**3GPP TSG-S4 Meeting # 127-bis-e S4-240xxx**

**Online, April 8th - 12th, 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **26.510** | **CR** |  | **rev** |  | **Current version:** | **1.1.4** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | pCR on Correction to Edge Resources | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Inc. | | | | | | | | | |
| ***Source to TSG:*** | S4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GMS\_Pro\_Ph2 | | | | |  | ***Date:*** | | | 2nd April 2024 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Correction to replace reference to non-existent activationTrigger | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.6.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First Change** |

#### 8.6.3.1 EdgeResourcesConfiguration resource type

Table 8.6.3.1-1: Definition of EdgeResourcesConfiguration resource type

| Property name | Type | Cardinality | Description |
| --- | --- | --- | --- |
| edgeResourcesConfigurationId | ResourceId | 1..1 | A resource identifier for this Edge Resources Configuration assigned by the Media AF when the resource is created that is unique within the scope of the enclosing Provisioning Session. |
| edgeManagementMode | Edge‌Management‌Mode | 1..1 | Indicates whether the management of edge resources is client-driven or AF-driven. (See clause 8.6.3.2.) |
| eligibilityCriteria | Edge‌Processing‌Eligibility‌Criteria‌ | 0..1 | Condition to activate edge resources for this Provisioning Session. If omitted, it shall be assumed that all media delivery sessions related to the parent Provisioning Session use edge resources. (See clause 7.3.3.10.) |
| easRequirements | EASRequirements | 1..1 | Requirements on the EAS Profile used by the Media AF or by the EEC to discover and select one or more Media EAS instances to serve media streaming sessions. (See clause 8.6.3.3.) |
| eas‌Relocation‌Requirements | M1EAS‌Relocation‌Requirements | 0..1 | EAS relocation tolerance and requirements.  If not present, the Media AF shall assume that the application is unaware of context transfer and that transfers to a target Media EAS are allowed. (See clause 8.6.3.4.) |