**3GPP TSG-SA5 Meeting #129e *S5-201217r1***

**e-meeting, 24 February – 4 March 2020**

**Source: Huawei**

**Title: Add requirements**

**Document for: Approval**

**Agenda Item: 7.4.3**

# 1 Decision/action requested

***In this box give a very clear / short /concise statement of what is wanted.***

# 2 References

3GPP TS 28.201

# 3 Rationale

This contribution is to provide some requirements for network slice performance and analytics charging.

# 4 Detailed proposal

|  |
| --- |
| ***First change*** |

### 5.1.2 Requirements

The following are high-level charging requirements specific to the network slice performance and analytics charging:

- The CSIF shall support subscription to specific network slice performance and analytics information.

- The CSIF shall support reporting charging information based on network slice performance and analytics information.

- The CSIF shall support reporting performance and analytics charging information per network slice.

- The CSIF shall support PEC scenario to report performance and analytics charging information.

- The CSIF shall support subscription to specific network slice performance and analytics information, this can be from NWDAF, using MnS or a combination. Editor’s note: The requirements are not complete.

|  |
| --- |
| **End of change** |