**3GPP TSG- Meeting # *rev1***

**20-28 April 2020, E-meeting** *Revision of S5-201183*

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **28.552** | **CR** | **0192** | **rev** | **2** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add measurements related to DL delay between PSA UPF and UE |
|  |  |
| ***Source to WG:*** | Intel, ETRI |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | 5G\_SLICE\_ePA |  | ***Date:*** | 2020-04-10 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The end to end UL delay in 5G networks between UE and PSA UPF has direct impact to users’ experience for some types of services (e.g., URLLC). In case the PSA UPF and NG-RAN are time synchronised, the UL delay between PSA UPF and UE can be measured at PSA UPF.The measurements on the UL delay between PSA UPF and NE can be used to evaluate the user plane delay performance in 5G networks and users’ experience.  |
|  |  |
| ***Summary of change:*** | Added measurements on UL one way packet delay between PSA UPF and NG-RAN. |
|  |  |
| ***Consequences if not approved:*** | The UL oacket delay between PSA UPF and NG-RAN cannot be monitored. |
|  |  |
| ***Clauses affected:*** | 5.4.x.y (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Implement the sub-clause 5.4.x.y of this CR to the clause 5.4.x of CR#0191.  |

|  |
| --- |
| **1st Modified Section** |

#### 5.4.x.y UL packet delay between PSA UPF and UE

##### 5.4.x.y.1 Average UL packet delay between PSA UPF and UE

a) This measurement provides the average UL packet delay between PSA UPF and UE. This measurement is split into subcounters per DSCP. This measurement is only applicable to the case the PSA UPF and NG-RAN are time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

 The UPF performs QoS monitoring per the request received from SMF during PDU Session Establishment or Modification procedure.

NOTE: The UPF may sample the GTP packets for QoS monitoring, the specific sampling rate is up to implementation.

For each received GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4] and 38.415 [31]):

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The UL Delay Result from UE to NG-RAN indicating the uplink delay measurement result which is the sum of the delay incurred in NG-RAN (including the delay at gNB-CU-UP, on F1-U and on gNB-DU) and the delay over Uu interface (see 38.415 [31], and the UL Delay Result is denoted by in the present document);

- The DSCP associated to the GTP PDU monitoring response packet.

 The PSA UPF counts the number (N) of GTP PDU monitoring response packets for each DSCP, and takes the following calculation for each DSCP:

d) Each measurement is a real representing the average delay in 0.1ms.

e) GTP.DelayUlPsaUpfUeMean.*DSCP,* where *DSCP* identifies the DSCP;

f) EP\_N3 (contained by UPFFunction);
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

##### 5.4.x.y.2 Distribution of UL packet delay between PSA UPF and UE

a) This measurement provides the distribution of UL packet delay between PSA UPF and UE. This measurement is split into subcounters per DSCP. This measurement is only applicable to the case the PSA UPF and NG-RAN are time synchronised.

b) DER (n=1).

c) The measurement is obtained by the following method:

 The UPF performs QoS monitoring per the request received from SMF during PDU Session Establishment or Modification procedure.

NOTE: The UPF may sample the GTP packets for QoS monitoring, the specific sampling rate is up to implementation.

 For each received GTP PDU monitoring response packet (packet i) for QoS monitoring, the PSA UPF records the following time stamps and information (see 23.501 [4] and 38.415 [31]):

- T3 received in the GTP-U header of the monitoring response packet indicating the local time that the monitoring response packet was sent by the NG-RAN;

- T4 that the monitoring response packet was received by the PSA UPF;

- The UL Delay Result from UE to NG-RAN indicating the uplink delay measurement result which is the sum of the delay incurred in NG-RAN (including the delay at gNB-CU-UP, on F1-U and on gNB-DU) and the delay over Uu interface (see 38.415 [31], and the UL Delay Result is denoted by in the present document);

- The DSCP associated to the GTP PDU monitoring response packet.

 The PSA UPF 1) takes the following calculation for each GTP PDU monitoring response packet (packet i) for each DSCP, and 2) increment the corresponding bin with the delay range where the result of 1) falls into by 1 for the subcounter per DSCP.

d) Each measurement is an integer representing the number of GTP PDUs measured with the delay within the range of the bin.

e) GTP.DelayUlPsaUpfUeDist.*DSCP.bin,* where *Bin* indicates a delay range which is vendor specific, and *DSCP* identifies the DSCP.

f) EP\_N3 (contained by UPFFunction);
EP\_N9 (contained by UPFFunction).

g) Valid for packet switched traffic.

h) 5GS.

|  |
| --- |
| **End of Modified Sections** |