3GPP TS 28.532 V16.6.0 (2020-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Management and orchestration;

Generic management services;

(Release 16)



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

Management and orchestration, Network Slicing, Provisioning

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 14

1 Scope 15

2 References 15

3 Definitions and abbreviations 17

3.1 Definitions 17

3.2 Abbreviations 17

4 Overview 17

5 Void 17

6 Void 17

7 Void 17

8 Void 17

9 Void 17

10 Void 18

11 Management services – Stage 2 18

11.1 Generic provisioning management service 18

11.1.1 Operations and notifications 18

11.1.1.1 createMOI operation 18

11.1.1.1.1 Description 18

11.1.1.1.2 Input parameters 18

11.1.1.1.3 Output parameters 18

11.1.1.1.4 Results 19

11.1.1.2 getMOIAttributes operation 20

11.1.1.2.1 Definition 20

11.1.1.2.2 Input Parameters 20

11.1.1.2.3 Output Parameters 21

11.1.1.2.4 Results 21

11.1.1.3 modifyMOIAttributes operation 21

11.1.1.3.1 Description 21

11.1.1.3.2 Input parameters 22

11.1.1.3.3 Output parameters 23

11.1.1.3.4 Results 23

11.1.1.4 deleteMOI operation 23

11.1.1.4.1 Description 23

11.1.1.4.2 Input parameters 23

11.1.1.4.3 Output parameters 24

11.1.1.4.4 Results 24

11.1.1.5 Void 24

11.1.1.6 Void 24

11.1.1.7 Notification notifyMOICreation 24

11.1.1.7.1 Definition 24

11.1.1.7.2 Input parameters 25

11.1.1.7.3 Triggering event 26

11.1.1.7.3.1 From-state 26

11.1.1.7.3.2 To-state 26

11.1.1.8 Notification notifyMOIDeletion 26

11.1.1.8.1 Definition 26

11.1.1.8.2 Input parameters 27

11.1.1.8.3 Triggering event 28

11.1.1.8.3.1 From-state 28

11.1.1.8.3.2 To-state 28

11.1.1.9 Notification notifyMOIAttributeValueChanges 28

11.1.1.9.1 Definition 28

11.1.1.9.2 Input parameters 29

11.1.1.9.3 Triggering event 30

11.1.1.9.3.1 From-state 30

11.1.1.9.3.2 To-state 30

11.1.1.10 Notification notifyEvent 30

11.1.1.10.1 Definition 30

11.1.1.10.2 Input parameters 30

11.1.1.11 Notification notifyMOIChanges 31

11.1.1.11.1 Definition 31

11.1.1.11.2 Input parameters 32

11.1.2 Managed Information 33

11.1.2.1 ManagedEntity 33

11.1.2.1.1 Definition 33

11.2 Generic fault supervision management service 33

11.2.1 Operations and notifications 33

11.2.1.1 Operation and notification of fault supervision data report management service 33

11.2.1.1.1 subscribe 33

11.2.1.1.1.1 Definition 33

11.2.1.1.1.2 Input parameters 33

11.2.1.1.1.3 Output parameters 34

11.2.1.1.1.4 Pre-condition 34

11.2.1.1.1.5 Post-condition 34

11.2.1.1.1.6 Exceptions 35

11.2.1.1.2 unsubscribe 35

11.2.1.1.2.1 Definition 35

11.2.1.1.2.2 Input parameters 35

11.2.1.1.2.3 Output parameters 35

11.2.1.1.2.4 Pre-condition 35

11.2.1.1.2.5 Post-condition 35

11.2.1.1.2.6 Exceptions 36

11.2.1.1.3 getAlarmList 36

11.2.1.1.3.1 Definition 36

11.2.1.1.3.2 Input parameters 37

11.2.1.1.3.3 Output parameters 38

11.2.1.1.3.4 Exceptions and constraints 40

11.2.1.1.4 notifyNewAlarm 40

11.2.1.1.4.1 Definition 40

11.2.1.1.4.2 Input parameters 40

11.2.1.1.4.2a Input parameters for notifications related to non-security alarms 42

11.2.1.1.4.3 Triggering event 42

11.2.1.1.4.3.1 From-state 42

11.2.1.1.4.3.2 To-state 43

11.2.1.1.5 notifyChangedAlarm 43

11.2.1.1.5.1 Definition 43

11.2.1.1.5.2 Input parameters 43

11.2.1.1.5.3 Triggering event 44

11.2.1.1.5.3.1 From-state 44

11.2.1.1.5.3.2 To-state 44

11.2.1.1.6 notifyAlarmListRebuilt 44

11.2.1.1.6.1 Definition 44

11.2.1.1.6.2 Input parameters 45

11.2.1.1.6.3 Triggering event 45

11.2.1.1.6.3.1 From-state 45

11.2.1.1.6.3.2 To-state 45

11.2.1.1.7 notifyCorrelatedNotificationChanged 46

11.2.1.1.7.1 Definition 46

11.2.1.1.7.2 Input parameters 46

11.2.1.1.7.3 Triggering event 46

11.2.1.1.7.3.1 From-state 46

11.2.1.1.7.3.2 To-state 46

11.2.1.1.8 getAlarmCount 46

11.2.1.1.8.1 Definition 46

11.2.1.1.8.2 Input parameters 47

11.2.1.1.8.3 Output parameters 47

11.2.1.1.8.4 Pre-condition 47

11.2.1.1.8.5 Post-condition 48

11.2.1.1.8.6 Exceptions 48

11.2.1.1.9 setComment 48

11.2.1.1.9.1 Definition 48

11.2.1.1.9.2 Input parameters 48

11.2.1.1.9.3 Output Parameters 48

11.2.1.2 Fault supervision data control management service 49

11.2.1.2.1 acknowledgeAlarms 49

11.2.1.2.1.1 Definition 49

11.2.1.2.1.2 Input parameters 49

11.2.1.2.1.3 Output parameters 49

11.2.1.2.1.4 Exceptions and constraints 50

11.2.1.2.2 unacknowledgeAlarms 50

11.2.1.2.2.1 Definition 50

11.2.1.2.2.2 Input parameters 50

11.2.1.2.2.3 Output parameters 51

11.2.1.2.2.4 Exceptions and constraints 51

11.2.1.2.3 clearAlarms 51

11.2.1.2.3.1 Definition 51

11.2.1.2.3.2 Input parameters 52

11.2.1.2.3.3 Output parameters 52

11.2.1.2.3.4 Exceptions and constraints 52

11.2.1.2.4 notifyClearedAlarm 52

11.2.1.2.4.1 Definition 52

11.2.1.2.4.2 Input parameters 53

11.2.1.2.4.3 Triggering event 53

11.2.1.2.4.3.1 From-state 53

11.2.1.2.4.3.2 To-state 53

11.2.1.2.5 notifyAckStateChanged 54

11.2.1.2.5.1 Definition 54

11.2.1.2.5.2 Input parameters 54

11.2.1.2.5.3 Triggering event 54

11.2.1.2.5.3.1 From-state 54

11.2.1.2.5.3.2 To-state 54

11.2.1.2.6 notifyComments 54

11.2.1.2.6.1 Definition 54

11.2.1.2.6.2 Input parameters 55

11.2.1.2.6.3 Trigger event 55

11.2.1.2.6.3.1 From-state 55

11.2.1.2.6.3.2 To-state 55

11.2.1.2.7 notifyPotentialFaultyAlarmList 55

11.2.1.2.7.1 Definition 55

11.2.1.2.7.2 Input parameters 56

11.2.1.2.7.3 Trigger event 56

11.2.1.2.7.3.1 From-state 56

11.2.1.2.7.3.2 To-state 56

11.2.1.2.8 notifyChangedAlarmGeneral 57

11.2.1.2.8.1 Definition 57

11.2.1.2.8.2 Input parameters for notifications related to non-security alarms 57

11.2.1.2.8.3 Input parameters for notifications related to security alarm 58

11.2.1.2.8.4 Trigger event 58

11.2.1.2.8.4.1 From-state 58

11.2.2 Managed information 59

11.2.2.1 Alarm information, alarm state change and Information Object Classes 59

11.2.2.1.1 Imported information entities and local labels 59

11.2.2.1.2 Class diagram 60

11.2.2.1.2.1 Introduction 60

11.2.2.1.2.2 Attributes and relationships 60

11.2.2.1.3 Information Object Class Definitions 60

11.2.2.1.3.1 AlarmInformation 60

11.2.2.1.3.1.1 Definition 60

11.2.2.1.3.1.2 Attribute 61

11.2.2.1.3.1.3 State diagram 61

11.2.2.1.3.2 AlarmList 63

11.2.2.1.3.2.1 Definition 63

11.2.2.1.3.2.2 Attribute 63

11.2.2.1.3.3 FSMnSProducer 64

11.2.2.1.3.3.1 Definition 64

11.2.2.1.3.3.2 Attribute 64

11.2.2.1.3.3.3 Notification Table 64

11.2.2.1.3.4 Comment 64

11.2.2.1.3.4.1 Definition 64

11.2.2.1.3.4.2 Attribute 64

11.2.2.1.3.5 CorrelatedNotification 64

11.2.2.1.3.5.1 Definition 64

11.2.2.1.3.5.2 Attribute 65

11.2.2.1.3.6 MonitoredEntity 65

11.2.2.1.3.6.1 Definition 65

11.2.2.1.3.6.2 Attribute 65

11.2.2.1.4 Information relationships definition 66

11.2.2.1.4.1 relation-FSMnSProducer-AlarmList (M) 66

11.2.2.1.4.1.1 Definition 66

11.2.2.1.4.1.2 Role 66

11.2.2.1.4.1.3 Constraint 66

11.2.2.1.4.2 relation-AlarmList-AlarmInformation (M) 66

11.2.2.1.4.2.1 Definition 66

11.2.2.1.4.2.2 Role 66

11.2.2.1.4.2.3 Constraint 66

11.2.2.1.4.3 relation-AlarmInformation-Comment (M) 66

11.2.2.1.4.3.1 Definition 66

11.2.2.1.4.3.2 Role 66

11.2.2.1.4.3.3 Constraint 66

11.2.2.1.4.4 relation-AlarmInformation-CorrelatedNotification (M) 66

11.2.2.1.4.4.1 Definition 66

11.2.2.1.4.4.2 Role 67

11.2.1.4.4.3 Constraint 67

11.2.2.1.4.5 relation-AlarmedObject-AlarmInformation (M) 67

11.2.2.1.4.5.1 Definition 67

11.2.2.1.4.5.2 Role 67

11.2.2.1.4.5.3 Constraint 67

11.2.2.1.4.6 relation-backUpObject-AlarmInformation (O) 67

11.2.2.1.4.6.1 Definition 67

11.2.2.1.4.6.2 Role 67

11.2.2.1.4.6.3 Constraint 67

11.2.2.1.5 Information attribute definition 68

11.2.2.1.5.1 Definition and legal values 68

11.2.2.1.5.2 Constraints 71

11.2.2.2 Subscription information, subscription state and Information Object Classes 71

11.2.2.2.1 Imported information entities and local labels 71

11.2.2.2.2 Class Diagram 71

11.2.2.2.2.1 Attributes and relationships 71

11.2.2.2.2.2 Inheritance 72

11.2.2.2.3 Information object classes definition 72

11.2.2.2.3.1 NtfSubscriber 72

11.2.2.2.3.1.1 Definition 72

11.2.2.2.3.1.2 Attributes 72

11.2.2.2.3.2 NtfSubscription 72

11.2.2.2.3.2.1 Definition 72

11.2.2.2.3.2.2 Attributes 72

11.2.2.2.3.2.3 Void 72

11.2.2.2.3.3 NotificationIRP 72

11.2.2.2.3.3.1 Definition 72

11.2.2.2.4 Information relationship definitions 73

11.2.2.2.4.1 relation-ntfSubscriber-ntfSubscription (M) 73

11.2.2.2.4.1.1 Definition 73

11.2.2.2.4.1.2 Roles 73

11.2.2.2.4.1.3 Constraints 73

11.2.2.2.4.2 relation-ntfIRP-ntfSubscriber (M) 73

11.2.2.2.4.2.1 Definition 73

11.2.2.2.4.2.2 Roles 73

11.2.2.2.4.2.3 Constraints 73

11.2.2.2.5 Information attribute definitions 74

11.2.2.2.5.0 Introduction 74

11.2.2.2.5.1 Definitions and legal values 74

11.2.2.2.5.2 Constraints 74

11.3 Generic performance assurance management service 74

11.3.1 Operations and notifications 74

11.3.1.1 Void 74

11.3.1.2 Operation and notification of performance threshold monitoring service 74

11.3.1.2.1 Notification notifyThresholdCrossing (M) 74

11.3.1.2.1.1 Definition 74

11.3.1.2.1.2 Notification information 75

11.3.2 Managed information 75

11.3.2.1 Performance data file definition 75

11.3.2.1.1 File generation and reporting 75

11.3.2.1.2 Performance data file content description 76

11.3.2.1.3 File naming convention 77

11.3.2.1.3.1 Generic file naming convention 77

11.3.2.1.3.2 Performance data file specific extension 78

11.3.2.1.4 Void 80

11.4 Heartbeat 80

11.4.1 Operations and notifications 80

11.4.1.1 Notification notifyHeartbeat 80

11.4.1.1.1 Definition 80

11.4.1.1.2 Input parameters 80

11.4.1.1.3 Triggering event 80

11.4.1.1.3.1 From-state 80

11.4.1.1.3.2 To-state 80

11.5 Streaming data reporting service 81

11.5.1 Operations and notifications 81

11.5.1.1 establishStreamingConnection operation (M) 81

11.5.1.1.1 Definition 81

11.5.1.1.2 Input parameters 82

11.5.1.1.3 Output parameters 82

11.5.1.1.4 Exceptions 83

11.5.1.2 terminateStreamingConnection operation (M) 83

11.5.1.2.1 Definition 83

11.5.1.2.2 Input parameters 83

11.5.1.2.3 Output parameters 83

11.5.1.2.4 Exceptions 83

11.5.1.3 reportStreamData operation (M) 83

11.5.1.3.1 Definition 83

11.5.1.3.2 Input parameters 84

11.5.1.3.3 Output parameters 84

11.5.1.3.4 Exceptions 84

11.5.1.4 addStream operation (M) 84

11.5.1.4.1 Definition 84

11.5.1.4.2 Input parameters 85

11.5.1.4.3 Output parameters 86

11.5.1.4.4 Exceptions 86

11.5.1.5 deleteStream operation (M) 87

11.5.1.5.1 Definition 87

11.5.1.5.2 Input parameters 87

11.5.1.5.3 Output parameters 87

11.5.1.5.4 Exceptions 87

11.5.1.6 getConnectionInfo operation (M) 87

11.5.1.6.1 Definition 87

11.5.1.6.2 Input parameters 87

11.5.1.6.3 Output parameters 88

11.5.1.6.4 Exceptions 88

11.5.1.7 getStreamInfo operation (M) 88

11.5.1.7.1 Definition 88

11.5.1.7.2 Input parameters 89

11.5.1.7.3 Output parameters 90

11.5.1.7.4 Exceptions 91

11.6 File data reporting service 91

11.6.1 Operations and notifications 91

11.6.1.1 Notification notifyFileReady (M) 91

11.6.1.1.1 Definition 91

11.6.1.1.2 Notification information 92

11.6.1.2 Notification notifyFilePreparationError (M) 93

11.6.1.2.1 Definition 93

11.6.1.2.2 Notification information 93

11.6.1.3 Operation subscribe (M) 94

11.6.1.3.1 Definition 94

11.6.1.3.2 Input parameters 94

11.6.1.3.3 Output parameters 94

11.6.1.3.4 Exceptions 94

11.6.1.4 Operation unsubscribe (M) 94

11.6.1.4.1 Definition 94

11.6.1.4.2 Input parameters 95

11.6.1.4.3 Output parameters 95

11.6.1.4.4 Exceptions 95

11.6.1.5 Operation listAvailableFiles (M) 95

11.6.1.5.1 Definition 95

11.6.1.5.2 Input parameters 96

11.6.1.5.3 Output parameters 96

11.6.1.5.4 Exceptions 96

12 Management services – Stage 3 96

12.1 Generic provisioning management service 96

12.1.1 RESTful HTTP-based solution set 96

12.1.1.1 Mapping of operations 96

12.1.1.1.1 Introduction 96

12.1.1.1.2 Operation "createMOI" 97

12.1.1.1.3 Operation "getMOIAttributes" 97

12.1.1.1.4 Operation "modifyMOIAttributes" 98

12.1.1.1.4.1 Mapping to HTTP PUT 98

12.1.1.1.4.2 Mapping to HTTP PATCH 99

12.1.1.1.5 Operation "deleteMOI" 100

12.1.1.1.6 Void 101

12.1.1.1.7 Void 101

12.1.1.2 Mapping of notifications 101

12.1.1.2.1 Introduction 101

12.1.1.2.2 Notification "notifyMOICreation" 101

12.1.1.2.3 Notification "notifyMOIDeletion" 101

12.1.1.2.4 Notification "notifyMOIAttributeValueChanges" 102

12.1.1.2.5 Notification "notifyMOIChanges" 102

12.1.1.3 Resources 102

12.1.1.3.1 Resource structure 102

12.1.1.3.1.1 Resource structure on the MnS consumer 103

12.1.1.3.2 Resource definitions 103

12.1.1.3.2.1 Resource "…/{className}={id}" 103

12.1.1.3.2.1.1 Description 103

12.1.1.3.2.1.2 URI 103

12.1.1.3.2.1.3 HTTP methods 104

12.1.1.3.2.2 Void 106

12.1.1.3.2.3 Void 106

12.1.1.3.2.4 Resource "{notificationTarget}" 106

12.1.1.3.2.4.1 Description 106

12.1.1.3.2.4.2 URI 106

12.1.1.3.2.4.3 HTTP methods 106

12.1.1.4 Data type definitions 107

12.1.1.4.1 General 107

12.1.1.4.1a Structured data types 109

12.1.1.4.1a.1 Type Resource 109

12.1.1.4.1a.2 Type Scope 109

12.1.1.4.1a.3 Type CorrelatedNotification 109

12.1.1.4.1a.4 Type MoiChange 110

12.1.1.4.1a.5 Type NotifyMoiCreation 111

12.1.1.4.1a.6 Type NotifyMoiDeletion 112

12.1.1.4.1a.7 Type NotifyMoiAttributeValueChanges 112

12.1.1.4.1a.8 Type NotifyMoiChanges 112

12.1.1.4.2 Void 112

12.1.1.4.3 Void 113

12.1.1.4.4 Simple data types and enumerations 113

12.1.1.4.4.6 Enumeration Operation 114

12.1.2 RESTful HTTP-based solution set for integration with ONAP VES API 114

12.1.2.1 Mapping of operations 114

12.1.2.2 Mapping of notifications 114

12.1.2.2.1 Introduction 114

12.1.2.2.1.1 General 114

12.1.2.2.1.2 Void 114

12.1.2.2.2 Notification notifyMOICreation 114

12.1.2.2.3 Notification notifyMOIDeletion 115

12.1.2.2.4 Notification notifyMOIAttributeValueChange 115

12.1.2.2.5 Notification notifyMOIChanges 115

12.1.2.3 Resources 115

12.1.2.3.1 Resource structure 115

12.1.2.3.2 Resource definitions 115

12.1.2.4 Data type definitions 115

12.1.3 YANG/Netconf-based solution set 116

12.1.3.1 Mapping of operations 116

12.1.3.1.1 Introduction 116

12.1.3.1.2 Operation createMOI 116

12.1.3.1.3 Operation getMOIAttributes 117

12.1.3.1.4 Operation modifyMOIAttributes 119

12.1.3.1.5 Operation deleteMOI 120

12.2 Generic fault supervision management service 121

12.2.1 RESTful HTTP-based solution set 121

12.2.1.1 Mapping of operations 121

12.2.1.1.1 Introduction 121

12.2.1.1.2 Operation getAlarmList 121

12.2.1.1.3 Operation getAlarmCount 122

12.2.1.1.4 Operation setComment 122

12.2.1.1.5 Operation acknowledgeAlarms 123

12.2.1.1.6 Operation unacknowledgeAlarms 125

12.2.1.1.7 Operation clearAlarms 126

12.2.1.1.8 Operation subscribe 127

12.2.1.1.9 Operation unsubscribe 128

12.2.1.2 Mapping of notifications 129

12.2.1.2.1 Introduction 129

12.2.1.2.2 Notification notifyNewAlarm (non-security alarm) 129

12.2.1.2.3 Notification notifyNewAlarm (security alarm) 130

12.2.1.2.4 Notification notifyAckStateChanged 130

12.2.1.2.5 Notification notifyClearedAlarm 131

12.2.1.2.6 Notification notifyAlarmListRebuilt 131

12.2.1.2.7 Notification notifyChangedAlarm 131

12.2.1.2.8 Notification notifyComments 132

12.2.1.2.9 Notification notifyPotentialFaultyAlarmList 132

12.2.1.2.10 Notification notifyCorrelatedNotificationChanged 132

12.2.1.2.11 Notification notifyChangedAlarmGeneral (non-security alarm) 133

12.2.1.2.12 Notification notifyChangedAlarmGeneral (security alarm) 133

12.2.1.3 Resources 134

12.2.1.3.1 Resource structure 134

12.2.1.3.1.2 Resource structure on the MnS consumer 134

12.2.1.3.2 Resource definitions 135

12.2.1.3.2.1 Resource "…/alarms" 135

12.2.1.3.2.1.1 Description 135

12.2.1.3.2.1.2 URI 135

12.2.1.3.2.1.3 HTTP methods 135

12.2.1.3.2.2 Resource "…/alarms /{alarmId}" 136

12.2.1.3.2.2.1 Description 136

12.2.1.3.2.2.2 URI 136

12.2.1.3.2.2.3 HTTP methods 136

12.2.1.3.2.3 Resource "…/alarms/alarmCount" 137

12.2.1.3.2.3.1 Definition 137

12.2.1.3.2.3.2 URI 137

12.2.1.3.2.3.3 HTTP methods 137

12.2.1.3.2.4 Resource "…/alarms/{alarmId}/comments" 138

12.2.1.3.2.4.1 Definition 138

12.2.1.3.2.4.2 URI 138

12.2.1.3.2.4.3 HTTP methods 138

12.2.1.3.2.5 Resource "…/comments/{commentId}" 139

12.2.1.3.2.5.1 Definition 139

12.2.1.3.2.5.2 URI 139

12.2.1.3.2.5.3 HTTP methods 139

12.2.1.3.2.6 Resource "…/subscriptions" 139

12.2.1.3.2.6.1 Description 139

12.2.1.3.2.6.2 URI 139

12.2.1.3.2.6.3 HTTP methods 139

12.2.1.3.2.7 Resource "…/subscriptions/{subscriptionId}" 140

12.2.1.3.2.7.1 Description 140

12.2.1.3.2.7.2 URI 140

12.2.1.3.2.7.3 HTTP methods 140

12.2.1.3.2.8 Resource "{notificationTarget}" 141

12.2.1.3.2.8.1 Description 141

12.2.1.3.2.8.2 URI 141

12.2.1.3.2.8.3 HTTP methods 141

12.2.1.4 Data type definitions 142

12.2.1.4.1 General 142

12.2.1.4.1a Structured data types 144

12.2.1.4.1a.1 Type ThresholdHysteresis 144

12.2.1.4.1a.2 Type ThresholdLevelInd 144

12.2.1.4.1a.3 Type ThresholdInfo 145

12.2.1.4.1a.4 Type CorrelatedNotification 145

12.2.1.4.1a.5 Type AlarmRecord 146

12.2.1.4.1a.6 Type AlarmCount 147

12.2.1.4.1a.7 Type Comment 147

12.2.1.4.1a.8 Type Subscription 148

12.2.1.4.1a.9 Type MergePatchAcknowledgeAlarm 148

12.2.1.4.1a.10 Type MergePatchClearAlarm 148

12.2.1.4.1a.11 Type FailedAlarm 148

12.2.1.4.1a.12 Type NotifyNewAlarm 149

12.2.1.4.1a.13 Type NotifyNewSecAlarm 150

12.2.1.4.1a.14 Type NotifyClearedAlarm 151

12.2.1.4.1a.15 Type NotifyChangedAlarm 151

12.2.1.4.1a.16 Type NotifyChangedAlarmGeneral 152

12.2.1.4.1a.17 Type NotifyChangedSecAlarmGeneral 153

12.2.1.4.1a.18 Type NotifyCorrelatedNotificationChanged 153

12.2.1.4.1a.19 Type NotifyAckStateChanged 154

12.2.1.4.1a.20 Type NotifyComments 154

12.2.1.4.1a.21 Type NotifyPotentialFaultyAlarmList 154

12.2.1.4.1a.22 Type NotifyAlarmListRebuilt 155

12.2.1.4.2 Void 155

12.2.1.4.3 Void 155

12.2.1.4.4 Simple data types and enumerations 155

12.2.1.4.4.1 General 155

12.2.1.4.4.2 Simple data types 155

12.2.1.4.4.3 Enumeration AlarmAckState 155

12.2.1.4.4.4 Enumeration AckState 156

12.2.1.4.4.5 Enumeration AlarmListAlignmentRequirement 156

12.2.1.4.4.6 Enumeration AlarmType 156

12.2.1.4.4.7 Enumeration ProbableCause 157

12.2.1.4.4.8 Enumeration AlarmNotificationTypes 157

12.2.1.4.4.9 Enumeration PerceivedSeverity 157

12.2.1.4.4.10 Enumeration TrendIndication 158

12.2.2 RESTful HTTP-based solution set for integration with ONAP VES API 158

12.2.2.1 Mapping of operations 158

12.2.2.2 Mapping of notifications 158

12.2.2.2.1 Introduction 158

12.2.2.2.1.1 General 158

12.2.2.2.1.2 Void 158

12.2.2.2.2 Notification notifyNewAlarm (non-security alarm) 158

12.2.2.2.3 Notification notifyNewAlarm (security alarm) 158

12.2.2.2.4 Notification notifyAckStateChanged 158

12.2.2.2.5 Notification notifyClearedAlarm 158

12.2.2.2.6 Notification notifyAlarmListRebuilt 159

12.2.2.2.7 Notification notifyChangedAlarm 159

12.2.2.2.8 Notification notifyComments 159

12.2.2.2.9 Notification notifyPotentialFaultyAlarmList 159

12.2.2.2.10 Notification notifyCorrelatedNotificationChanged 159

12.2.2.2.11 Notification notifyChangedAlarmGeneral (non-security alarm) 159

12.2.2.2.12 Notification notifyChangedAlarmGeneral (security alarm) 159

12.2.2.3 Resources 159

12.2.2.3.1 Resource structure 159

12.2.2.3.2 Resource definitions 160

12.2.2.4 Data type definitions 160

12.3 Generic performance assurance management service 160

12.3.1 RESTful HTTP-based solution set 160

12.3.1.1 Void 160

12.3.1.2 Performance threshold monitoring service 160

12.3.1.2.1 Mapping of operations 160

12.3.1.2.2 Mapping of notifications 160

12.3.1.2.2.1 Introduction 160

12.3.1.2.2.2 Notification "notifyThresholdCrossing" 160

12.3.1.2.3 Resources 161

12.3.1.2.3.1 Resource structure 161

12.3.1.2.3.2 Resource definitions 161

12.3.1.2.3.2.1 Resource "/notificationSink" 161

12.3.1.2.4 Data type definitions 162

12.3.1.2.4.1 General 162

12.3.1.2.4.2 Structured data types 163

12.3.1.2.4.2.1 Type NotifyThresholdCrossing 163

12.3.1.2.4.4 Void 163

12.3.1.2.4.5 Void 163

12.3.1.2.4.6 Simple data types and enumerations 163

12.3.1.2.4.6.1 General 163

12.3.1.2.4.6.2 Simple data types 163

12.3.1.2.4.6.3 Enumeration PerfNotificationTypes 164

12.3.1.2.4.6.4 Enumeration PerfMetricDirection 164

12.3.2 XML file format definition 164

12.3.2.1 Introduction 164

12.3.2.2 Mapping table 164

12.3.2.3 XML schema 165

11.3.2.3.1 Performance data file XML schema 165

12.3.2.3.2 Performance data file XML header 167

12.4 Heartbeat 167

12.4.1 RESTful HTTP-based solution set 167

12.4.1.1 Mapping of operations 167

12.4.1.2 Mapping of notifications 167

12.4.1.2.1 Introduction 167

12.4.1.2.2 Notification "notifyHeartbeat" 168

12.4.1.3 Usage of HTTP 168

12.4.1.4 Resources 168

12.4.1.5 Data type definitions 168

12.4.1.5.1 General 168

12.4.1.5.2 Structured data types 168

12.4.1.5.3 Simple data types and enumerations 169

12.4.1.5.3.1 General 169

12.4.1.5.3.2 Simple data types 169

12.4.1.5.3.3 Enumeration HeartbeatNotificationTypes 169

12.4.2 RESTful HTTP-based solution set for integration with ONAP VES API 169

12.4.2.1 Mapping of operations 169

12.4.2.2 Mapping of notifications 169

12.4.2.2.1 Introduction 169

12.4.2.2.1.1 General 169

12.4.2.2.1.2 Notification parameter mapping principles 169

12.4.2.2.2 Notification notifyHeartbeat 169

12.5 Streaming data reporting service 170

12.5.1 RESTful HTTP-based solution set 170

12.5.1.1 Mapping of operations 170

12.5.1.1.1 Introduction 170

12.5.1.1.2 Operation "establishStreamingConnection" 170

12.5.1.1.3 Operation "terminateStreamingConnection" 173

12.5.1.1.4 Operation "reportStreamData" 173

12.5.1.1.5 Operation "addStream" 174

12.5.1.1.6 Operation "deleteStream" 174

12.5.1.1.7 Operation "getConnectionInfo" 175

12.5.1.1.8 Operation "getStreamInfo" 175

12.5.1.2 Mapping of notifications 176

12.5.1.3 Resources 176

12.5.1.3.1 Resources structure 176

12.5.1.3.2 Resources definitions 176

12.5.1.4 Data type definitions 183

12.5.1.4.1 General 183

12.5.1.4.2 Query, message body and resource data types 184

12.5.1.4.3 Simple data types and enumerations 185

12.6 File data reporting service 186

12.6.1 RESTful HTTP-based solution set 186

12.6.1.1 Mapping of operations 186

12.6.1.1.1 Introduction 186

12.6.1.1.2 Operation "listAvailableFiles" 186

12.6.1.1.3 Operation "subscribe" 187

12.6.1.1.4 Operation "unsubscribe" 187

12.6.1.2 Mapping of notifications 187

12.6.1.2.1 Introduction 187

12.6.1.2.2 Notification "notifyFileReady" 187

12.6.1.2.3 Notification "notifyFilePreparationError" 187

12.6.1.3 Resources 188

12.6.1.3.1 Resource structure 188

12.6.1.3.2 Resource definitions 188

12.6.1.4 Data type definitions 192

12.6.1.4.1 General 192

12.6.1.4.2 Structured general data types 193

12.6.1.4.3 Structured path data types 193

12.6.1.4.4 Query, message body and resource data types 193

12.6.1.4.5 Referenced structured data types 195

12.6.1.4.6 Simple data types and enumerations 195

Annex A (normative): OpenAPI specification 197

A.0 Introduction 197

A.1 Provisioning management service 197

A.1.0 Introduction 197

A.1.1 OpenAPI document "provMnS.yaml" 197

A.1.2 Integration with ONAP VES 203

A.2 Generic fault supervision management service 204

A.2.0 Introduction 204

A.2.1 OpenAPI document "faultMnS.yaml" 204

A.2.2 Integration with ONAP VES 217

A.3 Void 218

A.4 Generic performance assurance management service 218

A.4.1 Void 218

A.4.2 OpenAPI document "perfMnS.yaml" 218

A.4.3 Integration with ONAP VES 219

A.5 Heartbeat 219

A.5.0 Introduction 219

A.5.1 OpenAPI document "heartbeatNtf.yaml" 219

A.5.2 Integration with ONAP VES 219

A.6 Streaming data reporting management service 220

A.6.1 Introduction 220

A.6.2 OpenAPI document "streamingDataMnS.yaml" 220

A.7 File data reporting management service 226

A.7.1 Introduction 226

A.7.2 OpenAPI document "FileDataReportingMnS.yaml" 226

A.7.3 Integration with ONAP VES 230

Annex B (Informative): Guidelines for the integration of 3GPP MnS notifications with ONAP VES 231

Annex C (informative): Change history 232

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the stage 2 and stage 3 of generic management services for mobile network.

# 2 References

- The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 28.526: "Telecommunication management; Life Cycle Management (LCM) for mobile networks that include virtualized network functions; Procedures".

[3] 3GPP TS 28.541: "Management and orchestration ; 5G Network Resource Model (NRM); Stage 2 and stage3".

[4] ITU-T Recommendation X.733 (02/92): "Information technology - Open Systems Interconnection - Systems Management: Alarm reporting function".

[5] 3GPP TS 28.531: "Management and orchestration ; Provisioning; ".

[6] 3GPP TS 28.554: "Management and orchestration ; 5G end to end Key Performance Indicators (KPI)".

[7] 3GPP TS 22.261: "Technical Specification Group Services and System Aspects; Service requirements for the 5G system; Stage 1".

[8] 3GPP TS 23.501: "Technical Specification Group Services and System Aspects; System Architecture for the 5G System; Stage 2".

[9] 3GPP TS 23.003: "Technical Specification Group Core Network and Terminals; Numbering, addressing and identification".

[10] ETSI GS NFV-IFA 013 V2.4.1 (2018-02) "Network Function Virtualization (NFV); Management and Orchestration; Os-Ma-nfvo Reference Point - Interface and Information Model Specification".

[11] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[12] ETSI GS NFV-IFA 015 (V2.4.1): "Network Function Virtualisation (NFV); Management and Orchestration; Report on NFV Information Model".

[13] 3GPP TS 28.533: "Management and orchestration; Architecture framework"

[14] ITU-T Recommendation X.734 (1992): "Information technology - Open Systems Interconnection - Systems management: Event report management function".

[15] 3GPP TS 32.158: "Management and orchestration; Design rules for REpresentational State Transfer (REST) Solution Sets (SS)".

[16] 3GPP TS 32.302: "Telecommunication management; Configuration Management (CM); Notification Integration Reference Point (IRP); Information Service (IS)".

[17] 3GPP TS 32.401: "Telecommunication management; Performance Management (PM); Concept and requirements".

[18] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[19] 3GPP TS 32.401: "Telecommunication management; Perfomance Measurement (PM); Concept and requirements".

[20] ISO 8601:2004: "Data elements and interchange formats – Information interchange – Representation of dates and times".

[21] Void.

[22] Void.

[23] Void.

[24] Void.

[25] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects ".

[26] W3C REC-xmlschema-0-20010502: "XML Schema Part 0: Primer".

[27] W3C REC-xmlschema-1-20010502: "XML Schema Part 1: Structures".

[28] W3C REC-xmlschema-2-20010502: "XML Schema Part 2: Datatypes".

[29] W3C REC-xml-names-19990114: "Namespaces in XML".

[30] Void.

[31] 3GPP TS 32.111-2: " Telecommunication management; Fault Management; Part 2: Alarm Integration Reference Point (IRP): Information Service (IS)".

[32] IETF RFC 6241 "Network Configuration Protocol (NETCONF)".

[33] 3GPP TS 32.160 " Management and orchestration; Management service template ".

[34] IETF RFC 7950 "The YANG 1.1 Data Modeling Language".

[35] OpenAPI: "OpenAPI 3.0.1 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.1.md>.

[36] IETF RFC 6902: "JavaScript Object Notation (JSON) Patch".

[37] IETF RFC 7396: "JSON Merge Patch".

[38] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[39] 3GPP TS 32.423: "Telecommunication management; Subscriber and equipment trace; Trace data definition and management".

[40] IETF RFC 6455: "The WebSocket Protocol".

[41] IETF RFC 793: "Transmission Control Protocol".

[42] 3GPP TS 28.550: "Management and orchestration; Performance assurance".

[43] ITU-T Recommendation X.733 (02/92): "Information technology - Open Systems Interconnection - Systems Management: Alarm reporting function".

[44] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[45] Text Attribution: Creator: ONAP, under Creative Commons Attribution 4.0 International License, https://creativecommons.org/licenses/by/4.0/, URI to access the text: <https://github.com/onap/vnfrqts-requirements/blob/05f26fac2b941513a7d0e856b99fd8c61d688299/docs/Chapter8/ves7_1spec.rst#resource-structure>.

[46] 3GPP SA5 FORGE OpenAPI definitions: <https://forge.3gpp.org/rep/sa5/MnS/tree/Rel-16/OpenAPI>.

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**Matching-Criteria-Attributes:** See its definition in [31].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

FS Fault Supervision

MnS Management Service

# 4 Overview

The generic management services concept follows the management service concepts as defined in TS 28.533 [13].

# 5 Void

# 6 Void

# 7 Void

# 8 Void

# 9 Void

# 10 Void

# 11 Management services – Stage 2

## 11.1 Generic provisioning management service

### 11.1.1 Operations and notifications

#### 11.1.1.1 createMOI operation

##### 11.1.1.1.1 Description

This operation is invoked by Generic Provisioning MnS consumer to request the Generic Provisioning MnS producer to create a Managed Object instance in the MIB maintained by Generic Provisioning MnS producer. This operation will create only one Managed Object instance.

The Generic Provisioning MnS consumer supplies the values of all attributes that are supported, i.e. a) attributes whose Support Qualifier is M and b) attributes whose Support Qualifier is O. The special cases are:

1) If the attribute has a default value specified. In such case, if the Generic Provisioning MnS consumer supplies a value, the supplied value is used; otherwise, the default value is used.

2) If the attribute is specified as capable of carrying a null value or carrying no information. In such case, if the Generic Provisioning MnS consumer supplies a (non-null) value, the supplied value is used; otherwise, the null value is used.

3) If the attribute does not have a default value specified and is specified as incapable of carrying null value and incapable of carrying no information, if there is a Generic Provisioning MnS producer defined default value, then that value will be used.

##### 11.1.1.1.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| managedObjectClass | M | class | This parameter specifies the class of the new managed object instance. |
| managedObjectInstance | M | DN | This parameter specifies the instance of the managed object that is to be created and registered. This is a full DN according to 3GPP TS 32.300 [5]. |
| attributeListIn | M | LIST OF SEQUENCE< attribute name, attribute value> | This parameter may have a null value. When this parameter is supplied, it contains a list of name/value pairs specifying attribute identifiers and their values to be assigned to the new managed object. These values override the values for the corresponding attributes derived from the default value set specified in the definition of the managed object's class. |

##### 11.1.1.1.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| attributeListOut | M | LIST OF SEQUENCE< attribute name, attribute value> | This list of name/value pairs contains the attributes of the new managed object and the actual value assigned to each. |
| status | M | ENUM (OperationSucceeded, OperationFailed) |  |

##### 11.1.1.1.4 Results

In case of success, the ManagedEntity instance has been created with the supplied DN. In case of failure, indication of the failure is provided in the Output parameters.

#### 11.1.1.2 getMOIAttributes operation

##### 11.1.1.2.1 Definition

This operation is invoked by Generic Provisioning MnS consumer to request the retrieval of management information (Managed Object attribute names and values) from the MIB maintained by Generic Provisioning MnS producer. One or several Managed Objects may be retrieved - based on the containment hierarchy.

A SS may choose to split this operation in several operations (e.g. operations to get "handlers" or "iterators" to Managed Objects fulfilling the scope/filter criteria and other operations to retrieve attribute names/values from these "handlers").

##### 11.1.1.2.2 Input Parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Qualifier | Information Type | Comment |
| baseObjectInstance | M | DN | This parameter specifies the base object instance.  If the "scope" parameter is absent, then either only the base object or the complete subtree below and including the base object shall be selected. The default behaviour is protocol specific. |
| scope | M | n/a | This parameter specifies the scope. It is a structured parameter and consists of the sub-parameters "scopeType" and "scopeLevel". The scope describes which object instances are selected with respect to a base object instance. The base object instance needs to be specified using a dedicated attribute. |
| > scopeType | M | ENUM {  BASE\_ONLY,  BASE\_ALL  } | If the optional "scopeLevel" parameter is not supported or absent, allowed values of "scopeType" are "BASE\_ONLY" and "BASE\_ALL".  The value "BASE\_ONLY" indicates only the base object is selected.  The value "BASE\_ALL" indicates the base object and all of its subordinate objects (incl. the leaf objects) are selected.  This parameter is redundant and can be omitted when confirming only the protocol specific default behaviour. |
|  |  | ENUM {  BASE\_NTH\_LEVEL,  BASE\_SUBTREE  } | If the "scopeLevel" parameter is supported and present, allowed values of "scopeType" are "BASE\_NTH\_LEVEL" and "BASE\_SUBTREE".  The value "BASE\_NTH\_LEVEL" indicates all objects on the level, which is specified by the "scopeLevel" parameter, below the base object are selected. The base object is at "scopeLevel" zero.  The value "BASE\_SUBTREE" indicates the base object and all of its subordinate objects down to and including the objects on the level, which is specified by the "scopeLevel" parameter, are selected. The base object is at "scopeLevel" zero. |
| > scopeLevel | O | Integer | See definition of "scopeType" parameter. |
| filter | O | See Comment. | This parameter defines filter criteria to be applied to the objects selected by the "baseObjectInstance", "scope" and "scopeLevel" parameters.  The actual syntax and capabilities of the filter is SS specific. However, each SS should support a filter consisting of one or several assertions that may be grouped using the logical operators AND, OR and NOT.  Each assertion is a logical expression of attribute existence, attribute value comparison ("equal to X, less than Y" etc.) and MO Class. |
| attributeListIn | O | LIST OF attribute name. | This parameter identifies the attributes to be returned by this operation. If the parmeter is absent or empty all attributes shall be returned. |

##### 11.1.1.2.3 Output Parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Qualifier | Matching Information | Comment |
| managedObjectClass | M | ManagedEntity class | For each returned MO: The class of the MO. |
| managedObjectInstance | M | ManagedEntity DN | For each returned MO: The name of the MO. This is a full DN according to 3GPP TS 32.300 [5]. |
| attributeListOut | M | LIST OF SEQUENCE< attribute name, attribute value > | For each returned MO: A list of name/value pairs for MO. |
| status | M | ENUM (OperationSucceeded, OperationFailed) | An operation may fail because of a specified or unspecified reason. |

##### 11.1.1.2.4 Results

In case of success, all of the ManagedEntity instances selected for retrieval are returned. In case of failure, a specified or unspecified reason may be provided in the Output parameters.

#### 11.1.1.3 modifyMOIAttributes operation

##### 11.1.1.3.1 Description

This service operation is invoked by Generic Provisioning MnS consumer to request the modification of one or more Managed Object instances from Generic Provisioning MnS producer. Attributes of one or several Managed Objects may be modified.

##### 11.1.1.3.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| baseObjectInstance | M | DN | The MO instance that is to be used as the starting point for the selection of managed objects to which the filter (when supplied) is to be applied. This is a full DN according to 3GPP TS 32.300 [5]. |
| scopeType | M | See corresponding parameter in getMOIAttributes. | See corresponding parameter in getMOIAttributes. |
| scopeLevel | O | See corresponding parameter in getMOIAttributes. | See corresponding parameter in getMOIAttributes. |
| filter | O | See comment. | See corresponding parameter in getMOIAttributes. |
| modificationList | M | LIST OF SEQUENCE <attribute identifier, [attribute values], ENUM( replace, add values, remove values, set to default)>  See Comment for when attribute values are require and when they are optional. | This parameter contains a set of attribute modification specifications, each of which contains:  1). attribute identifier: the identifier of the attribute whose value(s) is (are) to be modified.  2). attribute value: the value(s) to be used in the modification of the attribute. The use of this parameter is defined by the modify operator. This parameter is optional when the set to default modify operator is specified and if supplied, shall be ignored.  3). modify operator: the way in which the attribute values(s) (if supplied) is(are) to be applied to the attribute. The possible operators are:  a) replace: the attribute value(s) specified shall be used to replace the current values(s) of the attribute;  b) add values: the attribute values(s) specified shall be added to the current value(s) of the attribute. This operator shall only be applied to a set-valued attribute and shall perform a set union (in the mathematical sense) between the current values(s) of the attribute and the attribute value(s) specified. Value(s) specified in the attribute value parameter which is(are) already in the current values of the attribute shall not cause an error to be returned.  c) remove values: the attribute value(s) specified shall be removed from the current values(s) of the attribute. This operator shall only be applied to a set-valued attribute and shall perform a set difference (in the mathematical sense) between the current value(s) of the attribute and the attribute values(s) specified. Value(s) specified in the attribute value parameter which is(are) not in the current value(s) of the attribute shall not cause an error to be returned;    d) set to default: when this operator is applied to a single-valued attribute, the value of the attribute shall be set to its default value. When this operator is applied to a set–valued attribute, the value(s) of the attribute shall be set to their default value(s) and only as many values as defined by the default shall be assigned. If there is no default value defined, an error shall be returned.  Note: Set is used here in the mathematical sense so that a set-valued attribute is an unordered set of unique values.  The modify operator is optional, and if it is not specified, the replace operator shall be assumed.  The modificationList parameter contains a single set of attribute modification specifications and this same set is applied to each MO instance to be modified. |

##### 11.1.1.3.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| modificationListOut | M | LIST OF SEQUENCE< ManagedEntity DN, ManagedEntity class, LIST OF SEQUENCE< attribute name, attribute value >> | This parameter will provide for each managed object instance the full DN of the managed object instance, the managedObjectClass, and a list of name/value pairs with the values of all the attributes of the modified managed object instance after modification. The form of this information is SS dependant and may be provided in one or many data structures. |
| status | M | ENUM (OperationSucceeded, OperationFailed, OperationPartiallySucceeded) | An operation may fail because of a specified or unspecified reason and no attributes have been updated. The operation is only successful if all specified attributes of all selected objects are actually modified. Otherwise, the operation is partially successful. |

In lieu of a synchronization parameter, best effort synchronization will apply; that is, all managed objects selected for this operation will perform the operation if possible regardless of whether some managed objects fail to perform it.

##### 11.1.1.3.4 Results

In case of success, all of the ManagedEntity instances selected for modification are modified. In case of failure, a specified or unspecified reason may be provided in the Output parameters.

#### 11.1.1.4 deleteMOI operation

##### 11.1.1.4.1 Description

This service operation is invoked by Generic Provisioning MnS consumer to request the deletion of one or more Managed Object instances in the MIB maintained by the Generic Provisioning MnS producer.

##### 11.1.1.4.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| baseObjectInstance | M | DN | The MO instance that is to be used as the starting point for the selection of managed objects to which the filter (when supplied) is to be applied. This is a full DN according to 3GPP TS 32.300 [5]. |
| scopeType | O | See corresponding parameter in getMOIAttributes. | See corresponding parameter in getMOIAttributes. |
| scopeLevel | O | See corresponding parameter in getMOIAttributes. | See corresponding parameter in getMOIAttributes. |
| filter | O | See comment. | See corresponding parameter in getMOIAttributes. |

##### 11.1.1.4.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter name | Support Qualifier | Matching Information / Legal Values | Comment |
| deletionList | M | LIST OF SEQUENCE< ManagedEntity DN, ManagedEntity class name> | If the base object alone is specified, then this parameter is optional; otherwise it contains a list of managedObjectInstance/managedObjectClass pairs identifying the managed objects deleted. |
| status | M | ENUM (OperationSucceeded, OperationFailed, OperationPartiallySucceeded) | An operation may fail because of a specified or unspecified reason. The operation is partially successful if some, but not all, objects selected to be deleted are actually deleted. |

In lieu of a synchronization parameter, best effort synchronization will apply; that is, all managed objects selected for this operation will perform the operation if possible regardless of whether some managed objects fail to perform it.

##### 11.1.1.4.4 Results

In case of success, all of the ManagedEntity instances selected for deletion are deleted. In case of failure, a specified or unspecified reason may be provided in the Output parameters.

#### 11.1.1.5 Void

#### 11.1.1.6 Void

#### 11.1.1.7 Notification notifyMOICreation

##### 11.1.1.7.1 Definition

This notification notifies the subscribed consumers that a new Managed Object Instance has been created.

##### 11.1.1.7.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| objectClass | M | It shall carry the ManagedEntity class name. | It specifies the class name of the IOC. A network event has occurred in an instance of this class. |
| objectInstance | M | It shall carry  the DN of the ManagedEntitiy. | It specifies a new instance of the above IOC in which the network event related to by carrying the Distinguished Name (DN) for the instance. |
| notificationId | M | This is an identifier for the notification, which may be used to correlate notifications. | The identifier of the notification shall be chosen to be unique across all notifications of a particular managed object instance throughout the time that correlation is significant, it uniquely identifies the notification from other notifications generated by the subject MOI. |
| notificationType | M | It specifies the type of provisioning management services related notifications. The value “notifyMOICreation” shall be carried. | It specifies the type of notification. |
| eventTime | M | It indicates the MOICreation event time. | The semantics of Generalised Time specified by ITU-T[17] shall be used here. |
| systemDN | M | It shall carry the DN of management service providers. | - |
| correlatedNotifications | CM | It specifies a set of notifications that are correlated to the subject notification. | The condition is that the MnS producer support the correlation of notifications |
| additionalText | O | It can contain further information in text on the event of the ManagedEntity(s). | - |
| sourceIndicator | O | ENUM(  Resource\_operation,  Management\_operation,  SON\_operation,Unknown) | This parameter, when present, indicates the source of the operation that led to the generation of this notification. It can have one of the following values:  1. resource operation: The notification was generated in response to an internal operation of the resource;  2. management operation: The notification was generated in response to a management operation applied across the managed object boundary external to the managed object;  3. SON operation: The notification was generated as result of a SON (Self Organising Network) process like self-configuration, self-optimization, self-healing etc. .  4. unknown: It is not possible to determine the source of the operation.  Remark: A provisioning MnS provider may not in any case be aware that SON operation lead to the generation of this generation. In this case another value than SON\_operation for sourceIndicator might be sent. |
| attributeList | O | LIST OF SEQUENCE <AttributeName, AttributeValue> | The attributes (name/value pairs) of the created MOI. |

##### 11.1.1.7.3 Triggering event

###### 11.1.1.7.3.1 From-state

stateBeforeObjectCreation.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateBeforeObjectCreation | The number of instances of the IOC ManagedEntity is equal to N. |

###### 11.1.1.7.3.2 To-state

stateAfterObjectCreation.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateAfterObjectCreation | The number of instances of the IOC ManagedEntity is equal to N + 1. |

#### 11.1.1.8 Notification notifyMOIDeletion

##### 11.1.1.8.1 Definition

This notification notifies the subscribed consumers that an existing Managed Object Instance has been deleted.

##### 11.1.1.8.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| objectClass | M | It shall carry the ManagedEntity class name. | It specifies the class name of the IOC. A network event has occurred in an instance of this class. |
| objectInstance | M | It shall carry  the DN of the ManagedEntitiy. | It specifies an existing instance of the above IOC in which the network event related to by carrying the Distinguished Name (DN) for the instance. |
| notificationId | M | This is an identifier for the notification, which may be used to correlate notifications. | The identifier of the notification shall be chosen to be unique across all notifications of a particular managed object throughout the time that correlation is significant, it uniquely identifies the notification from other notifications generated by the subject MOI. |
| notificationType | M | It specifies the type of provisioning management services related notifications. The value “notifyMOIDeletion” shall be carried. | It specifies the type of notification. |
| eventTime | M | It indicates the MOIDeletion event time. | The semantics of Generalised Time specified by ITU-T[17] shall be used here. |
| systemDN | M | It shall carry the DN of management service providers. | - |
| correlatedNotifications | CM | It specifies a set of notifications that are correlated to the subject notification. | The condition is that the MnS producer support the correlation of notifications |
| additionalText | O | It can contain further information in text on the event of the ManagedEntity(s). | - |
| sourceIndicator | O | ENUM(  Resource\_operation,  Management\_operation,  SON\_operation,Unknown) | This parameter, when present, indicates the source of the operation that led to the generation of this notification. It can have one of the following values:  1. resource operation: The notification was generated in response to an internal operation of the resource;  2. management operation: The notification was generated in response to a management operation applied across the managed object boundary external to the managed object;  3. SON operation: The notification was generated as result of a SON (Self Organising Network) process like self-configuration, self-optimization, self-healing etc. .  4. unknown: It is not possible to determine the source of the operation.  Remark: A provisioning MnS provider may not in any case be aware that SON operation lead to the generation of this generation. In this case another value than SON\_operation for sourceIndicator might be sent. |
| attributeList | O | LIST OF SEQUENCE <AttributeName, AttributeValue> | The attributes (name/value pairs) of the deleted MOI. |

##### 11.1.1.8.3 Triggering event

###### 11.1.1.8.3.1 From-state

stateBeforeObjectDeletion.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateBeforeObjectDeletion | The number of instances of the IOC ManagedEntity is equal to N. |

###### 11.1.1.8.3.2 To-state

stateAfterObjectDeletion.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateAfterObjectDeletion | The number of instances of the IOC ManagedEntity is equal to N - 1. |

#### 11.1.1.9 Notification notifyMOIAttributeValueChanges

##### 11.1.1.9.1 Definition

This notification notifies the subscribed consumers that changes of one or several attributes of a Managed Object Instance in the NRM.

##### 11.1.1.9.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| objectClass | M | It shall carry the ManagedEntity class name. | It specifies the class name of the IOC. A network event has occurred in an instance of this class. |
| objectInstance | M | It shall carry  the DN of the ManagedEntitiy. | It specifies the existing instance of the above IOC in which the network event related to by carrying the Distinguished Name (DN) for the instance. |
| notificationId | M | This is an identifier for the notification, which may be used to correlate notifications. | The identifier of the notification shall be chosen to be unique across all notifications of a particular managed object throughout the time that correlation is significant, it uniquely identifies the notification from other notifications generated by the subject Information Object. |
| notificationType | M | It specifies the type of provisioning management services related notifications. The value “notifyMOIAttributeValueChange” shall be carried. | It specifies the type of notification. |
| eventTime | M | It indicates the MOIAttributeValueChange event time. | The semantics of Generalised Time specified by ITU-T[17] shall be used here. |
| systemDN | M | It shall carry the DN of management service providers. | - |
| correlatedNotifications | CM | It specifies a set of notifications that are correlated to the subject notification. | The condition is that the MnS producer support the correlation of notifications |
| additionalText | O | It can contain further information in text on the event of the ManagedEntity(s). | - |
| sourceIndicator | O | ENUM(  Resource\_operation,  Management\_operation,  SON\_operation,Unknown) | This parameter, when present, indicates the source of the operation that led to the generation of this notification. It can have one of the following values:  1. resource operation: The notification was generated in response to an internal operation of the resource;  2. management operation: The notification was generated in response to a management operation applied across the managed object boundary external to the managed object;  3. SON operation: The notification was generated as result of a SON (Self Organising Network) process like self-configuration, self-optimization, self-healing etc. .  4. unknown: It is not possible to determine the source of the operation.  Remark: A provisioning MnS provider may not in any case be aware that SON operation lead to the generation of this generation. In this case another value than SON\_operation for sourceIndicator might be sent. |
| attributeValueChange | M | LIST OF SEQUENCE <AttributeName, NewAttributeValue,  CHOICE [NULL, OldAttributeValue]> | The changed attributes (name/value pairs) of the MOI (with both new and, optionally, old values). |

##### 11.1.1.9.3 Triggering event

###### 11.1.1.9.3.1 From-state

stateBeforeAttributeValueChange.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateBeforeAttributeValueChange | The subject attribute has a value at time T1. |

###### 11.1.1.9.3.2 To-state

stateAfterAttributeValueChange.

|  |  |  |
| --- | --- | --- |
| Assertion Name | Definition | |
| stateAfterAttributeValueChange | | The subject attribute has been changed to a value other than the value at time T1. |

#### 11.1.1.10 Notification notifyEvent

##### 11.1.1.10.1 Definition

This notification notifies the consumer, who has a subscription receiving this type of notification, that certain network events has occurred with potential service impact, for example, system restart and system redundancy shift (backup).

This notification definition is generic in the sense that the specific types of network event are not defined.

##### 11.1.1.10.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| objectClass | M | It carries the IOC of an instance where an alert occurs. | -- |
| objectInstance | M | It carries the DN of an instance where an alert occurs. | -- |
| notificationId | M | It carries the identifier for the subject notification. | See Note 1. |
| eventTime | M | It indicates the time of the event. | The semantics of Generalised Time specified by ITU-T [17] shall be used here. |
| systemDN | M | It carries the DN of producer of the notification. | -- |
| notificationType | M | "notifyEvent" | -- |
| specificProblem | M | It indicates a problem detected. | -- |
| additionalText | O | It carries additional information. | -- |
| additionalInformation | O | It carries additional information. | -- |
| NOTE 1: If consumer receives notifications from one producer, consumer can use the notificationId and the objectInstance to uniquely identify all received notifications.  If consumer receives notifications from multiple producers and notifications of each objectInstance are reported to at most by one producer, consumer can use the notificationId and objectInstance to uniquely identify all received notifications.  If consumer receives notifications from multiple producers and notifications of one or more objectInstance(s) are reported byo two or more producers, consumer can use the notificationId together with objectInstance and the identity of producer (systemDN), to uniquely identify all received notifications. If the information systemDN is absent, consumer needs other means, which are outside the scope of this TS, to determine the identity of producer.  How notificationId of notifications are re-used to correlate notifications is outside of the scope of this specification. | | | |

#### 11.1.1.11 Notification notifyMOIChanges

##### 11.1.1.11.1 Definition

This notification notifies subscribed MnS consumers that Managed Object Instances have been created or deleted, or that values of Managed Object Instance attributes have been replaced. This notification can report multiple updates that happened at the same time.

The MnS producer decides whether to send notifications of type notifyMOICreation, notifyMOIDeletion or notifyMOIAttributesValueChange, or a single notifyMOIChanges reporting all changes in a single notification. The MnS producer should take subscription information into account when deciding the notification types to be sent, and not try to send notifications that the MnS consumer did not subscribe to.

The notification header includes a notificationId. This identifier shall not be used in the parameter correlatedNotifications potentially carried in other notifications. The notificationId in mOIChanges shall be used instead. This is because the latter notification id is associated to a single MOI only, whereas the former notification id can be associated to changes of multiple MOIs. The correlatedNotifications associates to a single MOI one or more notification ids identifying notifications reporting events for that MOI.

##### 11.1.1.11.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | Support Qualifier | Information Type / Legal Values | Comment |
| objectClass | M | See clause 11.1.1.7.2 | This parameter specifies the class name of the local root in the MIB |
| objectInstance | M | See clause 11.1.1.7.2 | This parameter specifies the instance of the local root in the MIB |
| notificationId | M | See clause 11.1.1.7.2 | See clause 11.1.1.7.2 |
| notificationType | M | const string “notifyMOIChanges” | See clause 11.1.1.7.2 |
| eventTime | M | See clause 11.1.1.7.2 | See clause 11.1.1.7.2 |
| systemDN | M | See clause 11.1.1.7.2 | See clause 11.1.1.7.2 |
| mOIChanges | M | SEQUENCE OF SET {  notificationId (M),  correlatedNotifications (O),  additionalText (O),  sourceIndicator (O),  path (M),  operation (M),  value (CM)  } | This parameter describes the NRM updates to be reported.  The notificationId is an identifier of one MOI change.  The path specifies the MOI created or deleted, or the MOI with replaced attribute values. The path may identify also parts of an attribute in case the attribute is a structured data type.  The operation specifies the type of operation that has been applied to the MOI specified by the path. It can have the values "CREATE", "DELETE" and "REPLACE". "CREATE" and "DELETE" refers to a MOI creation or deletion, respectively. "REPLACE" refers to the replacement of a complete attribute value of an existing MOI, or parts thereof in case the attribute is a structured data type.  When a MOI creation is reported, the value carries an (optional) complete MOI representation.  When a MOI deletion is reported, the value carries an (optional) complete MOI representation.  When the replacement of the value of one or more attributes of a MOI is reported, the value carries the MOI representation without the attributes not changed.  When the replacement of the value of a part of an attribute is reported, the value carries the new value of that part.  When arrays are modified (by e.g. adding an array item, removing an array item or replacing an array item) the complete array shall be included in value.  The reported MOI changes is an ordered list, since the creation of parent objects needs to be reported before the creation of child objects, and, vice versa, the deletion of child objects needs to be reported before the deletion of parent objects. |

### 11.1.2 Managed Information

#### 11.1.2.1 ManagedEntity

##### 11.1.2.1.1 Definition

The ProxyClass ManagedEntity represents the role that can be played by an instance of an IOC defined in NRMs, e.g. Generic NRM, NR and NG-RAN NRM, or 5GC NRM. ManagedEntity is used in the specification of provisioning operations and notifications to represent an instance of an IOC defined in these NRMs.

## 11.2 Generic fault supervision management service

### 11.2.1 Operations and notifications

#### 11.2.1.1 Operation and notification of fault supervision data report management service

##### 11.2.1.1.1 subscribe

###### 11.2.1.1.1.1 Definition

A MnS consumer invokes this operation to establish subscription to receive network events via notifications, under the filter constraint specified in this operation.

###### 11.2.1.1.1.2 Input parameters

| Parameter Name | S | Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| consumerReference | M | NtfSubscriber.ntfManagerReference | It specifies the reference of the authorized consumer to which notifications shall be sent. |
| timeTick | O | NtfSubscription.ntfTimeTick | It specifies the value of a timer held for the subject management service consumer.  The value is in unit of whole minute.  A special infinite value is assumed when parameter is absent or present but equal to zero. |
| filter | O | This attribute represents the filter of a subscription. | It specifies a filter constraint that service provider shall use to filter notification of the alarms.  If this parameter is absent, then no filter constraint shall be applied. |

###### 11.2.1.1.1.3 Output parameters

| Parameter Name | S | Matching Information /  Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| subscriptionId | M | NtfSubscription.ntfSubscriptionId. | It holds an unambiguous identity of this subscription. |
| status | M | ENUM (OperationSucceeded, OperationFailedExistingSubscription, OperationFailed) | If subscriptionCreated is true, status = OperationSuceeded.  If operation\_failed\_existing\_subscription is true, status = OperationFailedExistingSubscription  If operation\_failed is true, status = OperationFailed. |

###### 11.2.1.1.1.4 Pre-condition

notificationCategoriesNotAllSubscribed OR notificationCategoriesParameterAbsentAndNotAllSubscribed.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| notificationCategoriesNotAllSubscribed | At least one notificationCategory identified in the notificationCategories input parameter is supported by management service producer and is not a member of the ntfNotificationCategorySet attribute of an NtfSubscription which is involved in a subscription relationship with the NtfSubscriber identified by the managerReference input parameter. |
| notificationCategoriesParameterAbsentAndNotAllSubscribed | The notificationCategories input parameter is absent and at least one notificationCategory supported by management service producer is not a member of the ntfNotificationCategorySet attribute of an ntfSsubscription which is involved in a subscription relationship with the NtfSubscriber identified by the managerReference input parameter. |

###### 11.2.1.1.1.5 Post-condition

subscriberPossiblyCreated AND subscriptionCreated.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| subscriberPossiblyCreated | An NtfSubscriber with an ntfManagerReference attribute equal to the value of the managerReference input parameter is involved in a subscriptionRegistration relationship. |
| subscriptionCreated | An NtfSubscription has been created according to the following rules:  - ntfSubscriptionState attribute value has been set to "notSuspended";  - ntfTimeTick attribute value has been set to the value of the timeTick input parameter if This value was higher or equal to 15, or set to 15 if this parameter value was between 1 and 15, or set to a special infinite value if the parameter value was lower or equal to 0 or if parameter was absent;  - ntfTimeTickTimer has been reset with the value of timeTick attribute;  - ntfFilter attribute value has been set to the value of the filter input parameter if present;  - NtfSubscription is involved in a subscription relationship with the NtfSubscriber identified by the managerReference input parameter;  - attribute ntfNotificationCategorySet of NtfSubscription contains EITHER the notification categories identified by the notificationCategories input parameter that were not already contained in the ntfNotificationCategorySet attribute of other NtfSubscription of the same NtfSubscriber identified by the managerReference input parameter OR if notificationCategories input parameter is absent, all notification categories supported by management service producer that were not already contained in the ntfNotificationCategorySet attribute of other subscriptions of the same NtfSubscriber identified by the managerReference input parameter. |

###### 11.2.1.1.1.6 Exceptions

|  |  |
| --- | --- |
| Name | Definition |
| operation\_failed\_existing\_subscription | **Condition:** (notificationCategoriesNotAllSubscribed OR notificationCategoriesParameterAbsentAndNotAllSubscribed) not true  **Returned Information:** The output parameter status  **Exit state:** Entry State |
| operation\_failed | **Condition:** Post-condition is false  **Returned Information:** The output parameter status  **Exit state:** Entry State |

##### 11.2.1.1.2 unsubscribe

###### 11.2.1.1.2.1 Definition

A MnS consumer invokes this operation to cancel subscriptions. The MnS consumer can cancel one subscription made with a consumerReference by providing the corresponding subscriptionId or all subscriptions made with the same consumerReference by leaving the subscriptionId parameter absent.

###### 11.2.1.1.2.2 Input parameters

| Parameter Name | S | Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| consumerReference | M | DN | It specifies the reference of the MnS consumer to which notifications shall be sent. |
| subscriptionId | O | A unique identifier that is SS dependent. | It holds a subscriptionId carried as the output parameter in the subscribe operation. |

###### 11.2.1.1.2.3 Output parameters

| Parameter Name | S | Matching Information /  Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| status | M | ENUM (OperationSucceeded, OperationFailed) | If (subscriptionDeleted OR allSubscriptionDeleted) is true, status = OperationSucceeded.  If operation\_failed is true, status = OperationFailed. |

###### 11.2.1.1.2.4 Pre-condition

validSubscriptionId&ManagerReference OR SubscriptionIdAbsent&ValidManagerReference.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| validSubscriptionId&ManagerReference | The NtfSubscription identified by subscriptionId input parameter is involved in a subscription relationship with the NtfSubscriber identified by the managerReference input parameter. |
| subscriptionIdAbsent&ValidManagerReference | The subscriptionId input parameter is absent and the NtfSubscriber identified by the managerReference input parameter exists. |

###### 11.2.1.1.2.5 Post-condition

subscriptionDeleted OR allSubscriptionDeleted.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| subscriptionDeleted | The NtfSubscription identified by subscriptionId input parameter is no more involved in a subscription relationship with the NtfSubscriber identified by the managerReference input parameter and has been deleted. If this NtfSubscriber has no more NtfSubscription, it is deleted as well. |
| allSubscriptionDeleted | "In the case subscriptionId input parameter was absent, the NtfSubscriber identified by the managerReference input parameter is no more involved in any subscription relationship and is deleted, the corresponding NtfSubscription have been deleted as well. |

###### 11.2.1.1.2.6 Exceptions

|  |  |
| --- | --- |
| Name | Definition |
| operation\_failed | **Condition:** Pre-condition is false or post-condition is false  **Returned Information:** The output parameter status  **Exit state:** Entry State |

##### 11.2.1.1.3 getAlarmList

###### 11.2.1.1.3.1 Definition

A MnS consumer invokes this operation to request the MnS producer to provide either the complete list of AlarmInformation instances in the AlarmList or only a part of this list (partial alarm alignment).

The parameters baseObjectClass and baseObjectInstance are used to identify the part of the alarm list to be returned. If they are absent, then the complete alarm list shall be provided (full alarm alignment). If they identify a particular class instance, then only a) the AlarmInformation instances related to this class instance and b) the AlarmInformation instances related to the subordinate class instances of this class instance shall be provided (partial alarm alignment). An instance-a is said to be subordinate to instance-b if the DN of the latter is part of the DN of the former.

There are two modes of operation. One mode is synchronous. In this mode, the list of AlarmInformation instances in AlarmList is returned synchronously with the operation. The other mode is asynchronous. In this mode, the list of AlarmInformation instances is returned via alarm notifications. In asynchronous mode of operation, the only information returned synchronously is the status of the operation. A method allowing to abort an ongoing alarm alignment process shall be available in the asynchronous mode. The mode of operation to be used is determined by means outside the scope of specification. To use asynchronous mode, the authorized consumer needs to have established a subscription via the subscribe operation.

###### 11.2.1.1.3.2 Input parameters

| Parameter Name | S | Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| alarmAckState | O | ENUM (all alarms, all active alarms, all active and acknowledged alarms, all active and unacknowledged, all Cleared and unacknowledged alarms, all unacknowledged) | It carries a constraint. The FaultSupervision MnS producer shall apply it on AlarmInformation instances in AlarmList when constructing its output parameter AlarmInformationList. |
| baseObjectClass | O, see note 1 | This parameter is either absent or carries the object class of a certain class. | See how this attribute is used to support full alarm alignment and partial alarm alignment in 11.1.2.3.3.1.  See note 2. |
| baseObjectInstance | O, see note 1 | This parameter is either absent or carries the DN of a certain class instance. | See how this attribute is used to support full alarm alignment and partial alarm alignment in 11.1.2.3.3.1.  See note 2. |
| filter | O | N/A | It carries a filter constraint.  If the filter is present, the service provider shall apply it on AlarmInformation instances in AlarmList when constructing its output parameter AlarmInformationList.  If the filter is not present, all of the AlarmInformation instances included by the scope are selected. |
| NOTE 1: If the notification notifyAlarmListRebuilt supports indicating that only a part of the alarm list has been rebuilt then the operation getAlarmList shall support partial alarm alignment.  NOTE 2: The legal values of the parameters baseObjectClass and baseObjectInstance are restricted to those carried by the parameters baseObjectClass and baseObjectInstance in the recent notifyAlarmListRebuilt notifications. The timeline for "recent" is vendor-specific. | | | |

###### 11.2.1.1.3.3 Output parameters

Table 11.2.1.1.3.3-1: Output parameters for the operation getAlarmList

| Parameter Name | S | Matching Information /  Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| alarmInformationList | M | List of AlarmInformation. | It carries the requested AlarmInformation instances.  Case when synchronous mode of operation is used:  (a) The service provider shall apply the constraints expressed in alarmAckState and filter to AlarmInformation instances when constructing this output parameter.  Case when asynchronous mode of operation is used (i.e. this output parameter is conveyed via notifications):  (a) If the filter parameter is present, the service provider shall apply the constraint when constructing this output parameter. Furthermore, if the alarmAckState constraint is present, the service provider shall apply that constraint as well. The filter constraint, if any, that is currently active in the notification channel is not used for the construction of this output parameter.  (b) If the filter parameter is absent, the service provider shall apply the filter constraint currently active in the notification channel when constructing this output parameter. If the alarmAckState constraint is present, the service provider shall apply that constraint as well. |
| status | M | ENUM (OperationSucceeded, OperationFailed) | If all the AlarmInformation are returned, status = OperationSucceeded.  If operation is failed, status = OperationFailed. |

The following table defines an item of alarmInformationList.

Table 11.2.1.1.3.3-2: Definition of an item of alarmInformationList

| **Parameter name** | **S** | **Matching information** | **Comment** |
| --- | --- | --- | --- |
| objectClass,  objectInstance | M | MonitoredEntity.objectClass,  MonitoredEntity.objectInstance | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation. |
| notificationId | M | AlarmInformation.notificationId |  |
| notificationType | M | "notifyNewAlarm"  or  "notifyChangedAlarm"  or  "notifyClearedAlarm" | The parameter carries  - notifyNewAlarm in case the alarm has not yet changed and has not yet been cleared.  - notifyChangedAlarm in case the alarm has changed but has not yet been cleared.  - notifyClearedAlarm in case the alarm has been cleared but not yet acknowledged. |
| eventTime | O | AlarmInformation.alarmRaisedTime or  AlarmInformation.alarmChangedTime or  AlarmInformation.alarmClearedTime | The parameter carries the  - alarmRaisedTime in case notificationType carries notifyNewAlarm  - alarmChangedTime in case notificationType carries notifyChangedAlarm  - alarmClearedTime in case notificationType carries notifyClearedAlarm |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| [objectClass],  [objectInstance] | n/a | MonitoredEntity.objectClass,  MonitoredEntity.objectInstance | Parmeter identical to the first parameter in this list, shown here to clarify all elements of AlarmInformation are present |
| [notificationId] | n/a | AlarmInformation.notificationId | Parmeter identical to the second parameter in this list, shown here to clarify all elements of AlarmInformation are present |
| alarmRaisedTime | M | AlarmInformation.alarmRaisedTime |  |
| alarmChangedTime | O | AlarmInformation.alarmChangedTime | not applicable if the severity of related alarm was not changed |
| alarmClearedTime | M | AlarmInformation.alarmClearedTime | not applicable if related alarm was not cleared |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probableCause |  |
| specificProblem | O | AlarmInformation.specificProblem |  |
| perceivedSeverity | M | AlarmInformation.perceivedSeverity |  |
| backedUpStatus | O | AlarmInformation.backedUpStatus | not applicable if related alarm is a security alarm |
| backUpObject | O | MonitoredEntity.objectInstance | The MonitoredEntity is identified by relation-BackUpObject-AlarmInformation.  Not applicable if related alarm is a security alarm |
| trendIndication | O | AlarmInformation.trendIndication | not applicable if related alarm is a security alarm |
| thresholdInfo | O | AlarmInformation.thresholdInfo | not applicable if related alarm is a security alarm |
| correlatedNotifications | O | The set of CorrelatedNotification instances related to this AlarmInformation. |  |
| stateChangeDefinition | O | AlarmInformation.stateChange | not applicable if related alarm is a security alarm |
| monitoredAttributes | O | AlarmInformation.monitoredAttributes | not applicable if related alarm is a security alarm |
| proposedRepairActions | O | AlarmInformation.proposedRepairActions | not applicable if related alarm is a security alarm |
| additionalText | O | AlarmInformation.additionalText |  |
| additionalInformation | O | AlarmInformation.additionalInformation |  |
| rootCauseIndicator | O | AlarmInformation.rootCauseIndicator |  |
| ackTime | M | AlarmInformation.ackTime | not applicable if related alarm was not acknowledged nor unacknowledged  The availability and accuracy of time carried by the time parameters in individual entries of the list (i.e. eventTime, alarmRaisedTime, alarmClearedTime and ackTime) shall be "best effort".  Reason: A Management System is not required to persistently store these times or other alarm information (as in case of synchronization information may be provided by the NE), while also some NE's do not keep these times (and a later attempt to retrieve the alarm data from the NEs will not deliver these time data). |
| ackUserId | M | AlarmInformation.ackUserId | not applicable if related alarm was not acknowledged nor unacknowledged |
| ackSystemId | O | AlarmInformation.ackSystemId | not applicable if related alarm was not acknowledged nor unacknowledged |
| ackState | M | AlarmInformation.ackState | not applicable if related alarm was not acknowledged nor unacknowledged |
| clearUserId | O | AlarmInformation.clearUserId | not applicable if related alarm was not cleared |
| clearSystemId | O | AlarmInformation.clearSystemId | not applicable if related alarm was not cleared |
| serviceUser | M | AlarmInformation.serviceUser | not applicable if related alarm is not a security alarm |
| serviceProvider | M | AlarmInformation.serviceProvider | not applicable if related alarm is not a security alarm |
| securityAlarmDetector | M | AlarmInformation.securityAlarmDetector | not applicable if related alarm is not a security alarm |
| comments | M | The set of Comment instances related to this AlarmInformation. | Not applicable if the related alarm has no related comments |

###### 11.2.1.1.3.4 Exceptions and constraints

| Exception Name | Definition |
| --- | --- |
| operation\_failed | **Condition:** Operation is failed  **Returned Information:** The output parameter status  **Exit state:** Entry State |

##### 11.2.1.1.4 notifyNewAlarm

###### 11.2.1.1.4.1 Definition

This notification is generated by the MnS producer when a new AlarmInformation is added to the AlarmList. The notification parameters depend on the alarmType and are different for non-security and security alarms.

###### 11.2.1.1.4.2 Input parameters

The notifyNewAlarm notification is defined by Table 11.2.1.1.4.2-1, if the alarmType is equal to "Communications Alarm", "Processing Error Alarm", "Environmental Alarm". "Quality Of Service Alarm" or "Equipment Alarm".

Table 11.2.1.1.4.2-1: Input parameters for notifications related to non-security alarms

| Parameter Name | Qualifier | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation of the new AlarmInformation. |
| objectInstance | M | MonitoredEntity.objectInstance | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation of the new AlarmInformation. |
| notificationId | M | -- |  |
| notificationType | M | "notifyNewAlarm" |  |
| eventTime | M | AlarmInformation.alarmRaisedTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probableCause |  |
| perceivedSeverity | M | AlarmInformation.perceivedSeverity |  |
| specificProblem | O | AlarmInformation.specificProblem |  |
| backedUpStatus | O | AlarmInformation.backedUpStatus |  |
| backUpObject | O | MonitoredEntity.objectInstance  It carries the DN of the back up object. | The object is identified by relation-BackUpObject-AlarmInformation of the new AlarmInformation. |
| trendIndication | O | AlarmInformation.trendIndication |  |
| thresholdInfo | O | AlarmInformation.thresholdInfo |  |
| correlatedNotifications | O | The CorrelatedNotification instances related to this AlarmInformation. |  |
| stateChangeDefinition | O | AlarmInformation.stateChangeDefinition |  |
| monitoredAttributes | O | AlarmInformation.monitoredAttributes |  |
| proposedRepairActions | O | AlarmInformaton.proposedRepairActions |  |
| additionalText | O | AlarmInformation.additionalText |  |
| additionalInformation | O | AlarmInformation.additionalInformation |  |
| rootCauseIndicator | O | AlarmInformation.rootCauseIndicator |  |

###### 11.2.1.1.4.2a Input parameters for notifications related to non-security alarms

The notifyNewAlarm notification is defined by Table 11.2.1.1.4.2a-1, if the alarmType is equal to "Integrity Violation", "Operational Violation", "Physical Violation", "Security Service or Mechanism Violation" or "Time Domain Violation".

Table 11.2.1.1.4.2a-1: Input parameters for notifications related to security alarms

| Parameter Name | Qualifier | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation of the new AlarmInformation. |
| objectInstance | M | MonitoredEntity.objectInstance | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation of the new AlarmInformation. |
| notificationId | M | -- |  |
| notificationType | M | "notifyNewAlarm" |  |
| eventTime | M | AlarmInformation.alarmRaisedTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probableCause |  |
| perceivedSeverity | M | AlarmInformation.perceivedSeverity |  |
| correlatedNotifications | O | The set of CorrelatedNotification related to this AlarmInformation. |  |
| additionalText | O | AlarmInformation.additionalText |  |
| additionalInformation | O | AlarmInformation.additionalInformation |  |
| rootCauseIndicator | O | AlarmIngormation.rootCauseIndicator |  |
| serviceUser | M | AlarmInformation.securityServiceUser | This may contain no information if the identify of the service-user (requesting the service) is not known. |
| serviceProvider | M | AlarmInformation.securityServiceProvider | This shall always identify the service-provider receiving a service request, from serviceUser, that provokes the security alarm. |
| securityAlarmDetector | M | AlarmInformation.securityAlarmDetector | This may contain no information if the detector of the security alarm is the serviceProvider. |

###### 11.2.1.1.4.3 Triggering event

11.2.1.1.4.3.1 From-state

noMatchedAlarm.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| noMatchedAlarm | AlarmList does not contain an AlarmInformation that has the following properties:  Its matching-criteria-attributes values are identical to that of the newly generated network alarm and it is involved in relation-AlarmObject-AlarmInformation with the same MonitoredEntity as the one identified by the newly generated network alarm. |

11.2.1.1.4.3.2 To-state

newAlarmInAlarmList.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| newAlarmInAlarmList | AlarmList contains an AlarmInformation holding information conveyed by the newly generated network alarm. This AlarmInformation is involved in relation-AlarmObject-AlarmInformation with the same MonitoredEntity as the one identified by the newly generated network alarm.  The following attributes of the AlarmInformation shall be populated with information in the newly generated alarm:  notificationId, alarmRaisedTime, alarmId, alarmType, , probableCause, perceivedSeverity.  The following attributes of the same AlarmInformation shall be populated with information of the newly generated alarm if the information is present (in the newly generated alarm) and if the attribute is supported:  specificProblem, backedUpStatus, trendIndication, thresholdInfo, stateChangeDefinition, monitoredAttributes, proposedRepairActions, additionalText, additionalInformation. |

##### 11.2.1.1.5 notifyChangedAlarm

###### 11.2.1.1.5.1 Definition

This notification is generated by the MnS producer when the perceivedSeverity of an existing AlarmInformation changes (except to the value "CLEARED").

11.2.1.1.5.2 Input parameters

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation. |
| objectInstance | M | MonitoredEntity.objectInstance | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation. |
| notificationId | M | -- |  |
| notificationType | M | "notifyChangedAlarm" |  |
| eventTime | M | AlarmInformation.alarmChangedTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probableCause |  |
| perceivedSeverity | M | AlarmInformation.perceivedSeverity |  |

###### 11.2.1.1.5.3 Triggering event

11.2.1.1.5.3.1 From-state

alarmMatched AND alarmNotCleared AND alarmChanged.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmMatched | The matching-criteria-attributes of the newly generated network alarm has values that are identical (matches) with ones in one AlarmInformation in AlarmList. |
| alarmNotCleared | The perceivedSeverity of the newly generated network alarm is not Cleared. |
| alarmChanged | The perceivedSeverity of the newly generated network alarm and of the matched AlarmInformation are different. |

11.2.1.1.5.3.2 To-state

informationUpdate.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| informationUpdate | The AlarmInformation identified in alarmMatched in from-state has been updated according to the following rules:  - notificationId is updated;  - alarmChangedTime is updated;  - perceivedSeverity is updated;  - ackTime, ackUserId and ackSystemId are updated to contain no information;  - ackState is updated to "unacknowledged"; |

##### 11.2.1.1.6 notifyAlarmListRebuilt

###### 11.2.1.1.6.1 Definition

This notification is generated by the MnS producer when the AlarmList has been completely or partially rebuilt.

###### 11.2.1.1.6.2 Input parameters

| Parameter Name | S | Legal type | Comment |
| --- | --- | --- | --- |
| objectClass | M | -- | Identifies, together with the objectInstance parameter, the part of the alarm list that has been rebuilt.  If this paramter specifies the class of the instance carried in systemDN, then all AlarmInformation instances in the AlarmList may have been rebuilt.  If this parameter specifies some class represented by MonitoredEntity, then a subset of the AlarmInformation instances in the AlarmList may have been rebuilt. |
| objectInstance | M | -- | Identifies, together with the objetClass parameter, the part of the alarm list that has been rebuilt.  If this parameter is equal to the instance carried in systemDN, then all AlarmInformation instances in the AlarmList may have been rebuilt.  If this parameter is equal to some instance represented by MonitoredEntity, then only AlarmInformation related to this instance and its descendants may have been rebuilt.. |
| notificationId | M | -- | -- |
| notificationType | M | "notifyAlarmListRebuilt" |  |
| eventTime | M | -- | The time when the alarm list has been rebuilt. |
| systemDN | M | -- | It identifies the DN of service providers. |
| reason | M | "System-NE communication error", "System restarts", "indeterminate". Other values can be added. | The reason why the system has rebuilt the AlarmList. This may carry different reasons than that carried by the immediate previous notifyPotentialFaultyAlarmList. |
| alarmListAlignmentRequirement | O | "alignmentRequired", "alignmentNotRequired". | It carries an enumeration of "alignmentRequired" and "alignmentNotRequired". |

###### 11.2.1.1.6.3 Triggering event

11.2.1.1.6.3.1 From-state

alarmListRebuilt\_0 OR alarmListRebuilt\_1.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmListRebuilt\_0 | Provider has cold-started, initialized, re-initialized or rebooted and it has initiated procedure to rebuild its AlarmList. |
| alarmListRebuilt\_1 | Provider loses confidence in part or whole of its AlarmList. Provider has initiated procedure to repair its AlarmList. |

11.2.1.1.6.3.2 To-state

alarmListRebuilt\_2.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmListRebuilt\_2 | Provider rebuilds the whole or part of AlarmList. |

##### 11.2.1.1.7 notifyCorrelatedNotificationChanged

###### 11.2.1.1.7.1 Definition

This notification is generated by the MnS producer when the set of CorrelatedNotification is created, updated or deleted.

###### 11.2.1.1.7.2 Input parameters

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation. |
| objectInstance | M | MonitoredEntity.objectInstance | The MonitoredEntity is identified by the relation-AlarmedObject-AlarmInformation. |
| notificationId | M | -- |  |
| notificationType | M | "notifyCorrelatedNotificationChanged" |  |
| eventTime | M | It carries the time when the CorrelatedNotification is created, updated or deleted. |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| correlatedNotifications | M | The CorrelatedNotification instances related to this AlarmInformation. |  |
| rootCauseIndicator | O | AlarmInformation.rootCauseIndicator |  |

###### 11.2.1.1.7.3 Triggering event

11.2.1.1.7.3.1 From-state

newAlarmCorrelationInfoIsAvailable AND alarmInformationExists.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| newAlarmCorrelationInfoIsAvailable | New alarm correlation information is available but not yet conveyed to any consumer. |
| alarmInformationExists | The AlarmInformation is in AlarmList. |

11.2.1.1.7.3.2 To-state

alarmCorrelatedInfoUpdated.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmCorrelatedInfoUpdated | The set of CorrelatedNotification network slice instances is created, updated or deleted. |

##### 11.2.1.1.8 getAlarmCount

###### 11.2.1.1.8.1 Definition

A MnS consumer invokes this operation to get the number of alarms in the alarm list. The alarms are counted separately for each perceived severity level. An input parameter allows to control which alarms are counted.

###### 11.2.1.1.8.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Name | S | Information Type | Comment |
| filter | O | N/A | It carries a filter constraint. The operation shall apply it when counting the AlarmInformation instances in AlarmList.  Case when synchronous mode of operation is used for getAlarmList:  (a) If this parameter is present, the operation shall count the AlarmInformation instances which satisfy both (a) this filter constraint and (b) the condition set by input parameter alarmAckState.  (b) If this parameter is absent, the operation shall count all AlarmInformation instances that satisfy the condition set by input parameter alarmAckState.  Case when asynchronous mode of operation is used for getAlarmList:  (a) If this parameter is present, the operation shall count all AlarmInformation instances that satisfy this filter constraint and the condition set by input parameter alarmAckState.  (b) If this parameter is absent, the operation shall count AlarmInformation instances that satisfy (a) the filter constraint currently active in the notification channel established between the authorized consumer and the service provider and (b) the condition set by input parameter alarmAckState. |
| alarmAckState | O | ENUM (all alarms, all active alarms, all active and acknowledged alarms, all active and unacknowledged, all cleared and unacknowledged alarms, all unacknowledged) | It carries a constraint. The operation shall apply it on AlarmInformation instances in AlarmList when counting. |

###### 11.2.1.1.8.3 Output parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Name | S | Matching Information | Comment |
| criticalCount, majorCount, minorCount, warningCount, indeterminateCount, clearedCount | M | N/A | They carry the number of AlarmInformation in AlarmList that has the following properties.  Case when synchronous mode of operation is used:  (a) The operation shall apply the constraints expressed in alarmAckState and filter to AlarmInformation instances when counting.  Case when asynchronous mode of operation is used (i.e. this output parameter is conveyed via notifications):  (a) If the filter parameter is present, the operation shall apply the constraint when counting. Furthermore, if the alarmAckState constraint is present, the operation shall apply that constraint as well. The filter constraint, if any, that is currently active in the notification channel is not used for the counting.  (b) If the filter parameter is absent, the operation shall apply the filter constraint currently active in the notification channel when counting. If the alarmAckState constraint is present, the operation shall apply that constraint as well. |
| status | M | ENUM (OperationSucceeded, OperationFailed) | If allAlarmInformationCounted is true, status = OperationSucceeded.  If operation\_failed is true, status = OperationFailed. |

###### 11.2.1.1.8.4 Pre-condition

There are no pre-conditions.

###### 11.2.1.1.8.5 Post-condition

allAlarmInformationCounted.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| allAlarmInformationCounted | All AlarmInformation that satisfy the constraints expressed in input parameters filter and alarmAckState and are present in the AlarmList at the moment of this operation invocation are counted and the result returned.  All AlarmInformation in AlarmList remains unchanged as the result of this operation. |

###### 11.2.1.1.8.6 Exceptions

|  |  |
| --- | --- |
| Name | Definition |
| operation\_failed | **Condition:** the pre-condition is false or the post-condition is true.  **Returned Information:** The output parameter status.  **Exit state:** Entry state. |
| filter\_complexity\_limit | **Condition:** Operation not performed because the filter parameter is too complex.  **Returned Information**: The output parameter status.  **Exit state:** Entry state. |

##### 11.2.1.1.9 setComment

###### 11.2.1.1.9.1 Definition

A MnS consumer invokes this operation to set a comment in one or more AlarmInformation instances in AlarmList.

###### 11.2.1.1.9.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Name | S | Information Type | Comment |
| alarmInformation ReferenceList | M | List of AlarmInformation.alarmId | It carries one or more identifiers identifying AlarmInformation instances in the AlarmList. |
| commentUserId | M | Comment.commentUserId | The Comment is identified by the relation-AlarmInformation-Comment. |
| commentSystemId | O | Comment.commentSystemId | The Comment is identified by the relation-AlarmInformation-Comment. |
| commentText | M | Comment.commentText | The Comment is identified by the relation-AlarmInformation-Comment. |

###### 11.2.1.1.9.3 Output Parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Qualifier | Matching Information | Comment |
| badAlarm Information ReferenceList | M | List of pair of AlarmInformation.alarmId and the failure reason. | If allUpdated is true, it contains no information.  If someUpdated is true, then it contains identifications of AlarmInformation that are not present in AlarmList or that they are present, but AlarmInformation.comments has not changed, in contrast to authorized consumer's request. |
| status | M | ENUM( Operation succeeded, Operation failed, Operation partially failed) | If allUpdated is true, then status = OperationSucceeded.  If someUpdated is true, then status = OperationPartiallyFailed.  If exception operationFailed is raised, then status = OperationFailed. |

#### 11.2.1.2 Fault supervision data control management service

##### 11.2.1.2.1 acknowledgeAlarms

###### 11.2.1.2.1.1 Definition

The MnS consumer invokes this operation to acknowledge one or more alarms.

When this operation is not supported, the MnS producer shall support acknowledging alarms.

###### 11.2.1.2.1.2 Input parameters

| Parameter Name | S | Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| alarmInformationReferenceList | M | SET OF SEQUENCE {  AlarmInformation.alarmId (M)  AlarmInformation.perceivedSeverity (O)  } | It identifies the alarms to be acknowledged. If an alarm id is qualified with an optional perceived severity, the alarm shall be acknowledged only when the perceived severity in the alarm list matches the perceived severity provided in the operation request. |
| ackUserId | M | AlarmInformation.ackUserId | The identifier of the user acknowledgeding the alarm. |
| ackSystemId | O | AlarmInformation.ackSystemId | The identifier of the system where the acknowledgement request was originated. |

###### 11.2.1.2.1.3 Output parameters

| Parameter Name | S | Matching Information /  Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| badAlarm Information ReferenceList | M | SET OF SEQUENCE {  AlarmInformation.alarmId (M)  errorReason (M)  }  errorReason ::= ENUM {  UnknownAlarmId,  AcknowledgmentFailed,  WrongPerceivedSeverity  } | If all alarms are acknowledged, it contains no information.  If only some alarms are acknowledged, then it contains identifications of AlarmInformation that are  (a) present in input parameter AlarmInformationReferenceList but absent in the AlarmList (errorReason = UnknownAlarmId; or  (b) present in input parameter AlarmInformationReferenceList and present in the AlarmList but the Acknowledgement Information (see note below table) has not changed despite the consumer's request (errorReason = AcknowledgmentFailed); or  (c) present in input parameter AlarmInformationReferenceList and present in the AlarmList but the perceivedSeverity to be acknowledged has changed and/or is different in the Alarm List (ErrorReason = WrongPerceivedSeverity), applicable only if perceivedSeverity is provided. |
| status | M | ENUM {  OperationSucceeded,  OperationPartiallySucceeded,  OperationFailed  } | If all alarms acknowledged, then  status = OperationSucceeded.  If some alarms are acknowledged, then status = OperationPartiallySuceeded.  If operation failed is true, then  status = OperationFailed. |

NOTE: Acknowledgement Information is defined as the information contained in AlarmInformation.ackTime, AlarmInformation.ackUserId, AlarmInformaton.ackSystemId, AlarmInformation.ackState.

###### 11.2.1.2.1.4 Exceptions and constraints

| Exception Name | Definition |
| --- | --- |
| operation\_failed | **Condition:** Operation is failed  **Returned Information:** The output parameter status  **Exit state:** Entry State |

##### 11.2.1.2.2 unacknowledgeAlarms

###### 11.2.1.2.2.1 Definition

The MnS consumer invokes this operation to remove acknowledgement information kept in one or more AlarmInformation instances.

###### 11.2.1.2.2.2 Input parameters

| Parameter Name | S | Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| alarmInformationReferenceList | M | List of AlarmInformation.alarmId | It carries one or more identifiers identifying AlarmInformation in AlarmList. |
| ackUserId | M | AlarmInformation.ackUserId | The identifier of the user unacknowledgeding the alarm. |
| ackSystemId | O | AlarmInformation.ackSystemId | The identifier of the system where the acknowledgement request was originated. |

###### 11.2.1.2.2.3 Output parameters

| Parameter Name | Support Qualifier | Matching Information /  Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| badAlarmInformation  ReferenceList | M | SET OF SEQUENCE {  AlarmInformation.alarmId (M)  errorReason (M)  }  errorReason ::= ENUM {  UnknownAlarmId,  AcknowledgmentFailed,  WrongPerceivedSeverity,  } | If all alarms are acknowledged, it contains no information.  If only some alarms are acknowledged, then it contains identifications of AlarmInformation that are  (a) present in input parameter AlarmInformationReferenceList but absent in the AlarmList (errorReason = UnknownAlarmId; or  (b) present in input parameter AlarmInformationReferenceList and present in the AlarmList but the Acknowledgement Information (see note below table) has not changed despite the consumer's request (errorReason = AcknowledgmentFailed); or  (c) present in input parameter AlarmInformationReferenceList and present in the AlarmList but the perceivedSeverity to be acknowledged has changed and/or is different in the Alarm List (ErrorReason = WrongPerceivedSeverity), applicable only if perceivedSeverity is provided. |
| status | M | ENUM {  OperationSucceeded,  OperationPartiallySucceeded,  OperationFailed | If all alarms acknowledged, then  status = OperationSucceeded.  If some alarms are acknowledged, then  status = OperationPartiallySuceeded.  If operation failed is true, then  status = OperationFailed. |

NOTE: Acknowledgement Information is defined as the information contained in AlarmInformation.ackTime, AlarmInformation.ackUserId, AlarmInformaton.ackSystemId, AlarmInformation.ackState.

###### 11.2.1.2.2.4 Exceptions and constraints

| Exception Name | Definition |
| --- | --- |
| Operation\_failed | **Condition:** Operation is failed  **Returned Information:** The output parameter status  **Exit state:** Entry State |

##### 11.2.1.2.3 clearAlarms

###### 11.2.1.2.3.1 Definition

The authorized consumer invokes this operation to clear one or more AlarmInformation instances in AlarmList. For example, this operation can be used to support the manual clearing of the ADMC (automatic detection and manual clearing, see also 3GPP TS 32.111-1 [3]) alarms.

###### 11.2.1.2.3.2 Input parameters

| Parameter Name | S | Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| alarmInformation ReferenceList | M | List of AlarmInformation.alarmId | It carries one or more identifiers identifying AlarmInformation instances in the AlarmList. |
| clearUserId | M | AlarmInformation.clearUserId | It identities the user clearing the alarm. |
| clearSystemId | O | AlarmInformation.clearSystemId | It identifies the authorized consumer. It may be absent implying that consumer does not wish this information be known to the service provider. |

###### 11.2.1.2.3.3 Output parameters

| Parameter Name | S | Matching Information /  Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| badAlarmInformation ReferenceList | M | List of pair of AlarmInformation.alarmId and the failure reason. | If all alarms are cleared, it contains no information.  If some alarms are cleared, then it contains identifications of AlarmInformation that are not present in AlarmList or that are present in AlarmList but remain unchanged, in contrast to consumer's request. |
| status | M | ENUM( OperationSucceeded, OperationFailed, OperationPartiallySucceeded) | If all alarms are cleared, then status = OperationSucceeded.  If some alarms are cleared, then status = OperationPartiallySucceeded.  If operation is failed, then status = OperationFailed. |

###### 11.2.1.2.3.4 Exceptions and constraints

| Exception Name | Definition |
| --- | --- |
| operation\_failed | **Condition:** Operation is failed  **Returned Information:** The output parameter status  **Exit state:** Entry State |

##### 11.2.1.2.4 notifyClearedAlarm

###### 11.2.1.2.4.1 Definition

This notification is generated by the MnS producer when the perceivedSeverity of an existing AlarmInformation changes to "CLEARED".

###### 11.2.1.2.4.2 Input parameters

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass |  |
| objectInstance | M | MonitoredEntity.objectInstance |  |
| notificationId | M | -- |  |
| notificationType | M | "notifyClearedAlarm" |  |
| eventTime | M | AlarmInformation.alarmClearedTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probablaCause |  |
| perceivedSeverity | M | AlarmInformation.perceivedSeverity | Value shall be "CLEARED" |
| correlatedNotifications | O | The CorrelatedNotification instances related to this AlarmInformation. | This parameter contains references to other AlarmInformation instances whose perceivedSeverity levels are cleared as well. In this way, the perceivedSeverity level of multiple AlarmInformation instances can be cleared by one notification. |
| clearUserId | O | AlarmInformation.clearUserId | This parameter shall be present and contain valid information if the AlarmInformation is cleared by a clearAlarms operation request. |
| clearSystemId | O | AlarmInformation.clearSystemId | This parameter is present if clearUserId is present and if AlarmInformation.clearSystemId contains valid information. |

###### 11.2.1.2.4.3 Triggering event

11.2.1.2.4.3.1 From-state

alarmMatchedAndCleared OR clearedByProvider.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmMatchedAndCleared | The matching-criteria-attributes of the newly generated network alarm have values that are identical (matched) with ones in one AlarmInformation in AlarmList and the perceivedSeverity of the matched AlarmInformation is not Cleared  AND  The perceivedSeverity of the newly generated network alarm is cleared. |
| clearedByProvider | Reception of a valid clearAlarms operation that identifies the subject AlarmInformation instances. This triggering event shall occur regardless of the perceivedSeverity state of the identified AlarmInformation instances. |

11.2.1.2.4.3.2 To-state

alarmInformationCleared\_1 OR alarmInformationCleared\_2.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmInformationCleared\_1 | Case if From-state is alarmMatchedAndCleared:  The following attributes of the subject AlarmInformation are updated:  notificationId, perceivedSeverity (updated to Cleared), alarmClearedTime. |
| alarmInformationCleared\_2 | Case if From-state is clearedByProvider:  The following attributes of the subject AlarmInformation are updated:  notificationId, alarmClearedTime, perceivedSeverity (updated to CLEARED), alarmClearedUserId, alarmClearedSystemId. |

##### 11.2.1.2.5 notifyAckStateChanged

###### 11.2.1.2.5.1 Definition

This notification is generated by the MnS producer when a the acknowledgement state of an alarm changes from "UNACKNOWLEDGED" to "ACKNOWLEDGED" or back from "ACKNOWLEDGED" to "UNACKNOWLEDGED".

###### 11.2.1.2.5.2 Input parameters

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass |  |
| objectInstance | M | MonitoredEntity.objectInstance |  |
| notificationId | M | -- |  |
| notificationType | M | "notifyAckStateChanged" |  |
| eventTime | M | AlarmInformation.ackTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probableCause |  |
| perceivedSeverity | M | AlarmInformation.perceivedSeverity |  |
| ackState | M | AlarmInformation.ackState |  |
| ackUserId | M | AlarmInformation.ackUserId | The identifier of the user who acknowledged or unacknowledged the alarm. |
| ackSystemId | O | AlarmInformation.ackSystemId | The identifier of the system where the acknowledgement or unacknowledgement request was originated. |

###### 11.2.1.2.5.3 Triggering event

11.2.1.2.5.3.1 From-state

ackedByConsumer OR ackedByProvider AND alarmInformationExists.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| ackedByConsumer | Reception of an acknowledgeAlarms operation and a subsequent operation success return. |
| ackedByProvider | Reception of a local (non-standard) acknowlegeAlarms equivalent operation and a subsequent operation success return. |
| alarmInformationExists | The AlarmInformation exists in AlarmList. |

11.2.1.2.5.3.2 To-state

alarmAckStateHasChanged.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmAckStateHasChanged | The AlarmInformation.ackState of the AlarmInformation identified by from-state assertion alarmInformationExists have been updated. Specifically, the following attributes of the subject AlarmInformation are updated:  -- notificationId, ackTime, ackUserId, ackState, ackSystemId. |

##### 11.2.1.2.6 notifyComments

###### 11.2.1.2.6.1 Definition

This notification is generated by the MnS producer when a Comment instance is added to an AlarmInformation instance in the AlarmList.

A MnS producer shall support this notification if it supports the operation setComment.

###### 11.2.1.2.6.2 Input parameters

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass |  |
| objectInstance | M | MonitoredEntity.objectInstance |  |
| notificationId | M | -- |  |
| notificationType | M | "notifyComments" |  |
| eventTime | M | Comment.commentTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | M | AlarmInformation.probableCause |  |
| perceived Severity | M | AlarmInformation.perceivedSeverity |  |
| comments | M | The Comment instances related to this AlarmInformation. |  |

###### 11.2.1.2.6.3 Trigger event

11.2.1.2.6.3.1 From-state

commentedByServiceprovider OR commentedByServiceprovider AND alarmInformationExists.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| commentedByServiceprovider | Reception of a setComment operation and a subsequent operation success return. |
| commentedByServiceprovider | Reception of a local (non-standard) setComment equivalent operation and a subsequent operation success return. |
| alarmInformationExists | The AlarmInformation is in AlarmList. |

11.2.1.2.6.3.2 To-state

commentInserted.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| commentInserted | One Comment has been created and it is involved in a relationship with the AlarmInformation identified by from-state assertion alarmInformationExists. The following attributes of the newly created Comment instance shall be populated:  commentTime, commentText, commentUserId and commentSystemId. |

##### 11.2.1.2.7 notifyPotentialFaultyAlarmList

###### 11.2.1.2.7.1 Definition

This notification is generated by the MnS producer when the MnS producer looses confidence in the integrity of its alarm list.

The MnS producer may then rebuilt the faulty alarm list. When the alarm List is rebuilt or confidence in the existing alarm list is re-established the MnS producer may generate a notifyAlarmListRebuilt notification.

The parameters objectClass and objectInstance are used to specify if the complete alarm list is unreliable or only parts thereof.

The MnS consumer behaviour, on reception of this notifyPotentialFaultyAlarmList notification, is not specified. The authorized consumer behaviour is considered not essential for the specification of the interface itself. However, the following are recommended actions the uthorized consumer should take, in case it receives this notification.

1) The uthorized consumer should not perform any task requiring the integrity of the AlarmInformation identified as faulty or unreliable by the subject notification.

2) The uthorized consumer should not invoke operations that require integrity of the AlarmList such as getAlarmList., acknolwedgeAlarms operations.

###### 11.2.1.2.7.2 Input parameters

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | It identifies  the class of the instance identified by systemDN or  the class of MonitoredEntity. | Identifies, together with the objectInstance parameter, the part of the alarm list that is not reliable.  If this paramter specifies the class of the instance carried in systemDN, then all AlarmInformation instances in the AlarmList may not be reliable.  If this parameter specifies some class represented by MonitoredEntity, then a subset of the AlarmInformation instances in the AlarmList is not reliable. |
| objectInstance | M | It identifies  the instance identified by systemDN or  an instance of MonitoredEntity. | Identifies, together with the objetClass parameter, the part of the alarm list that may not be reliable.  If this parameter is equal to the instance carried in systemDN, then all AlarmInformation instances in the AlarmList may not be reliable.  If this parameter is equal to some instance represented by MonitoredEntity, then only AlarmInformation related to this instance and its descendants may not be reliable. |
| notificationId | M | -- |  |
| notificationType | M | "notifyPotentialFaultyAlarmList" |  |
| eventTime | M | -- | Time when the MnS producer lost confidence in the integrity of the alarm list |
| systemDN | M | -- |  |
| reason | M | "serviceprovider-NE communication error", " serviceprovider restarts", "indeterminate". Other values can be added. | Reason why the MnS producer has to rebuild its AlarmList. |

###### 11.2.1.2.7.3 Trigger event

11.2.1.2.7.3.1 From-state

faultyAlarmListDetected.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| faultyAlarmListDetected | Service provider detects faults in part or whole of its AlarmList. |

11.2.1.2.7.3.2 To-state

faultyAlarmList

|  |  |
| --- | --- |
| Assertion Name | Definition |
| faultyAlarmList | Service provider initiates the AlarmList rebuild process. |

##### 11.2.1.2.8 notifyChangedAlarmGeneral

###### 11.2.1.2.8.1 Definition

This notification is generated by the MnS producer when one or more of the following attributes of an AlarmInformation instance in the AlarmList changes its value: perceivedSeverity, backedUpStatus, backUpObject, trendIndication, thresholdInfo, stateChangeDefinition, monitoredAttributes, proposedRepairActions, additionalText, additionalInformation, serviceUser, serviceProvider or securityAlarmDetector. From the attributes listed above, only those that changed value shall be included in the notification.

The notification parameters depend on the alarmType and are different for non-security and security alarms.

###### 11.2.1.2.8.2 Input parameters for notifications related to non-security alarms

The notifyChangedAlarmGeneral notification is defined by Table 11.2.1.2.8.2-1, if the alarmType is equal to "Communications Alarm", "Processing Error Alarm", "Environmental Alarm",, "Quality Of Service Alarm" or "Equipment Alarm".

Table 11.2.1.2.8.2-1: Input parameters for notifications related to non-security alarms

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass |  |
| objectInstance | M | MonitoredEntity.objectInstance |  |
| notificationId | M | -- |  |
| notificationType | M | "notifyChangedAlarmGeneral" |  |
| eventTime | M | AlarmInformation.alarmChangedTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | O | AlarmInformation.probableCause |  |
| specificProblem | O | AlarmInformation.specificProblem |  |
| perceivedSeverity | O | AlarmInformation.perceivedSeverity |  |
| backedUpStatus | O | AlarmInformation.backedUpStatus |  |
| backUpObject | O | MonitoredEntity.objectInstance | The DN of the back up object. The object is identified by relation-BackUpObject-AlarmInformation of the new AlarmInformation. |
| trendIndication | O | AlarmInformation.trendIndication |  |
| thresholdInfo | O | AlarmInformation.thresholdInfo |  |
| correlatedNotifications | O | Set of CorrelatedNotification related to this AlarmInformation. |  |
| stateChangeDefinition | O | AlarmInformation.stateChange |  |
| monitoredAttributes | O | AlarmInformation.monitoredAttributes |  |
| proposedRepairActions | O | AlarmInformaton.proposedRepairActions |  |
| additionalText | O | AlarmInformation.additionalText |  |
| additionalInformation | O | AlarmInformation.additionalInformation |  |
| rootCauseIndicator | O | alarmInformation.rootCauseIndicator |  |
| changedAlarmAttributes | O | LIST OF SEQUENCE <AttributeName, OldAttributeValue> | The changed alarm attributes (name/value pairs) (with old values). |

###### 11.2.1.2.8.3 Input parameters for notifications related to security alarm

The notifyChangedAlarmGeneral notification is defined by Table 11.2.1.1.4.2a-1, if the alarmType is equal to "Integrity Violation", "Operational Violation", "Physical Violation", "Security Service or Mechanism Violation" or "Time Domain Violation".

Table 11.2.1.2.8.3-1: Input parameters for notifications related to security alarms

| Parameter Name | S | Matching Information/ Information Type / Legal Values | Comment |
| --- | --- | --- | --- |
| objectClass | M | MonitoredEntity.objectClass |  |
| objectInstance | M | MonitoredEntity.objectInstance |  |
| notificationId | M | -- |  |
| notificationType | M | "notifyChangedAlarmGeneral". |  |
| eventTime | M | AlarmInformation.alarmChangedTime |  |
| systemDN | M | -- |  |
| alarmId | M | AlarmInformation.alarmId |  |
| alarmType | M | AlarmInformation.alarmType |  |
| probableCause | O | AlarmInformation.probableCause |  |
| perceivedSeverity | O | AlarmInformation.perceivedSeverity |  |
| correlatedNotifications | O | Set of CorrelatedNotification related to this AlarmInformation. |  |
| additionalText | O | AlarmInformation.additionalText |  |
| additionalInformation | O | AlarmInformation.additionalInformation |  |
| rootCauseIndicator | O | alarmInformation.rootCauseIndicator |  |
| serviceUser | M | AlarmInformation.serviceUser | This may contain no information if the identify of the service-user (requesting the service) is not known. |
| serviceProvider | M | AlarmInformation.serviceProvider | This shall always identify the service-provider receiving a service request, from serviceUser, that provokes the security alarm. |
| securityAlarmDetector | M | AlarmInformation.securityAlarmDetector | This may contain no information if the detector of the security alarm is the serviceProvider. |
| changedAlarmAttributes | O | LIST OF SEQUENCE <AttributeName, OldAttributeValue> | The changed alarm attributes (name/value pairs) (with old values). |

###### 11.2.1.2.8.4 Trigger event

11.2.1.2.8.4.1 From-state

alarmMatched AND alarmNotCleared AND alarmChanged.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| alarmMatched | The matching-criteria-attributes of the newly generated network alarm has values that are identical (matches) with ones in one AlarmInformation in AlarmList. |
| alarmChanged | One or more of perceivedSeverity, backedUpStatus, backUpObject, trendIndication, thresholdInfo, stateChangeDefinition, monitoredAttributes, proposedRepairActions, additionalText, additionalInformation, serviceUser, serviceProvider or securityAlarmDetector of the newly generated network alarm and of the matched AlarmInformation are different. |

11.2.1.2.8.4.2 To-state

informationUpdate.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| informationUpdate | The AlarmInformation identified in alarmMatched in from-state has been updated according to the following rules: perceivedSeverity, backedUpStatus, backUpObject, trendIndication, thresholdInfo, stateChangeDefinition, monitoredAttributes, proposedRepairActions, additionalText, additionalInformation, serviceUser, serviceProvider or securityAlarmDetector is updated;  notificationId is updated;  alarmChangedTime is updated;  ackTime, ackUserId and ackSystemId are updated to contain no information;  ackState is updated to "unacknowledged"; |

### 11.2.2 Managed information

#### 11.2.2.1 Alarm information, alarm state change and Information Object Classes

##### 11.2.2.1.1 Imported information entities and local labels

None.

##### 11.2.2.1.2 Class diagram

###### 11.2.2.1.2.1 Introduction

This clause introduces the fault supervision related classes (i.e. IOCs, SupportIOCs). The intent is to identify the information required for the Fault management service implementation of its operations and notification emission. This clause provides the overview of all support object classes in UML. Subsequent clauses provide more detailed specification of various aspects of these support object classes.

###### 11.2.2.1.2.2 Attributes and relationships



##### 11.2.2.1.3 Information Object Class Definitions

###### 11.2.2.1.3.1 AlarmInformation

11.2.2.1.3.1.1 Definition

AlarmInformation contains information about alarm conditions of an alarmed MonitoredEntity.

A MnS producer is related to at most one AlarmList. The MnS producer assigns an identifier, called alarmId, to each AlarmInformation in the AlarmList. An alarmId unambiguously identifies one AlarmInformation in the AlarmList.

11.2.2.1.3.1.2 Attribute

|  |  |
| --- | --- |
| **Attribute name** | **S** |
| alarmId | M |
| objectClass/objectInstance (attribute related to role) | M |
| notificationId | M |
| alarmRaisedTime | M |
| alarmChangedTime | O |
| alarmClearedTime | M |
| alarmType | M |
| probableCause | M |
| specificProblem | O |
| perceivedSeverity | M |
| backedUpStatus | O |
| backUpObject (attribute related to role) | O |
| trendIndication | O |
| thresholdInfo | O |
| correlatedNotifications (attribute related to role) | O |
| stateChangeDefinition | O |
| monitoredAttributes | O |
| proposedRepairActions | O |
| additionalText | O |
| additionalInformation | O(see note 3) |
| rootCauseIndicator | O |
| ackTime | M |
| ackUserId | M |
| ackSystemId | O |
| ackState | M |
| clearUserId | O (see note 1) |
| clearSystemId | O (see note 1) |
| serviceUser | O (see note 2) |
| serviceProvider | O (see note 2) |
| securityAlarmDetector | O (see note 2) |
| NOTE 1: These attributes and qualifiers are applicable only if the management service producer supports clearAlarms() (they are absent if clearAlarms() is not supported).  NOTE 2: These attributes are supported if the management service producer emits notifyNewAlarm that carries security alarm information.  NOTE 3: This attribute is optionally populated whenever vendor specific attributes are needed. | |

11.2.2.1.3.1.3 State diagram

Alarms have states. The alarm state information is captured in AlarmInformation in AlarmList.

The solid circle icon represents the Start State. The double circle icon represents the End State. In this state, the alarm is Cleared and acknowledged. The AlarmInformation shall not be accessible via the Service interface and is removed from the AlarmList.

Note the state diagram uses " X / Y ^ Z " to label the arc that indicates state transition. The meanings of X, Y and Z are:

- X identifies the triggering event;

- Y identifies the action of FaultSupervision MnS producer because of the triggering event;

- Z is the notification to be emitted by FaultSupervision MnS producer because of the triggering event.

Note that acknowledgeAlarm^notifyAckStateChanged and the unacknowledgeAlarm^notifyAckStateChanged refer to cases when the request of the management service consumer is successful for the AlarmInformation concerned. They do not refer to the cases when the request is a failure since in the failure cases, no state transition would occur.

Note that, to reduce cluttering to the diagram, the setComment^notifyComment is not included in the figure . One transition should be applied from unack&unclear to itself. Similarly, another transition should be applied from ack&unclear to itself. Another one is from unack&clear to itself.

"PS" used in the state diagram stands for "perceived severity".

Figure 11.2.2.1.3.1.3-1 is used if it supports ^notifyChangedAlarm and Figure 11.2.2.1.3.1.3-2 is used if it does not support ^notifyChangedAlarm.



Figure 11.2.2.1.3.1.3-1 notifyChangedAlarm supported



Figure 11.2.2.1.3.1.3-2 notifyChangedAlarm not supported

###### 11.2.2.1.3.2 AlarmList

11.2.2.1.3.2.1 Definition

The MnS producer maintains an AlarmList that contains currently active alarms (i.e. AlarmInformation whose perceivedSeverity is not Cleared) and alarms that are Cleared but not yet acknowledged.

11.2.2.1.3.2.2 Attribute

There is no additional attribute defined for this class besides those inherited.

###### 11.2.2.1.3.3 FSMnSProducer

11.2.2.1.3.3.1 Definition

FSMnSProducer is the representation of the entity who provides the fault supervision management service(s) and contains the AlarmList.

11.2.2.1.3.3.2 Attribute

There is no additional attribute defined for this class besides those inherited.

11.2.2.1.3.3.3 Notification Table

| **Name** | **S** | **Notes** |
| --- | --- | --- |
| notifyAlarmListRebuilt | M |  |
| notifyPotentialFaultyAlarmList | O | . |

###### 11.2.2.1.3.4 Comment

11.2.2.1.3.4.1 Definition

Comment contains commentary and associated information such as the time when the commentary is made.

11.2.2.1.3.4.2 Attribute

|  |  |
| --- | --- |
| **Attribute Name** | **S** |
| commentTime | M |
| commentUserId | M |
| commentSystemId | O |
| commentText | M |

###### 11.2.2.1.3.5 CorrelatedNotification

11.2.2.1.3.5.1 Definition

The sourceObjectInstance attribute of CorrelatedNotification identifies one MonitoredEntity. For the MonitoredEntity identified, a set of notification identifiers is also identified. One or more CorrelatedNotification instances can be related to an AlarmInformation. In this case, the information of the AlarmInformation is said to be correlated to information carried in the notifications identified by the CorrelatedNotification instances. See further definition of correlated notification in ITU-T Recommendation X.733 [4], clause 8.1.2.9.

The notification identified by the CorrelatedNotification, as defined in ITU-T and used here, can carry all types of information and is not restricted to carrying alarm information only. For example, a notification, identified by the CorrelatedNotification, can indicate a managed instance attribute value change. In this case, the information of the AlarmInformation is said to be correlated to the managed instance attribute value change event.

The meaning of correlation is dependent on the type of notification itself. See the comment column of the correlatedNotification input parameter for each type of notification, such as notifyNewAlarm.

Notification carries AlarmInformation. The AlarmInformation instances referred to by the correlatedNotification may or may not exist in the AlarmList. For example, the AlarmInformation carried by the identified notification may have been acknowledged and Cleared and therefore, no longer exist in the AlarmList.

11.2.2.1.3.5.2 Attribute

|  |  |
| --- | --- |
| **Attribute Name** | **S** |
| sourceObjectInstance | M |
| notificationIdSet | M |

###### 11.2.2.1.3.6 MonitoredEntity

11.2.2.1.3.6.1 Definition

It represents classes that can have an alarmed state. The types of classes that can have alarmed state are:

a) All classes whose Notification Tables include alarm notifications.

b) VSE subclass of 3GPP defined classes and VSE defined classes that can have alarmed state.

The objectClass and objectInstance of this class identifies an instance of this class. The AlarmInformation uses this information in two places. In one place, the information is used to identify the instance that is in alarmed state. In another place, the information is used to identify an instance that can be used as the back up network resource for the instance that is in alarmed state.

11.2.2.1.3.6.2 Attribute

There is no attribute for this class.

##### 11.2.2.1.4 Information relationships definition

###### 11.2.2.1.4.1 relation-FSMnSProducer-AlarmList (M)

11.2.2.1.4.1.1 Definition

This represents the relationship between FSMnSProducer and AlarmList.

11.2.2.1.4.1.2 Role

There is no role defined for this relationship.

11.2.2.1.4.1.3 Constraint

There is no constraint for this relationship.

###### 11.2.2.1.4.2 relation-AlarmList-AlarmInformation (M)

11.2.2.1.4.2.1 Definition

This represents the relationship between AlarmList and AlarmInformation.

11.2.2.1.4.2.2 Role

|  |  |
| --- | --- |
| **Name** | **Definition** |
| identifyAlarmInformation | It represents a capability to obtain the information contained in AlarmInformation. |

11.2.2.1.4.2.3 Constraint

|  |  |
| --- | --- |
| **Name** | **Definition** |
| inv\_ hasAlarmInformation1 | No AlarmInformation playing the role of theAlarmInformation shall have its perceivedSeverity = "cleared" and its ackState = "acknowledged". |
| inv\_ hasAlarmInformation2 | The alarmId of all AlarmInformation instances playing the role of theAlarmInformation are distinct. |

###### 11.2.2.1.4.3 relation-AlarmInformation-Comment (M)

11.2.2.1.4.3.1 Definition

This represents the relationship between AlarmInformation and Comment.

11.2.2.1.4.3.2 Role

|  |  |
| --- | --- |
| **Name** | **Definition** |
| comment | It represents a capability to obtain the information contained in Comment. |

11.2.2.1.4.3.3 Constraint

There is no constraint.

###### 11.2.2.1.4.4 relation-AlarmInformation-CorrelatedNotification (M)

11.2.2.1.4.4.1 Definition

This represents the relationship between AlarmInformation and CorrelatedNotification.

11.2.2.1.4.4.2 Role

|  |  |
| --- | --- |
| **Name** | **Definition** |
| correlatedNotification | It represents a capability to obtain the information contained in CorrelatedNotification. |

11.2.1.4.4.3 Constraint

There is no constraint.

###### 11.2.2.1.4.5 relation-AlarmedObject-AlarmInformation (M)

11.2.2.1.4.5.1 Definition

This represents the relationship between MonitoredEntity and AlarmInformation.

11.2.2.1.4.5.2 Role

|  |  |
| --- | --- |
| **Name** | **Definition** |
| objectClass/objectInstance | It represents the capability to obtain the identification, in terms of objectClass and objectInstance, of alarmed network resource. |

11.2.2.1.4.5.3 Constraint

|  |  |
| --- | --- |
| **Name** | **Definition** |
| inv\_relation-AI-ME | All AlarmInformation involved in this relationship with the same MonitoredEntity shall have at least one different value in the following attributes: alarmType, probableCause and specificProblem. |

###### 11.2.2.1.4.6 relation-backUpObject-AlarmInformation (O)

11.2.2.1.4.6.1 Definition

The relationship represents the relationship between AlarmInformation and the backUpObject.

11.2.2.1.4.6.2 Role

|  |  |
| --- | --- |
| **Name** | **Definition** |
| backUpObject | It represents a capability to obtain the identification, in terms of objectClass and objectInstance, of the backUpObject. |

11.2.2.1.4.6.3 Constraint

|  |  |
| --- | --- |
| **Name** | **Definition** |
| inv\_identifyBackUpObject | This relationship is present if and only if the AlarmInformation.backedUpStatus attribute is present and is indicating true. |

##### 11.2.2.1.5 Information attribute definition

###### 11.2.2.1.5.1 Definition and legal values

| **Name** | **Definition** | **Legal Values** |
| --- | --- | --- |
| alarmId | It identifies one AlarmInformation in the AlarmList. |  |
| notificationId | It identifies the notification that carries the AlarmInformation. |  |
| alarmRaisedTime | It indicates the date and time when the alarm is first raised by the alarmed resource. | All values indicating valid date and time. |
| alarmChangedTime | It indicates the last date and time when the AlarmInformation is changed by the alarmed resource. Changes to AlarmInformation caused by invocations of the management service consumer would not change this date and time. | All values indicating valid date and time. |
| alarmClearedTime | It indicates the date and time when the alarm is cleared. | All values indicating valid date and time. |
| alarmType | It indicates the type of alarm.  Communications Alarm:  An alarm of this type is associated with the procedure and/or process required conveying information from one point to another (ITU-T Recommendation X.733 [x]).  Processing Error Alarm:  An alarm of this type is associated with a software or processing fault (ITU T Recommendation X.733 [x]).  Environmental Alarm:  An alarm of this type is associated with a condition related to an enclosure in which the equipment resides (ITU-T Recommendation X.733 [x]).  Quality of Service Alarm:  An alarm of this type is associated with degradation in the quality of a service (ITU T Recommendation X.733 [x]).  Equipment Alarm:  An alarm of this type is associated with an equipment fault (ITU-T Recommendation X.733 [x]).  Integrity Violation:  An indication that information may have been illegally modified, inserted or deleted.  Operational Violation:  An indication that the provision of the requested service was not possible due to the unavailability, malfunction or incorrect invocation of the service.  Physical Violation:  An indication that a physical resource has been violated in a way that suggests a security attack.  Security Service or Mechanism Violation:  An indication that a security attack has been detected by a security service or mechanism.  Time Domain Violation: An indication that an event has occurred at an unexpected or prohibited time. |  |
| probableCause | It qualifies alarm and provides further information than alarmType. Probable causes are ouside the scope of the present document. |  |
| specificProblem | It provides further refinement to the probableCause. This attribute value shall be single-valued and of simple type such as integer or string. See definition in ITU-T Recommendation X.733 [4] clause 8.1.2.2. | Provided by vendor. |
| perceivedSeverity | It indicates the relative level of urgency for operator attention. | Critical, Major, Minor, Warning, Indeterminate, Cleared: see ITU-T Recommendation X.733 [4]. The present document does not recommend the use of indeterminate. |
| backedUpStatus | It indicates if an object (the MonitoredEntity) has a back up. See definition in ITU-T Recommendation X.733 [4] clause 8.1.2.4. | All values that carry the semantics of backedUpStatus defined by ITU-T X.733 [4] clause 8.1.2.4. |
| trendIndication | It indicates if some observed condition is getting better, worse, or not changing. | "Less severe", "no change", "more severe": see definition in ITU-T Recommendation X.733 [4] clause 8.1.2.6. |
| thresholdInfo | It indicates the crossed threshold information such as:  - The identifier of the monitored attribute whose value has crossed a threshold,  - The threshold settings,  - The observed value that have crossed a threshold, etc.  See definition in ITU-T Recommendation X.733 [4] clause 8.1.2.7. See also for information in TS 32.401 [19] clause 5.6. |  |
| stateChangeDefinition | It indicates attribute value changes associated with the alarm for state attributes of the monitored entity (state transitions). The change is reported with the name of the state attribute, the new value and an optional old value. See definition in ITU-T Recommendation X.733 [4] clause 8.1.2.11. |  |
| monitoredAttributes | It indicates attributes of the monitored entity and their values at the time the alarm occurred that are of interest for the alarm report. How these attributes are chosen is outside of the scope of the present document. See definition in ITU-T Recommendation X.733 [4] clause 8.1.2.11. |  |
| proposedRepairActions | Used if the cause is known and the system being managed can suggest one or more solutions to fix the problem causing the alarm as defined in ITU-T Rec. X. 733 [4] |  |
| additionalText | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4]. | N/A |
| additionalInformation | This attribute when present allows the inclusion of a set of vendor specific alarm information in the alarm.  A specific condition for this optional population is when an alarm presented by the Management System (e.g. via the user interface) has different values of perceived severity, and / or alarm type, compared with the values presented to the Itf-N.  Any other uses of additional information on the alarm and its semantics is outside the scope of the present document | The additional information field is a list of one or more information parts.  The present document allows the support of two such information parts to carry  - vendor defined perceived severity  - vendor defined alarm type  using defined identification.  Other vendor specific information parts are allowed by using vendor specific identifications. |
| rootCauseIndicator | It indicates that this AlarmInformation is the root cause of the events captured by the notifications whose identifiers are in the related CorrelatedNotification instances. | boolean |
| ackTime | It identifies the time when the alarm has been acknowledged or unacknowledged the last time, i.e. it registers the time when ackState changes. | All values that indicate valid time that are later than that carried in alarmRaisedTime. |
| ackUserId | It identifies the last user who has changed the acknowledgement state. | It can be used to identify the human operator such as "John Smith" or it can identify a group, such as "Team Six", or it can contain no information such as "". |
| ackSystemId | It identifies the system that last changed the ackState of an alarm, i.e. acknowledged or unacknowledged the alarm. | It can be used to identify the system, such as "system 6" or it can contain no information such as "". |
| ackState | It identifies the acknowledgement state of an alarm. | Acknowledged: the alarm has been acknowledged.  Unacknowledged: the alarm has been unacknowledged or the alarm has never been acknowledged. |
| commentTime | It carries the time when the comment has been added to the alarm. |  |
| commentText | It carries the textual comment. |  |
| commentUserId | It carries the identification of the user who made the comment. |  |
| commentSystemId | It carries the identification of the system (Management System) from which the comment is made. That system supports the user that made the comment. |  |
| clearUserId | It carries the identity of the user who invokes the clearAlarms operation. | It can be used to identify the human operator such as "John Smith" or it can identify a group, such as "Team Six", or it can contain no information such as "". |
| clearSystemId | It carries the identity of the system in consuming the fault management service. That management service consumer supports the user who invokes the clearAlarms(). | It can be used to identify the system, such as "system 6" or it can contain no information such as "". |
| serviceUser | It identifies the service-user whose request for service provided by the serviceProvider led to the generation of the security alarm. | This attribute may carry no information if the server user is not identifiable. |
| serviceProvider | It identifies the service-provider whose service is requested by the serviceUser and the service request provokes the generation of the security alarm. |  |
| securityAlarmDetector | It carries the identity of the detector of the security alarm. | This attribute may carry no information if the security alarm detector is not identifiable. |
| sourceObjectInstance | It identifies one MonitoredEntity. | All values that carry the semantics of DN. |
| notificationIdSet | It carries one or more notification identifiers. |  |

###### 11.2.2.1.5.2 Constraints

|  |  |
| --- | --- |
| **Name** | **Definition** |
| inv\_alarmChangedTime | Time indicated shall be later than that carried in alarmRaisedTime. |
| inv\_alarmClearedTime | Time indicated shall be later than that carried in alarmRaisedTime. |
| inv\_ackTime | Time indicated shall be later than that carried in alarmRaisedTime. |
| inv\_notificationId | NotificationIds shall be chosen to be unique across all notifications of a particular Managed Object throughout the time that alarm correlation is significant. The algorithm by which alarm correlation is accomplished is outside the scope of the present document. |

#### 11.2.2.2 Subscription information, subscription state and Information Object Classes

##### 11.2.2.2.1 Imported information entities and local labels

None.

##### 11.2.2.2.2 Class Diagram

###### 11.2.2.2.2.1 Attributes and relationships

This clause depicts the set of Support IOCs that encapsulate information within the notification IRP. The intent is to identify the information required for the notification IRP implementation of its operations and notification emission. This clause provides the overview of all Support IOCs in UML. Subsequent clauses provide more detailed specification of various aspects of these Support IOCs.



###### 11.2.2.2.2.2 Inheritance

This clause depicts the inheritance relationships that exist between Support IOCs.



##### 11.2.2.2.3 Information object classes definition

###### 11.2.2.2.3.1 NtfSubscriber

11.2.2.2.3.1.1 Definition

This Support IOC represents a Subscriber from a notification perspective: a subscriber is fully identified by a management service consumer reference. A management service consumer using multiple management service consumer reference attributes to subscribe will result in multiple NtfSubscriber instances.

11.2.2.2.3.1.2 Attributes

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Support Qualifier | Read Qualifier | Write Qualifier |
| ntfConsumerReference | M | M | M |

###### 11.2.2.2.3.2 NtfSubscription

11.2.2.2.3.2.1 Definition

This Support IOC represents a subscription that has been requested by a management service consumer and created.

11.2.2.2.3.2.2 Attributes

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Support Qualifier | Read Qualifier | Write Qualifier |
| ntfSubscriptionId | M | M | - |
| ntfSubscriptionState | M | M | M |
| ntfTimeTick | M | M | M |
| ntfTimeTickTimer | M | - | - |
| ntfNotificationCategorySet | M | M | M |
| ntfFilter | M | M | M |

11.2.2.2.3.2.3 Void

###### 11.2.2.2.3.3 NotificationIRP

11.2.2.2.3.3.1 Definition

This Support IOC represents a notification IRP. It inherits from Support IOC ManagedGenericIRP.

##### 11.2.2.2.4 Information relationship definitions

###### 11.2.2.2.4.1 relation-ntfSubscriber-ntfSubscription (M)

11.2.2.2.4.1.1 Definition

This relationship defines the relationship between a NtfSubscriber and its current subscriptions.

11.2.2.2.4.1.2 Roles

|  |  |
| --- | --- |
| Name | Definition |
| theNtfSubscriber | This role represents the one who has subscribed. It can be played by instances of Support IOC NtfSubscriber |
| theNtfSubscription | This role represents the subscriptions which were made and not unsubscribed. It can be played by instances of Support IOC NtfSubscription |

11.2.2.2.4.1.3 Constraints

|  |  |
| --- | --- |
| Name | Definition |
| inv\_notificationCategoriesAllDistinct | The notification categories contained in the ntfNotificationCategorySet attribute of NtfSubscription playing the role theNtfSubscription are all distinct from each other. |

###### 11.2.2.2.4.2 relation-ntfIRP-ntfSubscriber (M)

11.2.2.2.4.2.1 Definition

This relationship defines the relationship between the NotificationIRP and the current subscribers of notifications.

11.2.2.2.4.2.2 Roles

|  |  |
| --- | --- |
| Name | Definition |
| theNtfSubscriber | This role represents the entities to which IRPAgent will notify events. It is played by instances of Support IOC NtfSubscriber |
| theNotificationIRP | This role represents the NotificationIRP to which an IRPManager has subscribed. It is played by instances of Support IOC NotificationIRP |

11.2.2.2.4.2.3 Constraints

|  |  |
| --- | --- |
| Name | Definition |
| inv\_uniqueManagerReference | All NtfSubscriber involved in the subscriptionRegistration relationship are distinguished from each other by their ntfManagerReference Attribute. |

##### 11.2.2.2.5 Information attribute definitions

###### 11.2.2.2.5.0 Introduction

This clause defines the semantics of the Attributes used in Support IOCs.

###### 11.2.2.2.5.1 Definitions and legal values

| Attribute Name | Definition | Legal Values |
| --- | --- | --- |
| ntfSubscriptionId | It identifies uniquely a subscription | N/A |
| ntfSubscriptionState | It indicates the activation state of a subscription | "suspended": the subscription is suspended  "notSuspended": the subscription is active |
| ntfTimeTick | This attribute represents the initial value of ntfTimeTickTimer. It is in unit of whole minute. This value defines a time window within which management service consumer intends to invoke getSubscriptionStatus (or subscribe) operation to confirm its subscription. A special value indicates infinity which is such that timer will never expire and management service producer needs other means to decide when to delete resources allocated to the management service consumer | Integer greater or equal to 15, OR special infinite value |
| ntfTimeTickTimer | This attribute represents the current value of a timer | integer greater or equal to zero |
| ntfNotificationCategorySet | This attribute represents a set of notification categories (see also Definition of notification category in clause 3.1) |  |
| ntfFilter | This attribute represents the filter of a subscription. The filter can be applied to parameters of notification header (see Notificationmaanagement service producer interface) and to parameters of notifications defined as filterable to  IManagement service producer shall notifymanagement service consumer if the event satisfies the filter constraint. |  |
| ntfConsumerReference | This attribute contains the reference of a consumer. It uniquely identifies a subscriber |  |

###### 11.2.2.2.5.2 Constraints

- "ntfTimeTickTimer is lower.

## 11.3 Generic performance assurance management service

### 11.3.1 Operations and notifications

#### 11.3.1.1 Void

#### 11.3.1.2 Operation and notification of performance threshold monitoring service

##### 11.3.1.2.1 Notification notifyThresholdCrossing (M)

###### 11.3.1.2.1.1 Definition

This notification supports the threshold monitoring notification target to be notified when the performance threshold is crossed or reached.

###### 11.3.1.2.1.2 Notification information

| **Parameter Name** | **S** | **Information Type** | **Comment** |
| --- | --- | --- | --- |
| objectClass | M | ManagedEntity.objectClass | Class of the managed object, where the threshold crossing occurred. |
| objectInstance | M | ManagedEntity.objectInstance | Instance of the managed object, where the threshold crossing occurred. |
| notificationId | M | -- |  |
| notificationType | M, Y | "notifyThresholdCrossing " |  |
| eventTime | M, Y | -- | Time when the threshold crossing occurred. |
| systemDN | M | -- |  |
| observedPerfMetricName | M | ThresholdMonitor.thresholdInfoList[x].\  performanceMetrics[y] | Name of the performance metric that has crossed the threshold |
| observedPerfMetricValue | M | -- | Value of the performance metric, that has crossed the threshold, when the threshold crossing was observed |
| observedPerfMetricDirection | M | -- | Direction ("UP" or "DOWN") of the performance metric, when the threshold crossing was observed |
| thresholdValue | M | ThresholdMonitor.thresholdInfoList[x].\  thresholdvalue | Threshold value of the triggered threshold |
| hysteresis | M | ThresholdMonitor.thresholdInfoList[x].\  hysteresis | Hysteresis of the triggered threshold |
| monitorGranularityPeriod | M | ThresholdMonitor.monitorGranularityPeriod | Granularity period of the threshold monitor |
| additionalText | O | -- | Vendor specific information |

### 11.3.2 Managed information

#### 11.3.2.1 Performance data file definition

##### 11.3.2.1.1 File generation and reporting

The performance data reporting related service producer generates the performance date file(s) for the consumer(s) and emits the "notifyFileReady" or "notifyFilePreparationError" notifications to the subject consumer(s) who have subscribed to these notifications.

How the measurement job control related service producer provides the measurement results to the performance data reporting related service producer is out of scope of the present specification.

The performance data reporting related service producer shall be able to allow the consumer to access the file using the following file transfer protocols, and the performance data reporting related service producer shall always act as the server while the consumer shall always act as the initiator (client) of file transfer actions:

- FTP;

- SFTP.

##### 11.3.2.1.2 Performance data file content description

Table 11.3.2.1.2-1 lists all the file content items. It also provides an explanation of the individual items.

Table 11.3.2.1.2-1: File Content Description

| File Content Item | Description |
| --- | --- |
| measDataCollection | This is the top-level tag, which identifies the file as a collection of measurement data. The file content is made up of a header ("measFileHeader"), the collection of measurement result items ("measData"), and a measurement file footer ("measFileFooter"). |
| measFileHeader | This is the measurement result file header to be inserted in each file. It includes a version indicator, the name, type and vendor name of the sending service producer, and a time stamp ("collectionBeginTime"). |
| measData | The "measData" construct represents the sequence of zero or more measurement result items contained in the file. It can be empty in case no measurement data can be provided. The individual "measData" elements can appear in any order.  Each "measData" element contains the identifier of the measured entity ("measuredEntityId") and the list of measurement results pertaining to that measured entity ("measInfo"). |
| measFileFooter | The measurement result file footer to be inserted in each file. It includes a time stamp, which refers to the end of the overall measurement collection interval that is covered by the collected measurement results being stored in this file. |
| fileFormatVersion | This parameter identifies the file format version applied by the sender. The format version defined in the present document shall be the abridged number and version of this 3GPP document (see below).  The abridged number and version of a 3GPP document is constructed from its version specific full reference "3GPP […] (yyyy-mm)" by:  - removing the leading "3GPP TS";  - removing everything including and after the version third digit, representing editorial only changes, together with its preceding dot character;  - from the resulting string, removing leading and trailing white space, replacing every multi character white space by a single space character and changing the case of all characters to uppercase. |
| senderName | The senderName uniquely identifies performance data reporting related service producer that assembled this measurement file. |
| senderType | This is a user configurable identifier of the type of performance data reporting related service producer that generated the file, e.g. NF performance data reporting service producer, or NSI performance data reporting service producer. The string may be empty (i.e. string size =0) in case the "senderType" is not configured in the sender. |
| vendorName | The "vendorName" identifies the vendor of the performance data reporting related service producer that provided the measurement file. The string may be empty (i.e. string size =0) if the "vendorName" is not configured in the sender. |
| collectionBeginTime | The "collectionBeginTime" is a time stamp that refers to the start of the first measurement collection interval (granularity period) that is covered by the collected measurement results that are stored in this file. |
| measuredEntityUserName | This is the user definable name ("userLabel") defined for the measured entity in 3GPP TS 28.622 [11]. The string may be empty (i.e. string size =0) if the "measuredEntityUserName" is not configured in the CM applications. |
| measuredEntityDn | This is the Distinguished Name (DN) defined for the measured entity in 3GPP TS 32.300 [25]. It is unique across an operator's network. The string may be empty (i.e. string size =0) if the "measuredEntityDn" is not configured in the CM applications. |
| measuredEntitySoftwareVersion | This is the software version ("swVersion") defined for the measured entity in 3GPP TS 28.622 [11]. This is an optional parameter which allows post-processing systems to take care of vendor specific measurements modified between software versions. |
| measInfo | The sequence of measurements, values and related information. It includes a list of measurement types ("measTypes") and the corresponding results ("measValues"), together with the time stamp ("measTimeStamp") and granularity period ("granularityPeriod") pertaining to these measurements. |
| measInfoId | This attribute associates a tag name with the set of measurements defined by a *measInfo* property. This is an optional parameter that may be used to assign unique names to categories of measurements grouped together by measInfo elements. It allows parsing tools to easily isolate measurement sets by name. |
| measTimeStamp | Time stamp referring to the end of the granularity period. |
| jobId | The "jobId" is an optional item represents the measurement job with which measurement result contained in the file is associated. |
| granularityPeriod | Granularity period of the measurement(s) in seconds. |
| reportingPeriod | Reporting period of the measurement(s) in seconds. |
| measTypes | This is the list of measurement types for which the following, analogous list of measurement values ("measValues") pertains. |
| measValues | This parameter contains the list of measurement results for the resource being measured, e.g. trunk, cell. It includes an identifier of the resource ("measObjInstId"), the list of measurement result values ("measResults") and a flag that indicates whether the data is reliable ("suspectFlag"). |
| measObjInstId | In case the measEntity is a ManagedElement, the "measObjInstId" field contains the local distinguished name (LDN) of the measured object within the scope defined by the "measuredEntityDn" (see 3GPP TS 32.300 [25]). The concatenation of the "measuredEntityDn" and the "measObjInstId" yields the DN of the measured object. The "measObjInstId" is therefore empty if the "measuredEntityDn" already specifies completely the DN of the measured object, which is the case for all measurements specified on measured entity (e.g., NF) level. For example, if the measured object is a "ManagedElement" representing RNC "RNC-Gbg-1", then the "measuredEntityDn" will be for instance "DC=a1.companyNN.com,SubNetwork=1,IRPAgent=1,SubNetwork=CountryNN,MeContext=MEC-Gbg-1,ManagedElement=RNC-Gbg-1", and the "measObjInstId" will be empty. On the other hand, if the measured object is a "UtranCell" representing cell "Gbg-997" managed by that RNC, then the "measuredEntityDn" will be for instance the same as above, i.e. "DC=a1.companyNN.com,SubNetwork=1,IRPAgent=1,SubNetwork=CountryNN,MeContext=MEC-Gbg-1,ManagedElement=RNC-Gbg-1", and the "measObjInstId" will be for instance "RncFunction=RF-1,UtranCell=Gbg-997". The class of the "measObjInstId" is defined in item F of each measurement definition template.  In case the measEntity is not a ManagedElement, the value of this attribute is empty (i.e. string size =0). |
| measResults | This parameter contains the sequence of result values for the observed measurement types. The "measResults" sequence shall have the same number of elements, which follow the same order as the measTypes sequence. The NULL value is reserved to indicate that the measurement item is not applicable or could not be retrieved for the object instance. |
| suspectFlag | Used as an indication of quality of the scanned data. FALSE in the case of reliable data, TRUE if not reliable. The default value is "FALSE", in case the suspect flag has its default value it may be omitted. |
| timestamp | This tag carries the time stamp that refers to the end of the measurement collection interval (granularity period) that is covered by the collected measurement results that are stored in this file. The minimum required information within timestamp is year, month, day, hour, minute, and second. |

The measInfo contains the sequence of measurements, values and related information, in a table-oriented structure.

The representation of all timestamps in PM files shall follow the representations allowed by the ISO 8601 [20].   
The precise format for timestamp representation shall be determined by the technology used for encoding the PM file (e.g. ASN.1, XML DTD, and XML Schema). The choice of technology should ensure that this representation is derived from ISO 8601 [20]. Based on the representation used, the timestamp shall refer to either UTC time or local time or local time with offset from UTC.

##### 11.3.2.1.3 File naming convention

###### 11.3.2.1.3.1 Generic file naming convention

The following generic convention shall be applied for naming the files containing different management data:

<managementData\_type><file\_ready\_date>< file\_ready\_time><file\_expiration\_delta\_time>  
[<specificData\_extension>][<separator><RC>]

1) The managementData\_type field is the type of the management data contained in the file, the value of managementData\_type field including:

"PM" for performance data files,

2) The file\_ready\_date field is of the form YYYYMMDD, where:

- YYYY is the year in four-digit notation;

- MM is the month in two digit notation (01 - 12);

- DD is the day in two digit notation (01 - 31).

The file\_ready\_date is the date when the file was last closed and made available for upload and the file content will not be changed.

3) The file\_ready\_time field is of the form HHMMshhmm, where:

- HH is the two digit hour of the day (local time), based on 24 hour clock (00 - 23);

- MM is the two digit minute of the hour (local time, 00 - 59);

- s is the sign of the local time differential from UTC (+ or -), in case the time differential to UTC is 0 then the sign may be arbitrarily set to "+" or "-";

- hh is the two digit number of hours of the local time differential from UTC (00 - 23);

- mm is the two digit number of minutes of the local time differential from UTC (00 - 59).

The file\_ready\_time is the time when the file was last closed and made available for upload and the file content will not be changed.

4) To reduce length of the file name, the file\_expiration\_delta\_time field could be a delta time interval from file ready time. The unit is hour.

5) The specificData\_extension field is used to extend the extra file naming convention for a specific type of management data.

6) The RC parameter is a running count, starting with the value of "1", and shall be appended only if the filename is not unique, i.e. more than one file is generated and all other parameters of the file name are identical.

7) The separator field is "\_-\_", which is an underscore character (\_), followed by a minus character (-), followed by an underscore character (\_).

###### 11.3.2.1.3.2 Performance data file specific extension

The following convention defined as <specificData\_extension> of the generic file naming convention (as defined annex A.3.1) shall be applied for performance data file naming:

<Type><Startdate>.<Starttime>-[<Enddate>.]<Endtime>[\_-<jobIdList>][\_<UniqueId>][\_-\_<RC>]

1) The Type field indicates if the file contains measurement results for single or multiple measured objects and/or granularity periods where:

- "A" means single measured object, single granularity period (this is used when granularity period is equal to reporting period);

- "B" indicates multiple measured objects, single granularity period (this is used when granularity period is equal to reporting period);

- "C" signifies single measured object, multiple granularity periods (this is used when reporting period is multiples of the granularity period and will contain multiple measurement reports);

- "D" stands for multiple measured objects, multiple granularity periods (this is used when reporting period is multiples of the granularity period and will contain multiple measurement reports).

2) The Startdate field indicates the date when the granularity period began if the Type field is set to A or B. If the Type field is either "C" or "D" then Startdate contains the date when the first granularity period of the measurement results contained in the file started. The Startdate field is of the form YYYYMMDD, where:

- YYYY is the year in four-digit notation;

- MM is the month in two digit notation (01 - 12);

- DD is the day in two-digit notation (01 - 31).

3) The Starttime field indicates the time when the granularity period began if the Type field is set to A or B. If the Type field is either "C" or "D" then Starttime contains the time when the first granularity period of the measurement results contained in the file began. The Starttime field is of the form HHMMshhmm, where:

- HH is the two-digit hour of the day (local time), based on 24-hour clock (00 - 23);

- MM is the two digit minute of the hour (local time), possible values are 00, 05, 10, 15, 20, 25, 30, 35, 40, 45, 50, and 55;

- s is the sign of the local time differential from UTC (+ or -), in case the time differential to UTC is 0 then the sign may be arbitrarily set to "+" or "-";

- hh is the two-digit number of hours of the local time differential from UTC (00-23);

- mm is the two digit number of minutes of the local time differential from UTC (00-59).

4) The Enddate field shall only be included if the Type field is set to "C" or "D", i.e. measurement results for multiple granularity periods are contained in the file. It identifies the date when the last granularity period of these measurements ended, and its structure corresponds to the Startdate field.

5) The Endtime field indicates the time when the granularity period ended if the Type field is set to A or B. If the Type field is either "C" or "D" then Endtime contains the time when the last granularity period of the measurement results contained in the file ended. Its structure corresponds to the Starttime field, however, the allowed values for the minute of the hour are 05, 10, 15, 20, 25, 30, 35, 40, 45, 50, 55, and 00.

6) UniqueId. This is the DN of the measured NF, NSI, NSSI, or network/subnetwork, as defined in annex A.2 (e.g. a measObjInstId). The field may be omitted only if the distinguishedName is not available from the CM applications.

7) The RC parameter is a running count, starting with the value of "1", and shall be appended only if the filename is otherwise not unique, i.e. more than one file is generated and all other parameters of the file name are identical. Therefore it may only be used by the EM, since the described situation cannot occur with NE generated files. Note that the delimiter for this field, \_-\_, is an underscore character (\_), followed by a minus character (-), followed by an underscore character (\_).

8) jobIdList indicates the measurement job id(s) that the performance data file is associated with.

Some examples describing file-naming convention:

1) file name: A20000626.2315+0200-2330+0200\_gNBId,   
meaning: file produced for gNB <gNBId> on June 26, 2000, granularity period 15 minutes from 23:15 local to 23:30 local, with a time differential of +2 hours against UTC.

2) file name: B20021224.1700-1130-1705-1130\_-job10\_S-NSSAI,  
meaning: file containing results for multiple measured objects, generated for measurement job job10, produced for NSI <S-NSSAI> on December 24, 2002, granularity period 5 minutes from 17:00 local to 17:05 local, with a time differential of –11:30 hours against UTC.

3) file name: D20050907.1030+0000-20050909.1500+0000\_SubnetworkId\_-\_2,  
meaning: file containing results subnetwork <SubnetworkId>, start of first granularity period 07 September 2005, 10:30 local, end of last granularity period 09 September 2005, 15:00 local, with a time differential of 0 against UTC. This is the second file for this subnetwork/granularity period combination.

4) file name: C20050907.1030+0000-20050909.1500+0000\_gNBId,  
meaning: file produced for the gNB <gNBId>, start of first granularity period 07 September 2005, 10:30 local, end of last granularity period 09 September 2005, 15:00 local, with a time differential of 0 against UTC.

#### 11.3.2.1.4 Void

## 11.4 Heartbeat

### 11.4.1 Operations and notifications

#### 11.4.1.1 Notification notifyHeartbeat

##### 11.4.1.1.1 Definition

This notification notifies the subscribed consumer(s) that the MnS producer heartbeat period has expired or that a MnS consumer requested the emission of an immediate heartbeat notification.

The emission of heartbeat notifications is controlled by the HeartbeatControl IOC (3GPP TS 28.622 [11]).

##### 11.4.1.1.2 Input parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter Name | S | Information Type / Legal Values | Comment |
| objectClass | M | HeartbeatControl.objectClass |  |
| objectInstance | M | HeartbeatControl.objectInstance | Instance  controlling the emission of this notifyHeartbeat notification. |
| notificationId | M | -- |  |
| notificationType | M | "notifyHeartbeat" |  |
| eventTime | M | -- | Time at which the notification is emitted.  The semantics of Generalised Time specified by ITU-T [17] shall be used here. |
| systemDN | M | -- |  |
| heartbeatNtfPeriod | M | HeartbeatControl.heartbeatNtfPeriod |  |

##### 11.4.1.1.3 Triggering event

###### 11.4.1.1.3.1 From-state

stateBeforeHeartbeatNotification1 OR stateBeforeHeartbeatNotification2.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateBeforeHeartbeatNotification1 | The internal countdown timer of the MOI emitting the notifyHeartbeat notification has reached the value ‘0’ (zero). |
| stateBeforeHeartbeatNotification2 | The value of the attribute triggerHeartbeatNtf of the MOI emitting the notifyHeartbeat notification is TRUE. |

###### 11.4.1.1.3.2 To-state

stateAfterOHeartbeatNotification1 OR stateAfterOHeartbeatNotification2.

|  |  |
| --- | --- |
| Assertion Name | Definition |
| stateAfterHeartbeatNotification1 | If From-state is stateBeforeHeartbeatNotification1 then:  the internal countdown timer of the MOI is reset to the value of its heartbeatNtfPeriod attribute. |
| stateAfterHeartbeatNotification2 | If From-state is stateBeforeHeartbeatNotification2 then:  the value of the internal countdown timer of the MOI is not affected. |

## 11.5 Streaming data reporting service

### 11.5.1 Operations and notifications

#### 11.5.1.1 establishStreamingConnection operation (M)

##### 11.5.1.1.1 Definition

This operation enables the streaming data reporting producer to establish a connection to the streaming data reporting consumer (i.e. streaming target). The connection establishement includes the exchange of meta-data (producer informs consumer about its own identity and the nature of the data to be reported via streaming) phase and the actual connection (a data pipe for streaming) establishment.

Established connection supports stream multiplexing (one connection supports one or more reporting streams simultaneously).

Upon successful connection establishment, the consumer is aware of the producer's identity, the list of reporting streams and the nature of data being reported on each of the streams.

The established connection may be kept "alive" either by built-in functionality of the solution set or by periodic reporting of empty stream data.

##### 11.5.1.1.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| producerId | M | The identity of the producer requesting the connection establishment. | DN of the streaming data reporting MnS producer. If the producer is not modeled as 3GPP NRM MOI, an alternative identifer other than DN may be used. |
| streamInfoList | M | List of StreamInfo | This parameter contains the list of meta-data about each reporting stream.  For streaming trace reporting each StreamInfo includes:  - StreamType carrying the value "TRACE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - Trace Reference (see clause 5.6 of TS 32.422 [38]) as stream identifier;  - TraceJob (see clause 4.3.30 of TS 28.622 [11]) providing the details about the configuration of the trace job for which the data is being reported.  For streaming performance data reporting each StreamInfo includes:  - StreamType carrying the value "PERFORMANCE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - measObjDn: the DN of the measured object instance;  - performanceMetrics: a list of performance metric names whose values are to be reported by the Performance Data Stream Units (see Annex C of TS 28.550 [42]) via this stream. Performance metrics include measurement and KPI;  - either:  - jobId defined in the PerfMetricJob MOI (see clause 4.3.31 of TS 28.622 [11]) for which the data is being reported;  - or:  - jobId globally unique identifier of a measurement job (see TS 28.550 [42]).  For streaming analytics reporting each StreamInfo includes:  - StreamType carrying the value "ANALYTICS";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - AnalyticsInfo providing the details about the analytics activity for which the data is being reported.  For proprietary data streaming reporting each StreamInfo includes:  - StreamType carrying the value "PROPRIETARY";  - streamId globally unique stream identifier;  - VsDataContainer (see clause 4.3.9 of TS 28.622 [11]) providing the details about the data being reported. |

##### 11.5.1.1.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| connectionId | M | Identifier of the established streaming connection. | It identifies the established streaming connection. The format may have dependency on the solution set. |
| status | M | ENUM (Success, Failure) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.1.4 Exceptions

| Exception Name | Definition |
| --- | --- |
| unexpectedStreams | **Condition:** Some information in the list of streamInfo was unexpected by the MnS consumer.  **Returned Information:** Name of the exception; status is set to "Failure". |

#### 11.5.1.2 terminateStreamingConnection operation (M)

##### 11.5.1.2.1 Definition

This operation enables the streaming data reporting producer to terminate the connection to the streaming data reporting consumer (i.e. streaming target).

Upon successful termination of the streaming connection, the producer stops reporting data to the consumer on this connection.

##### 11.5.1.2.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| connectionId | M | See clause 11.5.1.1.3 | It identifies the streaming connection being terminated. The format may have dependency on the solution set. |

##### 11.5.1.2.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| status | M | ENUM (Success, Failure) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.2.4 Exceptions

| Exception Name | Definition |
| --- | --- |
| unknownConnection | **Condition:** the connectionId is invalid.  **Returned Information:** Name of the exception; status is set to "Failure". |

#### 11.5.1.3 reportStreamData operation (M)

##### 11.5.1.3.1 Definition

This operation enables the streaming data reporting producer to send a unit of streaming data to the streaming data reporting consumer.

##### 11.5.1.3.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| connectionId | M | See clause 11.5.1.1.3 | It identifies the streaming connection on which the reported data are being sent. The format may have dependency on the solution set. |
| streamingData | M | Unit of streaming data | This parameter contains the actual data (payload) being reported via stream.  For streaming trace reporting each streamingData is encoded according to the format specified in the clause 5 of 3GPP TS 32.423 [39].  For streaming performance data reporting each streamingData is encoded according to the format specified in the Annex C of 3GPP TS 28.550 [42].  For proprietary data streaming reporting each streamingData is encoded according to the format specified in the product documentation. |

##### 11.5.1.3.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| status | M | ENUM (Success, Failure) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.3.4 Exceptions

| Exception Name | Definition |
| --- | --- |
|  |  |

#### 11.5.1.4 addStream operation (M)

##### 11.5.1.4.1 Definition

This operation allows the producer to add one or more reporting streams to an already established streaming connection.

##### 11.5.1.4.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| connectionId | M | See clause 11.5.1.1.3 | It identifies the streaming connection to which new reporting streams are being added. The format may have dependency on the solution set. |
| streamInfoList | M | List of StreamInfo | This parameter contains the list of meta-data about each reporting stream being added to the already established connection.  For streaming trace reporting each StreamInfo includes:  - StreamType carrying the value "TRACE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - Trace Reference (see clause 5.6 of TS 32.422 [38]) as stream identifier;  - TraceJob (see clause 4.3.30 of TS 28.622 [11]) providing the details about the configuration of the trace job for which the data is being reported.  For streaming performance data reporting each StreamInfo includes:  - StreamType carrying the value "PERFORMANCE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - measObjDn: the DN of the measured object instance;  - performanceMetrics: a list of performance metric (i.e. measurement or KPI) names whose values are to be reported by the Performance Data Stream Units (see Annex C of TS 28.550 [42]) via this stream;  - either:  - jobId defined in the PerfMetricJob MOI (see clause 4.3.31 of TS 28.622 [11]) for which the data is being reported;  - or:  - jobId globally unique identifier of a measurement job (see TS 28.550 [42]).  For streaming analytics reporting each StreamInfo includes:  - StreamType carrying the value "ANALYTICS";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - AnalyticsInfo providing the details about the analytics activity for which the data is being reported.  For proprietary data streaming reporting each StreamInfo includes:  - StreamType carrying the value "PROPRIETARY";  - streamId globally unique stream identifier;  - VsDataContainer (see clause 4.3.9 of TS 28.622 [11]) providing the details about the data being reported. |

##### 11.5.1.4.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| streamInfoList | M | List of StreamInfo | This parameter contains the list of meta-data about each reporting stream that has been successfully added as a result of this operation.  For streaming trace reporting each StreamInfo includes:  - StreamType carrying the value "TRACE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - Trace Reference (see clause 5.6 of 3GPP TS 32.422 [38]) as stream identifier;  - TraceJob (see clause 4.3.30 of 3GPP TS 28.622 [11]) providing the details about the configuration of the trace job for which the data is being reported.  For streaming performance data reporting each StreamInfo includes:  - StreamType carrying the value "PERFORMANCE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - measObjDn: the DN of the measured object instance;  - performanceMetrics: a list of performance metric names whose values are to be reported by the Performance Data Stream Units (see Annex C of TS 28.550 [42]) via this stream. Performance metrics include measurement and KPI;  - either:  - jobId defined in the PerfMetricJob MOI (see clause 4.3.31 of 3GPP TS 28.622 [11]) for which the data is being reported;  - or:  - jobId globally unique identifier of a measurement job (see TS 28.550 [42]).  For streaming analytics reporting each StreamInfo includes:  - StreamType carrying the value "ANALYTICS";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - AnalyticsInfo providing the details about the analytics activity for which the data is being reported.  For proprietary data streaming reporting each StreamInfo includes:  - StreamType carrying the value "PROPRIETARY";  - streamId globally unique stream identifier;  - VsDataContainer (see clause 4.3.9 of 3GPP TS 28.622 [11]) providing the details about the data being reported. |
| status | M | ENUM (Success, Failure, PartialSuccess) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.4.4 Exceptions

| Exception Name | Definition |
| --- | --- |
| duplicateStream | **Condition:** One or more of stream identifiers in the streamInfoList already exist on this connection.  **Returned Information:** Name of the exception; status is set to "Failure" or "PartialSuccess". |
| unexpectedStreams | **Condition:** Some information in the list of streamInfo was unexpected by the MnS consumer.  **Returned Information:** Name of the exception; status is set to "Failure". |
| unknownConnection | **Condition:** the connectionId is invalid.  **Returned Information:** Name of the exception; status is set to "Failure". |

#### 11.5.1.5 deleteStream operation (M)

##### 11.5.1.5.1 Definition

This operation allows the producer to remove one or more reporting streams from an already established streaming connection.

##### 11.5.1.5.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| connectionId | M | See clause 11.5.1.1.3 | It identifies the streaming connection from which the reporting streams are being removed. The format may have dependency on the solution set. |
| streamIdList | M | List of stream identifiers | This parameter contains the list of identifiers for streams being removed from the already established connection.  For streaming trace reporting Trace Reference (see clause 5.6 of 3GPP TS 32.422 [38]) is used as stream identifier.  For streaming performance data reporting streamId globally unique stream identifier.  For streaming analytics reporting streamId globally unique stream identifier.  For proprietary data streaming reporting streamId globally unique stream identifier. |

##### 11.5.1.5.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| status | M | ENUM (Success, Failure, PartialSuccess) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.5.4 Exceptions

| Exception Name | Definition |
| --- | --- |
| unknownStreamId | **Condition:** One or more of stream identifiers in the streamIdList does not exist on this connection.  **Returned Information:** Name of the exception; status is set to "Failure" or "PartialSuccess". |
| unknownConnection | **Condition:** the connectionId is invalid.  **Returned Information:** Name of the exception; status is set to "Failure". |

#### 11.5.1.6 getConnectionInfo operation (M)

##### 11.5.1.6.1 Definition

This operation enables the streaming data reporting service producer to obtain information about one or more streaming connections.

##### 11.5.1.6.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| connectionIdList | M | List of streaming connection identifiers | This parameter contains the list of streaming connection identifiers for which the stream information is to be returned.  The empty list indicates the stream information for all connections are to be returned. |

##### 11.5.1.6.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| connectionInfoList | M | List of <connectionId, streamReporter, streamIdList> tuples | This parameter contains the list of meta-data about each streaming connection requested by this operation. Each entry in this list is a tuple of connectionId, streamReporter and streamIdList.  For streaming trace reporting:  - streamReporter is the identity of the streaming data reporting MnS producer reporting data for this connectionId;  - streamIdList is the list of Trace References (see clause 5.6 of 3GPP TS 32.422 [38]) used as stream identifiers.  For streaming performance data reporting:  - streamReporter is the identity of the streaming data reporting MnS producer reporting data for this connectionId;  - streamIdList is the list of streamId globally unique stream identifiers.  For streaming analytics reporting:  - streamReporter is the identity of the streaming data reporting MnS producer reporting data for this connectionId;  - streamIdList is the list of streamId globally unique stream identifiers.  For streaming proprietary data reporting:  - streamReporter is the identity of the streaming data reporting MnS producer reporting data for this connectionId;  - streamIdList is the list of streamId globally unique stream identifiers. |
| status | M | ENUM (Success, Failure, PartialSuccess) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.6.4 Exceptions

| Exception Name | Definition |
| --- | --- |
| unknownConnectionId | **Condition:** One or more of connection identifiers in the connectionIdList is not known to this MnS consumer.  **Returned Information:** Name of the exception; status is set to "Failure" or "PartialSuccess". |

#### 11.5.1.7 getStreamInfo operation (M)

##### 11.5.1.7.1 Definition

This operation enables the streaming data reporting service producer to obtain information about one or more reporting streams.

##### 11.5.1.7.2 Input parameters

| Parameter Name | Qualifier | Information type | Comment |
| --- | --- | --- | --- |
| streamIdList | M | List of stream identifiers | This parameter contains the list of stream identifiers for which the stream information is to be returned.  The empty list indicates the stream information for all streams are to be returned.  For streaming trace reporting Trace Reference (see clause 5.6 of 3GPP TS 32.422 [38]) is used as stream identifier.  For streaming performance data reporting streamId globally unique stream identifier.  For streaming analytics reporting streamId globally unique stream identifier.  For proprietary data streaming reporting streamId globally unique stream identifier. |

##### 11.5.1.7.3 Output parameters

| Parameter Name | Qualifier | Matching Information | Comment |
| --- | --- | --- | --- |
| streamInfoSumList | M | List of <StreamInfo, StreamReporters> tuples | This parameter contains the list of meta-data about each reporting stream requested by this operation. Each entry in this list is a tuple of StreamInfo and StreamReporters.  For streaming trace reporting each StreamInfo includes:  - StreamType carrying the value "TRACE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - Trace Reference (see clause 5.6 of TS 32.422 [38]) as stream identifier;  - TraceJob (see clause 4.3.30 of TS 28.622 [11]) providing the details about the configuration of the trace job for which the data is being reported.  For streaming trace the StreamReporters is a list of the identities of the streaming data reporting MnS producer(s) reporting data for this Trace Reference to this MnS consumer.  For streaming PM reporting each StreamInfo includes:  - StreamType carrying the value "PERFORMANCE";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - measObjDn: the DN of the measured object instance;  - performanceMetrics: a list of performance metric names whose values are to be reported by the Performance Data Stream Units (see Annex C of TS 28.550 [42]) via this stream. Performance metrics include measurement and KPI;  - either:  - jobId defined in the PerfMetricJob MOI (see clause 4.3.31 of TS 28.622 [11]) for which the data is being reported;  - or:  - jobId globally unique identifier of a measurement job (see TS 28.550 [42]).  For streaming performance data the StreamReporters is a list of the identities of the streaming data reporting MnS producer(s) reporting data for this streamId to this MnS consumer.  For streaming analytics reporting each StreamInfo includes:  - StreamType carrying the value "ANALYTICS";  - SerializationFormat carrying the value "GPB" or "ASN1";  - streamId globally unique stream identifier;  - AnalyticsInfo providing the details about the analytics activity for which the data is being reported.  For streaming analytics the StreamReporters is a list of the identities of the streaming data reporting MnS producer(s) reporting data for this streamId to this MnS consumer.  For proprietary data streaming reporting each StreamInfo includes:  - StreamType carrying the value "PROPRIETARY";  - streamId globally unique stream identifier;  - VsDataContainer (see clause 4.3.9 of TS 28.622 [11]) providing the details about the data being reported.  For proprietary data streaming the StreamReporters is a list of the identities of the streaming data reporting MnS producer(s) reporting data for this streamId to this MnS consumer. |
| status | M | ENUM (Success, Failure, PartialSuccess) | An operation may fail because of a specified or unspecified reason. |

##### 11.5.1.7.4 Exceptions

| Exception Name | Definition |
| --- | --- |
| unknownStreamId | **Condition:** One or more of stream identifiers in the streamIdList is not known to this MnS consumer.  **Returned Information:** Name of the exception; status is set to "Failure" or "PartialSuccess". |

## 11.6 File data reporting service

### 11.6.1 Operations and notifications

#### 11.6.1.1 Notification notifyFileReady (M)

##### 11.6.1.1.1 Definition

This notification supports the authorized file data reporting service consumer to be notified about the readiness of the file data by the file data reporting service producer.

After the file data has been prepared ready for the consumer(s), the file data reporting service producer emits the notification to the subject consumer(s) who have subscribed to this notification.

##### 11.6.1.1.2 Notification information

Table 11.6.1.1.2-1: Notification Information

| Parameter Name | Qualifier | Information Type | Comment |
| --- | --- | --- | --- |
| objectClass | M, Y | Type of the file data reporting related producer, e | It indicates the class, whose instance emitted this notification. The class indicates the type of the file data reporting service producer. |
| objectInstance | M, Y | Identifier of the file data reporting service producer | It identifies the file data reporting related service producer, who actually emitted the notification. |
| notificationId | M, N | This is an identifier of the notification, which may be used to correlate notifications. | The unique identifier of the notification across all notifications sent by a particular management service producer throughout the time that correlation is significant.  How identifiers of notifications are re-used to correlate notifications is outside of the scope of the present document. |
| eventTime | M, Y | It indicates the event occurrence time. | The semantics of Generalised Time specified by ITU-T shall be used here. |
| notificationType | M, Y | "notifyFileReady " | The type of notification, and it shall be assigned to "notifyFileReady" for this notification. |
| fileInfoList | M, N | List of struct <  fileLocation,  fileSize  fileReadyTime  fileExpirationTime  fileCompression,  fileFormat,  fileType,  >.  Each element is defined as following:  - fileLocation: It identifies the location of the file. The location may be a directory path or a URL.  E.g.:  "\\202.112.101.1\D:\user\Files\<xxx>" or  "[ftp://nms.telecom\_org.com/datastore/<xxx>](ftp://nms.telecom_org.com/datastore/%3cxxx%3e), where <xxx> is the filename and the file naming convention is defined in Annex A.3.  - fileSize: It identifies the size of the file. Its value is positive Integer (the unit is byte).  - fileReadyTime: It identifies the date and time when the file was last closed and made available in the management service producer and the file content will not be changed.  - fileExpirationTime: It identifies the date and time beyond which the file may be deleted. It shall not be empty and shall be later than fileReadyTime.  - fileCompression: It identifies the name of the compression algorithm used for the file. An empty fileCompression means that there is no compression on the file. Choice of compression algorithm is vendor-specific but is encouraged to use industrial standard algorithm such as GZIP.  - fileFormat: It identifies the encoding technique used by the file. Its value should indicate the version of the file format specification plus to indicate if "ASN1" or "XML-schema" is used.  - fileType: It identifies the type of the management data stored in the file. Following are the allowed values:  - For performance data (including measurement data and KPI) files, the value is assigned to "PERFORMANCE".  - For trace data files, the value is assigned to "TRACE".  - For analytic data files, the value is assigned to "ANALYTICS".  - For proprietary data files, the value is assigned to "PROPRIETARY". | It specifies the information of each available file. |
| additionalText | O, N | It provides additional information for this notification. | It carries vendor-specific semantics not defined in the present document. |

#### 11.6.1.2 Notification notifyFilePreparationError (M)

##### 11.6.1.2.1 Definition

This notification supports the authorized file data reporting service consumer to be notified about the occurrence of an error during the preparation of the data file by the file data reporting service producer. When such error occurs, the the file data reporting service producer emits the notification to the authorized consumer(s) who have subscribed to this notification when the reporting period arrives.

##### 11.6.1.2.2 Notification information

| Parameter Name | Qualifier | Information Type | Comment |
| --- | --- | --- | --- |
| objectClass | M, Y | See Table 11.6.1.1.2-1. | See Table 11.6.1.1.2-1. |
| objectInstance | M, Y | See Table 11.6.1.1.2-1. | See Table 11.6.1.1.2-1. |
| notificationId | M, N | See Table 11.6.1.1.2-1. | See Table 11.6.1.1.2-1. |
| eventTime | M, Y | See Table 11.6.1.1.2-1. | See Table 11.6.1.1.2-1. |
| notificationType | M, Y | "notifyFilePreparationError" | The type of notification, and it shall be assigned to "notifyFilePreparationError" for this notification. |
| fileInfoList | M, N | See Table 11.6.1.1.2-1. | If file is kept, this parameter identifies the file whose preparation provoked an error. If file is not generated, this parameter is empty. |
| reason | M, N | It specifies the reason of the error occurred during the file data preparation. | The detailed reason is given, including  errorInPreparation  hardDiskFull  hardDiskFailure  tooManyFiles  collectionTimeOut  incompleteTruncatedFile  corruptedFile  lowMemory  dataNotAvailable |
| additionalText | O, N | See Table Table 11.6.1.1.2-1. | See Table 11.6.1.1.2-1. |

#### 11.6.1.3 Operation subscribe (M)

##### 11.6.1.3.1 Definition

This operation enables the authorized file data reporting service consumer to subscribe to the notification(s) related to the services provided by the file data reporting service producer.

##### 11.6.1.3.2 Input parameters

| Parameter Name | Qualifier | Information Type | Comment |
| --- | --- | --- | --- |
| consumerReference | M | It specifies the reference of the consumer to which the notifications shall be sent. | The format of the reference may have dependency on the solution set. |
| timeTick | O | It specifies the value of a timer the subscription is hold by the file data reporting service producer for the subject consumer.  The value is in unit of whole minute. | A special infinite value is assumed when parameter is absent or present but equal to zero. |
| filter | O | It specifies a filter constraint that the file data reporting service producer shall use to filter notification(s).  Filter constraint grammar is solution set dependent | If this parameter is absent, then no filter constraint shall be applied. |

##### 11.6.1.3.3 Output parameters

| **Parameter Name** | **Qualifier** | **Matching Information** | **Comment** |
| --- | --- | --- | --- |
| subscriptionId | M | An unambiguous identity of this subscription. |  |
| status | M | ENUM (OperationSucceeded, OperationFailedExistingSubscription, OperationFailed) | If subscription is successfully created, status = OperationSuceeded.  If subscription is not created because it is duplicated or conflict with existing subscription(s), status = OperationFailedExistingSubscription  If the operation is failed for any other reason than being duplicated or conflict with existing subscription(s), status = OperationFailed. |

##### 11.6.1.3.4 Exceptions

|  |  |
| --- | --- |
| **Name** | **Definition** |
| operation\_failed\_existing\_subscription | **Condition:** The subscription is duplicated or conflict with existing subscription(s)  **Returned Information:** The output parameter status |
| operation\_failed | **Condition:** The operation is failed for any other reason than being duplicated or conflict with subscription(s)  **Returned Information:** The output parameter status |

#### 11.6.1.4 Operation unsubscribe (M)

##### 11.6.1.4.1 Definition

This operation enables the authorized file data reporting service consumer cancel subscription(s) at a management service producer.

The authorized file data reporting service consumer can cancel one subscription made with a consumerReference by providing the corresponding subscriptionId or all subscriptions made with the same consumerReference by leaving the subscriptionId parameter absent.

##### 11.6.1.4.2 Input parameters

| **Parameter Name** | **Qualifier** | **Information Type** | **Comment** |
| --- | --- | --- | --- |
| consumerReference | M | It specifies the reference of the authorized file data reporting service consumer whose subscription(s) are to be cancelled. | The format of the reference may have dependency on the solution set. |
| subscriptionId | O | It holds a subscriptionId carried as the output parameter in the subscribe operation. | If this parameter is absent, all subscriptions made with the same consumerReference shall be cancelled. |

##### 11.6.1.4.3 Output parameters

| **Parameter Name** | **Qualifier** | **Matching Information** | **Comment** |
| --- | --- | --- | --- |
| status | M | ENUM (OperationSucceeded, OperationFailed) | If subscription(s) as identified in the input parameter are cancelled, status = OperationSucceeded.  If the operation is failed, status = OperationFailed. |

##### 11.6.1.4.4 Exceptions

|  |  |
| --- | --- |
| **Name** | **Definition** |
| operation\_failed | **Condition:** the operation is failed  **Returned Information:** The output parameter status |

#### 11.6.1.5 Operation listAvailableFiles (M)

##### 11.6.1.5.1 Definition

This operation allows the authorized file data reporting service consumer to list all or specified available data files stored in the file data reporting service producer.

The file data reporting service producer shall only provide the information about the available management data files that are created for the subject consumer.

A Solution Set may choose to split this operation in several operations (e.g. operations to get "iterator" which fulfil the criteria and other operations to retrieve the detailed information of the files from the "iterator").

##### 11.6.1.5.2 Input parameters

| **Parameter Name** | **Qualifier** | **Information type** | **Comment** |
| --- | --- | --- | --- |
| fileType | M | It specifies the type of the management data stored in the file. | For performance data (including measurement data and KPI) files, the value is assigned to "PERFORMANCE".  For trace data files, the value is assigned to "TRACE".  For analytic data files, the value is assigned to "ANALYTICS".  For proprietary data files, the value is assigned to "PROPRIETARY". |
| beginTime | M | The consumer requests to list information about the available file(s) whose ready time(s) are later or equal to this time.  This parameter is expressed in UTC time. | This parameter indicates date and time.  If this parameter is empty, no restriction on begin time is applied on the file ready time. |
| endTime | M | The consumer requests to list information about the available file(s) whose ready time(s) are earlier than this time.  This parameter is expressed in UTC time. | This parameter indicates date and time.  If this parameter is empty, no restriction on end time is applied on the file ready time. |

##### 11.6.1.5.3 Output parameters

| **Parameter Name** | **Qualifier** | **Matching Information** | **Comment** |
| --- | --- | --- | --- |
| fileInfoList | M | See the fileInfoList defined in notifyFileReady notification (clause 11.3.1.1.1) | See the fileInfoList defined in notifyFileReady notification (clause 11.3.1.1.1) |
| status | M | ENUM (Success, Failure) |  |

##### 11.6.1.5.4 Exceptions

| **Exception Name** | **Definition** |
| --- | --- |
| invalidTimes | **Condition:** Either beginTime or endTime is invalid.  **Returned information:** output parameter status is set to Failure. |

# 12 Management services – Stage 3

## 12.1 Generic provisioning management service

### 12.1.1 RESTful HTTP-based solution set

#### 12.1.1.1 Mapping of operations

##### 12.1.1.1.1 Introduction

The IS operations are mapped to SS equivalents according to table 12.1.1.1.1-1.

Table 12.1.1.1.1-1: Mapping of IS operations to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation** | **HTTP Method** | **Resource URI** | **S** |
| createMOI | PUT | {MnSRoot}/ProvMnS/{MnSVersion}/{URI-LDN-first-part}/{className}={id} | M |
| getMOIAttributes | GET | {MnSRoot}/ProvMnS/{MnSVersion}/{URI-LDN-first-part}/{className}={id} | M |
| modifyMOIAttributes | PUT  PATCH | {MnSRoot}/ProvMnS/{MnSVersion}/{URI-LDN-first-part}/{className}={id} | M |
| deleteMOI | DELETE | {MnSRoot}/ProvMnS/{MnSVersion}/{URI-LDN-first-part}/{className}={id} | M |

##### 12.1.1.1.2 Operation "createMOI"

This operation creates a single resource representing a managed object instance.

Table 12.1.1.1.2-1: Mapping of IS operation input parameters to SS equivalents (HTTP PUT)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| managedObjectClass  managedObjectInstance | path | …/{className}={id} | className: string  id: string | M |
| attributeListIn | request body | n/a | Resource | M |

Note 1: Void.

Table 12.1.1.1.2-2: Mapping of IS operation output parameters to SS equivalents (HTTP PUT)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| attributeListOut | response body | n/a | Resource | M |
| status | response status codes | n/a | n/a | M |
| response body | error | ErrorResponse | O |

The message flow for creating a resource is as follows:

1. The MnS consumer sends a HTTP PUT request to the MnS producer.

- The target URI identifies the location of the new resource to be created.

- The message body shall carry the complete representation of the resource to be created.

2. The MnS producer sends a HTTP PUT response to the MnS consumer.

- On success, "201 Created" shall be returned. The Location header shall carry the URI of the new resource and the message body the complete representation of the new resource.

- On failure, an appropriate error code shall be returned. The response message body may provide additional error information

##### 12.1.1.1.3 Operation "getMOIAttributes"

This operation retrieves one or multiple resources representing managed object instances.

Table 12.1.1.1.3-1: Mapping of IS operation input parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| baseObjectInstance | path | /{className}={id} | className: string  id: string | M |
| scope | query | scope | Scope  style: form  explode: true | O |
| filter | query | filter | Filter | O |
| attributeListIn | query | attributes | array(string)  style: form  explode: false | O |
| fields | array(string)  style: form  explode: false | O |

The SS parameters "scope", "filter", "attributes" and "fields" are defined in TS 32.158 [15].

Note 1: Void.

Note 2: Void.

Table 12.1.1.1.3-2: Mapping of IS operation output parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| attributeListOut | response body | n/a | Resource | M |
| status | response status codes | n/a | n/a | M |
| response body | error | ErrorResponse | O |

The message flow for retrieval of one or multiple resources is as follows:

1. The MnS consumer sends a HTTP GET request to the MnS producer.

- The authority and path component of the target URI identify the base resource.

- If present, the scope query parameter identifies other resources besides the base resource.

- The filter query parameter is applied to the set of scoped resources. Only resources passing the filter criteria are targeted.

- The attributes and fields query parameters identify the attributes and sub-attributes to be returned.

2. The MnS producer sends a HTTP GET response to the MnS consumer.

- On success, "200 OK" shall be returned. The response message body is constructed according to the hierarchical response construction method (TS 32.158 [15]).

- On failure, an appropriate error code shall be returned. The response message body shall provide additional error information

##### 12.1.1.1.4 Operation "modifyMOIAttributes"

###### 12.1.1.1.4.1 Mapping to HTTP PUT

HTTP PUT is used for a full update of a single resource.

Table 12.1.1.1.4.1-1: Mapping of IS operation input parameters to SS equivalents (HTTP PUT)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| baseObjectInstance | path | /{className}={id} | className: string  id: string | M |
| scope | n/a | n/a | n/a | n/a |
| filter | n/a | n/a | n/a | n/a |
| modificationList | request body | n/a | Resource | M |

The IS parameters "scope" and "filter" have no meaning when targeting a single resource with the target URI and are not mapped.

Table 12.1.1.1.4.1-2: Mapping of IS operation output parameters to SS equivalents (HTTP PUT)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| attributeListOut | response body | n/a | Resource | O |
| status | response status codes | n/a | n/a | M |
| response body | error | ErrorResponse | O |

The message flow is as follows:

1. The MnS consumer sends a HTTP PUT request to the MnS producer.

- The target URI identifies the target resource.

- The message body shall contain the representation the target resource shall be replaced with.

2. The MnS producer sends a HTTP PUT response to the MnS consumer.

- On success, "200 OK" or "204 No Content" shall be returned. In the former case the response carries the representation of the updated resource in the message body. In the latter case the response has no message body. A "200 OK" response including the representation of the updated resource shall be sent in case the updated representation of the resource is not identical to the representation received in the request.

- On failure, an appropriate error code shall be returned. The response message body may provide additional error information.

###### 12.1.1.1.4.2 Mapping to HTTP PATCH

HTTP PATCH is used to create, update or delete one or multiple resources.

Table 12.1.1.1.4.2-1: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| baseObjectInstance | path | …/{className}={id} | className: string  id: string | M |
| scope | n/a | n/a | n/a | n/a |
| filter | n/a | n/a | n/a | n/a |
| modificationList | request body | n/a | Resource, or  array(object) | M |

Four patch media types are available. They are listed below together with their request body data types:

- "application/merge-patch+json" (RFC 7396 [37]), request body type: Resource

- "application/3gpp-merge-patch+json" (TS 32.158 [15]), request body type: Resource

- "application/json-patch+json" (RFC 6902 [36]), request body type: array(object)

- "application/3gpp-json-patch+json" (TS 32.158 [15]), request body type: array(object)

The IS parameters "scope" and "filter" have no SS equivalents in the present document.

Table 12.1.1.1.4.2-2: Mapping of IS operation output parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| attributeListOut | n/a | n/a | n/a | n/a |
| status | response status codes | n/a | n/a | M |
| response body | error | ErrorResponse | O |

The message flow for modification of one or multiple resources is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The path component of the target URI identifies the base resource.

- The message body shall contain the patch document.

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success, "200 OK" or "204 No Content" shall be returned. When "200 OK" is returned the message body shall include a representation of the updated resources constructed according to the hierarchical response construction method (TS 32.158 [15]).

- On failure, an appropriate error code shall be returned. The response message body may provide additional error information

Note 1: Void.

##### 12.1.1.1.5 Operation "deleteMOI"

This operation deletes one or multiple resources representing managed object instances.

Table 12.1.1.1.5-1: Mapping of IS operation input parameters to SS equivalents (HTTP DELETE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| baseObjectInstance | path | /{className}={id} | className: string  id: string | M |
| scope | query | scope | Scope  style: form  explode: true | O |
| filter | query | filter | Filter | O |

Note 1: Void.

Note 2: Void.

Table 12.1.1.1.5-2: Mapping of IS operation output parameters to SS equivalents (HTTP DELETE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| deletionlist | response body | n/a | array(Uri) | O |
| status | response status codes | n/a | n/a | M |
| response body | error | ErrorResponse | O |

The message flow for deletion of one or multiple resources is as follows:

1. The MnS consumer sends a HTTP DELETE request to the MnS producer.

- The authority and path components of the target URI identify the base resource.

- If present, the scope query parameter identifies other resources besides the base resource.

- The filter query parameter may be applied to the set of scoped resources. Only resources passing the filter criteria are targeted.

2. The MnS producer sends a HTTP DELETE response to the MnS consumer.

- On success, when no query parameters are present in the request and only one resource is deleted, "204 No Content" shall be returned. Otherwise, when query parameters are present in the request, "200 OK" shall be returned and the response message body shall carry the URIs of the deleted resources.

- On failure, an appropriate error code shall be returned. The response message body shall provide additional error information

##### 12.1.1.1.6 Void

##### 12.1.1.1.7 Void

#### 12.1.1.2 Mapping of notifications

##### 12.1.1.2.1 Introduction

The IS notifications are mapped to SS equivalents according to table 12.1.1.2.1-1.

**Table 12.1.1.2.1-1: Mapping of IS notifications to SS equivalents**

|  |  |  |  |
| --- | --- | --- | --- |
| **IS notification** | **HTTP Method** | **Resource URI** | **S** |
| notifyMOICreation | POST | /notificationTarget | M |
| notifyMOIDeletion | POST | /notificationTarget | M |
| notifyMOIAttributeValueChanges | POST | /notificationTarget | M |
| notifyMOIChanges | POST | /notificationTarget | M |

##### 12.1.1.2.2 Notification "notifyMOICreation"

The IS notification parameters are mapped to SS equivalents according to table 12.1.1.2.2-1.

Table 12.1.1.2.2-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| objectClass  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| additionalText | request body | additionalText | AdditionalText | O |
| sourceIndicator | request body | sourceIndicator | SourceIndicator | O |
| attributeList | request body | attributeList | AttributeNameValuePairSet | O |

##### 12.1.1.2.3 Notification "notifyMOIDeletion"

The IS notification parameters are mapped to SS equivalents according to table 12.1.1.2.3-1.

Table 12.1.1.2.3-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| objectClass  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| additionalText | request body | additionalText | AdditionalText | O |
| sourceIndicator | request body | sourceIndicator | SourceIndicator | O |
| attributeList | request body | attributeList | AttributeNameValuePairSet | O |

##### 12.1.1.2.4 Notification "notifyMOIAttributeValueChanges"

The IS notification parameters are mapped to SS equivalents according to table 12.1.1.2.4-1.

Table 12.1.1.2.4-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| objectClass  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| additionalText | request body | additionalText | AdditionalText | O |
| sourceIndicator | request body | sourceIndicator | SourceIndicator | O |
| attributeListValueChanges | request body | attributeListValueChange | AttributeValueChangeSet | M |

##### 12.1.1.2.5 Notification "notifyMOIChanges"

The IS notification parameters are mapped to SS equivalents according to table 12.1.1.2.5-1.

Table 12.1.1.2.5-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| objectClass  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| mOIChanges | request body | mOIChanges | array(MoiChange) | M |

#### 12.1.1.3 Resources

##### 12.1.1.3.1 Resource structure

12.1.1.3.1.1 Resource structure on the MnS producer

Figure 12.1.1.3.1.1-1 shows the resource structure of the Provisioning MnS on the MnS producer.



Figure 12.1.1.3.1.1-1: Resource URI structure of the Provisioning MnS on the MnS producer

Table 12.1.1.3.1.1-1 provides an overview of the resources and applicable HTTP methods.

Table 12.1.1.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| MOI | …/{className}={id} | PUT | Create a resource representing a managed object instance |
| MOI | …/{className}={id} | GET | Retrieve one or multiple resources representing managed object instances |
| MOI | …/{className}={id} | PATCH | Modifiy one or multiple resources representing managed object instances |
| MOI | …/{className}={id} | DELETE | Delete one or multiple resources representing managed object instances |

###### 12.1.1.3.1.1 Resource structure on the MnS consumer

Figure 12.1.1.3.1.2-1 shows the resource structure of the Provisioning MnS on the MnS consumer.



Figure 12.1.1.3.1.2-1: Resource URI structure of the Provisioning MnS on the MnS consumer

Table 12.1.1.3.1.2-1 provides an overview of the resources and applicable HTTP methods.

Table 12.1.1.3.1.2-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Notification Target | {notificationTarget} | POST | Send a notification to the notification target |

##### 12.1.1.3.2 Resource definitions

###### 12.1.1.3.2.1 Resource "…/{className}={id}"

12.1.1.3.2.1.1 Description

This resource represents a managed object instance.

12.1.1.3.2.1.2 URI

Resource URI: {MnSRoot}/ProvMnS/{MnSVersion}/{URI-LDN-first-part}/{className}={id}

The resource URI variables are defined in table 12.1.1.3.2.1.2-1.

Table 12.1.1.3.2.1.2-1: URI variables

|  |  |
| --- | --- |
| **Name** | **Definition** |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |
| URI-LDN-first-part | See clause 4.4.2 of TS 32.158 [15] |
| className | Class name of the targeted resource |
| id | Identifier of the targeted resource |

12.1.1.3.2.1.3 HTTP methods

12.1.1.3.2.1.3.1 HTTP PUT

This method shall support the URI query parameters specified in the following table.

Table 12.1.1.3.2.1.3.1-1: URI query parameters supported by the PUT method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

Table 12.1.1.3.2.1.3.1-2: Data structures supported by the PUT request body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| Resource | Resource representation of the resource to be created or replaced | M |

Table 12.1.1.3.2.1.3.1-3: Data structures supported by the PUT Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| Resource | 200 OK | Status code returned when the resource is replaced, and when the replaced resource representation is not identical to the resource representation in the request.  This status code may be retourned when the resource is updated and when the updated resource representation is identical to the resource representation in the request.  The representation of the updated resource is returned in the response message body. | M |
| Resource | 201 Created | Status code returned when the resource is created. The representation of the created resource is returned in the response message body. | M |
| n/a | 204 No Content | Status code that may be returned only when the replaced resource representation is identical to the representation in the request. The response has no message body. | M |
| ErrorResponse | 4xx/5xx | Returned in case of an error | O |

12.1.1.3.2.1.3.2 HTTP GET

This method shall support the URI query parameters specified in the following table.

Table 12.1.1.3.2.1.3.2-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| scope | Scope  style: form  explode: true | Extends the set of targeted resources beyond the base resource identified with the authority and path component of the URI. | O |
| filter | Filter | Reduces the targeted set of resources by applying a filter to the scoped set of resource representations. Only resources representations for which the filter construct evaluates to "true" are targeted. | O |
| attributes | array(string)  style: form  explode: false | Attributes of the scoped resources to be returned. The value is a comma-separated list of attribute names. | O |
| fields | array(string)  style: form  explode: false | Attribute fields of the scoped resources to be returned. The value is a comma-separated list of JSON pointers to the attribute fields. | O |

This method shall support the request data structures, the response data structures and response codes specified in the following tables.

Table 12.1.1.3.2.1.3.2-2: Data structures supported by the GET request body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
|  |  |  |

Table 12.1.1.3.2.1.3.2-3: Data structures supported by the GET response body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| Resource | 200 OK | Resources identified in the request for retrieval. In case the attributes or fields query parameters are used, only the selected attributes or sub-attributes are returned. The response message body is constructed according to the hierarchical response construction method (TS 32.158 [15]) | M |
| ErrorResponse | 4xx/5xx | Returned in case of an error | M |

12.1.1.3.2.1.3.3 HTTP PATCH

This method shall support the URI query parameters specified in the following table.

Table 12.1.1.3.2.1.3.3-1: URI query parameters supported by the PATCH method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures, the response data structures and response codes specified in the following tables.

Table 12.1.1.3.2.1.3.3-2: Data structures supported by the PATCH request body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| Resource, or  array(object) | Patch document describing the set of modifications to be applied to the targeted resources.  The following patch media types are available:  - "application/merge-patch+json" (RFC 7396 [37])  - "application/3gpp-merge-patch+json" (TS 32.158 [15])  - "application/json-patch+json" (RFC 6902 [36])  - "application/3gpp-json-patch+json" (TS 32.158 [15]) | M |

Table 12.1.1.2.1.1.3.3-3: Data structures supported by the PATCH response body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| ErrorResponse | 4xx/5xx | Returned in case of an error | M |

12.1.1.3.2.1.3.4 HTTP DELETE

This method shall support the URI query parameters specified in the following table.

Table 12.1.1.3.2.1.3.4-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| scope | Scope  style: form  explode: true | Extends the set of targeted resources beyond the base resource identified with the authority and path component of the URI. | O |
| filter | Filter | Reduces the targeted set of resources by applying a filter to the scoped set of resource representations. Only resources representations for which the filter construct evaluates to "true" are targeted. | O |

This method shall support the request data structures, the response data structures and response codes specified in the following tables.

Table 12.1.1.3.2.1.3.4-2: Data structures supported by the DELETE request body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| n/a | n/a | n/a |

Table 12.1.1.3.2.1.3.4-3: Data structures supported by the DELETE response body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| array(Uri) | 200 OK | Status code returned, when query parameters are present in the request and one or multiple resources are deleted. The URIs of the deleted resources are returned in the response message body. | M |
| n/a | 204 No Content | Status code returned, when no query parameters are present in the request and only one resource is deleted. The message body is empty. | M |
| ErrorResponse | 4xx/5xx | Returned in case of an error | M |

###### 12.1.1.3.2.2 Void

###### 12.1.1.3.2.3 Void

###### 12.1.1.3.2.4 Resource "{notificationTarget}"

12.1.1.3.2.4.1 Description

This resource represents a notification target on the MnS consumer.

12.1.1.3.2.4.2 URI

Resource URI: {notificationTarget}

The resource URI variables are defined in table12.1.1.3.2.4.2-1.

Table 12.1.1.3.2.4.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| notificationTarget | URI of the notification target on the MnS consumer, contained in the notification subscription |

12.1.1.3.2.4.3 HTTP methods

12.1.1.3.2.4.3.1 POST

This method shall support the URI query parameters specified in table 12.1.1.3.2.4.3.1-1.

Table 12.1.1.3.2.4.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | S |
| n/a |  |  |  |

This method shall support the request data structures specified in table 12.1.1.3.2.4.3.1-2 and the response data structures and response codes specified in table 12.1.1.3.2.4.3.1-3.

Table 12.1.1.3.2.4.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Data type | | Description | | S | |
| NotifyMOICreation | | Type for a notifyMOICreation notification | | M | |
| NotifyMOIDeletion | | Type for a notifyMOIDeletion notification | | M | |
| NotifyAttributeValueChanges | | Type for a notifyAttributeValueChanges notification | | M | |
| NotifyMOIChanges | | Type for a notifyMOIChanges notification | | M | |

Table 12.1.1.3.2.4.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | S |
| n/a | 204 No Content | In case of success no message body is returned | M |
| ErrorResponse | 4xx/5xx | In case of failure the error object is returned. | M |

#### 12.1.1.4 Data type definitions

##### 12.1.1.4.1 General

This clause defines the data types used by the Provisioning MnS. Table 12.1.1.4.1-1 specifies the data types defined in the present document and Table table 12.1.1.4.1-2 the data types imported.

Table 12.1.1.4.1-1: Data types defined in this specification

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Description |
| Scope | 12.1.1.4.1a.2 | Used in the query part of HTTP GET and HTTP DELETE to extend the set of targeted resources beyond the base resource identified with the authority and path component of the URI |
| ScopeType | 12.1.1.4.4.5 | Scope type of a scope |
| CmNotificationTypes | 12.1.1.4.4.3 | Notification type (notifyMOICreation, etc.) |
| SourceIndicator | 12.1.1.4.4.4 | Indicates the source of the operation that led to the generation of the notification. |
| CorrelatedNotification | 12.1.1.4.1a.3 | Describes the correlated notifications of a single source |
| Resource | 12.1.1.4.1a.1 | Used for resource representations |
| Operation | 12.1.1.4.4.6 | Enum with "create", "delete" and "replace" |
| MoiChange | 12.1.1.4.1a.4 | Single MOI change reported by notifyMOIChanges |
| NotifyMOICreation | 12.1.1.4.1a.5 | Used in the request body of HTTP POST for the notification type notifyMOICreation |
| NotifyMOIDeletion | 12.1.1.4.1a.5 | Used in the request body of HTTP POST for the notification type notifyMOIDeletion |
| NotifyMOIAttributeValueChanges | 12.1.1.4.1a.5 | Used in the request body of HTTP POST for the notification type notifyMOIAttributeValueChanges |
| NotifyMOIChanges | 12.1.1.4.1a.5 | Used in the request body of HTTP POST for the notification type notifyMOIChanges |

Table 12.1.1.4.1-2: Data types imported

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Description |
| DateTime | TS 28.623 [44] | Date and time |
| Dn | TS 28.623 [44] | DN type |
| SystemDN | TS 28.623 [44] | systemDN type |
| Uri | TS 28.623 [44] | URI type |
| AttributeNameValuePairSet | TS 28.623 [44] | Set of attribute name/value pairs |
| AttributeValueChangeSet | TS 28.623 [44] | Set of attribute names with their old and new values |
| Filter | TS 28.623 [44] | Filter type |
| NotificationId | TS 28.623 [44] | Notification identifier as defined in ITU-T Rec. X. 733 [4] |
| NotificationType | TS 28.623 [44] | Notification type |
| NotificationHeader | TS 28.623 [44] | Notification header |
| ErrorResponse | TS 28.623 [44] | Used in the response body of multiple HTTP methods in case of error |

##### 12.1.1.4.1a Structured data types

###### 12.1.1.4.1a.1 Type Resource

**Table 12.1.1.4.1a.1 -1: Definition of type Resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| id | string | Identifier of the resource object | M |
| attributes | object | Attributes object whose members are the class attributes and values. | M |
| n/a | map(array(object)) | Name contained objects | M |

This definition of "Resource" does not specify any attributes or name contained objects. Resource representations with specific attributes and name contained objects are contained in the NRM definitions. These definitions should be used in implementations of the Provisioning MnS instead of this generic definition.

###### 12.1.1.4.1a.2 Type Scope

Table 12.1.1.4.1a.2-1: Definition of type Scope

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| scopeType | ScopeType | Used in the query component of HTTP GET and HTTP DELETE together with scopeLevel to extend the set of targeted resources beyond the base resource identified with the authority and path component of the URI | M |
| scopeLevel | integer | Used in the query component of HTTP GET and HTTP DELETE together with scopeType to extend the set of targeted resources beyond the base resource identified with the path component of the URI | M |

###### 12.1.1.4.1a.3 Type CorrelatedNotification

Table 12.1.1.4.1a.3 -1: Definition of type CorrelatedNotification

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| source | Dn | Source of the correlated notifications | M |
| notificationIds | array(NotificationId) | Notification identifiers of correlated notifications of that source | M |

###### 12.1.1.4.1a.4 Type MoiChange

Table 12.1.1.4.1a.4 -1: Definition of type MoiChange

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| sourceIndicator | SourceIndicator | Indicates the source of the operation that led to the generation of this notification. | O |
| path | Uri | URI specifying the created, deleted or updated resource | M |
| operation | Operation | Operation associated to the reported change ("CREATE", "DELETE", "REPLACE") | M |
| value | oneOf(AttributeNameValuePairSet, AttributeValueChangeSet) | For reporting resource creation or deletion, the optional resource representation (MOC attributes only). In this case, the data type of value is "AttributeNameValuePairSet".  For reporting attribute value changes, the (mandatory) new values and (optional) old values. In this case, the data type of value is "AttributeValueChangeSet". | M |

For a "CREATE" or "DELETE" operation only the host and path components are present in the URI carried by the "path" attribute of "MoiChange". They identify the created or deleted resource. The "value" attribute of "MoiChange" may optionally carry the MOC attribute name value pairs of the created or deleted resource in the format of a map. The keys of the map are equal to the MOC attribute names, and the values are equal to the MOC attribute values.

For a "REPLACE" operation, two cases need to be distinguished.

In the first case, one or more value changes of complete MOC attributes are reported. Only the host and path components are present in the URI carried by the "path" attribute of "MoiChanges". They identify the resource, where attribute value changes occured. The "value" attribute is an array of minimum one and maximum two items. If only one array item is present, it carries the MOC attribute names that changed value and their new values. If the optional second array item is present as well, it carries the MOC attribute names that changed value and their old values. The order of items in the array carries semantics and shall therefore not be reversed.

In the second case, a single value change of an attribute part (sub-attribute) is reported. Here the URI needs to carry, besides the host and path components, also the fragment component. The host and path components identify the resource, where the attribute part value change occured. The fragment component identifies the attribute part inside the resource. The URI fragment is specified using JSON pointer in the URI fragment identifier representation as defined in clause 6 of of RFC 6901 [x]. The context for JSON pointer is the updated resource. The "value" is an array of minimum one and maximum two items. If only one item is present, it carries the name of the attribute part that changed value and its new value. If the optional second array item is present as well, it carries the name of the attribute part that changed value and its old value. Hence also in this case, the order of items in the array carries semantics and shall not be reversed.

For example, the following instance of a "moiChanges" array item reports an object creation

notificationId: 123456789

path: 'https://example.com/3GPP/ClassA=1'

operation: CREATE

value:

attrA:

subAttrA1: ABC

subAttrA2: 56

attrB: XYZ

attrC: 123

or, when omitting the optional attribute name vale pairs of the created object, the instance looks like

notificationId: 123456789

path: 'https://nokia.com/3GPP/ClassA=1'

operation: CREATE

The following instance reports a change of the attributes "attrA" and " attrC" with new and old values

notificationId: 123456789

path: 'https://example.com/3GPP/ClassA=1'

operation: REPLACE

value:

- attrA:

subAttrA1: ABC

subAttrA2: 56

attrC: 123

- attrA:

subAttrA1: DEF

subAttrA2: 67

attrC: 345

and the following with new values only

notificationId: 123456789

path: 'https://example.com/3GPP/ClassA=1'

operation: REPLACE

value:

- attrA:

subAttrA1: ABC

subAttrA2: 56

attrC: 123

When a change of the attribute part "attrA:subAttrA1" shall be reported, the instance looks like

notificationId: 123456789

path: 'https://example.com/3GPP/ClassA=1?attributes/attrA/subAttrA1'

operation: REPLACE

value:

- subAttrA1: ABC

- subAttrA1: DEF

or, with the new value only, like

notificationId: 123456789

path: 'https://example.com/3GPP/ClassA=1?attributes/attrA/subAttrA1'

operation: REPLACE

value:

- subAttrA1: ABC

###### 12.1.1.4.1a.5 Type NotifyMoiCreation

Table 12.1.1.4.1a.5 -1: Definition of type NotifyMoiCreation

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyMOICreation) | M |
| eventTime | DateTime | Event (MOI creation) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| sourceIndicator | SourceIndicator | Indicates the source of the operation that led to the generation of this notification. | O |
| attributeList | AttributeNameValuePairSet | The attributes (name/value pairs) of the created MOI. | O |

###### 12.1.1.4.1a.6 Type NotifyMoiDeletion

Table 12.1.1.4.1a.6 -1: Definition of type NotifyMoiDeletion

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyMOIDeletion) | M |
| eventTime | DateTime | Event (MOI creation) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| sourceIndicator | SourceIndicator | Indicates the source of the operation that led to the generation of this notification. | O |
| attributeList | AttributeNameValuePairSet | Attributes (name/value pairs) of the deleted MOI. | O |

###### 12.1.1.4.1a.7 Type NotifyMoiAttributeValueChanges

Table 12.1.1.4.1a.7 -1: Definition of type NotifyMoiAttributeValueChanges

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyMOIAttributeValueChanges) | M |
| eventTime | DateTime | Event (MOI creation) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| sourceIndicator | SourceIndicator | Indicates the source of the operation that led to the generation of this notification. | O |
| attributeListValueChanges | AttributeValueChangeSet | List with names of changed attributes, together with new value and optionally old value | M |

###### 12.1.1.4.1a.8 Type NotifyMoiChanges

**Table 12.1.1.4.1a.8 -1: Definition of type NotifyMoiChanges**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the local root in the MIB | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4]. | M |
| notificationType | NotificationType | Notification type (notifyMOIChanges) | M |
| eventTime | DateTime | Event (NRM updates) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| moiChanges | array(MoiChange) | MOI changes to be reported | M |

##### 12.1.1.4.2 Void











































































##### 12.1.1.4.3 Void







##### 12.1.1.4.4 Simple data types and enumerations

12.1.1.4.4.1 General

This clause defines simple data types and enumerations that are used by the data structures defined in the previous clauses.

12.1.1.4.4.2 Simple data types

Table 12.1.1.4.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type name | Type definition | Description |

12.1.1.4.4.3 Enumeration CmNotificationTypes

Table 12.1.1.4.4.3-1: Enumeration CmNotificationTypes

|  |  |
| --- | --- |
| Enumeration value | Description |
| notifyMOICreation | Notification type is notifyMOICreation |
| notifyMOIDeletion | Notification type is notifyMOIDeletion |
| notifyMOIAttributeValueChanges | Notification type is notifyMOIAttributeValueChange |
| noitifyMOIChanges | Notification type is notifyMOIChanges |

12.1.1.4.4.4 Enumeration SourceIndicator

Table 12.1.1.4.4.4-1: Enumeration SourceIndicator

|  |  |
| --- | --- |
| Enumeration value | Description |
| RESOURCE\_OPERATION | The notification was generated in response to an internal operation of the resource. |
| MANAGEMENT\_OPERATION | The notification was generated in response to a management operation applied across the managed object boundary external to the managed object |
| SON\_OPERATION | The notification was generated as result of a SON (Self Organising Network) process like self-configuration, self-optimization, self-healing etc. . |
| UNKNOWN | It is not possible to determine the source of the operation. |

12.1.1.4.4.5 Enumeration ScopeType

Table 12.1.1.4.4.4.1-1: Enumeration ScopeType

|  |  |
| --- | --- |
| Enumeration value | Description |
| BASE\_ONLY | Selects only the base resource. The "scopeLevel" parameter shall be absent or ignored if present. |
| BASE\_ALL | Selects the base resource and all of its subordinate resources (incl. the leaf resources). The "scopeLevel" parameter shall be absent or ignored if present. |
| BASE\_NTH\_LEVEL | Selects all resources on the level, which is indicated by the "scopeLevel" parameter, below the base resource. The base resource is at "scopeLevel" zero. |
| BASE\_SUBTREE | Selects the base resource and all of its subordinate resources down to and including the resources on the level indicated by the "scopeLevel" parameter. The base resource is at "scopeLevel" zero. |

12.1.1.4.4.6 Enumeration Operation

Table 12.1.1.4.4.4.6-1: Enumeration Operation

|  |  |
| --- | --- |
| Enumeration value | Description |
| CREATE | Create operation |
| DELETE | Delete operation |
| REPLACE | Replace operation |

### 12.1.2 RESTful HTTP-based solution set for integration with ONAP VES API

#### 12.1.2.1 Mapping of operations

NOTE: this mapping is not part of the present document.

#### 12.1.2.2 Mapping of notifications

##### 12.1.2.2.1 Introduction

###### 12.1.2.2.1.1 General

The 3GPP IS notifications are mapped to SS equivalents according to table 12.1.2.2.1.1-1.

Table 12.1.2.2.1.1-1: Mapping of 3GPP IS notifications to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **3GPP IS notifications** | **HTTP Method** | **Resource URI** | **SQ** |
| notifyMOICreation | POST | /eventListener | M |
| notifyMOIDeletion | POST | /eventListener | M |
| notifyMOIAttributeValueChanges | POST | /eventListener | M |
| notifyMOIChanges | POST | /eventListener | M |

###### 12.1.2.2.1.2 Void

##### 12.1.2.2.2 Notification notifyMOICreation

See clause 12.1.1.2.2..

##### 12.1.2.2.3 Notification notifyMOIDeletion

See clause 12.1.1.2.3.

##### 12.1.2.2.4 Notification notifyMOIAttributeValueChange

See clause 12.1.1.2.4.

##### 12.1.2.2.5 Notification notifyMOIChanges

See clause 12.1.1.2.5.

#### 12.1.2.3 Resources

##### 12.1.2.3.1 Resource structure

Figure 12.1.2.3.1-1 shows the resource structure of the provisioning MnS in the context of its integration with VES Event Listener 7.1.1 [45].



Figure 12.1.2.3.1-1: Resource URI structure of the provisioning MnS for integration with ONAP VES Event Listener 7.1.1 (Resource structure section) [45]

Table 12.1.2.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 12.1.2.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| eventListener | /eventListener | POST | Send notifications |

##### 12.1.2.3.2 Resource definitions

See Resource structure section in [45].

#### 12.1.2.4 Data type definitions

See clause 12.1.1.4.

### 12.1.3 YANG/Netconf-based solution set

#### 12.1.3.1 Mapping of operations

##### 12.1.3.1.1 Introduction

The YANG/Netconf based solution set is based on the 3GPP TS 32.160 [33] clause 6.2 and the IETF RFC 6241 [32] including the Xpath capability.

NOTE: The clauses below omit namespaces for brevity. In NETCONF operations namespaces are included following [34]

##### 12.1.3.1.2 Operation createMOI

The operation is mapped to a NETCONF <edit-config> operation, with XML elements representing the DN path to the MOI, the MOI itself, its id/key and its attributes.

The NETCONF operation attribute on the list representing the newly created MOI should be set to ‘create’.

The default-operation parameter of the <edit-config> operation should be set to none.

The IS operation parameters are mapped to SS equivalents according to table 12.1.3.1.2-1 and table 12.1.3.1.2-2.

Table 12.1.3.1.2-1: Mapping from IS createMOI input parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| IS operation parameter name | SS parameter name | SQ | Remark |
| managedObjectClass | config | M | XML element’s name inside the <config> element. |
| managedObjectInstance | config | M | A sequence of embedded XML elements inside the <config> element. XML elements for all containing MOIs and their ids(keys) shall be included together wilt the XML elements representing the to be created MOI and its key. |
| attributeListIn | config | M | The key leaf, the “attributes container” and leaf, leaf-list or list entries of YANG models representing the attributes. |

Table 12.1.3.1.2-2: Mapping from IS createMOI output parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| IS operation parameter name | SS parameter name | SQ | Remark |
| attributeListOut | no corresponding SS parameter | M | Not supported.  (note 1) |
| status | - | M | OperationSucceeded if NETCONF rpc-reply contains <ok> element.  OperationFailed if NETCONF-reply contains <rpc-error>. |

NOTE 1: Successful Netconf <edit-config> operations only return an <ok> element. Therefore, the attributeListOut can be retrieved via a separate <get-config> operation.

**Examples**

Create ManagedElement=myNode, GNBDUFunction=1

<rpc message-id="101">

<edit-config>

<target>

<running/>

</target>

<default-operation>none</default-operation>

<config>

< ManagedElement>

<id>myNode</id>

<GNBDUFunction operation=”create”>

<id>1</id>

<attributes>

<gNBIdLength>25</gNBIdLength>

<gNBId>357</gNBId>

<priorityLabel>1</priorityLabel>

<gNBDUName>du-south-1</gNBDUName>

<!-- other attributes --->

</attributes>

</GNBDUFunction>

</ManagedElement>

</config>

</edit-config>

</rpc>

<!-- createMO Response -->

<rpc-reply message-id="101" xmlns="urn:ietf:params:xml:ns:netconf:base:1.0">

<ok/>

</rpc-reply>

##### 12.1.3.1.3 Operation getMOIAttributes

This IS operation is mapped to NETCONF <get> or <get-config> operation, depending on whether all configuration and state information is to be retrieved, or configuration data only. (In the next paragraphs only <get> operation is mentioned but <get-config> is always an alternative).

The IS operation patameters baseObjectInstance , (3GPP-)filter, scope, level and attributeListIn are all combined and mapped into the Netconf-filter element. The scopes BASE\_ONLY and BASE\_ALL can be mapped to both subtree and Xpath filtering. The scopes BASE\_NTH\_LEVEL and BASE\_SUBTREE can only be mapped to Xpath filtering.

The IS operation parameters are mapped to SS equivalents according to table 12.1.3.1.3-1 and table 12.1.3.1.3-2.

Table 12.1.3.1.3-1: Mapping of IS getMOIAttributes input parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| IS operation parameter name | SS parameter name | SQ | Remark |
| baseObjectInstance | filter | M | Initial part of the filter element.  For subtree filter this is a set of XML element representing lists containing MOIs together with the leafs representing key values for these MOIs from the root MOI (e.g. ManagedElement) to the baseObjectInstance.  For Xpath filter it is the initial parts of the Xpath expression representing the same information. |
| scope | filter | M | BASE\_ONLY and BASE\_ALL realized by the initial XML elements of the <get> operation. BASE\_SUBTREE and BASE\_NTH\_LEVEL is encoded in the Xpath filter. |
| level | filter | M | Included in the Xpath filter, see examples. (If level is used Xpath filtering must be used.  For BASE\_SUBTREE the levels number is transformed into a number of filter sub-expressions joined by the OR operator.  For BASE\_NTH\_LEVEL included in the Xpath expression as a sequence of ‘\*’ parts (descendant axis) The number of ‘\*’ correspond to the number of levels. |
| filter | filter | M | Netconf Subtree or Xpath filter |
| attributeListIn | filter | M | add the attributes to the subtree or Xpath filter |

Table 12.1.3.1.3-2: Mapping of IS getMOIAttributes output parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| IS operation parameter name | SS parameter name | SQ | Remark |
| managedObjectClass | data | M | Can be extracted from the NETCONF <rpc-reply> <data> elements |
| managedObjectInstance | data | M | Can be extracted from the NETCONF <rpc-reply> <data> elements |
| attributeListOut | data | M | Can be extracted from the NETCONF <rpc-reply> <data> elements |
| status | data | M | rpc-reply or rpc-error indicates general status. |

If scope is ***BASE\_ONLY*** the <get> shall be directed against the “attributes” container of the baseObjectInstance.

**Example 1**

A getMOIAttributes for base object ManagedElement=myNode, scope = BASE\_ONLY, filter=none, attributesListIn=empty is mapped into the following <get-config> operation -

<rpc message-id="101"

xmlns="urn:ietf:params:xml:ns:netconf:base:1.0">

<get-config>

<source>

<running/>

</source>

<filter type="subtree">

<ManagedElement>

<id>myNode</id>

<attributes/>

</ManagedElement>

</filter>

</get-config>

</rpc>

If scope is ***BASE\_ALL*** the <get> shall be directed against the list representing the baseObjectInstance.

**Example 2**

A getMOIAttributes for base object ManagedElement=myNode, scope = BASE\_ALL, filter=, MeasurementControl.pMAdministrativeState=UNLOCKED, attributesListIn=empty.

<rpc message-id="101"

xmlns="urn:ietf:params:xml:ns:netconf:base:1.0">

<get>

<source>

<running/>

</source>

<filter type="subtree">

<ManagedElement>

<id>myNode</id>

<MeasurementControl>

<pMAdministrativeState>

UNLOCKED

</pMAdministrativeState>

</MeasurementControl>

</ManagedElement>

</filter>

</get>

</rpc>

If scope is ***BASE\_SUBTREE*** the <get> shall be directed against the list representing the baseObjectInstance. The Xpath filter expression will need a sub-expression for each level joined by the OR operator.

**Example 3**

A getMOIAttributes for base object ManagedElement=me1, scope = BASE\_ SUBTREE, level=2, filter=none, attributesListIn=empty.

<rpc xmlns="urn:ietf:params:xml:ns:netconf:base:1.0" message-id="101">

<get>

<source>

<running/>

</source>

<filter type="xpath"

select="/me3gpp:ManagedElement[id='me1']/attributes |

/me3gpp:ManagedElement[id='me1']/\*/attributes |

/me3gpp:ManagedElement[id='me1']/\*/\*/attributes" />

</get>

</rpc>

If scope is ***BASE\_NTH\_LEVEL*** the <get> shall be directed against the list representing classes at the N*th* level under the baseObjectInstance. The number of ‘\*’ parts (descendant axis) will correspond to the number of levels.

**Example 4**

A getMOIAttributes for base object ManagedElement=myNode, scope = BASE\_NTH\_LEVEL, level=2, filter=none, attributesListIn=empty.

<rpc xmlns="urn:ietf:params:xml:ns:netconf:base:1.0" message-id="101">

<get>

<source>

<running/>

</source>

<filter type="xpath"

select="/me3gpp:ManagedElement[id='me1']/\*/\*/attributes"/>

</get>

</rpc>

##### 12.1.3.1.4 Operation modifyMOIAttributes

This IS operation modifies one or multiple managed object instances. It is mapped to the NETCONF <edit-config> operation. The NETCONF <edit-config> operation can modify attributes in a given MOI or set of MOIs but only indirectly supports scope or filtered sets of MOIs that are part of the modifyMOIAttributes 3GPP operation specification. <edit-config> needs a config block, containing the explicit config changes to be made for each MOI.

The default-operation parameter should be set to none.

The Netconf operation attribute on the list representing modified MOI(s) should be set to create, replace or delete according to the ENUM in the modificationList.

The IS operation parameters are mapped to SS equivalents according to table 12.1.3.1.4-1 and table 12.1.3.1.4-2.

Table 12.1.3.1.4-1: Mapping of IS modifyMOIAttributes input parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| IS operation parameter name | SS parameter name | SQ | Remark |
| baseObjectInstance | config | M | A sequence of embedded XML elements inside the <config> element. XML elements for all containing MOIs and their ids(keys) shall be included together with the XML elements representing the to be modified MOI and its key. |
| scope | config | M | BASE\_ONLY supported as default. Multiple MOIs can be specified in the same operation, emulating other scopes. |
| filter | config | M | Multiple MOIs can be specified in the same operation, emulating filtering. |
| modificationList | config | M | The “attributes container” and leaf, leaf-list or list entries representing the attributes. |

Table 12.1.3.1.4-2: Mapping of IS modifyMOIAttributes output parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter name** | **SQ** | **Remark** |
| modificationListOut | no corresponding SS parameter | M | Not supported.  (note 1) |
| status | - | M | rpc-reply or rpc-error indicates general status.  The following elements give detailed error information:  <error-tag>  <error-path> |

Note 1: Successful Netconf <edit-config> operations only return an <ok> element. Therefore, the attributeListOut can be retrieved via a separate <get-config> operation.

##### 12.1.3.1.5 Operation deleteMOI

This IS operation deletes one or multiple managed object instances. It is mapped to the NETCONF <edit-config> operation. <edit-config> can delete one or more specific MOIs but only indirectly supports scope or filtered sets of MOIs that are part of the generic deleteMOI 3GPP operation specification. <edit-config> uses a config block, indicating the MOI(s) to be deleted.

The Netconf operation attribute on the list representing the baseObjectInstance should be set to delete or remove.

The default-operation parameter should be set to none.

The IS operation parameters are mapped to SS equivalents according to table 12.1.3.1.5-1 and table 12.1.3.1.5-2.

Table 12.1.3.1.5-1: Mapping of IS deleteMOI input parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter name** | **SQ** | **Remark** |
| baseObjectInstance | config | M | A sequence of embedded XML elements inside the <config> element. XML elements for all containing MOIs and their ids(keys) shall be included together wilt the XML elements representing the to be deleted MOI and its key. |
| scope | config | M | BASE\_ONLY supported as default. Multiple MOIs can be specified in the same operation, emulating other scopes. |
| filter | config | M | Multiple MOIs can be specified in the same operation, emulating filtering. |

Table 12.1.3.1.5-2: Mapping of IS deleteMOI output parameters to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter name** | **SQ** | **Remark** |
| deletionList | no corresponding SS parameter | M | Not supported.  (note 1) |
| status | - | M | rpc-reply or rpc-error indicates general status.  The following elements give detailed error information:  <error-tag>  <error-path> |

NOTE 1: Successful Netconf <edit-config> operations only return an <ok> element. Therefore, the deletionList can be retrieved via a separate <get-config> operation.

## 12.2 Generic fault supervision management service

### 12.2.1 RESTful HTTP-based solution set

#### 12.2.1.1 Mapping of operations

##### 12.2.1.1.1 Introduction

The IS operations are mapped to SS equivalents according to table 12.2.1.1.1-1.

Table 12.2.1.1.1-1: Mapping of IS operations to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation** | **HTTP Method** | **Resource URI** | **S** |
| getAlarmList | GET | /alarms | M |
| getAlarmCount | GET | /alarms/alarmCount | O |
| acknowledgeAlarms | PATCH | /alarms | M |
| PATCH | /alarms/{alarmId} | M |
| unacknowledgeAlarms | PATCH | /alarms | M |
| PATCH | /alarms/{alarmId} | M |
| clearAlarms | PATCH | /alarms | M |
| PATCH | /alarms/{alarmId} | M |
| setComment | POST | /alarms/{alarmId}/comment | O |
| subscribe | POST | /subscriptions | M |
| unsubscribe | DELETE | /subscriptions/{subscriptionId} | M |

##### 12.2.1.1.2 Operation getAlarmList

The IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.2-1 and table 12.2.1.1.2-2.

Table 12.2.1.1.2-1: Mapping of IS operation input parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ISparameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| alarmAckState | query | alarmAckState | AlarmAckState- | O |
| baseObjectClass  baseObjectInstance | query | baseObjectInstance | Dn | O |
| filter | query | filter | Filter | O |

Table 12.2.1.1.2-2: Mapping of IS operation output parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| alarmInformationList | response body | n/a | map(NotificationHeader, AlarmRecord, comments(map(Comment))) | M |
| status | response status codes | n/a | n/a | M |

The message flow is as follows:

1. The MnS consumer sends a HTTP GET request to the MnS producer.

- The URI identifies the "…/alarms" collection resource.

- The querycomponent may contain three optional parameters: "alarmAckstate", "baseObjectInstance" and "filter". Absence of the query component means all alarms shall be returned.

- The request message body shall be empty.

2. The MnS producer sends a HTTP GET response to the MnS consumer.

- On success "200 OK" shall be returned. The response message body shall contain the queried alarm records, the notification headers of the last "notifyNewAlarm", "notifyChangedAlarm" or "notifyClearedAlarm" notifications, which were sent related to the alarms, and the comments associated to the alarms.

- On failure, an appropriate error code shall be returned. The response message body may carry additional error information.

##### 12.2.1.1.3 Operation getAlarmCount

The IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.3-1 and table 12.2.1.1.3-2.

Table 12.2.1.1.3-1: Mapping of IS operation input parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| alarmAckState | query | alarmAckState | AlarmAckState- | O |
| filter | query | filter | string | O |

Table 12.2.1.1.3-2: Mapping of IS operation output parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| criticalCount, majorCount, minorCount, warningCount, indeterminateCount, clearedCount | response body | n/a | AlarmCount | M |
| status | response status codes | n/a | n/a | M |

The message flow is as follows:

1. The MnS consumer sends a HTTP GET request to the MnS producer.

- The URI identifies the "…/alarms/alarmsCount" collection resource.

- The query component may contain two optional parameters: "alarmAckstate" and "filter". Absence of the query component means all alarms shall be counted.

- The request message body shall be empty.

2. The MnS producer sends a HTTP GET response to the MnS consumer.

- On success "200 OK" shall be returned. The response message body shall carry the alarm count for all perceived severity values. The response format is defined by "AlarmsCount".

- On failure, an appropriate error code shall be returned. The response message body may carry additional error information.

##### 12.2.1.1.4 Operation setComment

In case a comment shall be added to a single alarm the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.4-1 and table 12.2.1.1.4-2.

Table 12.2.1.1.4-1: Mapping of IS operation input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| alarmInformationReferenceList | path | /alarms/{alarmId}/comment | string | M |
| commentUserId | request body | commentUserId | commentUserId | M |
| commentSystemId | request body | commentSystemId | commentSystemId | O |
| commentText | request body | commentText | commentText | M |

Table 12.2.1.1.4-2: Mapping of IS operation output parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| badAlarmInformationReferenceList | response body | n/a | ErrorResponse | M |
| status | response status codes | n/a | n/a | M |

The message flow for adding a comment to a single alarm is as follows:

1. The MnS consumer sends a HTTP POST request to the MnS producer.

- The URI identifies the "…/alarms/{alarmId}/comment" alarm resource the comment shall be added to.

- The query component shall be absent.

- The request message body shall contain a JSON object with "commentUserId" and "commentText" properties. In addition to that the request object may contain the "commentSystemId" property. .

2. The MnS producer sends a HTTP POST response to the MnS consumer.

- On success "201 Created " shall be returned. The response message body shall carry the representation of the created comment resource. The Location header shall be present and carry the URI of the created comment resource.

- On failure, an appropriate error code shall be returned. The response message body may carry additional error information.

The stage 3 solution does not support adding a comment to multiple alarms.

##### 12.2.1.1.5 Operation acknowledgeAlarms

In case a single alarm shall be acknowledged the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.5-1 and table 12.2.1.1.5-2.

Table 12.2.1.1.5-1: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| alarmInformationAndSeverityReferenceList | path | /{alarmId} | string | M |
| ackUserId | request body | ackUserId | AckUserId | M |
| ackSystemId | request body | ackSystemId | AckSystemId | O |

The perceived severity is not mapped in the present documet.

Table 12.2.1.1.5-2: Mapping of IS operation output parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| badAlarmInformationReferenceList | response body | n/a | errorResponse | M |
| status | response status codes | n/a | n/a | M |

The message flow for acknowledging a single alarm is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The URI identifies the "…/alarms/{alarmId}" alarm resource to be acknowledged.

- The query component is absent..

- The request message body contains a merge patch document. The document shall patch the "ackState" and "ackUserId" property of the identified alarm resource, and may patch the "ackSystemId" property. The patch document is defined by "MergePatchAcknowledgeAlarms".

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success "204 No Content" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body shall return the alarmId, together with failure reason. The response message body may carry additional error information.

In case multiple alarms shall be acknowledged the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.5-3 and table 12.2.1.1.5-4.

Table 12.2.1.1.5-3: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| alarmInformationAndSeverity  ReferenceList | path  request body | /alarms  alarmId (key in map) | n/a  string | M  M |
| ackUserId | request body | ackUserId | ackUserIdType | M |
| ackSystemId | request body | ackSystemId | ackSystemIdType | O |

The perceived severity is not mapped in the present document.

Table 12.2.1.1.5-4: Mapping of IS operation output parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| badAlarmInformationReferenceList | response body | n/a | array(failedAlarm) | M |
| status | response status codes | n/a | n/a | M |

The message flow for acknowledging multiple alarms is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The URI identifies the "…/alarms" collection resource.

- The query component is absent..

- The request message body contains a merge patch document. The document shall patch the "ackState" and "ackUserId" property of the identified alarm resources, and my patch the "ackSystemId" property. The patch document is defined by "MergePatchAcknowledgeAlarms".

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success "200 OK" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body shall return a list with the alarmId's that did not exist or were identifying alarms that could not be acknowledged, together with the failure reasons.

##### 12.2.1.1.6 Operation unacknowledgeAlarms

In case a single alarm shall be unacknowledged the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.6-1 and table 12.2.1.1.6-2.

Table 12.2.1.1.6-1: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| alarmInformationReferenceList | path | /{alarmId} | string | M |
| ackUserId | request body | ackUserId | AckUserId | M |
| ackSystemId | request body | ackSystemId | AckSystemId | O |

Table 12.2.1.1.6-2: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| badAlarmInformationReferenceList | response body | n/a | errorResponse | M |
| status | response status codes | n/a | n/a | M |

The message flow for unacknowledging a single alarm is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The URI identifies the "…/alarms/{alarmId}" alarm resource to be acknowledged.

- The query component is absent.

- The request message body contains a merge patch document. The document shall patch the "ackState" and "ackUserId" property of the identified alarm resource, and may patch the "ackSystemId" property. The patch document is defined by "MergePatchAcknowledgeAlarms".

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success "204 No Content" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body may carry additional error information.

In case multiple alarms shall be unacknowledged the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.6-3 and table 12.2.1.1.6-4.

Table 12.2.1.1.6-3: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| alarmInformationReferenceList | path  request body | /alarms  alarmId (key in map) | n/a  string | M  M |
| ackUserId | request body | ackUserId | AckUserId | M |
| ackSystemId | request body | ackSystemId | AckSystemId | O |

Table 12.2.1.1.6-4: Mapping of IS operation output parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| badAlarmInformationReferenceList | response body | error | array(failedAlarm) | M |
| status | response status codes | n/a | n/a | M |

The message flow for unacknowledging multiple alarms is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The URI identifies the "…/alarms" collection resource.

- The query component is absent.

- The request message body contains a merge patch document. The document shall patch the "ackState" and "ackUserId" property of the identified alarm resources, and my patch the "ackSystemId" property. The patch document is defined by "MergePatchAcknowledgeAlarms".

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success "200 OK" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body shall return a list with the alarmId's that did not exist or were identifying alarms that could not be unacknowledged, together with the failure reasons.

##### 12.2.1.1.7 Operation clearAlarms

In case a single alarm shall be cleared the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.7-1 and table 12.2.1.1.7-2.

Table 12.2.1.1.7-1: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| alarmInformationReferenceList | path | /{alarmId} | string | M |
| clearUserId | request body | clearUserId | ClearUserId | M |
| clearSystemId | request body | clearSystemId | ClearSystemId | O |

Table 12.2.1.1.7-2: Mapping of IS operation output parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| badAlarmInformationReferenceList | response body | n/a | errorResponse | M |
| status | response status codes | n/a | n/a | M |

The message flow for clearing a single alarm is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The URI identifies the "…/alarms/{alarmId}" alarm resource.

- The query component is absent.

- The request message body contains a merge patch document. The document shall patch the "clearUserId" property, may patch the "clearSystemId" property and shall patch the "perceivedSeverity" property of the identified alarm resource represented by an "alarmRecord" object. The patch document is defined by "MergePatchClearAlarms".

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success "204 No content" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body shall return the alarmId that did not exist or was identifying an alarm that could not be cleared together with a failure reason. The JSON document carried in the response shall comply to "FailedAlarms-Response" .

In case multiple alarms shall be cleared the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.7-3 and table 12.2.1.1.7-4.

Table 12.2.1.1.7-3: Mapping of IS operation input parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| alarmInformationReferenceList | path  request body | /alarms  alarmId (key in map) | n/a  string | M  M |
| clearUserId | request body | clearUserId | ClearUserId | M |
| clearSystemId | request body | clearSystemId | ClearSystemId | O |

Table 12.2.1.1.7-4: Mapping of IS operation output parameters to SS equivalents (HTTP PATCH)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| badAlarmInformationReferenceList | response body | n/a | array(failedAlarm) | M |
| status | response status codes | n/a | n/a | M |

The message flow for clearing multiple alarms is as follows:

1. The MnS consumer sends a HTTP PATCH request to the MnS producer.

- The URI identifies the "…/alarms" collection resource.

- The query component is absent..

- The request message body contains a merge patch document. The document shall patch the "clearUserId" property, may patch the "clearSystemId" property and shall patch the "perceivedSeverity" property of the identified alarm resources . The patch document is defined by "patchClearAlarms-RequestType".

2. The MnS producer sends a HTTP PATCH response to the MnS consumer.

- On success "200 OK" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body shall return a list with the alarmId's that did not exist or were identifying alarms that could not be cleared, together with the failure reasons.

##### 12.2.1.1.8 Operation subscribe

The IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.8-1 and table 12.2.1.1.8-2.

Table 12.2.1.1.8-1: Mapping of IS operation input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| consumerReference | request body | consumerReference | Uri | M |
| timeTick | request body | timeTick | integer | O |
| filter | request body | filter | Filter | O |

Table 12.2.1.1.8-2: Mapping of IS operation output parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| subscriptionId | Location header | n/a | Uri | M |
| status | response status code | n/a | n/a | M |

The procedure for subscribing to notifications is as follows:

1. The MnS consumer sends a HTTP POST request to the MnS producer.

- The URI identifies the "…/subscriptions" collection resource.

- The query component shall be absent.

- The request message body shall carry a data structure of type "Subscription". This data structure contains filtering criteria and a consumer side URI to which the provider will subsequently send notifications about events that match the filter.

2. The MnS producer creates a new subscription for notifications related to fault management, and a resource that represents this subscription.

3. The MnS producer sends a HTTP POST response to the MnS consumer.

- On success "201 Created " shall be returned. The response message body shall carry the representation of the created subscription resource. The Location header shall be present and carry the URI of the created subscription resource.

- On failure, an appropriate error code shall be returned. The response message body may carry additional error information.

##### 12.2.1.1.9 Operation unsubscribe

In case one subscription shall be cancelled the IS operation parameters are mapped to SS equivalents according to table 12.2.1.1.9-1 and table 12.2.1.1.9-2.

Table 12.2.1.1.9-1: Mapping of IS operation input parameters to SS equivalents (HTTP DELETE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| consumerReference | -- | -- | -- | -- |
| subscriptionId | path | /subscriptions/{subscriptionId} | string | M |

Table 12.2.1.1.9-2: Mapping of IS operation output parameters to SS equivalents (HTTP DELETE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| status | response status codes | n/a | n/a | M |

The consumer reference is not mapped in the present document.

The procedure for unsubscribing from one subscription is as follows:

1. The MnS consumer sends a HTTP DELETE request to the MnS producer.

- The URI identifies the "…/subscriptions/{subscriptionId}" subscription resource.

- The querycomponent shall be absent.

- The request message body shall be empty.

2. The MnS producer sends a HTTP DELETE response to the MnS consumer.

- On success "204 No Content" shall be returned. The response message body shall be empty.

- On failure, an appropriate error code shall be returned. The response message body may carry an error object.

#### 12.2.1.2 Mapping of notifications

##### 12.2.1.2.1 Introduction

The IS notifications are mapped to SS equivalents according to table 12.2.1.2.1-1.

**Table 12.2.1.2.1-1: Mapping of IS notifications to SS equivalents**

|  |  |  |  |
| --- | --- | --- | --- |
| IS operations | HTTP Method | Resource URI | S |
| notifyNewAlarm | POST | /notificationTarget | M |
| notifyAckStateChanged | POST | /notificationTarget | M |
| notifyClearedAlarm | POST | /notificationTarget | M |
| notifyAlarmListRebuilt | POST | /notificationTarget | M |
| notifyChangedAlarm | POST | /notificationTarget | M |
| notifyComments | POST | /notificationTarget | M |
| notifyPotentialFaultyAlarmList | POST | /notificationTarget | M |
| notifyCorrelatedNotificationChanged | POST | /notificationTarget | M |
| notifyChangedAlarmGeneral | POST | /notificationTarget | O |

##### 12.2.1.2.2 Notification notifyNewAlarm (non-security alarm)

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.2-1.

**Table 12.2.1.2.2-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | M |
| specificProblem | request body | specificProblem | SpecificProblem | O |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| backedUpStatus | request body | backedUpStatus | boolean | O |
| backUpObject | request body | backUpObject | Dn | O |
| trendIndication | request body | trendIndication | TrendIndication | O |
| thresholdInfo | request body | thresholdInfo | ThresholdInfo | O |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| stateChangeDefinition | request body | stateChangeDefinition | AttributeValueChangeSet | O |
| monitoredAttributes | request body | monitoredAttributes | AttributeNameValuePairSet | O |
| proposedRepairActions | request body | proposedRepairActions | string | O |
| additionalText | request body | additionalText | string | O |
| additionalInformation | request body | additionalInformation | AttributeNameValuePairSet | O |

##### 12.2.1.2.3 Notification notifyNewAlarm (security alarm)

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.3-1.

**Table 12.2.1.2.3-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | M |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| additionalText | request body | additionalText | string | O |
| additionalInformation | request body | additionalInformation | AttributeNameValuePairSet | O |
| rootCauseIndicator | request body | rootCauseIndicator | boolean | O |
| serviceUser | request body | serviceUser | string | M |
| serviceProvider | request body | serviceProvider | string | M |
| securityAlarmDetector | request body | securityAlarmDetector | string | M |

##### 12.2.1.2.4 Notification notifyAckStateChanged

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.4-1.

**Table 12.2.1.2.4-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri- | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType- | M |
| eventTime | request body | eventTime | DdteTime- | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId- | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | M |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | M |
| ackState | request body | ackState | AckState | M |
| ackUserId | request body | ackUserId | string | M |
| ackSystemId | request body | ackSystemId | string | O |

##### 12.2.1.2.5 Notification notifyClearedAlarm

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.5-1.

**Table 12.2.1.2.5-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri- | M |
| notificationId | request body | notificationId | NotificationId- | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN- | M |
| alarmId | request body | alarmId | AalarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | M |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification | O |
| clearUserId | request body | clearUserId | string | O |
| clearSystemId | request body | clearSystemId | string | O |

##### 12.2.1.2.6 Notification notifyAlarmListRebuilt

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.6-1.

**Table 12.2.1.2.6-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| reason | request body | reason | string | M |
| alarmListAlignmentRequirement | request body | alarmListAlignmentRequirement | AlarmListAlignmentRequirement | O |

##### 12.2.1.2.7 Notification notifyChangedAlarm

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.7-1.

**Table 12.2.1.2.7-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri-e | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType- | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | M |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | M |

##### 12.2.1.2.8 Notification notifyComments

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.8-1.

**Table 12.2.1.2.8-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri-e | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | M |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | M |
| comments | request body | comments | map(Comment) | M |

##### 12.2.1.2.9 Notification notifyPotentialFaultyAlarmList

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.9-1.

**Table 12.2.1.2.9-1: Mapping of IS notification parameters to SS equivalents**

| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| --- | --- | --- | --- | --- |
| objectClass,  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| reason | request body | reason | string | M |

##### 12.2.1.2.10 Notification notifyCorrelatedNotificationChanged

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.10-1.

**Table 12.2.1.2.10-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri- | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | M |
| rootCauseIndicator | request body | rootCauseIndicator | boolean | O |

##### 12.2.1.2.11 Notification notifyChangedAlarmGeneral (non-security alarm)

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.11-1.

**Table 12.2.1.2.11-1: Mapping of IS notification parameters to SS equivalents**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | O |
| specificProblem | request body | specificProblem | SpecificProblem | O |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | O |
| backedUpStatus | request body | backedUpStatus | booleanbackedUpStatus | O |
| backUpObject | request body | backUpObject | Dn | O |
| trendIndication | request body | trendIndication | TrendIndication | O |
| thresholdInfo | request body | thresholdInfo | ThresholdInfo | O |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| stateChangeDefinition | request body | stateChangeDefinition | AttributeValueChangeSet | O |
| monitoredAttributes | request body | monitoredAttributes | AttributeNameValuePairSet | O |
| proposedRepairActions | request body | proposedRepairActions | string | O |
| additionalText | request body | additionalText | string | O |
| additionalInformation | request body | additionalInformation | AttributeNameValuePairSet | O |
| rootCauseIndicator | request body | rootCauseIndicator | booleanr | O |
| changedAlarmAttributes | request body | changedAlarmAttributes | AttributeNameValuePairSet | O |

##### 12.2.1.2.12 Notification notifyChangedAlarmGeneral (security alarm)

The IS notification parameters are mapped to SS equivalents according to table 12.2.1.2.12-1.

Table 12.2.1.2.12-1: Mapping of IS notification parameters to SS equivalents

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS parameter name | SS parameter location | SS parameter name | SS parameter type | S |
| objectClass,  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | SystemDN | M |
| alarmId | request body | alarmId | AlarmId | M |
| alarmType | request body | alarmType | AlarmType | M |
| probableCause | request body | probableCause | ProbableCause | O |
| perceivedSeverity | request body | perceivedSeverity | PerceivedSeverity | O |
| correlatedNotifications | request body | correlatedNotifications | array(CorrelatedNotification) | O |
| additionalText | request body | additionalText | string | O |
| additionalInformation | request body | additionalInformation | AttributeNameValuePairSet | O |
| rootCauseIndicator | request body | rootCauseIndicator | boolean | O |
| serviceUser | request body | serviceUser | string | M |
| serviceProvider | request body | serviceProvider | string | M |
| securityAlarmDetector | request body | securityAlarmDetector | string | M |
| changedAlarmAttributes | request body | changedAlarmAttributes | AttributeNameValuePairSet | M |

#### 12.2.1.3 Resources

##### 12.2.1.3.1 Resource structure

12.2.1.3.1.1 Resource structure on the MnS producer

Figure 12.2.1.3.1.1-1 shows the resource structure of the Fault Supervision MnS on the MnS producer.



Figure 12.2.1.3.1-1: Resource URI structure of the Fault Supervision MnS on the MnS producer

Table 12.2.1.3.1.1-1 provides an overview of the resources and applicable HTTP methods.

Table 12.2.1.3.1.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Alarms | .../alarms | GET | Retrieve all alarms or a filtered subset |
| PATCH | Clear, acknowledge or unacknowledge multiple alarms |
| Alarm Count | .../alarms/alarmCount | GET | Retrieve the alarm count per perceived severity |
| Alarm | .../alarms/{alarmId} | PATCH | Clear, acknowledge or unacknowledge an alarm |
| Comments | .../alarms/{alarmId}/comments | POST | Add a comment to an alarm |
| Subscriptions | .../subscriptions | POST | Create a subscription |
| Subscription | .../subscriptions/{subscriptionId} | DELETE | Delete a subscription |

###### 12.2.1.3.1.2 Resource structure on the MnS consumer

Figure 12.2.1.3.1.2-1 shows the resource structure of the Fault Supervision MnS on the MnS consumer.



Figure 12.2.1.3.1.2-1: Resource URI structure of the Fault Supervision MnS on the MnS consumer

Table 12.2.1.3.1.2-1 provides an overview of the resources and applicable HTTP methods.

Table 12.2.1.3.1.2-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Notification Target | {notificationTarget} | POST | Send a notification to the notification target |

##### 12.2.1.3.2 Resource definitions

###### 12.2.1.3.2.1 Resource "…/alarms"

12.2.1.3.2.1.1 Description

This resource represents a collection of alarms.

12.2.1.3.2.1.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/alarms

The resource URI variables are defined in table 12.2.1.3.2.1.2-1.

Table 12.2.1.3.2.1.2-1: URI variables

|  |  |
| --- | --- |
| **Name** | **Definition** |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |

12.2.1.3.2.1.3 HTTP methods

12.2.1.3.2.1.3.1 HTTP GET

This method shall support the URI query parameters specified in the following table.

Table 12.2.1.3.2.1.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| alarmAckState | AlarmAckState |  | O |
| href | Dn |  | O |
| filter | string |  | O |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

Table 12.2.1.3.2.1.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| n/a |  |  |

Table 12.2.1.3.2.1.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| GetAlarmsResponse | 200 OK | The alarms returned. | M |
| ErrorResponse | 4xx/5xx | Returned in case of an error | O |

12.2.1.3.2.1.3.2 Void

12.2.1.3.2.1.3.3 HTTP PATCH

This method shall support the URI query parameters specified in the following table.

Table 12.2.1.3.2.1.3.3-1: URI query parameters supported by the PATCH method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

Table 12.2.1.3.2.1.3.3-2: Data structures supported by the PATCH Request Body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| map(MergePatchAcknowledgeAlarm) | Patch document for acknowledging one or multiple alarms | M |
| map(MergePatchClearAlarm) | Patch document for clearing one or multiple alarms | M |

Table 12.2.1.3.2.1.3.3-3: Data structures supported by the PATCH Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| n/a | 204 No Content | In case of success the response body shall be empty. | M |
| FailedAlarms-Response | 4xx/5xx | In case of failure, the response body shall carry a JSON object described by the "FailedAlarmsResponse" format. | M |

###### 12.2.1.3.2.2 Resource "…/alarms /{alarmId}"

12.2.1.3.2.2.1 Description

This resource represents an alarm.

12.2.1.3.2.2.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/alarms/{alarmId}

The resource URI variables are defined in table 12.2.1.3.2.2.2-1.

Table 12.2.1.3.2.2.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |
| alarmId | Alarm identifier |

12.2.1.3.2.2.3 HTTP methods

12.2.1.3.2.2.3.1 HTTP PATCH

This method shall support the URI query parameters specified in the following table.

Table 12.2.1.3.2.2.3.1-1: URI query parameters supported by the PATCH method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| n/a |  |  |  |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

Table 12.2.1.3.2.2.3.1-2: Data structures supported by the PATCH Request Body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| MergePatchAcknowledgeAlarm | Patch document for acknowledging an alarm | M |
| MergePatchClearAlarm | Patch document for clearing an alarm | M |

Table 12.2.1.3.2.2.3.1-3: Data structures supported by the PATCH Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **S** |
| n/a | 200 OK | In case of success the response body shall be empty. |  |
| ErrorResponse | 4xx/5xx | In case of failure, the response body shall carry a JSON object described by "ErrorResponse". |  |

###### 12.2.1.3.2.3 Resource "…/alarms/alarmCount"

12.2.1.3.2.3.1 Definition

This resource holds metadata about the /alarms collection resource like the alarm count per perceived severity.

12.2.1.3.2.3.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/alarms/alarmCount

The resource URI variables are defined in table 12.2.1.3.2.3.2-1.

Table 12.2.1.3.2.3.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |

12.2.1.3.2.3.3 HTTP methods

12.2.1.3.2.3.3.1 GET

This method shall support the URI query parameters specified in table 12.2.1.3.2.3.3.1-1.

Table 12.2.1.3.2.3.3.3-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | S |
| alarmAckState | AlarmAckState | Allows to control which alarms are counted based on acknowledgement state | O |
| filter | string | Allows to control which alarms are counted based on a general filter applied to the alarm records. | O |

This method shall support the request data structures specified in table 12.2.1.3.2.3.3.1-2 and the response data structures and response codes specified in table 12.2.1.3.2.3.3.1-3.

Table 12.2.1.3.2.3.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | S |
| n/a |  |  |

Table 12.2.1.3.2.3.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | S |
| AlarmsCount | 200 OK | The alarm count per severity level returned. | M |
| ErrorResponse | 4xx/5xx | Returned in case of an error | O |

###### 12.2.1.3.2.4 Resource "…/alarms/{alarmId}/comments"

12.2.1.3.2.4.1 Definition

This resource is a collection resource for comments attached to an alarm.

12.2.1.3.2.4.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/alarms/{alarmId}/comments

The resource URI variables are defined in table 12.2.1.3.2.4.2-1.

Table 12.2.1.3.2.4.2-1: URI variables

|  |  |
| --- | --- |
| **Name** | **Definition** |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |
| alarmId | Alarm identifier |

12.2.1.3.2.4.3 HTTP methods

12.2.1.3.2.4.3.1 POST

This method shall support the URI query parameters specified in the following table.

Table 12.2.1.3.2.4.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **S** |
| n/a |  |  |  |

This method shall support the request data structures, and the response data structures and response codes specified in the following tables.

Table 12.2.1.3.2.4.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **S** |
| Comment | The representation of the comment to be added to an alarm. | M |

Table 12.2.1.3.2.4.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | S |
| Comment-ResponseType | 201 Created | In case of success, the response body shall be carry the representation of a comment. The "commentTime" shall be set by the MnS producer. | M |
| ErrorResponse | 4xx/5xx | In case of failure, the response body shall be described by "ErrorResponse". | M |

###### 12.2.1.3.2.5 Resource "…/comments/{commentId}"

12.2.1.3.2.5.1 Definition

This resource represents a comment attached to an alarm.

12.2.1.3.2.5.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/alarms/{alarmId}/comments/{commentId}

The resource URI variables are defined in table 12.2.1.3.2.4.5-1.

Table 12.2.1.3.2.4.5-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |
| alarmId | Alarm identifier |
| commentId | Comment identifier |

12.2.1.3.2.5.3 HTTP methods

None.

###### 12.2.1.3.2.6 Resource "…/subscriptions"

12.2.1.3.2.6.1 Description

This resource is a container resource for individual subscriptions.

12.2.1.3.2.6.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/subscriptions

The resource URI variables are defined in table 12.2.1.3.2.6.2-1.

Table 12.2.1.3.2.6.2-1: URI variables

|  |  |  |
| --- | --- | --- |
| **Name** | | **Definition** |
| MnSRoot | | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] | |

12.2.1.3.2.6.3 HTTP methods

12.2.1.3.2.6.3.1 POST

This method shall support the URI query parameters specified in table 12.2.1.3.2.6.3.1-1.

Table 12.2.1.3.2.6.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | S |
| n/a |  |  |  |

This method shall support the request data structures specified in table 12.2.1.3.2.6.3.1-2 and the response data structures and response codes specified in table 12.2.1.3.2.6.3.1-3.

Table 12.2.1.3.2.6.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | S |
| Subscription | Details of the subscription to be created | M |

Table 12.2.1.3.2.6.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | S |
| Subscription | 201 Created | In case of success the representation of the created subscription is returned. | M |
| ErrorResponse | 4xx/5xx | In case of failure the error object is returned. | M |

12.2.1.3.2.6.3.2 Void

###### 12.2.1.3.2.7 Resource "…/subscriptions/{subscriptionId}"

12.2.1.3.2.7.1 Description

This resource represents a subscription.

12.2.1.3.2.7.2 URI

Resource URI: {MnSRoot}/FaultSupervisionMnS/{MnSVersion}/ subscriptions/{subscriptionId}

The resource URI variables are defined in table 12.2.1.3.2.7.2-1.

Table 12.2.1.3.2.7.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| MnSRoot | See clause 4.4.2 of TS 32.158 [15] |
| MnSVersion | See clause 4.4.2 of TS 32.158 [15] |
| subscriptionId | Subscription identifier |

12.2.1.3.2.7.3 HTTP methods

12.2.1.3.2.7.3.1 DELETE

This method shall support the URI query parameters specified in table 12.2.1.3.2.7.3.1-1.

Table 12.2.1.3.2.7.3.1-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | S |
| n/a |  |  |  |

This method shall support the request data structures specified in table 12.2.1.3.2.7.3.1-2 and the response data structures and response codes specified in table 12.2.1.3.2.7.3.1-3.

Table 12.2.1.3.2.7.3.1-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | S |
| n/a |  |  |

Table 12.2.1.3.2.7.3.1-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | S |
| n/a | 204 No Content | In case of success no message body is returned | M |
| ErrorResponse | 4xx/5xx | In case of failure the error object is returned. | M |

###### 12.2.1.3.2.8 Resource "{notificationTarget}"

12.2.1.3.2.8.1 Description

This resource represents a notification target on the MnS consumer.

12.2.1.3.2.8.2 URI

Resource URI: {notificationTarget}

The resource URI variables are defined in table 12.2.1.3.2.8.2-1.

Table 12.2.1.3.2.8.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| notificationTarget | URI of the notification target on the MnS consumer, contained in the notification subscription |

12.2.1.3.2.8.3 HTTP methods

12.2.1.3.2.8.3.1 POST

This method shall support the URI query parameters specified in table 12.2.1.3.2.8.3.1-1.

Table 12.2.1.3.2.8.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | S |
| n/a |  |  |  |

This method shall support the request data structures specified in table 12.2.1.3.2.8.3.1-2 and the response data structures and response codes specified in table 12.2.1.3.2.8.3.1-3.

Table 12.2.1.3.2.8.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Data type | | Description | | S | |
| NotifyNewAlarm | | Type for a notifyNewAlarm notification (non-security alarm) | | M | |
| NotifyNewSecurityAlarm- | | Type for a notifyNewAlarm notification (security alarm) | | M | |
| NotifyAckStateChanged | | Type for a notifyAckStateChanged notification | | M | |
| NotifyClearedAlarm | | Type for a notifyClearedAlarm notification | | M | |
| NotifyAlarmListRebuilt | | Type for a notifyAlarmListRebuilt notification | | M | |
| NotifyChangedAlarm | | Type for a notifyChangedAlarm notification | | M | |
| NotifyComments | | Type for a notifyComments notification | | M | |
| NotifyPotentialFaultyAlarmList | | Type for a notifyPotentialFaultyAlarmList notification is sent | | M | |
| NotifyCorrelatedNotificationChanged | | Type for a notifyCorrelatedNotificationChanged notification (non-security alarm) | | M | |
| NotifyChangedAlarmGeneral | | Type for a notifyChangedAlarmGeneral notification is sent | | M | |
| NotifyChangedSecAlarmGeneral | | Type for a notifyChangedAlarmGeneral notification (security alarm) | | M | |

Table 12.2.1.3.2.8.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | S |
| n/a | 204 No Content | In case of success no message body is returned | M |
| ErrorResponse | 4xx/5xx | In case of failure the error object is returned. | M |

#### 12.2.1.4 Data type definitions

##### 12.2.1.4.1 General

This clause defines the data types used by the Fault Supervision MnS. Table 12.2.1.4.1-1 specifies the data types defined in the present document and table 12.2.1.4.1-2 the data types imported.

Table 12.2.1.4.1-1: Data types defined in the present document

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Description |
| AlarmAckState | 12.2.1.4.3.4 | Used in the query part of HTTP GET on /alarms to discriminate alarms to be returned or counted |
| AlarmId | 12.2.1.4.4.2 | Alarm identifier, see clause 11.2.2.1.5.1 |
| AlarmType | 12.2.1.4.4.6 | Alarm type as defined in ITU-T Rec. X. 733 [4] |
| ProbableCause | 12.2.1.4.4.7 | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] |
| PerceivedSeverity | 12.2.1.4.4.9 | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] |
| TrendIndication | 12.2.1.4.4.10 | Severity trend of the alarmed object as defined in ITU-T Rec. X. 733 [4] |
| ThresholdHysteresis | 12.2.1.4.1a.1 | Used in the definition of ThresholdInfo as defined in ITU-T Rec. X. 733 [4] |
| ThresholdLevelInd | 12.2.1.4.1a.2 | Used in the definition of ThresholdInfo as defined in ITU-T Rec. X. 733 [4] |
| ThresholdInfo | 12.2.1.4.1a.3 | Provides information for threshold crossing alarms as defined in ITU-T Rec. X. 733 [4] |
| CorrelatedNotification | 12.2.1.4.1a.4 | Describes the correlated notifications of a single source |
| AckState | 12.2.1.4.4.4 | Acknowledgement state, see clause 11.2.2.1.5.1 |
| AlarmNotificationTypes | 12.2.1.4.4.8 | Alarm notification types (notifyNewAlarm, etc.) |
| AlarmListAlignmentRequirement | 12.2.1.4.4.5 | Indicating if alarm list alignment is required or not |
| AlarmRecord | 12.2.1.4.1a.5 | Representation of an alarm resource |
| AlarmCount | 12.2.1.4.1a.6 | Representation of an alarmCout resource |
| Comment | 12.2.1.4.1a.7 | Representation of a comment resource |
| Subscription | 12.2.1.4.1a.8 | Representation of a subscription resource |
| MergePatchAcknowledgeAlarm | 12.2.1.4.1a.9 | Used in the request message body of HTTP PATCH to acknowledge or unacknowledge an alarm |
| MergePatchClearAlarm | 12.2.1.4.1a.10 | Used in the request body of HTTP PATCH to clear an alarm |
| FailedAlarm | 12.2.1.4.1a.11 | Used in the response body of multiple HTTP methods to indicate error reasons per alarm id |
| NotifyNewAlarm | 12.2.1.4.1a.12 | Used in the request body of HTTP POST for the notification type notifyNewAlarm |
| NotifyNewSecAlarm | 12.2.1.4.1a.13 | Used in the request body of HTTP POST for the notification type notifyNewAlarm |
| NotifyClearedAlarm | 12.2.1.4.1a.14 | Used in the request body of HTTP POST for the notification type notifyClearedAlarm |
| NotifyChangedAlarm | 12.2.1.4.1a.15 | Used in the request body of HTTP POST for the notification type notifyChangedAlarm |
| NotifyChangedAlarmGeneral | 12.2.1.4.1a.16 | Used in the request body of HTTP POST for the notification type notifyChangedAlarmGeneral |
| NotifyChangedSecAlarmGeneral | 12.2.1.4.1a.17 | Used in the request body of HTTP POST for the notification type notifyChangedAlarmGeneral |
| NotifyCorrelatedNotificationChanged | 12.2.1.4.1a.18 | Used in the request body of HTTP POST for the notification type notifyCorrelatedNotificationChanged |
| NotifyAckStateChanged | 12.2.1.4.1a.19 | Used in the request body of HTTP POST for the notification type notifyAckStateChanged |
| NotifyComments | 12.2.1.4.1a.20 | Used in the request body of HTTP POST for the notification type notifyComments |
| NotifyPotentialFaultyAlarmList | 12.2.1.4.1a.21 | Used in the request body of HTTP POST for the notification type notifyPotentialFaultyAlarmList |
| NotifyAlarmListRebuilt | 12.2.1.4.1a.22 | Used in the request body of HTTP POST for the notification type notifyAlarmListRebuilt |

Table 12.2.1.4.1-2: Data types imported

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Description |
| DateTime | TS 28.623 [44] | Date and time |
| Float | TS 28.623 [44] | Float type |
| Dn | TS 28.623 [44] | DN type |
| SystemDN | TS 28.623 [44] | systemDN type |
| Uri | TS 28.623 [44] | URI type |
| AttributeNameValuePairSet | TS 28.623 [44] | Set of attribute name/value pairs |
| AttributeValueChangeSet | TS 28.623 [44] | Set of attribute names with their old and new values |
| Filter | TS 28.623 [44] | Filter type |
| NotificationId | TS 28.623 [44] | Notification identifier as defined in ITU-T Rec. X. 733 [4] |
| NotificationType | TS 28.623 [44] | Notification type |
| NotificationHeader | TS 28.623 [44] | Notification header |
| ErrorResponse | TS 28.623 [44] | Used in the response body of multiple HTTP methods in case of error |

##### 12.2.1.4.1a Structured data types

###### 12.2.1.4.1a.1 Type ThresholdHysteresis

Table 12.2.1.4.1a.1-1: Definition of type ThresholdHysteresis

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| high | oneOf(integer, Float) | Higher value of a threshold with hysteris, the integer type is used for counter thresholds and the float type for gauge thresholds. | M |
| low | Float | Lower value of a threshold with hysteresis, applicable only to gauge thresholds. | M |

###### 12.2.1.4.1a.2 Type ThresholdLevelInd

Table 12.2.1.4.1a.2-1: Definition of type ThresholdLevelInd

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name (choice) | Data type | Description | S |
| up | ThresholdHysteresis | Indicates for counter and gauge thresholds that the threshold crossing occurred when going up. | M |
| down | ThresholdHysteresis | Indicates for gauge thresholds that the threshold crossing occurred when going down, applicable only to gauge thresholds. | M |

###### 12.2.1.4.1a.3 Type ThresholdInfo

Table 12.2.1.4.1a.3-1: Definition of type ThresholdInfo

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| observedMeasurement | string | The name of the monitored measurement that crossed the threshold and that caused the notification (Rec. ITU-T X. 733 [4]). | M |
| observedValue | oneOf(integer, Float) | The value of the gauge or counter which crossed the threshold. This may be different from the threshold value if, for example, the gauge may only take on discrete values. The integer type is used for counters and the float type for gauges (Rec. ITU-T X. 733 [4]). | M |
| thresholdLevel | ThresholdLevelInd | In the case of a gauge the threshold level specifies a pair of threshold values, the first being the value of the crossed threshold and the second, its corresponding hysteresis; in the case of a counter the threshold level specifies only the threshold value (Rec. ITU-T X. 733 [4]). | O |
| armTime | DateTime | For a gauge threshold, the time at which the threshold was last re-armed, namely the time after the previous threshold crossing at which the hysteresis value of the threshold was exceeded thus again permitting generation of notifications when the threshold is crossed. For a counter threshold, the later of the time at which the threshold offset was last applied, or the time at which the counter was last initialized (for resettable counters) (Rec. ITU-T X. 733 [4]). | O |

###### 12.2.1.4.1a.4 Type CorrelatedNotification

Table 12.2.1.4.1a.4-1: Definition of type CorrelatedNotification

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| sourceObjectInstance | Dn | Source oject instance of the notifications identified by notificationIds. The sourceObjectInstance shall be present if the sourceObjectInstance is not identical to the alarmed objectInstance of the alarmRecord | O |
| notificationIds | array(NotificationId) | Notification identifiers of notifications related to the sourceObjectInstance that are considered to be correlated to the alarmRecord | M |

###### 12.2.1.4.1a.5 Type AlarmRecord

Table 12.2.1.4.1a.5-1: Definition of type AlarmRecord

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| alarmId | key(AlarmId) | Alarm identifier, see clause 11.2.2.1.5.1. The alarmId is used as key in alarm record maps. | M |
| objectInstance | Dn | Alarmed object instance | M |
| notificationId | NotificationId | Notification identifier of the last notifyNewAlarm, notifyChangedAlarm or notifyClearedAlarm | M |
| alarmRaisedTime | DateTime | Date and time the alarm was raised the first time, see clause 11.2.2.1.5.1 | M |
| alarmChangedTime | DateTime | Date and time the perceived severity of the alarm changed the last time, see clause 11.2.2.1.5.1 | O |
| alarmClearedTime | DateTime | Date and time the alarm was cleared, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| specificProblem | oneOf(string, integer) | Refinements to the probable cause of the alarm as defined in ITU-T Rec. X. 733 [4] | O |
| perceivedSeverity | PerceivedSeverity | Perceived severity of the alarm as defined in ITU-T Rec. X. 733 [4] | M |
| backedUpStatus | boolean | Indicating if the object emitting the alarm has been backed up as defined in ITU-T Recommendation X. 733 [4] | O |
| backUpObject | Dn | Backup object of the alarmed object as defined in ITU-T Rec. X. 733 [4] | O |
| trendIndication | TrendIndication | Severity trend of the alarmed object as defined in ITU-T Rec. X. 733 [4] | O |
| thresholdInfo | ThresholdInfo | Additional information for threshold crossing alarms as defined in ITU-T Rec. X. 733 [4] | O |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| stateChangeDefinition | AttributeValueChangeSet | State transition associated to an alarm as defined in ITU-T Rec. X. 733 [4] | O |
| monitoredAttributes | AttributeNameValuePairSet | Attributes of the alarmed manged object and their corresponding values at the time of the alarm as defined in ITU-T Rec. X. 733 [4]. | O |
| proposedRepairActions | string | Proposed repair action, used if the cause is known and the system being managed can suggest one or more solutions to fix the problem causing the alarm as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| additionalInformation | AttributeNameValuePairSet | Allows the inclusion of a set of additional information in the event report as defined in ITU-T Rec. X. 733 [4] | O |
| rootCauseIndicator | boolean | Indicates if this event is the root cause of the events captured by the notifications whose identifiers are in the related correlatedNotifications attribute, see clause 11.2.2.1.5.1 | O |
| ackTime | DateTime | Time when the alarm has been acknowledged or unacknowledged the last time, see clause 11.2.2.1.5.1 | M |
| ackUserId | string | Identifier of a user acknowledging an alarm, see clause 11.2.2.1.5.1 | M |
| ackSystemId | string | Identifier of a system acknowledging an alarm, see clause 11.2.2.1.5.1 | O |
| ackState | AckState | Acknowledgement state, see clause 11.2.2.1.5.1 | M |
| clearUserId | string | Identifier of a system clearing an alarm, see clause 10.2.2.1.5.1 | O |
| clearSystemId | string | Identifier of a user clearing an alarm, see clause 11.2.2.1.5.1 | O |
| serviceUser | string | Identifies the service-user whose request for service provided by the serviceProvider led to the generation of the security alarm, see clause 11.2.2.1.5.1 | O |
| serviceProvider | string | Identifies the service-provider whose service is requested by the serviceUser and the service request provokes the generation of the security alarm, see clause 11.2.2.1.5.1 | O |
| securityAlarmDetector | string | Identity of the detector of the security alarm, see clause 11.2.2.1.5.1 | O |

###### 12.2.1.4.1a.6 Type AlarmCount

Table 12.2.1.4.1a.6-1: Definition of type AlarmCount

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| criticalCount | integer | Number of alarms with perceived severity equal to critical | M |
| majorCount | integer | Number of alarms with perceived severity equal to major | M |
| minorCount | integer | Number of alarms with perceived severity equal to minor | M |
| warningCount | integer | Number of alarms with perceived severity equal to warning | M |
| indeterminateCount | integer | Number of alarms with perceived severity equal to indeterminate | M |
| clearedCount | integer | Number of alarms with perceived severity equal to cleared | M |

###### 12.2.1.4.1a.7 Type Comment

Table 12.2.1.4.1a.7-1: Definition of type Comment

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| commentTime | DateTime | Time when the comment has been added to the alarm. | M |
| commentText | string | Comment in text form | M |
| commentUserId | string | Identifier of the user who makes the comment | M |
| commentSystemId | string | Identifier of the system which makes the comment | O |

###### 12.2.1.4.1a.8 Type Subscription

Table 12.2.1.4.1a.8-1: Definition of type Subscription

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| consumerReference | Uri | URI of the notification target on the MnS consumer | M |
| timeTick | integert | Time window within which the subscriber intends to subscribe again to confirm its subscription, see clause 11.2.2.2.5.1 | O |
| filter | Filter | Filter settings for this subscription, to define the subset of all notifications this subscription relates to. A notification is sent to the subscriber if the filter matches, or if there is no filter. | O |

###### 12.2.1.4.1a.9 Type MergePatchAcknowledgeAlarm

Table 12.2.1.4.1a.9-1: Definition of type MergePatchAcknowledgeAlarm

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| ackUserId | string | User acknowledging an alarm | M |
| ackSystemId | string | System acknowledging an alarm | O |
| ackState | AckState | Indicates the ackState shall be set to "ACKNOWLEDGED" or "UNACKNOWLEDGED" | M |

###### 12.2.1.4.1a.10 Type MergePatchClearAlarm

Table 12.2.1.4.1a.10-1: Definition of type MergePtchClearAlarm

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| clearUserId | clearUserId-Type | User clearing an alarm | M |
| clearSystemId | clearSystemId-Type | System clearing an alarm | O |
| perceivedSeverity | type string, enum "CLEARED" | Indicates the perceivedSeverity shall be set to "CLEARED" | M |

###### 12.2.1.4.1a.11 Type FailedAlarm

Table 12.2.1.4.1a.11-1: Definition of type FailedAlarm

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| alarmId | AlarmId | Indicating the alarms for which the action on the alarm could not be performed | M |
| failureReason | string | Indicating the reason why the action could not be performed | M |

###### 12.2.1.4.1a.12 Type NotifyNewAlarm

Table 12.2.1.4.1a.12-1: Definition of type NotifyNewAlarm

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyNewAlarm) | M |
| eventTime | DateTime | Event (alarm) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| specificProblem | SpecificProblem | Identifies further refinements to the Probable cause of the alarm as defined in ITU-T Rec. X. 733 [4] | O |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | M |
| backedUpStatus | boolean | Indicating if the object emitting the alarm has been backed up as defined in ITU-T Recommendation X. 733 [4] | O |
| backUpObject | Dn | Indicating the backup object of the alarmed object as defined in ITU-T Rec. X. 733 [4] | O |
| trendIndication | TrendIndication | Severity trend of the alarmed object as defined in ITU-T Rec. X. 733 [4] | O |
| thresholdInfo | ThresholdInfo | Provides additional information for threshold crossing alarms as defined in ITU-T Rec. X. 733 [4] | O |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| stateChangeDefinition | AttributeValueChangeSet | Indicates a state transition associated to an alarm as defined in ITU-T Rec. X. 733 [4] | O |
| monitoredAttributes | AttributeNameValuePairSet | Defines one or more attributes of the alarmed manged object and their corresponding values at the time of the alarm as defined in ITU-T Rec. X. 733 [4]. | O |
| proposedRepairActions | string | Used if the cause is known and the system being managed can suggest one or more solutions to fix the problem causing the alarm as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| additionalInformation | AttributeNameValuePairSet | Allows the inclusion of a set of additional information in the event report as defined in ITU-T Rec. X. 733 [4] | O |
| rootCauseIndicator | boolean | Indicates if this event is the root cause of the events captured by the notifications whose identifiers are in the related correlatedNotifications attribute, see clause 11.2.2.1.5.1 | O |

###### 12.2.1.4.1a.13 Type NotifyNewSecAlarm

**Table 12.2.1.4.1a.13-1: Definition of type NotifyNewSecAlarm**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyNewAlarm) | M |
| eventTime | DateTime | Event (alarm) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | M |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| additionalInformation | AttributeNameValuePairSet | Allows the inclusion of a set of additional information in the event report as defined in ITU-T Rec. X. 733 [4] | O |
| rootCauseIndicator | boolean | Indicates if this event is the root cause of the events captured by the notifications whose identifiers are in the related correlatedNotifications attribute, see clause 11.2.2.1.5.1 | O |
| serviceUser | string | Identifies the service-user whose request for service provided by the serviceProvider led to the generation of the security alarm, see clause 11.2.2.1.5.1 | M |
| serviceProvider | string | Identifies the service-provider whose service is requested by the serviceUser and the service request provokes the generation of the security alarm, see clause 11.2.2.1.5.1 | M |
| securityAlarmDetector | string | Identity of the detector of the security alarm, see clause 11.2.2.1.5.1 | M |

###### 12.2.1.4.1a.14 Type NotifyClearedAlarm

Table 12.2.1.4.1a.14-1: Definition of type NotifyClearedAlarm

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyClearedAlarm) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | M |
| correlatedNotifications | array(correlatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| clearUserId | string | Identifier of a user clearing an alarm, see clause 11.2.2.1.5.1 | O |
| clearSystemId | string | Identifier of a system clearing an alarm, see clause 11.2.2.1.5.1 | O |

###### 12.2.1.4.1a.15 Type NotifyChangedAlarm

Table 12.2.1.1a.14.15-1: Definition of type NotifyChangedAlarm

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyChangedAlarm) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | M |

###### 12.2.1.4.1a.16 Type NotifyChangedAlarmGeneral

Table 12.2.1.4.1a.16-1: Definition of type NotifyChangedAlarmGeneral

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyChangedAlarmGeneral) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | O |
| specificProblem | SpecificProblem | Identifies further refinements to the Probable cause of the alarm as defined in ITU-T Rec. X. 733 [4] | O |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | O |
| backedUpStatus | boolean | Indicating if the object emitting the alarm has been backed up as defined in ITU-T Recommendation X. 733 [4] | O |
| backUpObject | Dn | Indicating the backup object of the alarmed object as defined in ITU-T Rec. X. 733 [4] | O |
| trendIndication | TrendIndication | Severity trend of the alarmed object as defined in ITU-T Rec. X. 733 [4] | O |
| thresholdInfo | ThresholdInfo | Provides additional information for threshold crossing alarms as defined in ITU-T Rec. X. 733 [4] | O |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| stateChangeDefinition | AttributeValueChangeSet | Indicates a state transition associated to an alarm as defined in ITU-T Rec. X. 733 [4] | O |
| monitoredAttributes | AttributeNameValuePairSet | Defines one or more attributes of the alarmed manged object and their corresponding values at the time of the alarm as defined in ITU-T Rec. X. 733 [4]. | O |
| proposedRepairActions | string | Used if the cause is known and the system being managed can suggest one or more solutions to fix the problem causing the alarm as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| additionalInformation | AttributeNameValuePairSet | Allows the inclusion of a set of additional information in the event report as defined in ITU-T Rec. X. 733 [4] | O |
| rootCauseIndicator | boolean | Indicates if this event is the root cause of the events captured by the notifications whose identifiers are in the related correlatedNotifications attribute, see clause 11.2.2.1.5.1 | O |
| changedAlarmAttributes | AttributeNameValuePairSet | Indicating the alarm attributes that have changed | O |

###### 12.2.1.4.1a.17 Type NotifyChangedSecAlarmGeneral

Table 12.2.1.4.1a.17-1: Definition of type NotifyChangedSecAlarmGeneral

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyChangedAlarmGeneral) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | O |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | O |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | O |
| additionalText | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |
| additionalInformation | AttributeNameValuePairSet | Allows the inclusion of a set of additional information in the event report as defined in ITU-T Rec. X. 733 [4] | O |
| rootCauseIndicator | boolean | Indicates if this event is the root cause of the events captured by the notifications whose identifiers are in the related correlatedNotifications attribute, see clause 11.2.2.1.5.1 | O |
| serviceUser | string | Identifies the service-user whose request for service provided by the serviceProvider led to the generation of the security alarm, see clause 11.2.2.1.5.1 | M |
| serviceProvider | string | Identifies the service-provider whose service is requested by the serviceUser and the service request provokes the generation of the security alarm, see clause 11.2.2.1.5.1 | M |
| securityAlarmDetector | string | Identity of the detector of the security alarm, see clause 11.2.2.1.5.1 | M |
| changedAlarmAttributes | AttributeNameValuePairSet | Indicating the alarm attributes that have changed | O |

###### 12.2.1.4.1a.18 Type NotifyCorrelatedNotificationChanged

Table 12.2.1.4.1a.18-1: Definition of type NotifyCorrelatedNotificationChanged

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyCorrelatedNotificationChanged) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| correlatedNotifications | array(CorrelatedNotification) | Set of all notifications to which this notification is considered to be correlated as defined in ITU-T Rec. X. 733 [4] | M |
| rootCauseIndicator | boolean | Indicates if this event is the root cause of the events captured by the notifications whose identifiers are in the related correlatedNotifications attribute, see clause 11.2.2.1.5.1 | O |

###### 12.2.1.4.1a.19 Type NotifyAckStateChanged

**Table 12.2.1.4.1a.19-1: Definition of type NotifyAckStateChanged**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyAckStateChanged) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | M |
| ackState | string | Acknowledgement state, see clause 11.2.2.1.5.1 | M |
| ackUserId | string | Identifier of a system acknowledging an alarm, see clause 11.2.2.1.5.1 | M |
| ackSystemId | string | Identifier of a user acknowledging an alarm, see clause 11.2.2.1.5.1 | O |

###### 12.2.1.4.1a.20 Type NotifyComments

Table 12.2.1.4.1a.20-1: Definition of type NotifyComments

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyComments) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| alarmId | AlarmId | Alarm identifier, see clause 11.2.2.1.5.1 | M |
| alarmType | AlarmType | Alarm type as defined in ITU-T Rec. X. 733 [4] | M |
| probableCause | ProbableCause | Probable cause of an alarm as defined in ITU-T Rec. X.733 [4] | M |
| perceivedSeverity | PerceivedSeverity | Perceived severity of an alarm as defined in ITU-T Rec. X. 733 [4] | M |
| comments | map(Comment) | Set of all comments related to an alarm | M |

###### 12.2.1.4.1a.21 Type NotifyPotentialFaultyAlarmList

Table 12.2.1.4.1a.21-1: Definition of type NotifyPotentialFaultyAlarmList

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyPotentialFaultyAlarmList) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| reason | string | Indicating the reason why the alarm list has to be rebuilt. | M |

###### 12.2.1.4.1a.22 Type NotifyAlarmListRebuilt

Table 12.2.1.4.1a.22-1: Definition of type NotifyAlarmListRebuilt

|  |  |  |  |
| --- | --- | --- | --- |
| Attribute name | Data type | Description | S |
| href | Uri | URI of the resource where the event (alarm) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyAlarmListRebuilt) | M |
| eventTime | DateTime | Event occurrence time | M |
| systemDN | SystemDN | System DN | M |
| reason | string | Indicating the reason why the alarm list has been rebuilt | M |
| alarmListAlignmentRequirement | alarmListAlignmentRequirement-Type | Indicating if alarm list alignment is required or not | O |

##### 12.2.1.4.2 Void

##### 12.2.1.4.3 Void

##### 12.2.1.4.4 Simple data types and enumerations

###### 12.2.1.4.4.1 General

This clause defines simple data types and enumerations that are used by the data structures defined in the previous clauses.

###### 12.2.1.4.4.2 Simple data types

Table 12.2.1.4.4.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type name | Type definition | Description |
| AlarmId | string | Alarm identifier, see clause 11.2.2.1.5.1 |

###### 12.2.1.4.4.3 Enumeration AlarmAckState

Table 12.2.1.4.4.3-1: Enumeration AlarmAckState

|  |  |
| --- | --- |
| Enumeration value | Description |
| ALL\_ALARMS | All alarms shall be returned or counted. |
| ALL\_ACTIVE\_ALARMS | All active alarms shall be returned or counted. |
| ALL\_ACTIVE\_AND\_ACKNOWLEDGED \_ALARMS | All active and acknowledged alarms shall be returned or counted. |
| ALL\_ACTIVE\_AND\_UNACKNOWLEDGED\_ALARMS | All active and unacknowledged alarms shall be returned or counted. |
| ALL\_CLEARED\_AND\_ACKNOWLEDGED\_ALARMS | All cleared and unacknowledged alarms shall be returned or counted. |
| ALL\_UNACKNOWLEDGED\_ALARMS | All unacknowledged alarms shall be returned or counted |

###### 12.2.1.4.4.4 Enumeration AckState

Table 12.2.1.4.4.4-1: Enumeration ackState

|  |  |
| --- | --- |
| Enumeration value | Description |
| ACKNOWLEDGED | State acknowledged. |
| UNACKNOWLEDGED | State unacknowledged. |

###### 12.2.1.4.4.5 Enumeration AlarmListAlignmentRequirement

Table 12.2.1.4.4.5-1: Enumeration AlarmListAlignmentRequirement

|  |  |
| --- | --- |
| Enumeration value | Description |
| ALIGNMENT\_REQUIRED | Alarm list alignment is required |
| ALIGNMENT\_NOT\_REQUIRED | Alarm list alignment is not required |

###### 12.2.1.4.4.6 Enumeration AlarmType

Table 12.2.1.4.4.6-1: Enumeration AlarmType

|  |  |
| --- | --- |
| Enumeration value | Description |
| COMMUNICATIONS\_ALARM | An alarm of this type is principally associated with the procedures and/or processes required to convey information from one point to another (Rec. ITU-T X. 733 [4]). |
| PROCESSING\_ERROR\_ALARM | An alarm of this type is principally associated with a software or processing fault (Rec. ITU-T X. 733 [4]). |
| ENVIRONMENTAL\_ALARM | An alarm of this type is principally associated with a condition relating to an enclosure in which the equipment resides (Rec. ITU-T X. 733 [4]). |
| QUALITY\_OF\_SERVICE\_ALARM | An alarm of this type is principally associated with a degradation in the  quality of a service (Rec. ITU-T X. 733 [4]). |
| EQUIPMENT\_ALARM | An alarm of this type is principally associated with an equipment fault (Rec. ITU-T X. 733 [4]). |
| INTEGRITY\_VIOLATION | An indication that information may have been illegally modified, inserted or deleted. |
| OPERATIONAL\_VIOLATION | An indication that the provision of the requested service was not possible due to the unavailability, malfunction or incorrect invocation of the service. |
| PHYSICAL\_VIOLATION | An indication that a physical resource has been violated in a way that suggests a security attack. |
| SECURITY\_SERVICE\_OR\_MECHANISM\_VIOLATION | An indication that a security attack has been detected by a security service or mechanism. |
| TIME\_DOMAIN\_VIOLATION | An indication that an event has occurred at an unexpected or prohibited time. |

###### 12.2.1.4.4.7 Enumeration ProbableCause

Table 12.2.1.4.4.7-1: Enumeration ProbableCause

|  |  |
| --- | --- |
| Enumeration value | Description |
| PROBABLE\_CAUSE\_001 | Generic probable cause string 001, mapping to a concrete probable cause is vendor specific |
| PROBABLE\_CAUSE\_002 | Generic probable cause string 002, mapping to a concrete probable cause is vendor specific |
| PROBABLE\_CAUSE\_003 | Generic probable cause string 003, mapping to a concrete probable cause is vendor specific |
| PROBABLE\_CAUSE\_004 | Generic probable cause string 004, mapping to a concrete probable cause is vendor specific |
| PROBABLE\_CAUSE\_005 | Generic probable cause string 005, mapping to a concrete probable cause is vendor specific |

###### 12.2.1.4.4.8 Enumeration AlarmNotificationTypes

Table 12.2.1.4.4.8-1: Enumeration AlarmNotificationTypes

|  |  |
| --- | --- |
| Enumeration value | Description |
| notifyNewAlarm | Notification type is notifyNewAlarm |
| notifyNewSecurityAlarm | Notification type is notifyNewSecurityAlarm |
| notifyAckStateChanged | Notification type is notifyAckStateChanged |
| notifyClearedAlarm | Notification type is notifyClearedAlarm |
| notifyAlarmListRebuiltAlarm | Notification type is notifyAlarmListRebuiltAlarm |
| notifyChangedAlarm | Notification type is notifyChangedAlarm |
| notifyComments | Notification type is notifyComments |
| notifyPotentialFaultyAlarmList | Notification type is notifyPotentialFaultyAlarmList |
| notifyCorrelatedNotificationChanged | Notification type is notifyCorrelatedNotificationChanged |
| notifyChangedAlarmGeneral | Notification type is notifyChangedAlarmGeneral |

###### 12.2.1.4.4.9 Enumeration PerceivedSeverity

Table 12.2.1.4.4.9-1: Enumeration PerceivedSeverity

|  |  |
| --- | --- |
| Enumeration value | Description |
| CRITICAL | The Critical severity level indicates that a service affecting condition has occurred and an immediate corrective action is required (Rec. ITU-T X. 733 [4]). |
| MAJOR | The Major severity level indicates that a service affecting condition has developed and an urgent corrective action is required (Rec. ITU-T X. 733 [4]). |
| MINOR | The Minor severity level indicates the existence of a non-service affecting fault condition and that corrective action should be taken in order to prevent a more serious (for example, service affecting) fault (Rec. ITU-T X. 733 [4]). |
| WARNING | The Warning severity level indicates the detection of a potential or impending service affecting fault, before any significant effects have been felt (Rec. ITU-T X. 733 [4]). |
| INDETERMINATE | The Indeterminate severity level indicates that the severity level cannot be determined (Rec. ITU-T X. 733 [4]). |
| CLEARED | The Cleared severity level indicates the clearing of one or more previously reported alarms (Rec. ITU-T X. 733 [4]). |

###### 12.2.1.4.4.10 Enumeration TrendIndication

Table 12.2.1.4.4.10-1: Enumeration TrendIndication

|  |  |
| --- | --- |
| Enumeration value | Description |
| MORE\_SEVERE | Severity trend of the alarmed object is more severe (Rec. ITU-T X.733 [4]) |
| NO\_CHANGE | Severity trend of the alarmed object is no change (Rec. ITU-T X.733 [4]) |
| LESS\_SEVERE | Severity trend of the alarmed object is less severe (Rec. ITU-T X.733 [4]) |

### 12.2.2 RESTful HTTP-based solution set for integration with ONAP VES API

#### 12.2.2.1 Mapping of operations

NOTE: no use case has been specified by ONAP. Therefore this mapping is not part of the present document.

#### 12.2.2.2 Mapping of notifications

##### 12.2.2.2.1 Introduction

###### 12.2.2.2.1.1 General

The 3GPP IS notifications are mapped to SS equivalents according to table 12.2.2.2.1.1-1.

Table 12.2.2.2.1.1-1: Mapping of 3GPP IS notifications to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **3GPP IS notifications** | **HTTP Method** | **Resource URI** | **SQ** |
| notifyNewAlarm | POST | /eventListener | M |
| notifyAckStateChanged | POST | /eventListener | M |
| notifyClearedAlarm | POST | /eventListener | M |
| notifyAlarmListRebuilt | POST | /eventListener | M |
| notifyChangedAlarm | POST | /eventListener | M |
| notifyComments | POST | /eventListener | M |
| notifyPotentialFaultyAlarmList | POST | /eventListener | M |
| notifyCorrelatedNotificationChanged | POST | /eventListener | M |
| notifyChangedAlarmGeneral | POST | /eventListener | O |

###### 12.2.2.2.1.2 Void

##### 12.2.2.2.2 Notification notifyNewAlarm (non-security alarm)

See clause 12.2.1.2.2.

##### 12.2.2.2.3 Notification notifyNewAlarm (security alarm)

See clause 12.2.1.2.3.

##### 12.2.2.2.4 Notification notifyAckStateChanged

See clause 12.2.1.2.4.

##### 12.2.2.2.5 Notification notifyClearedAlarm

See clause 12.2.1.2.5.

##### 12.2.2.2.6 Notification notifyAlarmListRebuilt

See clause 12.2.1.2.6.

##### 12.2.2.2.7 Notification notifyChangedAlarm

See clause 12.2.1.2.7.

##### 12.2.2.2.8 Notification notifyComments

See clause 12.2.1.2.8.

##### 12.2.2.2.9 Notification notifyPotentialFaultyAlarmList

See clause 12.2.1.2.9.

##### 12.2.2.2.10 Notification notifyCorrelatedNotificationChanged

See clause 12.2.1.2.10.

##### 12.2.2.2.11 Notification notifyChangedAlarmGeneral (non-security alarm)

See clause 12.2.1.2.11.

##### 12.2.2.2.12 Notification notifyChangedAlarmGeneral (security alarm)

See clause 12.2.1.2.12.

#### 12.2.2.3 Resources

##### 12.2.2.3.1 Resource structure

Figure 12.2.2.3.1-1 shows the resource structure of the fault supervision data report MnS in the context of its integration with VES Event Listener 7.1.1 [45].



Figure 12.2.2.3.1-1: Resource URI structure of the fault supervision data report MnS for integration with ONAP VES Event Listener 7.1.1 (Resource structure section) [45]

Table 12.2.2.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 12.2.2.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| eventListener | /eventListener | POST | Send notifications |

##### 12.2.2.3.2 Resource definitions

See Resource structure section in [45].

##### 12.2.2.4 Data type definitions

See clause 12.2.1.4.

## 12.3 Generic performance assurance management service

### 12.3.1 RESTful HTTP-based solution set

#### 12.3.1.1 Void

#### 12.3.1.2 Performance threshold monitoring service

##### 12.3.1.2.1 Mapping of operations

None.

##### 12.3.1.2.2 Mapping of notifications

###### 12.3.1.2.2.1 Introduction

The IS notifications are mapped to SS equivalents according to table 12.3.1.2.2.1-1.

**Table 12.3.1.2.2.1-1: Mapping of IS notifications to SS equivalents**

|  |  |  |  |
| --- | --- | --- | --- |
| **IS notifications** | **HTTP Method** | **Resource URI** | **S** |
| notifyThresholdCrossing | POST | /notificationSink | M |

###### 12.3.1.2.2.2 Notification "notifyThresholdCrossing"

The IS notification parameters are mapped to SS equivalents according to table 12.3.1.2.2.2-1.

Table 12.3.1.2.2.2-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| objectClass | request body | href | Uri | M |
| objectInstance |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | Request body | systemDN | SystemDN | M |
| observedPerfMetricName | request body | observedPerfMetricName | string | M |
| observedPerfMetricValue | request body | observedPerfMetricValue | PerfMetricValue | M |
| observedPerfMetricDirection | request body | observedPerfMetricDirection | PerfMetricDirection | M |
| thresholdValue | request body | thresholdValue | PerfMetricValue | M |
| hysteresis | request body | hysteresis | PerfMetricValue) | M |
| monitorGranularityPeriod | request body | monitorGranularityPeriod | integer | M |
| additionalText | request body | additionalText | string | O |

##### 12.3.1.2.3 Resources

###### 12.3.1.2.3.1 Resource structure

Table 12.3.1.2.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 12.3.1.2.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| notificationSink | /notificationSink | POST | Send notifications |

###### 12.3.1.2.3.2 Resource definitions

12.3.1.2.3.2.1 Resource "/notificationSink"

12.3.1.2.3.2.1.1 Description

This resource represents a resource on a MnS consumer to which notifications are sent to.

12.3.1.2.3.2.1.2 URI

The resource URI is provided by the notification subscription.

12.3.1.2.3.2.1.3 HTTP methods

12.3.1.2.3.2.1.3.1 POST

This method shall support the URI query parameters specified in table 12.3.1.2.3.2.1.3.1-1.

Table 12.3.1.2.3.2.1.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | Qualifier |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures specified in table 12.3.1.2.3.2.1.3.1-2 and the response data structures and response codes specified in table 12.3.1.2.3.2.1.3.1-3.

Table 12.3.1.2.3.2.1.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | SQ |
| notifyThresholdCrossing-NotifType | Type in case a notifyThresholdCrossing notification is sent | M |

Table 12.3.1.2.3.2.1.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | SQ |
| n/a | 204 No Content | In case of success no message body is returned | M |
| error-ResponseType | 4xx/5xx | In case of failure the error object is returned. | M |

##### 12.3.1.2.4 Data type definitions

###### 12.3.1.2.4.1 General

Table 12.3.1.2.4.1-1: Data types defined in this specification

|  |  |  |
| --- | --- | --- |
| **Data type** | **Reference** | **Description** |
| NotifyThresholdCrossing | 12.3.1.2.4.2.1 | Used in the request body of HTTP POST for the notification type notifyThresholdCrossing |
| PerfNotificationTypes | 12.3.1.2.4.6.4 | Performance notification types (notifyThresholdCrossing) |

Table 12.3.1.1.4.1-2: Data types imported

|  |  |  |
| --- | --- | --- |
| **Data type** | **Reference** | **Description** |
| DateTime | TS 28.623 [44] | Date and time |
| Float | TS 28.623 [44] | Float type |
| Uri | TS 28.623 [44] | URI type |
| SystemDN | TS 28.623 [44] | systemDN type |
| NotificationId | TS 28.623 [44] | Notification identifier as defined in ITU-T Rec. X. 733 [4] |
| NotificationHeader | TS 28.623 [44] | Notification header |
| ErrorResponse | TS 28.623 [44] | Used in the response body of multiple HTTP methods in case of error |

###### 12.3.1.2.4.2 Structured data types

12.3.1.2.4.2.1 Type NotifyThresholdCrossing

Table 12.3.1.2.4.2.1-1: Definition of NotifyThresholdCrossing

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **S** |
| href | Uri | URI of the resource where the event (threshold crossing) occurred | M |
| notificationId | NotificationId | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| notificationType | NotificationType | Notification type (notifyThresholdCrossing) | M |
| eventTime | DateTime | Event (threshold crossing) occurrence time | M |
| systemDN | SystemDN | System DN | M |
| observedPerfMetricName | string | Name of the performance metric that has crossed the threshold | M |
| observedPerfMetricValue | PerfMetricValue | Value of the performance metric, that has crossed the threshold, when the threshold crossing was observed | M |
| observedPerfMetricDirection | PerfMetricDirection | Direction ("UP" or "DOWN") of the performance metric, when the threshold crossing was observed | M |
| thresholdValue | PerfMetricValue | Threshold value of the triggered threshold | M |
| hysteresis | PerfMetricValue | Hysteresis of the triggered threshold |  |
| monitorGranularityPeriod | integer | Granularity period of the threshold monitor | M |
| additionalText | string | Vendor specific information | O |

12.3.1.2.4.3 Void

###### 12.3.1.2.4.4 Void



###### 12.3.1.2.4.5 Void



###### 12.3.1.2.4.6 Simple data types and enumerations

12.3.1.2.4.6.1 General

This clause defines simple data types and enumerations that are used by the data structures defined in the previous clauses.

12.3.1.2.4.6.2 Simple data types

Table 12.3.1.2.4.6.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type name | Type definition | Description |
| PerfMetricValue | Union(integer, Float) | The type of a performance metric is either integer or Float |

12.3.1.2.4.6.3 Enumeration PerfNotificationTypes

Table 12.3.1.2.4.6.3-1: Enumeration PerfNotificationTypes-Type

|  |  |
| --- | --- |
| Enumeration value | Description |
| notifyThresholdCrossing | Notification type is notifyThresholdCrossing |

12.3.1.2.4.6.4 Enumeration PerfMetricDirection

Table 12.3.1.2.4.6.4-1: Enumeration PerfMetricDirection

|  |  |
| --- | --- |
| Enumeration value | Description |
| UP | Performance metric values are going up |
| DOWN | Performance metric values are going down |

### 12.3.2 XML file format definition

#### 12.3.2.1 Introduction

This clause describes the format of performance data file. The XML file format definition is based on XML schema (see [26], [27], [28] and [29]).

#### 12.3.2.2 Mapping table

Table 12.3.2.2-1 maps the file content items in the clause 11.3.2.1.2 to those used in the XML schema based file format definitions. XML tag attributes are useful where data values bind tightly to its parent element. They have been used where appropriate.

Table 12.3.2.2-1: Mapping of File Content Items to XML tags

| File Content Item | XML schema based XML tag | Description |
| --- | --- | --- |
| measDataCollection | measDataFile |  |
| measFileHeader | fileHeader |  |
| measData | measData |  |
| measFileFooter | fileFooter |  |
| fileFormatVersion | fileHeader fileFormatVersion |  |
| senderName | fileSender senderName |  |
| senderType | fileSender senderType | For the XML schema based XML format, XML attribute specification "senderType " may be absent in case the "senderType" is not configured in the sender. |
| vendorName | fileHeader vendorName | For the XML schema based XML format, XML attribute specification "vendorName" may be absent in case the "vendorName" is not configured in the sender. |
| collectionBeginTime | measData beginTime |  |
| measuredEntityUserName | measEntity userLabel | For the XML schema based XML format, XML attribute specification "userLabel" may be absent in case the "nEUserName" is not configured in the CM applications. |
| measuredEntityDn | fileHeader dnPrefix  and measuredEntity  localDn | For the XML schema based XML format, the DN is split into the DN prefix and the Local DN (LDN) (see 3GPP TS 32.300 [25]). XML attribute specification "localDn" may be absent in case the LDN is not configured in the CM applications. |
| measuredEntitySoftwareVersion | measEntity swVersion | For the XML schema based XML format, XML attribute specification "swVersion" may be absent in case the "nESoftwareVersion" is not configured in the CM applications. |
| measInfo | measInfo |  |
| measInfoId | measInfoId |  |
| measTimeStamp | granPeriod endTime |  |
| jobId | jobId | This item is optional. |
| granularityPeriod | granPeriod duration | For the XML schema based XML format, the value of XML attribute specification "duration" shall use the truncated representation "PT*n*S" (see [28]). |
| reportingPeriod | repPeriod duration | For the XML schema based XML format, the value of XML attribute specification "duration" shall use the truncated representation "PT*n*S" (see [28]). |
| measTypes | measTypes  or measType | For the XML schema based XML format, depending on sender's choice for optional positioning presence, either XML element "measTypes" or XML elements "measType" will be used. |
| measValues | measValue |  |
| measObjInstId | measValue measObjLdn |  |
| measResults | measResults  or  r | For the XML schema based XML format, depending on sender's choice for optional positioning presence, either XML element "measResults" or XML elements "r" will be used. |
| suspectFlag | suspect |  |
| timeStamp | measData endTime |  |
| There is no corresponding File Content Item. | measType p | An optional positioning XML attribute specification of XML element "measType" (XML schema based), used to identify a measurement type for the purpose of correlation to a result. The value of this XML attribute specification is expected to be a non-zero, non-negative integer value that is unique for each instance of XML element "measType" that is contained within the measurement data collection file. |
| There is no corresponding File Content Item. | r p | An optional positioning XML attribute specification of XML element "r", used to correlate a result to a measurement type. The value of this XML attribute specification should match the value of XML attribute specification "p" of the corresponding XML element "measType" (XML schema based). |

#### 12.3.2.3 XML schema

##### 11.3.2.3.1 Performance data file XML schema

The following XML schema measData.xsd is the schema for performance measurements data XML files:

<?xml version="1.0" encoding="UTF-8"?>

<!--

3GPP TS 28.532 Measurements data XML file format definition

data file XML schema

measData.xsd

-->

<schema xmlns="http://www.w3.org/2001/XMLSchema" xmlns:md="http://www.3gpp.org/ftp/specs/archive/28\_series/28.532#measData" targetNamespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.532#measData" elementFormDefault="qualified">

<!-- Measurement collection data file root XML element -->

<element name="measDataFile">

<complexType>

<sequence>

<element name="fileHeader">

<complexType>

<sequence>

<element name="fileSender">

<complexType>

<attribute name="senderName" type="string" use="optional"/>

<attribute name="senderType" type="string" use="optional"/>

</complexType>

</element>

<element name="measData">

<complexType>

<attribute name="beginTime" type="dateTime" use="required"/>

</complexType>

</element>

</sequence>

<attribute name="fileFormatVersion" type="string" use="required"/>

<attribute name="vendorName" type="string" use="optional"/>

<attribute name="dnPrefix" type="string" use="optional"/>

</complexType>

</element>

<element name="measData" minOccurs="0" maxOccurs="unbounded">

<complexType>

<sequence>

<element name="measEntity">

<complexType>

<attribute name="userLabel" type="string" use="optional"/>

<attribute name="localDn" type="string" use="optional"/>

<attribute name="swVersion" type="string" use="optional"/>

</complexType>

</element>

<element name="measInfo" minOccurs="0" maxOccurs="unbounded">

<complexType>

<sequence>

<element name="job" minOccurs="0">

<complexType>

<attribute name="jobId" type="string" use="required"/>

</complexType>

</element>

<element name="granPeriod">

<complexType>

<attribute name="duration" type="duration" use="required"/>

<attribute name="endTime" type="dateTime" use="required"/>

</complexType>

</element>

<element name="repPeriod" minOccurs="0">

<complexType>

<attribute name="duration" type="duration" use="required"/>

</complexType>

</element>

<choice>

<element name="measTypes">

<simpleType>

<list itemType="Name"/>

</simpleType>

</element>

<element name="measType" minOccurs="0" maxOccurs="unbounded">

<complexType>

<simpleContent>

<extension base="Name">

<attribute name="p" type="positiveInteger" use="required"/>

</extension>

</simpleContent>

</complexType>

</element>

</choice>

<element name="measValue" minOccurs="0" maxOccurs="unbounded">

<complexType>

<sequence>

<choice>

<element name="measResults">

<simpleType>

<list itemType="md:measResultType"/>

</simpleType>

</element>

<element name="r" minOccurs="0" maxOccurs="unbounded">

<complexType>

<simpleContent>

<extension base="md:measResultType">

<attribute name="p" type="positiveInteger" use="required"/>

</extension>

</simpleContent>

</complexType>

</element>

</choice>

<element name="suspect" type="boolean" minOccurs="0"/>

</sequence>

<attribute name="measObjLdn" type="string" use="required"/>

</complexType>

</element>

</sequence>

<attribute name="measInfoId" type="string" use="optional"/>

</complexType>

</element>

</sequence>

</complexType>

</element>

<element name="fileFooter">

<complexType>

<sequence>

<element name="measData">

<complexType>

<attribute name="endTime" type="dateTime" use="required"/>

</complexType>

</element>

</sequence>

</complexType>

</element>

</sequence>

</complexType>

</element>

<simpleType name="measResultType">

<union memberTypes="integer float string">

<simpleType>

<restriction base="string">

<enumeration value="NULL"/>

</restriction>

</simpleType>

</union>

</simpleType>

</schema>

##### 12.3.2.3.2 Performance data file XML header

The following header shall be used in actual XML measurement result files:

<?xml version="1.0" encoding="UTF-8"?>  
<?xml-stylesheet type="text/xsl" href="measData.xsl"?>  
<measDataFile  
 xmlns=  
"http://www.3gpp.org/ftp/specs/archive/28\_series/28.532#measData"  
>

## 12.4 Heartbeat

### 12.4.1 RESTful HTTP-based solution set

#### 12.4.1.1 Mapping of operations

N/A

#### 12.4.1.2 Mapping of notifications

##### 12.4.1.2.1 Introduction

The IS notifications are mapped to SS equivalents according to table 12.4.1.2.1-1.

**Table 12.4.1.2.1-1: Mapping of IS notifications to SS equivalents**

|  |  |  |  |
| --- | --- | --- | --- |
| **IS notifications** | **HTTP Method** | **Resource URI** | **S** |
| notifyHeartbeat | POST | /notificationSink | M |

##### 12.4.1.2.2 Notification "notifyHeartbeat"

The IS notification parameters are mapped to SS equivalents according to table 12.4.1.2.2-1.

Table 12.4.1.2.2-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **S** |
| objectClass  objectInstance | request body | href | Uri | M |
| notificationId | request body | notificationId | NotificationId | M |
| notificationType | request body | notificationType | NotificationType (notifyHeartbeat) | M |
| eventTime | request body | eventTime | DateTime | M |
| systemDN | request body | systemDN | systemDN | M |
| heartbeatNtfPeriod | request body | heartbeatNtfPeriod | integer | M |

#### 12.4.1.3 Usage of HTTP

N/A.

#### 12.4.1.4 Resources

N/A.

#### 12.4.1.5 Data type definitions

##### 12.4.1.5.1 General

Table 12.4.1.5.1-1: Data types defined in the present document

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Description |
| HeartbeatNotificationTypes | 12.4.1.4.2.2 | Haertbeat notification types |

Table 12.4.1.5.1-2: Data types imported

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Description |
| Uri | TS 28.623 [44] | URI type |
| NotificationId | TS 28.623 [44] | Notification identifier as defined in ITU-T Rec. X. 733 [4] |
| NotificationType | TS 28.623 [44] | Notification type |
| DateTime | TS 28.623 [44] | Date and time |
| SystemDN | TS 28.623 [44] | systemDN type |
| NotificationHeader | TS 28.623 [44] | Notification header |

##### 12.4.1.5.2 Structured data types

None.

##### 12.4.1.5.3 Simple data types and enumerations

###### 12.4.1.5.3.1 General

This subclause defines simple data types and enumerations that are used by the data structures defined in the previous subclauses.

###### 12.4.1.5.3.2 Simple data types

Table 12.4.1.4.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
|  |  |  |

###### 12.4.1.5.3.3 Enumeration HeartbeatNotificationTypes

Table 12.4.1.4.3.3-1: Enumeration HeartbeatNotificationTypes

|  |  |
| --- | --- |
| Enumeration value | Description |
| notifyHeartbeat | Notification type is notifyHeartbeat |

### 12.4.2 RESTful HTTP-based solution set for integration with ONAP VES API

NOTE: Void.

#### 12.4.2.1 Mapping of operations

See clause 12.1.1.1.

#### 12.4.2.2 Mapping of notifications

##### 12.4.2.2.1 Introduction

###### 12.4.2.2.1.1 General

The 3GPP IS heartbeat notifications are mapped to SS equivalents according to table 12.4.2.2.1.1-1.

Table 12.4.2.2.1.1-1: Mapping of 3GPP IS notifications to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **3GPP IS notifications** | **HTTP Method** | **Resource URI** | **SQ** |
| notifyHeartbeat | POST | /eventListener | M |

###### 12.4.2.2.1.2 Notification parameter mapping principles

3GPP IS fault supervision alarm notification parameters are mapped to solution set equivalent as follows:

##### 12.4.2.2.2 Notification notifyHeartbeat

See clause 12.4.1.2.2.

## 12.5 Streaming data reporting service

### 12.5.1 RESTful HTTP-based solution set

#### 12.5.1.1 Mapping of operations

##### 12.5.1.1.1 Introduction

The IS operations are mapped to SS equivalents according to table 12.5.1.1.1-1.

Table 12.5.1.1.1-1: Mapping of IS operations to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation** | **Method/frame** | **Resource/URI** | **Qualifier** |
| establishStreamingConnection | HTTP POST (see NOTE) | /connections | M |
| HTTP GET (Upgrade, see NOTE) | /connections/{connectionId} | M |
| terminateStreamingConnection | WebSocket Close frame sent (frame with opcode of 0x8), and  WebSocket Close frame received (frame with opcode of 0x8 for successful case) | /connections/{connectionId} | M |
| reportStreamData | WebSocket Data frame sent (frame with opcode of 0x2) | /connections/{connectionId} | M |
| addStream | HTTP POST | /connections/{connectionId}/streams | M |
| deleteStream | HTTP DELETE | /connections/{connectionId}/streams | M |
| getConnectionInfo | HTTP GET | /connections | M |
| HTTP GET | /connections/{connectionId} | M |
| getStreamInfo | HTTP GET | /connections/{connectionId}/streams | M |
|  | HTTP GET | /connections/{connectionId}/streams/{streamId} | M |
| Note: the establishStreamingConnection is mapped to a HTTP POST operation followed by a HTTP GET operation. The HTTP POST operation is to provide the information in streamInfoList parameter to the consumer and receive the connectionId assigned by the consumer, while the HTTP GET (Upgrade) operation is to establish the WebSocket connection. | | | |

##### 12.5.1.1.2 Operation "establishStreamingConnection"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.2-1 through 12.5.1.1.2-4.

Table 12.5.1.1.2-1: Mapping of IS operation input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS operation parameter name | SS parameter location | SS parameter name | SS parameter type | Qualifier |
| producerId | request body | producerId | String | M |
| streamInfoList | request body | streamInfoList | array(streamInfo-Type) | M |

Table 12.5.1.1.2-2: Mapping of IS operation output parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IS operation parameter name | SS parameter location | SS parameter name | SS parameter type | Qualifier |
| connectionId | location header | n/a | uri-Type | M |
| status | response status codes  response body | n/a  error | n/a  error-ResponseType | M |

Table 12.5.1.1.2-3: Mapping of IS operation input parameters to SS equivalents (HTTP GET (Upgrade))

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | Headers | Request-URI | String | n/a |
| -- | HTTP-Version (Request-Line) | -- | String (see Note 1) | M |
| -- | Upgrade Header | -- | Constant string: websocket | M |
| -- | Connection Header | -- | Constant string: Upgrade | M |
| -- | Sec-WebSocket-Key Header | -- | String (see Note 2) | M |
| -- | Sec-WebSocket-Version Header | -- | String (see Note 3) | M |
| -- | See Note 4. | | | |
| NOTE 1: The HTTP version shall be not earlier than HTTP/1.1.  NOTE 2: The valid value needs to be assigned according to WebSocket protocol (see IETF RFC 6455 [40]).  NOTE 3: The valid value needs to be assigned according to WebSocket protocol (see IETF RFC 6455 [40]).  NOTE 4: Other SS parameters (not listed in this table) independent from the Stage 2 may be used, according to the WebSocket protocol (see IETF RFC 6455 [40]). | | | | |

Table 12.5.1.1.2-4: Mapping of IS operation output parameters to SS equivalents (HTTP GET (Upgrade))

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | n/a | -- | n/a | n/a |
| status | HTTP-Version (Response-Line) | -- | String (see Note 1) | M |
| Status-Code | -- | String |
| response body | error | error-ResponseType |
| -- | Upgrade Header |  | Constant string: websocket | M |
| -- | Connection Header | -- | Constant string: Upgrade | M |
|  | Sec-WebSocket-Accept Header | -- | String (see Note 2) | M |
| -- | See Note 3. | | | |
| NOTE 1: The HTTP version shall be not earlier than HTTP/1.1.  NOTE 2: The valid value needs to be assigned according to WebSocket protocol (see IETF RFC 6455 [40]).  NOTE 3: Other SS parameters (not listed in this table) independent from the Stage 2 may be used, according to the WebSocket protocol (see IETF RFC 6455 [40]). | | | | |



Figure 12.5.1.1.2-1: Message flow for establishing a streaming connection

The message flow for establishing a streaming connection illustrated on Figure 12.5.1.1.2-1 is as follows:

1. The performance data streaming service producer sends a HTTP POST request to the consumer.

- The URI identifies the "…/connections" collection resource.

- The request message body carries the information about the connecting producer identity via parameter "producerId" and about streams supported by the new connection via parameter "StreamInfoList".

2. The consumer sends a HTTP POST response to the producer.

- On success "201 Posted" shall be returned with the identifier of a newly created ".../connections/{connectionId}" resource.

- On failure, an appropriate error code shall be returned. The response message body may carry an error object.

3. If step 2 is successful, the performance data streaming service producer sends a HTTP GET (upgrade) request to the consumer to establish the WebSocket connection.

- The URI identifies the ".../connections/{connectionId}" resource with the /secure/flag;

- The HTTP-version in the Request-line indicates the HTTP version which is no earlier than HTTP/1.1;

- The Upgrade header is with value "websocket";

- The Connection header is with value "Upgrade";

- The Sec-WebSocket-Key header is with a valid value according to IETF RFC 6455 [40].

- The Sec-WebSocket-Version header is with a valid according to IETF RFC 6455 [40].

4. The consumer sends a HTTP GET (Upgrade) response to the producer.

- On success, "101 Switching Protocols" shall be returned;

- On failure, an appropriate error code shall be returned. The response message body may carry an error object.

- The HTTP-version in the Response-line indicates the HTTP version which is no earlier than HTTP/1.1;

- The Upgrade header is with value "websocket";

- The Connection header is with value "Upgrade";

- The Sec-WebSocket-Accept header is with a valid value according to IETF RFC 6455 [40].

##### 12.5.1.1.3 Operation "terminateStreamingConnection"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.3-1 and 12.5.1.1.3-2.

Table 12.5.1.1.3-1: Mapping of IS operation input parameters to SS equivalents (WebSocket Close frame sent)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | n/a | -- | n/a | n/a |
| -- | Opcode (see clause 5 of IETF RFC 6455 [40]) | -- | Constant value: 0x8 | M |

Table 12.5.1.1.3-2: Mapping of IS operation output parameters to SS equivalents (WebSocket Close frame received)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| status | Opcode | -- | For a successful operation, the Opcode is 0x8, and for an unsuccessful operation, the Opcode has a value other than 0x8 (see clause 5 of IETF RFC 6455 [40]). | M |

##### 12.5.1.1.4 Operation "reportStreamData"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.4-1 and 12.5.1.1.4-2.

Table 12.5.1.1.4-1: Mapping of IS operation input parameters to SS equivalents (WebSocket Data frame sent with Opcode of 0x2)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | n/a | -- | n/a | n/a |
| -- | Opcode (see clause 5 of IETF RFC 6455 [40]) | -- | Constant value: 0x2 ("binary") | M |
| streamingData | Payload data | Streaming Trace Payload  or  streaming performance data payload  or  streaming analytics payload  or  proprietary data payload | See clause 5 of 3GPP TS 32.423 [39] for detailed definition of the Streaming Trace Payload format and Annex G of 3GPP TS 28.550 [40] for detailed definition of the streaming performance data payload format. | M |

The protocol stack with Streaming Trace Payloads formatted as per clause 5 of 3GPP TS 32.423 [39] carried by WebSocket binary data frames (see clause 5.6 of IETF RFC 6455 [40]) is illustrated on Figure 12.5.1.1.4-1.

The protocol stack with streaming performance data payloads formatted as per Annex G of 3GPP TS 28.550 [42] carried by WebSocket binary data frames (see clause 5.6 of IETF RFC 6455 [40]) is illustrated on Figure 12.5.1.1.4-2.

Table 12.5.1.1.4-2: Mapping of IS operation output parameters to SS equivalents

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| status | n/a | -- See Note 1. | n/a | n/a |
| NOTE 1: The delivery of WebSocket Data frame is taken care of by the underlying TCP (see IETF RFC 793 [41]) which provides reliable data transmission and ensures the data delivery. There is no mechanism at WebSocket protocol level to report the delivery status for WebSocket Data frame. | | | | |



Figure 12.5.1.1.4-1: Protocol stack for streaming trace data reporting



Figure 12.5.1.1.4-2: Protocol stack for streaming performance data reporting

##### 12.5.1.1.5 Operation "addStream"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.5-1 and 12.5.1.1.5-2.

Table 12.5.1.1.5-1: Mapping of IS operation input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | Headers | Request-URI | String | n/a |
| streamInfoList | request body | streamInfoList | array(streamInfo-Type) | M |

Table 12.5.1.1.5-2: Mapping of IS operation output parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| streamInfoList | response body | streamInfoList | array(streamInfo-Type) | M |
| status | response status codes  response body | n/a  error | n/a  error-ResponseType | M |

##### 12.5.1.1.6 Operation "deleteStream"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.6-1 and 12.5.1.1.6-2.

Table 12.5.1.1.6-1: Mapping of IS operation input parameters to SS equivalents (HTTP DELETE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | headers | Request-URI | String | n/a |
| streamIdList | path,  query | /connections/{connectionId}/streams,  streamIdList | array(streamId-Type) | M |

Table 12.5.1.1.6-2: Mapping of IS operation output parameters to SS equivalents (HTTP DELETE)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| status | response status codes  response body | n/a  error | n/a  error-ResponseType | M |

##### 12.5.1.1.7 Operation "getConnectionInfo"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.7-1 and 12.5.1.1.7-2.

Table 12.5.1.1.7-1: Mapping of IS operation input parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | headers | Request-URI | String | n/a |
| connectionIdList | path,  query | /connections,  /connections/{connectionId} | array(uri-Type) | M |

Table 12.5.1.1.7-2: Mapping of IS operation output parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionInfoList | response body | connectionInfoList | array(uri-Type, streamReporter-Type, streamIdList-Type) | M |
| status | response status codes  response body | n/a  error | n/a  error-ResponseType | M |

##### 12.5.1.1.8 Operation "getStreamInfo"

The IS operation parameters are mapped to SS equivalents according to the tables 12.5.1.1.8-1 and 12.5.1.1.8-2.

Table 12.5.1.1.8-1: Mapping of IS operation input parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| connectionId | headers | Request-URI | String | n/a |
| streamIdList | path,  query | /connections/{connectionId}/streams,  streamIdList | array(streamId-Type) | M |

Table 12.5.1.1.8-2: Mapping of IS operation output parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| streamInfoSumList | response body | streamInfoSumList | array(streamInfo-Type, streamReporters-Type) | M |
| status | response status codes  response body | n/a  error | n/a  error-ResponseType | M |

#### 12.5.1.2 Mapping of notifications

Not applicable (no notifications defined in IS).

#### 12.5.1.3 Resources

##### 12.5.1.3.1 Resources structure

Figure 12.5.1.3.1-1 shows the resource structure of the Streaming data reporting service.



Figure 12.5.1.3.1-1: Resource URI structure of the Streaming data reporting service

Table 12.5.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| connections | /connections | POST | Inform consumer about reporting streams to be carried by the new connection and receive a new connection id. |
| GET | Obtain information about connections |
| connection | /connections/{connectionId} | GET (Upgrade) | Establish WebSocket for a given connection |
| GET | Obtain information about connection |
| WebSocket 0x2 | Send a unit of streaming data |
| WebSocket 0x8 | Terminate a WebSocket connection |
| streams | /connections/{connectionId}/streams | POST | Inform consumer about new reporting streams on an existing connection. |
| DELETE | Remove reporting streams from an existing connection |
| GET | Obtain information about streams |
| stream | /connections/{connectionId}/streams/{streamId} | GET | Obtain information about stream |

##### 12.5.1.3.2 Resources definitions

12.5.1.3.2.1 Resource "/connections"

12.5.1.3.2.1.1 Description

This resource represents a collection of connections and can be used to establish new connections or to obtain information about existing connections.

12.5.1.3.2.1.2 URI

The resource URI is: {MnSRroot}/StreamingDataReportingMnS/{version}/connections

This resource shall support the resource URI variables defined in the table 12.5.1.3.2.1.2-1.

Table 12.5.1.3.2.1.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| root | indicates the scheme ("http" or "https"), the host name and optional port, and an optional sequence of path segments that together represent a prefix path |

12.5.1.3.2.1.3 HTTP methods

12.5.1.3.2.1.3.1 HTTP POST

This method shall support the URI query parameters specified in the following table.

**Table 12.5.1.3.2.1.3.1-1: URI query parameters supported by the POST method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| none supported |  |  |  |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

**Table 12.5.1.3.2.1.3.1-2: Data structures supported by the POST request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| producerId | String representing the DN of the streaming data reporting MnS producer. | M |
| array(streamInfo-Type) | List of meta-data about each reporting stream. Where each reporting stream is represented by a streamInfo. |  |

**Table 12.5.1.3.2.1.3.1-3: Data structures supported by the POST Response Body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |
| uri-Type | 201 Posted | Connection identifier assigned by the MnS consumer | M |

12.5.1.3.2.1.3.2 HTTP GET

This method shall support the URI query parameters specified in the following table.

**Table 12.5.1.3.2.1.3.2-1: URI query parameters supported by the GET method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| connectionIdList | array(uri-Type) | The list of connectionId for which the connection information is to be returned. | O |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

**Table 12.5.1.3.2.1.3.2-2: Data structures supported by the GET request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| n/a | n/a | n/a |

**Table 12.5.1.3.2.1.3.2-3: Data structures supported by the GET Response Body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |
| array(uri-Type, streamReporter-Type, streamIdList-Type) | 200 OK | In case of success the representation of the retrieved information is returned. | M |
| 202 Partially retrieved | In case of partial success the representation of the retrieved information is returned. | M |

12.5.1.3.2.2 Resource "/connections/{connectionId}"

12.5.1.3.2.2.1 Description

This resource represents an individual connection and can be used for an "upgrade" to WebSocket as part of the connection establishment, or to obtain information about an existing connection, or to terminate an existing connection, or to send a unit of streaming data.

12.5.1.3.2.2.2 URI

The resource URI is: {MnSRoot}/StreamingDataReportingMnS/{version}/connections/{connectionId}

This resource shall support the resource URI variables defined in the table 12.5.1.3.2.2.2-1.

Table 12.5.1.3.2.2.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| root | See table 12.5.1.3.2.1.2-1 |
| connectionId | Represents identifier of an individual connection assigned by the MnS consumer during connection establishment |

12.5.1.3.2.2.3 HTTP methods

12.5.1.3.2.2.3.1 HTTP GET (Upgrade)

This method shall support the URI header parameters specified in the following table.

**Table 12.5.1.3.2.2.3.2-1: Header parameters supported by the GET request on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| connectionId | uri-Type | To indicate the ID (URI) of the connection being upgraded to WebSocket | M |
| Upgrade | Upgrade-HeaderType | To indicate the HTTP GET operation is to upgrade the connection to WebSocket protocol | M |
| Connection | Connection-HeaderType | To indicate the HTTP GET operation is to upgrade the connection to another protocol | M |
| Sec-WebSocket-Key | Sec-WebSocket-Key-HeaderType | The Sec-WebSocket-Key needed for establishing the WebSocket connection. | M |
| Sec-WebSocket-Version | Sec-WebSocket-Version-HeaderType | The Sec-WebSocket-Version needed for establishing the WebSocket connection. | M |

This method shall support the URI query parameters specified in the following table.

**Table 12.5.1.3.2.2.3.2-2: URI query parameters supported by the GET method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| none supported |  |  |  |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

**Table 12.5.1.3.2.2.3.2-3: Data structures supported by the GET request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| n/a | n/a | n/a |

**Table 12.5.1.3.2.2.3.2-4: Header parameters supported by the GET response on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| Upgrade | Upgrade-HeaderType | To indicate the HTTP GET operation is to upgrade the connection to WebSocket protocol | M |
| Connection | Connection-HeaderType | To indicate the HTTP GET operation is to upgrade the connection to another protocol | M |
| Sec-WebSocket-Accept | Sec-WebSocket-Accept-HeaderType | The Sec-WebSocket-Accept responded when establishing the WebSocket connection. | M |

**Table 12.5.1.3.2.2.3.2-5: Data structures supported by the GET response body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| n/a | 101 Switching Protocols | The status code indicating the connection has been successfully upgraded to WebSocket. | M |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |

12.5.1.3.2.2.3.2 HTTP GET

This method shall support the URI query parameters specified in the following table.

**Table 12.5.1.3.2.1.3.2-1: URI query parameters supported by the GET method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| none supported |  |  |  |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

**Table 12.5.1.3.2.1.3.2-2: Data structures supported by the GET request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| n/a | n/a | n/a |

**Table 12.5.1.3.2.1.3.2-3: Data structures supported by the GET Response Body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |
| uri-Type | 200 OK | In case of success the representation of the connectionId is returned. | M |
| streamReporter-Type | 200 OK | In case of success the representation of the streamReporter is returned. | M |
| streamIdList-Type | 200 OK | In case of success the representation of the streamIdList is returned. | M |

12.5.1.3.2.3 Resource "/connections/{connectionId}/streams"

12.5.1.3.2.3.1 Description

This resource represents a collection of reporting streams on a particular connection and can be used to add a new reporting stream to an existing connection, or to remove a reporting stream from an existing connection, or to obtain information about reporting streams.

12.5.1.3.2.3.2 URI

The resource URI is: {MnSR}/StreamingDataReportingMnS/{version}/connections/{connectionId}/streams

This resource shall support the resource URI variables defined in the table 12.5.1.3.2.3.2-1.

Table 12.5.1.3.2.3.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| root | See table 12.5.1.3.2.1.2-1 |
| connectionId | See table 12.5.1.3.2.2.2-1 |

12.5.1.3.2.3.3 HTTP methods

12.5.1.3.2.3.3.1 HTTP POST

This method shall support the URI query parameters specified in the following table.

**Table 12.5.1.3.2.3.3.1-1: URI query parameters supported by the POST method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| none supported |  |  |  |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

**Table 12.5.1.3.2.3.3.1-2: Data structures supported by the POST request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| array(streamInfo-Type) | The resource representation of the set of information about streams to be posted. | M |

**Table 12.5.1.3.2.3.3.1-3: Data structures supported by the POST Response Body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| array(streamInfo-Type) | 201 Posted | In case of success the representation of the posted information about streams is returned. | M |
| 202 Partially posted | In case of partial success the representation of the posted information about streams is returned. | M |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |

12.5.1.3.2.3.3.2 HTTP DELETE

This method shall support the URI query parameters specified in the following table.

Table 12.5.1.3.2.3.3.2-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| streamIdList | array(streamId-Type) | The list of streamId for the stream(s) to be deleted. | M |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

Table 12.5.1.3.2.3.3.2: Data structures supported by the DELETE request body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| n/a | n/a | n/a |

Table 12.5.1.3.2.3.3.2-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| n/a | 204 No Content | In case of success no message body is returned | M |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |

12.5.1.3.2.3.3.3 HTTP GET

This method shall support the URI query parameters specified in the following table.

Table 12.5.1.3.2.3.3.3-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| streamIdList | array(streamId-Type) | The list of streamId for which the stream information are to be returned. | O |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

Table 12.5.1.3.2.3.3.3-2: Data structures supported by the GET request body on this resource

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| n/a | n/a | n/a |

Table 12.5.1.3.2.3.3.3-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| array(streamInfo-Type, streamReporters-Type) | 200 OK | In case of success the representation of the retrieved stream information is returned. | M |
| 202 Partially retrieved | In case of partial success the representation of the retrieved stream information is returned. | M |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |

12.5.1.3.2.4 Resource "/connections/{connectionId}/streams/{streamId}"

12.5.1.3.2.4.1 Description

This resource represents an individual reporting stream on an existing connection and can be used to obtain information about reporting stream.

12.5.1.3.2.4.2 URI

The resource URI is: {MnSR}/StreamingDataReportingMnS/{version}/connections/{connectionId}/streams/{streamId}

This resource shall support the resource URI variables defined in the table 12.5.1.3.2.4.2-1.

Table 12.5.1.3.2.4.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| root | See table 12.5.1.3.2.1.2-1 |
| connectionId | See table 12.5.1.3.2.2.2-1 |
| streamId | Represents identifier of an individual stream. For Streaming Trace reporting, the Trace Reference (see clause 5.6 of 3GPP TS 32.422 [38]) is used as stream identifier |

12.5.1.3.2.4.3 HTTP methods

12.5.1.3.2.4.3.1 HTTP GET

This method shall support the URI query parameters specified in the following table.

**Table 12.5.1.3.2.4.3.1-1: URI query parameters supported by the GET method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| none supported |  |  |  |

This method shall support the request data structures, the response data structures and response codes specified in the following table.

**Table 12.5.1.3.2.4.3.1-2: Data structures supported by the GET request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
| n/a | n/a | n/a |

**Table 12.5.1.3.2.4.3.1-3: Data structures supported by the GET Response Body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| streamInfo-Type | 200 OK | In case of success the representation of the retrieved stream information is returned. | M |
| streamReporters-Type | 200 OK | In case of success the representation of the retrieved stream reporters information is returned. | M |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |

#### 12.5.1.4 Data type definitions

##### 12.5.1.4.1 General

Table 12.5.1.4.1-1: Data types defined

|  |  |  |
| --- | --- | --- |
| **Data type** | **Reference** | **Description** |
| **General types** | | |
| uri-Type | 12.5.1.4.3 | Used to represent a URI |
| **Types used in paths** | | |
| connectionId-Type | 12.5.1.4.3 | Used to indicate the connection as a context of the operation |
| streamId-Type | 12.5.1.4.3 | Used to indicate the stream as a context of the operation |
| **Types used in headers** | | |
| websocketHeaderConnection-Type | 12.5.1.4.3 | Header value for the upgrade request and response |
| websocketHeaderUpgrade-Type | 12.5.1.4.3 | Header value for the upgrade to WebSocket request and response |
| websocketHeader-Sec-WebSocket-Accept-Type | 12.5.1.4.3 | Header value for secure WebSocket response. Carries hash. |
| websocketHeader-Sec-WebSocket-Extensions-Type | 12.5.1.4.3 | Header value for secure WebSocket request. Carries protocol extensions. |
| websocketHeader-Sec-WebSocket-Key-Type | 12.5.1.4.3 | Header value for secure WebSocket request. Provides information to the server which is needed in order to confirm that the client is entitled to request an upgrade to WebSocket. |
| websocketHeader-Sec-WebSocket-Protocol-Type | 12.5.1.4.3 | Header value for secure WebSocket request. Carries a comma-separated list of subprotocol names, in the order of preference. |
| websocketHeader-Sec-WebSocket-Version-Type | 12.5.1.4.3 | Header value for secure WebSocket request and response. Carries the WebSocket protocol version to be used. |
| **Types used in query parts** | | |
| connectionId-Type | 12.5.1.4.3 | Used to indicate the connection as a context of the operation |
| streamId-Type | 12.5.1.4.3 | Used to indicate the stream as a context of the operation |
| **Types used in request bodies** | | |
| connectionRequest-Type | 12.5.1.4.2.2 | Used to carry the meta-data during connection establishment |
| streamInfo-Type | 12.5.1.4.2.5 | Reporting stream meta-data. |
| **Types used in response bodies** | | |
| failedConnectionResponse-Type | 12.5.1.4.2.4 | Used to carry the details of a failed connection establishment |
| connectionInfo-Type | 12.5.1.4.2.1 | Used to carry connection meta-data |
| errorResponse-Type | 12.5.1.4.2.3 | Used to carry the details of an error |
| streamInfo-Type | 12.5.1.4.2.5 | Used to carry the stream meta-data |
| streamInfoWithReporters-Type | 12.5.1.4.2.6 | Used to carry the augmented stream meta-data |
| **Types used for resources** | | |
| uri-Type | 12.5.1.4.3 | Used to represent resource URI |
| **Types referenced by the definitions above** | | |
| systemDN-Type | 12.5.1.4.3 | Used to represent DN of the reporting entity |
| traceJob-Type | Generic NRM | Used to represent Trace configuration |
| producerId-Type | 12.5.1.4.3 | Used to identify the reporting entity |
| streamType-Type | 12.5.1.4.3 | Used to identify the type of a reporting stream |
| serializationFormat-Type | 12.5.1.4.3 | Used to identify serialization method |
| measObjDn-Type | 12.5.1.4.3 | Used to represent DN of the measured object instance |
| measTypes-Type | 12.5.1.4.3 | Used to represent an ordered list of measurement types or KPI |
| analyticsInfo-Type | 12.5.1.4.3 | Used to represents information about streamed analytics |
| vsDataContainer-Type | Generic NRM | Used to represent details about proprietary data |

Table 12.5.1.4.1-2: Data types imported

|  |  |  |
| --- | --- | --- |
| **Data type** | **Reference** | **Description** |
| traceJob-Type | Generic NRM | Attributes container of the TraceJob IOC (see 3GPP TS 28.622 [11]). |
| vsDataContainer-Type | Generic NRM | Vendor specific data container (see 3GPP TS 28.622 [11]). |

##### 12.5.1.4.2 Query, message body and resource data types

12.5.1.4.2.1 Type connectionInfo-Type

Table 12.5.1.4.2.1-1: Definition of type connectionInfo-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| connection | connectionId-Type | Connection identifier | M |
| producer | producerId-Type | Producer identifier | M |
| streams | array(streamId-Type) | List of stream identifiers | M |

12.5.1.4.2.2 Type connectionRequest-Type

Table 12.5.1.4.2.2-1: Definition of type connectionRequest-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| producer | producerId-Type | Producer identifier | M |
| streams | array(streamInfo-Type) | List of stream meta-data | M |

12.5.1.4.2.3 Type errorResponse-Type

Table 12.5.1.4.2.3-1: Definition of type errorResponse-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| error | object | Key indicating the response body containing an error | M |
| > errorInfo | string | Attribute allowing to convey error information in string format | M |

12.5.1.4.2.4 Type failedConnectionResponse-Type

Table 12.5.1.4.2.4-1: Definition of type failedConnectionResponse-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| error | object | Key indicating the response body containing an error | M |
| > streamId | array(streamId-Type) | Attribute conveying the list of "problematic" stream IDs | M |
| > errorReason | string | Attribute allowing to convey error information in string format |  |

12.5.1.4.2.5 Type streamInfo-Type

Table 12.5.1.4.2.5-1: Definition of type streamInfo-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| streamId | streamId-Type | Stream identifier | M |
| streamType | streamType-Type | Enumerated stream type | M |
| serializationFormat | serializationFormat-Type | Enumerated serialization method | M |
| measObjDn | measObjDn-Type | DN of the measured object instance. Used for streaming performance data only. | CM |
| measTypes | measTypes-Type | Ordered list of measurement types or KPI. Used for streaming performance data only. | CM |
| analyticsInfo | analyticsInfo-Type | Information about streamed analytics. Used for streaming analytics only. | CM |
| vsDataContainer | vsDataContainer-Type | Details about proprietary data. Mandatory for proprietary data streaming only. | CM |
| traceInfo | traceJob-Type | Trace configuration. Used for streaming trace data reporting streams only. | CM |

Table 12.5.1.4.2.5-2: Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| measObjDn (support qualifier) | Attribute shall be present for streaming performance data only. |
| measTypes (support qualifier) | Attribute shall be present for streaming performance data only. |
| analyticsInfo (support qualifier) | Attribute shall be present for streaming analytics only. |
| vsDataContainer (support qualifier) | Attribute shall be present for proprietary data streaming. |
| traceInfo (support qualifier) | Attribute shall be present for streaming trace data only. |

12.5.1.4.2.6 Type streamInfoWithReporters-Type

Table 12.5.1.4.2.6-1: Definition of type streamInfoWithReporters-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| streamInfo | streamInfo-Type | Stream meta-data | M |
| reporters | producerId-Type | List of entities reporting streaming data | M |

##### 12.5.1.4.3 Simple data types and enumerations

12.5.1.4.3.1 General

This subclause defines simple data types and enumerations that are used by the data structures defined in the previous subclauses.

12.5.1.4.3.2 Simple data types

Table 12.5.1.4.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type name | Type definition | Description |
| analyticsInfo-Type | string | Information about streamed analytics. |
| measObjDn-Type | DN | See 3GPP TS 32.300 [25] |
| measTypes-Type | string | See 3GPP TS 28.550 [42] |
| websocketHeaderConnection-Type | Constant string "Upgrade" | Header value for the upgrade request and response. |
| websocketHeaderUpgrade-Type | Constant string "websocket" | Header value for the upgrade to WebSocket request and response. |
| websocketHeader-Sec-WebSocket-Accept-Type | string | Header value for secure WebSocket response. Carries hash. |
| websocketHeader-Sec-WebSocket-Extensions-Type | string | Header value for secure WebSocket request. Carries protocol extensions. |
| websocketHeader-Sec-WebSocket-Key-Type | string | Header value for secure WebSocket request. Provides information to the server which is needed in order to confirm that the client is entitled to request an upgrade to WebSocket. |
| websocketHeader-Sec-WebSocket-Protocol-Type | string | Header value for secure WebSocket request. Carries a comma-separated list of subprotocol names, in the order of preference. |
| websocketHeader-Sec-WebSocket-Version-Type | string | Header value for secure WebSocket request and response. Carries the WebSocket protocol version to be used. |
| connectionId-Type | uri-Type | Used to indicate the connection as a context of the operation |
| producerId-Type | systemDN-Type | Used to identify the reporting entity |
| serializationFormat-Type | enum | Enumerated serialization method with values: "GPB", "ASN1" |
| streamId-Type | Trace Reference | See 3GPP TS 32.422 [38] |
| streamType-Type | enum | Enumerated stream type with values: "TRACE", "PERFORMANCE", "ANALYTICS", "PROPRIETARY" |
| systemDN-Type | DN | See 3GPP TS 32.300 [25] |
| uri-Type | string | Used to represent resource URI |

## 12.6 File data reporting service

### 12.6.1 RESTful HTTP-based solution set

#### 12.6.1.1 Mapping of operations

##### 12.6.1.1.1 Introduction

The IS operations are mapped to SS equivalents according to table 12.6.1.1.1-1.

Table 12.6.1.1.1-1: Mapping of IS operations to SS equivalents

|  |  |  |  |
| --- | --- | --- | --- |
| **IS operation** | **HTTP Method** | **Resource URI** | **Qualifier** |
| listAvailableFiles | GET | /Files | M |
| subscribe | POST | /subscriptions | M |
| unsubscribe | DELETE | /subscriptions | M |
| DELETE | /subscriptions/{subscriptionId} | M |

##### 12.6.1.1.2 Operation "listAvailableFiles"

The IS operation parameters are mapped to SS equivalents according to table 12.6.1.1.2-1 and table 12.6.1.1.2-2.

Table 12.6.1.1.2-1: Mapping of IS operation input parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| fileType | query | fileType | fileType-Type | M |
| beginTime | query | beginTime | dateTime-Type | M |
| endTime | query | endTime | dateTime-Type | M |

Table 12.6.1.1.2-2: Mapping of IS operation output parameters to SS equivalents (HTTP GET)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **Qualifier** |
| fileInfoList | response body | n/a | fileInfoRetrieval-ResponseType | M |
| status | response status codes  response body | n/a  error | n/a  error-ResponseType | M |

The message flow is as follows:

- 1. The Service Consumer sends a HTTP GET request to the Service Provider.

- The URI identifies the "…/Files" collection resource.

- The query part may contain filter parameter. Absence of the query part means all available management data files shall be returned.

- The request message body shall be empty.

2. The Service Provider sends a HTTP GET response to the Service Consumer.

- On success "200 OK" shall be returned. The response message body shall carry the information of available files. The response format is defined by "fileInfoRetrieval-ResponseType ".

- On failure, an appropriate error code shall be returned. The response message body may carry an error object.

##### 12.6.1.1.3 Operation "subscribe"

See clause 12.2.1.1.8, with the discrepance that the subscribe operation in this clause is for file data reporting related notifications (i.e., notifyFileReady and notifyFilePreparationError).

##### 12.6.1.1.4 Operation "unsubscribe"

See clause 12.2.1.1.9, with the discrepance that the unsubscribe operation in this clause is for file data reporting related notifications (i.e., notifyFileReady and notifyFilePreparationError).

#### 12.6.1.2 Mapping of notifications

##### 12.6.1.2.1 Introduction

The IS notifications are mapped to SS equivalents according to table 12.6.1.2.1-1.

**Table 12.6.1.2.1-1: Mapping of IS notifications to SS equivalents**

|  |  |  |  |
| --- | --- | --- | --- |
| **IS notifications** | **HTTP Method** | **Resource URI** | **SQ** |
| notifyFileReady | POST | /notificationSink | M |
| notifyFilePreparationError | POST | /notificationSink | M |

##### 12.6.1.2.2 Notification "notifyFileReady"

The IS notification parameters are mapped to SS equivalents according to table 12.6.1.2.2-1.

Table 12.6.1.2.2-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **SQ** |
| objectClass | request body | href | uri-Type | M |
| objectInstance |
| notificationId | request body | notificationId | notificationId-Type | M |
| eventTime | request body | eventTime | dateTime-Type | M |
| notificationType | request body | notificationType | notificationType-Type | M |
| fileInfoList | request body | fileInfoList | array(fileInfo-Type) | M |
| additionalText | request body | additionalText | additionalText-Type | O |

##### 12.6.1.2.3 Notification "notifyFilePreparationError"

The IS notification parameters are mapped to SS equivalents according to table 12.6.1.2.3-1.

Table 12.6.1.2.3-1: Mapping of IS notification input parameters to SS equivalents (HTTP POST)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IS operation parameter name** | **SS parameter location** | **SS parameter name** | **SS parameter type** | **SQ** |
| objectClass | request body | href | uri-Type | M |
| objectInstance |
| notificationId | request body | notificationId | notificationId-Type | M |
| eventTime | request body | eventTime | dateTime-Type | M |
| notificationType | request body | notificationType | notificationType-Type | M |
| fileInfoList | request body | fileInfoList | array(fileInfo-Type) | M |
| reason | request body | reason | reason-Type | O |
| additionalText | request body | additionalText | additionalText-Type | O |

#### 12.6.1.3 Resources

##### 12.6.1.3.1 Resource structure

Figure 12.6.1.3.1-1 shows the resource structure of the file data reporting service.




Figure 12.6.1.3.1-1: Resource URI structure of the file data reporting service

Table 12.6.1.3.1-2 provides an overview of the resources and applicable HTTP methods.

Table 12.6.1.3.1-2: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Files | /Files | GET | Retrieve the information of the available files |
| subscriptions | /subscriptions | POST | Create a subscription |
| subscriptions | /subscriptions | DELETE | Delete all subscriptions made with a consumerReferenceId |
| subscription | /subscriptions/{subscriptionId} | DELETE | Delete a single subscription |
| notificationSink | /notificationSink | POST | Send notifications |

##### 12.6.1.3.2 Resource definitions

12.6.1.3.2.1 Resource “/Files”

12.6.1.3.2.1.1 Description

This resource represents the information about a collection of available files.

12.6.1.3.2.1.2 URI

Resource URI = {MnSRoot}/FileDataReportingMnS/{MnSVersion}/Files

The resource URI variables a defined in the following table.

Table 12.6.1.3.2.1.1-1: URI variables

|  |  |
| --- | --- |
| **Name** | **Definition** |
| MnSRoot | See clause 4.4 of TS 32.158 [15] |

12.6.1.3.2.1.3 HTTP methods

12.6.1.3.2.1.3.1 HTTP GET

This method shall support the URI query parameters specified in the following table.

**Table 12.6.1.3.2.1.3.1-1: URI query parameters supported by the GET method on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Data type** | **Description** | **SQ** |
| fileType | fileType | To filter the available files based on the file type. | M |
| beginTime | dateTime-Type | To filter the available files who became ready no later than this time stamp. | M |
| endTime | dateTime-Type | To filter the available files who became ready no earlier than this time stamp. | M |

This method shall support the request data structures, the response data structures and response codes specified in the following tables.

**Table 12.6.1.3.2.1.3.1-2: Data structures supported by the GET request body on this resource**

|  |  |  |
| --- | --- | --- |
| **Data type** | **Description** | **SQ** |
|  |  |  |

**Table 12.6.1.3.2.1.3.1-3: Data structures supported by the GET response body on this resource**

|  |  |  |  |
| --- | --- | --- | --- |
| **Data type** | **Response**  **codes** | **Description** | **SQ** |
| fileInfoRetrieval-ResponseType | 200 OK | The resource representation of the infomraiton about the available files retrieved. | M |
| error-ResponseType | 4xx/5xx | Returned in case of an error | M |

12.6.1.3.2.2 Resource "/subscriptions"

12.6.1.3.2.2.1 Description

This resource is a container resource for individual subscriptions.

12.6.1.3.2.2.2 URI

The resource URI is:

Resource URI: {MnSRoot}/FileDataReportingMnS/{MnSVersion}/subscriptions

The resource URI variables a defined in the following table.

Table 12.6.1.3.3.2.2.2-1: URI variables

|  |  |
| --- | --- |
| **Name** | **Definition** |
| MnSRoot | See clause 4.4 of TS 32.158 [15] |

12.6.1.3.2.2.3 HTTP methods

12.6.1.3.2.2.3.1 POST

This method shall support the URI query parameters specified in table 12.6.1.3.2.2.3.1-1.

Table 12.6.1.3.2.2.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | Qualifier |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures specified in table 12.6.1.3.2.2.3.1-2 and the response data structures and response codes specified in table 12.6.1.3.2.2.3.1-3.

Table 12.6.1.3.2.2.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | SQ |
| subscription-RequestType | Details of the subscription to be created | M |

Table 12.6.1.3.2.2.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | SQ |
| subscription-ResponseType | 201 Created | In case of success the representation of the created subscription is returned. | M |
| error-ResponseType | 4xx/5xx | In case of failure the error object is returned. | M |

12.6.1.3.2.2.3.2 DELETE

This method shall support the URI query parameters specified in table 12.6.1.3.2.2.3.2-1.

Table 12.6.1.3.2.2.3.2-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | Qualifier |
| consumerReferenceId | consumerReferenceId-QueryType | Identifies the consumer whose subscriptions shall be deleted | M |

This method shall support the request data structures specified in table 12.6.1.3.2.2.3.2-2 and the response data structures and response codes specified in table 12.6.1.3.2.2.3.2-3.

Table 12.6.1.3.2.2.3.2-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | SQ |
| n/a | n/a | n/a |

Table 12.6.1.3.2.2.3.2-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | SQ |
| n/a | 204 No Content | In case of success no message body is returned | n/a |
| error-ResponseType | 4xx/5xx | In case of failure the error object is returned. | M |

12.6.1.3.2.3 Resource "/subscriptions/{subscriptionId}"

12.6.1.3.2.3.1 Description

This resource represents a subscription.

12.6.1.3.2.3.2 URI

The resource URI is:

Resource URI: {MnSRoot}/FileDataReportingMnS/{MnSVersion}/subscriptions/{subscriptionId}

Table 12.6.1.3.2.3.2-1: URI variables

|  |  |
| --- | --- |
| Name | Definition |
| MnSRoot | See clause 4.4 of TS 32.158 [15] |
| subscriptionId | Subscription identifier |

12.6.1.3.2.3.3 HTTP methods

12.6.1.3.2.3.3.1 DELETE

This method shall support the URI query parameters specified in table 12.6.1.3.2.3.3-1.

Table 12.6.1.3.2.3.3-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | Qualifier |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures specified in table 12.6.1.3.2.3.3-2 and the response data structures and response codes specified in table 12.6.1.3.2.3.3-3.

Table 12.6.1.3.2.3.3-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | SQ |
| n/a | n/a | n/a |

Table 12.6.1.3.2.3.3-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | SQ |
| n/a | 204 No Content | In case of success no message body is returned | M |
| error-ResponseType | 4xx/5xx | In case of failure the error object is returned. | M |

12.6.1.3.2.4 Resource "/notificationSink"

12.6.1.3.2.4.1 Description

This resource represents a resource to which notifications are sent to.

12.6.1.3.2.4.2 URI

The resource URI is provided by the notification subscriber when creating the subscription.

12.6.1.3.2.4.3 HTTP methods

12.6.1.3.2.4.3.1 POST

This method shall support the URI query parameters specified in table 12.6.1.3.2.4.3.1-1.

Table 12.6.1.3.2.4.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Data type | Description | Qualifier |
| n/a | n/a | n/a | n/a |

This method shall support the request data structures specified in table 12.6.1.3.2.4.3.1-2 and the response data structures and response codes specified in table 12.6.1.3.2.4.3.1-3.

Table 12.6.1.3.2.4.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |
| --- | --- | --- |
| Data type | Description | SQ |
| notifyFileReady-NotifType | Type in case a notifyFileReady notification is sent | M |
| notifyFilePreparationError-NotifType | Type in case a notifyFilePreparationError notification is sent | M |

Table 12.6.1.3.2.4.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Response  codes | Description | SQ |
| n/a | 204 No Content | In case of success no message body is returned | M |
| error-ResponseType | 4xx/5xx | In case of failure the error object is returned. | M |

#### 12.6.1.4 Data type definitions

##### 12.6.1.4.1 General

Table 12.6.1.4.1-1: Data types defined in this specification

|  |  |  |
| --- | --- | --- |
| **Data type** | **Reference** | **Description** |
| **General types** | | |
| dataTime-Type | 12.6.1.4.6.2 | Data type of date and time. |
| uri-Type | 12.6.1.4.6.2 | The data type of a URI. |
| **Types used in paths** | | |
|  |  |  |
| **Types used in query parts** | | |
| file-Type | 12.6.1.4.6.3 | Used in listing the information of available files describing the type of the files. |
| consumerReferenceId-QueryType | 12.6.1.4.6.2 | Used in the query part of HTTP DELETE on /Subscriptions to delete all subscriptions made with a specific consumerReferenceId |
| **Types used in request bodies** | | |
| subscription-RequestType | 12.6.1.4.4.1 | Used in the request body of HTTP POST on /subscriptions to create file data reporting notifications subscriptions. |
| **Types used in response bodies** | | |
| fileInfoRetrieval-ResponseType | 12.6.1.4.4.2 | Used in the response body of HTTP GET describing the information of the listed files. |
| error-ResponseType | 12.6.1.4.4.3 | Used in the response body describing the error. |
| **Types used for resources** | | |
| subscription-ResourceType | 12.6.1.4.4.4 | Representation of a subscription resource. |
| **Types used in notifications** |  |  |
| notifyFileReady-NotifType | 12.6.1.4.4.5 | Used in the request body of HTTP POST for the notification type notifyFileReady. |
| notifyFilePreparationError-NotifType | 12.6.1.4.4.6 | Used in the request body of HTTP POST for the notification type notifyFilePreparationError. |
| **Types referenced by the definitions above** | | |
| fileInfo-Type | 12.6.1.4.5.1 | Used for describing the file information. |
| notificationId-Type | 12.6.1.4.6.2 | Notification identifier as defined in ITU-T Rec. X. 733 [4] |
| notificationType-Type | 12.6.1.4.6.2 | Notification type (notifyFileReady, etc.) |
| additionalText-Type | 12.6.1.4.6.2 | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] |
| reason-Type | 12.6.1.4.6.2 | Used to describe the reason causing the file preparation error. |

Table 12.6.1.4.1-2: Data types imported

|  |  |  |
| --- | --- | --- |
| **Data type** | **Reference** | **Description** |
|  |  |  |

##### 12.6.1.4.2 Structured general data types

None.

##### 12.6.1.4.3 Structured path data types

None.

##### 12.6.1.4.4 Query, message body and resource data types

12.6.1.4.4.1 Type subscription-RequestType

**Table 12.6.1.4.4.1-1: Definition of type subscription-RequestType**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| data | subscription-ResourceType | Used in the request body of HTTP POST on /subscriptions describing the representation of the subscription to be created | M |

12.6.1.4.4.2 Type fileInfoRetrieval-ResponseType

Table 12.6.1.4.4.2-1: Definition of type fileInfoRetrieval-ResponseType

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| data | array(fileInfoType) | The information of the available files | M |

12.6.1.4.4.3 Type error-ResponseType

Table 12.6.1.4.4.3-1: Definition of type error-ResponseType

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| error | object | Key indicating the response body containing an error | M |
| > errorInfo | string | Attribute allowing to convey error information in string format | M |

12.6.1.4.4.4 Type subscription-ResourceType

**Table 12.6.1.4.4.4-1: Definition of type subscription-ResourceType**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| consumerReference | uri-Type | The URI of the endpoint to send the notification to (/notificationSink). | M |
| timeTick | long-Type | Time window within which the subscriber intends to subscribe again to confirm its subscription, see clause 11.2.2.2.5.1 | O |
| filter | filter-Type | Filter settings for this subscription, to define the subset of all notifications this subscription relates to. A notification is sent to the subscriber if the filter matches, or if there is no filter. | O |

12.6.1.4.4.5 Type notifyFileReady-NotifType

**Table 12.6.1.4.4.5-1: Definition of type notifyFileReady-NotifType**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| header |  |  |  |
| > href | uri-Type | URI of the resource indicating the file data reporting service | M |
| > notificationId | notificationId-Type | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| > notificationType | notificationType-Type | Notification type (notifyFileReady, etc.) | M |
| > eventTime | dateTime-Type | Event occurrence time (e.g., the file ready time) | M |
| body |  |  |  |
| > fileInfoList | array(fileInfo-Type) | The information of the available files | M |
| > additionalText | additionalText-Type | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |

12.6.1.4.4.6 Type notifyFilePreparationError-NotifType

**Table 12.6.1.4.4.6-1: Definition of type notifyFilePreparationError-NotifType**

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| header |  |  |  |
| > href | uri-Type | URI of the resource indicating the file data reporting service | M |
| > notificationId | notificationId-Type | Notification identifier as defined in ITU-T Rec. X. 733 [4] | M |
| > notificationType | notificationType-Type | Notification type (notifyFileReady, etc.) | M |
| > eventTime | dateTime-Type | Event occurrence time (e.g., the file ready time) | M |
| body |  |  |  |
| > fileInfoList | array(fileInfo-Type) | The information of the available files | M |
| > reason | reason-Type | The reason that caused the error of the file preparation. |  |
| > additionalText | additionalText-Type | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] | O |

##### 12.6.1.4.5 Referenced structured data types

12.6.1.4.5.1 Type fileInfo-Type

Table 12.6.1.4.5-1: Definition of fileInfo-Type

|  |  |  |  |
| --- | --- | --- | --- |
| **Attribute name** | **Data type** | **Description** | **SQ** |
| fileLocation | uri-Type | Usd to indicate the location of the file. | M |
| fileSize | long-Type | The size of the file with positive Integer value (the unit is byte). | M |
| fileReadyTime | dataTime-Type | Indicates the date and time when the file was last closed and made available in the management service producer and the file content will not be changed. | M |
| fileExpirationTime | dataTime-Type | Indicates the date and time beyond which the file may be deleted. | M |
| fileCompression | string | Identifies the name of the compression algorithm used for the file. | M |
| fileFormat | string | Identifies the encoding technique used by the file. Its value should indicate the version of the file format specification plus to indicate if "ASN1" or "XML-schema" is used. | M |
| fileType | file-Type | It identifies the the type of the management data stored in the file. Following are the allowed values:  - For performance data (including measurement data and KPI) files, the value is assigned to "PERFORMANCE".  - For trace data files, the value is assigned to "TRACE".  - For analytic data files, the value is assigned to "ANALYTICS".  - For proprietary data files, the value is assigned to "PROPRIETARY". | M |

##### 12.6.1.4.6 Simple data types and enumerations

12.6.1.4.6.1 General

This clause defines simple data types and enumerations that are used by the data structures defined in the previous clauses.

12.6.1.4.6.2 Simple data types

Table 12.6.1.4.6.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type name | Type definition | Description |
| dataTime-Type | string | The data type for date and time in “date-time” format. |
| uri-Type | string | The type of a URI. |
| consumerReferenceId-QueryType | uri-Type | Used in the query part of HTTP DELETE on /subscriptions to delate all subscriptions made with a specific consumerReferenceId. |
| filter-Type | string | Filter of a subscription resource. |
| notificationId-Type | long | Notification identifier as defined in ITU-T Rec. X. 733 [4] |
| additionalText-Type | string | Allows a free form text description to be reported as defined in ITU-T Rec. X. 733 [4] |
| reason-Type | string | THe type for describing the reason that caused the file preparation error. |

12.6.1.4.6.3 Enumeration fileType-Type

Table 12.6.1.4.6.3-1: Enumeration fileType-Type

|  |  |
| --- | --- |
| Enumeration value | Description |
| PERFORMANCE | It indicates that the file type is “Performance data file” |
| TRACE | It indicates that the file type is “Trace data file” |
| ANALYTICS | It indicates that the file type is “Analytics data file” |
| PROPRIETARY | It indicates that the file type is “Proprietary data file” |

12.6.1.4.6.4 Enumeration notificationType-Type

Table 12.6.1.4.6.4-1: Enumeration notificationType-Type

|  |  |
| --- | --- |
| Enumeration value | Description |
| notifyFileReady | Notification type is notifyFileReady |
| notifyFilePreparationError | Notification type is notifyFilePreparationError |

Annex A (normative):  
OpenAPI specification

# A.0 Introduction

This clause describes the capabilities of the service in the structure of the OpenAPI Specification Version 3.0.1 [A9]. The OpenAPI definitions are provided in YAML or JSON format.

# A.1 Provisioning management service

## A.1.0 Introduction

Clause A.1.1 contains the OpenAPI definition of the provisioning MnS which includes the provisioning MnS operations and the provisioning MnS notifications.

Clause A.1.2 provides indications regarding the content of the generic provisioning MnS notifications when the consumer of these notifications supports the ONAP VES API. This content is sent as payload of VES events (see Annex B).

## A.1.1 OpenAPI document "provMnS.yaml"

openapi: 3.0.1

info:

title: Provisioning MnS

version: 16.5.0

description: >-

OAS 3.0.1 definition of the Provisioning MnS

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.532; Generic management services

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.532/

servers:

- url: '{MnSRoot}/ProvMnS/{MnSVersion}/{URI-LDN-first-part}'

variables:

MnSRoot:

description: See clause 4.4.2 of TS 32.158

default: http://example.com/3GPPManagement

MnSVersion:

description: Version number of the OpenAPI definition

default: XXX

URI-LDN-first-part:

description: See clause 4.4.2 of TS 32.158

default: ''

paths:

'/{className}={id}':

parameters:

- name: className

in: path

required: true

schema:

type: string

- name: id

in: path

required: true

schema:

type: string

put:

summary: Replaces a complete single resource or creates it if it does not exist

description: >-

With HTTP PUT a complete resource is replaced or created if it does not

exist. The target resource is identified by the target URI.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/Resource'

responses:

'200':

description: >-

Success case ("200 OK").

This status code shall be returned when the resource is replaced, and

when the replaced resource representation is not identical to the resource

representation in the request.

This status code may be retourned when the resource is updated and when the

updated resource representation is identical to the resource representation

in the request.

The representation of the updated resource is returned in the response

message body.

content:

application/json:

schema:

$ref: '#/components/schemas/Resource'

'201':

description: >-

Success case ("201 Created").

This status code shall be returned when the resource is created.

The representation of the created resource is returned in the response

message body.

content:

application/json:

schema:

$ref: '#/components/schemas/Resource'

'204':

description: >-

Success case ("204 No Content").

This status code may be returned only when the replaced resource

representation is identical to the representation in the request.

The response has no message body.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

callbacks:

notifyMOICreation:

'{request.body#/notificationRecipientAddress}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyMoiCreation'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response

has no message body.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyMOIDeletion:

'{request.body#/notificationRecipientAddress}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyMoiDeletion'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response

has no message body.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyMOIAttributeValueChanges:

'{request.body#/notificationRecipientAddress}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyMoiAttributeValueChanges'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response

has no message body.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyMOIChanges:

'{request.body#/notificationRecipientAddress}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyMoiChanges'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response

has no message body.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/Error-Response'

get:

summary: Reads one or multiple resources

description: >-

With HTTP GET resources are read. The resources to be retrieved are

identified with the target URI. The attributes and fields parameter

of the query components allow to select the resource properties to be returned.

parameters:

- name: scope

in: query

description: >-

This parameter extends the set of targeted resources beyond the base

resource identified with the path component of the URI. No scoping

mechanism is specified in the present document.

required: false

schema:

$ref: '#/components/schemas/Scope'

style: form

explode: true

- name: filter

in: query

description: >-

This parameter reduces the targeted set of resources by applying a

filter to the scoped set of resource representations. Only resource

representations for which the filter construct evaluates to "true"

are targeted. No filter language is specified in the present

document.

required: false

schema:

$ref: 'comDefs.yaml#/components/schemas/Filter'

- name: attributes

in: query

description: >-

This parameter specifies the attributes of the scoped resources that

are returned.

required: true

schema:

type: array

items:

type: string

style: form

explode: false

- name: fields

in: query

description: >-

This parameter specifies the attribute field of the scoped resources

that are returned.

required: false

schema:

type: array

items:

type: string

style: form

explode: false

responses:

'200':

description: >-

Success case ("200 OK").

The resources identified in the request for retrieval are returned

in the response message body. In case the attributes or fields query

parameters are used, only the selected attributes or sub-attributes are

returned. The response message body is constructed according to the

hierarchical response construction method (TS 32.158 [15]).

content:

application/json:

schema:

$ref: '#/components/schemas/Resource'

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

patch:

summary: Patches one or multiple resources

description: >-

With HTTP PATCH resources are created, updated or deleted. The resources

to be modified are identified with the target URI (base resource) and

the patch document included in the request message body.

requestBody:

description: >-

The request body describes changes to be made to the target resources.

The following patch media types are available

- "application/merge-patch+json" (RFC 7396)

- "application/3gpp-merge-patch+json" (TS 32.158)

- "application/json-patch+json" (RFC 6902)

- "application/3gpp-json-patch+json" (TS 32.158)

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/Resource'

application/3gpp-merge-patch+json:

schema:

$ref: '#/components/schemas/Resource'

application/json-patch+json:

schema:

type: array

items:

type: object

application/3gpp-json-patch+json:

schema:

type: array

items:

type: object

responses:

'200':

description: >-

Success case ("200 OK").

This status code is returned when the updated the resource representations

shall be returned for some reason.

The resource representations are returned in the response message body. The

response message body is constructed according to the hierarchical response

construction method (TS 32.158 [15])

content:

application/json:

schema:

$ref: '#/components/schemas/Resource'

'204':

description: >-

Success case ("204 No Content").

This status code is returned when there is no need to return the updated

resource representations.

The response message body is empty.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefsy.yaml#/components/schemas/ErrorResponse'

delete:

summary: Deletes one or multiple resources

description: >-

With HTTP DELETE resources are deleted. The resources to be deleted are

identified with the target URI.

parameters:

- name: scope

in: query

description: >-

This parameter extends the set of targeted resources beyond the base

resource identified with the path component of the URI. No scoping

mechanism is specified in the present document.

required: false

schema:

$ref: '#/components/schemas/Scope'

style: form

explode: true

- name: filter

in: query

description: >-

This parameter reduces the targeted set of resources by applying a

filter to the scoped set of resource representations. Only resources

representations for which the filter construct evaluates to "true"

are returned. No filter language is specified in the present

document.

required: false

schema:

$ref: 'comDefs.yaml#/components/schemas/Filter'

responses:

'200':

description: >-

Success case ("200 OK").

This status code shall be returned, when query parameters are present in

the request and one or multiple resources are deleted.

The URIs of the deleted resources are returned in the response message body.

'204':

description: >-

Success case ("204 No Content").

This status code shall be returned, when no query parameters are present in

the request and only one resource is deleted.

The message body is empty.

content:

application/json:

schema:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/Uri'

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

components:

schemas:

CorrelatedNotification:

type: object

properties:

source:

$ref: 'comDefs.yaml#/components/schemas/Dn'

notificationIds:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/NotificationId'

required:

- source

- notificatioIds

CmNotificationTypes:

type: string

enum:

- notifyMOICreation

- notifyMOIDeletion

- notifyMOIAttributeValueChanges

- notifyMOIChanges

SourceIndicator:

type: string

enum:

- RESOURCE\_OPERATION

- MANAGEMENT\_OPERATION

- SON\_OPERATION

- UNKNOWN

Operation:

type: string

enum:

- CREATE

- DELETE

- REPLACE

ScopeType:

type: string

enum:

- BASE\_ONLY

- BASE\_NTH\_LEVEL

- BASE\_SUBTREE

- BASE\_ALL

Scope:

type: object

properties:

scopeType:

$ref: '#/components/schemas/ScopeType'

scopeLevel:

type: integer

Resource:

oneOf:

- type: object

properties:

id:

type: string

attributes:

type: object

additionalProperties:

type: array

items:

type: object

- anyOf:

- $ref: 'genericNrm.yaml#/components/schemas/resources-genericNrm'

- $ref: 'nrNrm.yaml#/components/schemas/resources-nrNrm'

- $ref: '5gcNrm.yaml#/components/schemas/resources-5gcNrm'

- $ref: 'sliceNrm.yaml#/components/schemas/resources-sliceNrm'

MoiChange:

type: object

properties:

notificationId:

$ref: 'comDefs.yaml#/components/schemas/NotificationId'

correlatedNotifications:

type: array

items:

$ref: '#/components/schemas/CorrelatedNotification'

additionalText:

type: string

sourceIndicator:

$ref: '#/components/schemas/SourceIndicator'

path:

$ref: 'comDefs.yaml#/components/schemas/Uri'

operation:

$ref: '#/components/schemas/Operation'

value:

oneOf:

- $ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

- $ref: 'comDefs.yaml#/components/schemas/AttributeValueChangeSet'

NotifyMoiCreation:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

properties:

correlatedNotifications:

type: array

items:

$ref: '#/components/schemas/CorrelatedNotification'

additionalText:

type: string

sourceIndicator:

$ref: '#/components/schemas/SourceIndicator'

attributeList:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

NotifyMoiDeletion:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

properties:

correlatedNotifications:

type: array

items:

$ref: '#/components/schemas/CorrelatedNotification'

additionalText:

type: string

sourceIndicator:

$ref: '#/components/schemas/SourceIndicator'

attributeList:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

NotifyMoiAttributeValueChanges:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

properties:

correlatedNotifications:

type: array

items:

$ref: '#/components/schemas/CorrelatedNotification'

additionalText:

type: string

sourceIndicator:

$ref: '#/components/schemas/SourceIndicator'

attributeListValueChanges:

$ref: 'comDefs.yaml#/components/schemas/AttributeValueChangeSet'

required:

- attributeValueChange

NotifyMoiChanges:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

properties:

moiChanges:

type: array

items:

$ref: '#/components/schemas/MoiChange'

required:

- moiChanges

## A.1.2 Integration with ONAP VES

Detailed guidelines for integration of provisioning MnS notifications with ONAP VES are provided in Annex B.

# A.2 Generic fault supervision management service

### A.2.0 Introduction

Clause A.2.1 contains the OpenAPI definition of the generic fault supervision MnS which includes the fault supervision MnS operations and the fault supervision MnS notifications.

Clause A.2.2 provides indications regarding the content of the generic fault supervision MnS notifications when the consumer of these notifications supports the ONAP VES API. This content is sent as payload of VES events (see Annex B).

## A.2.1 OpenAPI document "faultMnS.yaml"

openapi: 3.0.1

info:

title: Fault Supervision MnS

version: 16.6.0

description: >-

OAS 3.0.1 definition of the Fault Supervision MnS

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.532; Generic management services

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.532/

servers:

- url: '{MnSRoot}/FaultSupervisionMnS/{MnSversion}'

variables:

MnSRoot:

description: See subclause 4.4.3 of TS 32.158

default: http://example.com/3GPPManagement

MnSversion:

description: Version number of the OpenAPI definition

default: XXX

paths:

/alarms:

get:

summary: Retrieve multiple alarms

description: >-

Retrieves the alarms identified by alarmAckState, baseObjectInstance

and filter.

parameters:

- name: alarmAckState

in: query

required: false

schema:

$ref: '#/components/schemas/AlarmAckState'

- name: baseObjectInstance

in: query

required: false

schema:

$ref: 'comDefs.yaml#/components/schemas/Dn'

- name: filter

in: query

required: false

schema:

$ref: 'comDefs.yaml#/components/schemas/Filter'

responses:

'200':

description: >-

Success case ("200 OK").

Returns the alarms identified in the request. The alarmId is the key

of the map.

content:

application/json:

schema:

type: object

additionalProperties:

type: object

allOf:

- type: object

properties:

lastNotificationHeader:

$ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- $ref: '#/components/schemas/AlarmRecord'

- type: object

properties:

comments:

$ref: '#/components/schemas/Comments'

default:

description: Response in case of error.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

patch:

summary: 'Clear, acknowledge or unacknowledge multiple alarms'

description: >-

Clears, acknowledges or unacknowledges multiple alarms using patch. Depending

on which action is to be performed, different merge patch documents need

to be used.

requestBody:

description: >-

Patch documents for acknowledging and unacknowledging, or clearing multiple

alarms. The keys in the map are the alarmIds to be patched.

content:

application/merge-patch+json:

schema:

oneOf:

- type: object

additionalProperties:

$ref: '#/components/schemas/MergePatchAcknowledgeAlarm'

- type: object

additionalProperties:

$ref: '#/components/schemas/MergePatchClearAlarm'

responses:

'204':

description: >-

Success case ("204 No content").

The response message body is empty.

default:

description: Response in case of error.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/FailedAlarm'

/alarms/alarmCount:

get:

summary: Get the alarm count per perceived severity

parameters:

- name: alarmAckState

in: query

required: false

schema:

$ref: '#/components/schemas/AlarmAckState'

- name: filter

in: query

required: false

schema:

type: string

responses:

'200':

description: >-

Success case ("200 OK").

The alarm count per perceived severity is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AlarmCount'

default:

description: Response in case of error. The error case needs rework.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

/alarms/{alarmId}:

patch:

summary: 'Clear, acknowledge or unacknowledge a single alarm'

description: >-

Clears, acknowledges or uncknowldeges a single alarm by patching the alarm

information. A conditional acknowledge request based on the perceived

severity is not supported.

parameters:

- name: alarmId

in: path

description: Identifies the alarm to be patched.

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

oneOf:

- $ref: '#/components/schemas/MergePatchAcknowledgeAlarm'

- $ref: '#/components/schemas/MergePatchClearAlarm'

responses:

'204':

description: >-

Success case (204 No content).

The response message body is absent.

default:

description: Response in case of error.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

/alarms/{alarmId}/comments:

post:

summary: Add a comment to a single alarm

description: >-

Adds a comment to an alarm identified by alarmId. The id of the new comment

is allocated by the producer.

parameters:

- name: alarmId

in: path

description: Identifies the alarm to which the comment shall be added.

required: true

schema:

type: string

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/Comment'

responses:

'201':

description: >-

Success case (201 Created).

The representation of the newly created comment resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/Comment'

headers:

Location:

description: URI of the newly created comment resource.

required: true

schema:

type: string

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

/subscriptions:

post:

summary: Create a subscription

description: >-

To create a subscription the representation of the subscription is

POSTed on the /subscriptions collection resource.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/Subscription'

responses:

'201':

description: >-

Success case ("201 Created").

The representation of the newly created subscription resource shall

be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/Subscription'

headers:

Location:

description: URI of the newly created subscription resource

required: true

schema:

type: string

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

callbacks:

notifyNewAlarm:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

oneOf:

- $ref: '#/components/schemas/NotifyNewAlarm'

- $ref: '#/components/schemas/NotifyNewSecAlarm'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyClearedAlarm:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyClearedAlarm'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyChangedAlarm:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyChangedAlarm'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyChangedAlarmGeneral:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

oneOf:

- $ref: '#/components/schemas/NotifyChangedAlarmGeneral'

- $ref: '#/components/schemas/NotifyChangedSecAlarmGeneral'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyCorrelatedNotificationChanged:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyCorrelatedNotificationChanged'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyAckStateChanged:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyAckStateChanged'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyComments:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyComments'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyPotentialFaultyAlarmList:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyPotentialFaultyAlarmList'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

notifyAlarmListRebuilt:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyAlarmListRebuilt'

responses:

'204':

description: >-

Success case ("204 No Content").

The notification is successfully delivered. The response message

body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

/subscriptions/{subscriptionId}:

delete:

summary: Delete a subscription

description: >-

The subscription is deleted by deleting the corresponding subscription

resource. The resource to be deleted is identified with the path

component of the URI.

parameters:

- name: subscriptionId

in: path

description: Identifies the subscription to be deleted.

required: true

schema:

type: string

responses:

'204':

description: >-

Success case ("204 No Content").

The subscription resource has been deleted. The response message body

is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

components:

schemas:

#---- Definition of AlarmRecord ----------------------------------------------------#

AlarmId:

type: string

AlarmType:

type: string

enum:

- COMMUNICATIONS\_ALARM

- QUALITY\_OF\_SERVICE\_ALARM

- PROCESSING\_ERROR\_ALARM

- EQUIPMENT\_ALARM

- ENVIRONMENTAL\_ALARM

- INTEGRITY\_VIOLATION

- OPERATIONAL\_VIOLATION

- PHYSICAL\_VIOLATION

- SECURITY\_SERVICE\_OR\_MECHANISM\_VIOLATION

- TIME\_DOMAIN\_VIOLATION

ProbableCause:

description: >-

The value of the probable cause may be a specific standardized string, or any

vendor provided string. Probable cause strings are not standardized in the

present document. They may be added in a future version. Up to then the

mapping of the generic probable cause strings "PROBABLE\_CAUSE\_001" to

"PROBABLE\_CAUSE\_005" is vendor specific.

The value of the probable cause may also be an integer. The mapping of integer

values to probable causes is vendor specific.

oneOf:

- anyOf:

- type: string

enum:

- PROBABLE\_CAUSE\_001

- PROBABLE\_CAUSE\_002

- PROBABLE\_CAUSE\_003

- PROBABLE\_CAUSE\_004

- PROBABLE\_CAUSE\_005

- type: string

- type: integer

SpecificProblem:

oneOf:

- type: string

- type: integer

PerceivedSeverity:

type: string

enum:

- INDETERMINATE

- CRITICAL

- MAJOR

- MINOR

- WARNING

- CLEARED

TrendIndication:

type: string

enum:

- MORE\_SEVERE

- NO\_CHANGE

- LESS\_SEVERE

ThresholdHysteresis:

type: object

required:

- high

properties:

high:

oneOf:

- type: integer

- $ref: 'comDefs.yaml#/components/schemas/Float'

low:

$ref: 'comDefs.yaml#/components/schemas/Float'

ThresholdLevelInd:

oneOf:

- type: object

properties:

up:

$ref: '#/components/schemas/ThresholdHysteresis'

- type: object

properties:

down:

$ref: '#/components/schemas/ThresholdHysteresis'

ThresholdInfo:

type: object

properties:

observedMeasurement:

type: string

observedValue:

oneOf:

- type: integer

- $ref: 'comDefs.yaml#/components/schemas/Float'

thresholdLevel:

$ref: '#/components/schemas/ThresholdLevelInd'

armTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

required:

- observedMeasurement

- observedValue

CorrelatedNotification:

type: object

properties:

sourceObjectInstance:

$ref: 'comDefs.yaml#/components/schemas/Dn'

notificationIds:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/NotificationId'

required:

- source

- notificationId

CorrelatedNotifications:

type: array

items:

$ref: '#/components/schemas/CorrelatedNotification'

AckState:

type: string

enum:

- ACKNOWLEDGED

- UNACKNOWLEDGED

AlarmRecord:

description: >-

The alarmId is not a property of an alarm record. It is used as key

in the map of alarm records instead.

type: object

properties:

# alarmId:

# $ref: '#/components/schemas/AlarmId'

objectInstance:

$ref: 'comDefs.yaml#/components/schemas/Dn'

notificationId:

$ref: 'comDefs.yaml#/components/schemas/NotificationId'

alarmRaisedTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

alarmChangedTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

alarmClearedTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

specificProblem:

$ref: '#/components/schemas/SpecificProblem'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

backedUpStatus:

type: boolean

backUpObject:

$ref: 'comDefs.yaml#/components/schemas/Dn'

trendIndication:

$ref: '#/components/schemas/TrendIndication'

thresholdinfo:

$ref: '#/components/schemas/ThresholdInfo'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

stateChangeDefinition:

$ref: 'comDefs.yaml#/components/schemas/AttributeValueChangeSet'

monitoredAttributes:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

proposedRepairActions:

type: string

additionalText:

type: string

additionalInformation:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

rootCauseIndicator:

type: boolean

ackTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

ackUserId:

type: string

ackSystemId:

type: string

ackState:

$ref: '#/components/schemas/AckState'

clearUserId:

type: string

clearSystemId:

type: string

serviceUser:

type: string

serviceProvider:

type: string

securityAlarmDetector:

type: string

#---- Definition of alarm notifications --------------------------------------------#

AlarmNotificationTypes:

type: string

enum:

- notifyNewAlarm

- notifyChangedAlarm

- notifyChangedAlarmGeneral

- notifyAckStateChanged

- notifyCorrelatedNotificationChanged

- notifyComments

- notifyClearedAlarm

- notifyAlarmListRebuiltAlarm

- notifyPotentialFaultyAlarmList

AlarmListAlignmentRequirement:

type: string

enum:

- ALIGNMENT\_REQUIRED

- ALIGNMENT\_NOT\_REQUIRED

NotifyNewAlarm:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- probableCause

- perceivedSeverity

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

specificProblem:

$ref: '#/components/schemas/SpecificProblem'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

backedUpStatus:

type: boolean

backUpObject:

$ref: 'comDefs.yaml#/components/schemas/Dn'

trendIndication:

$ref: '#/components/schemas/TrendIndication'

thresholdInfo:

$ref: '#/components/schemas/ThresholdInfo'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

stateChangeDefinition:

$ref: 'comDefs.yaml#/components/schemas/AttributeValueChangeSet'

monitoredAttributes:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

proposedRepairActions:

type: string

additionalText:

type: string

additionalInformation:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

rootCauseIndicator:

type: boolean

NotifyNewSecAlarm:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- probableCause

- perceivedSeverity

- serviceUser

- serviceProvider

- securityAlarmDetector

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

additionalText:

type: string

additionalInformation:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

rootCauseIndicator:

type: boolean

serviceUser:

type: string

serviceProvider:

type: string

securityAlarmDetector:

type: string

NotifyClearedAlarm:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- probableCause

- perceivedSeverity

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

clearUserId:

type: string

clearSystemId:

type: string

NotifyChangedAlarm:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- probableCause

- perceivedSeverity

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

NotifyChangedAlarmGeneral:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

specificProblem:

$ref: '#/components/schemas/SpecificProblem'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

backedUpStatus:

type: boolean

backUpObject:

$ref: 'comDefs.yaml#/components/schemas/Dn'

trendIndication:

$ref: '#/components/schemas/TrendIndication'

thresholdInfo:

$ref: '#/components/schemas/ThresholdInfo'

stateChangeDefinition:

$ref: 'comDefs.yaml#/components/schemas/AttributeValueChangeSet'

monitoredAttributes:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

proposedRepairActions:

type: string

additionalText:

type: string

additionalInformation:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

rootCauseIndicator:

type: boolean

changedAlarmAttributes:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

NotifyChangedSecAlarmGeneral:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- serviceUser

- serviceProvider

- securityAlarmDetector

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

additionalText:

type: string

additionalInformation:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

rootCauseIndicator:

type: boolean

serviceUser:

type: string

serviceProvider:

type: string

securityAlarmDetector:

type: string

changedAlarmAttributes:

$ref: 'comDefs.yaml#/components/schemas/AttributeNameValuePairSet'

NotifyCorrelatedNotificationChanged:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- correlatedNotifications

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

correlatedNotifications:

$ref: '#/components/schemas/CorrelatedNotifications'

rootCauseIndicator:

type: boolean

NotifyAckStateChanged:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- probableCause

- perceivedSeverity

- ackState

- ackUserId

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

ackState:

$ref: '#/components/schemas/AckState'

ackUserId:

type: string

ackSystemId:

type: string

NotifyComments:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- alarmId

- alarmType

- probableCause

- perceivedSeverity

- comments

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

alarmType:

$ref: '#/components/schemas/AlarmType'

probableCause:

$ref: '#/components/schemas/ProbableCause'

perceivedSeverity:

$ref: '#/components/schemas/PerceivedSeverity'

comments:

$ref: '#/components/schemas/Comments'

NotifyPotentialFaultyAlarmList:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- reason

properties:

reason:

type: string

NotifyAlarmListRebuilt:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

required:

- reason

properties:

reason:

type: string

alarmListAlignmentRequirement:

$ref: '#/components/schemas/AlarmListAlignmentRequirement'

#---- Definition of query parameters -----------------------------------------------#

AlarmAckState:

type: string

enum:

- ALL\_ALARMS

- ALL\_ACTIVE\_ALARMS

- ALL\_ACTIVE\_AND\_ACKNOWLEDGED\_ALARMS

- ALL\_ACTIVE\_AND\_UNACKNOWLEDGED\_ALARMS

- ALL\_CLEARED\_AND\_UNACKNOWLEDGED\_ALARMS

- ALL\_UNACKNOWLEDGED\_ALARMS

#---- Definition of patch documents ------------------------------------------------#

MergePatchAcknowledgeAlarm:

description: >-

Patch document acknowledging or unacknowledging a single alarm. For

acknowleding an alarm the value of ackState is ACKNOWLEDGED, for unacknowleding

an alarm the value of ackState is UNACKNOWLEDGED.

type: object

required:

- ackUserId

- ackState

properties:

ackUserId:

type: string

ackSystemId:

type: string

ackState:

$ref: '#/components/schemas/AckState'

MergePatchClearAlarm:

description: Patch document for clearing a single alarm

type: object

required:

- clearUserId

- perceivedSeverity

properties:

clearUserId:

type: string

clearSystemId:

type: string

perceivedSeverity:

type: string

enum:

- CLEARED

#---- Definition of method responses -----------------------------------------------#

FailedAlarm:

type: object

required:

- alarmId

- failureReason

properties:

alarmId:

$ref: '#/components/schemas/AlarmId'

failureReason:

type: string

#---- Definition of resources ------------------------------------------------------#

AlarmCount:

type: object

required:

- criticalCount

- majorCount

- minorCount

- warningCount

- indeterminateCount

- clearedCount

properties:

criticalCount:

type: integer

majorCount:

type: integer

minorCount:

type: integer

warningCount:

type: integer

indeterminateCount:

type: integer

clearedCount:

type: integer

Comment:

type: object

properties:

commentTime:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

commentUserId:

type: string

commentSystemId:

type: string

commentText:

type: string

Comments:

description: >-

Collection of comments. The comment identifiers are allocated by the

MnS producer and used as key in the map.

type: object

additionalProperties:

$ref: '#/components/schemas/Comment'

Subscription:

type: object

properties:

consumerReference:

$ref: 'comDefs.yaml#/components/schemas/Uri'

timeTick:

type: integer

filter:

$ref: 'comDefs.yaml#/components/schemas/Filter'

## A.2.2 Integration with ONAP VES

Detailed guidelines for integration of fault supervision MnS notifications with ONAP VES are provided in Annex B.

# A.3 Void

# A.4 Generic performance assurance management service

## A.4.1 Void

## A.4.2 OpenAPI document "perfMnS.yaml"

openapi: 3.0.1

info:

title: TS 28.532 Performance Threshold Monitoring MnS

version: 16.6.0

description: >-

OAS 3.0.1 definition of the Performance Threshold Monitoring MnS

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.532 V16.6.0; Generic management services

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.532/

servers:

- url: '{root}'

variables:

root:

description: >-

The open API server of the performance threshold monitoring service is

located in the consumer side, see monitoringNotifTarget attribute of

the IOC ThresholdMonitor defined in 3GPP TS 28.622 [11].

default: http://example.com/3GPPManagement

paths:

/notificationSink:

post:

summary: Send notifications about performance threshold crossing

description: To send a notifyThresholdCrossing notification

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NotifyThresholdCrossing'

responses:

'204':

description: >-

Success case ("204 No Content"). The notification is successfully

delivered. The response message body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: 'comDefs.yaml#/components/schemas/ErrorResponse'

components:

schemas:

PerfNotificationTypes:

type: string

enum:

- notifyThresholdCrossing

PerfMetricValue:

oneOf:

- type: integer

- $ref: 'comDefs.yaml#/components/schemas/Float'

PerfMetricDirection:

type: string

enum:

- UP

- DOWN

NotifyThresholdCrossing:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

properties:

observedPerfMetricName:

type: string

observedPerfMetricValue:

$ref: '#/components/schemas/PerfMetricValue'

observedPerfMetricDirection:

$ref: '#/components/schemas/PerfMetricDirection'

thresholdValue:

$ref: '#/components/schemas/PerfMetricValue'

hysteresis:

$ref: '#/components/schemas/PerfMetricValue'

monitorGranularityPeriod:

type: integer

additionalText:

type: string

## A.4.3 Integration with ONAP VES

Detailed guidelines for integration of performance assurance MnS notifications with ONAP VES are provided in Annex B.

# A.5 Heartbeat

### A.5.0 Introduction

Clause A.5.1 contains the OpenAPI definition of the heartbeat management capability.

Clause A.5.2 provides indications regarding the content of the heartbeat management capability notifications when the consumer of these notifications supports the ONAP VES API. This content is sent as payload of VES events (see Annex B).

## A.5.1 OpenAPI document "heartbeatNtf.yaml"

openapi: 3.0.1

info:

title: Heartbeat notification

version: 16.6.0

description: >-

OAS 3.0.1 definition of the heartbeat notification

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.532 V16.6.0; Generic management services

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.6532/

paths: {}

components:

schemas:

HeartbeatNotificationTypes:

type: string

enum:

- notifyHeartbeat

NotifyHeartbeat:

allOf:

- $ref: 'comDefs.yaml#/components/schemas/NotificationHeader'

- type: object

properties:

heartbeatNtfPeriod:

type: integer

## A.5.2 Integration with ONAP VES

NOTE: Void.

Detailed guidelines for integration of heartbeat notifications with ONAP VES are provided in Annex B.

# A.6 Streaming data reporting management service

## A.6.1 Introduction

Clause A.6.2 contains the OpenAPI specification of the Streaming data reporting MnS.

## A.6.2 OpenAPI document "streamingDataMnS.yaml"

openapi: 3.0.1

info:

title: TS 28.532 Streaming data reporting service

version: 16.6.0

description: OAS 3.0.1 specification for the Streaming data reporting service (Streaming MnS)

servers:

- url: '{MnSRoot}/StreamingDataReportingMnS/{version}'

variables:

MnSRoot:

description: See subclause 4.4 of TS 32.158.

default: https://example.com/3GPPManagement

version:

description: Indicates the current version of the specification

default: 16.5.0

paths:

'/connections':

post:

summary: Inform consumer about reporting streams to be carried by the new connection and receive a new connection id.

description: Exchange of meta-data (producer informs consumer about its own identity and the nature of the data to be reported via streaming) phase of the connection establishement by streaming data reporting producer to the streaming data reporting consumer (i.e. streaming target).

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/connectionRequest-Type'

responses:

'201':

description: Success case (201 Created).

headers:

Location:

description: Location of the created connection resource.

schema:

$ref: '#/components/schemas/connectionId-Type'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/failedConnectionResponse-Type'

get:

summary: Obtain information about connections.

description: Enables the streaming data reporting service producer to obtain information about one or more streaming connections.

parameters:

- name: connectionIdList

in: query

description: The list of connectionId for which the connection information is to be returned.

required: false

schema:

type: array

items:

$ref: '#/components/schemas/connectionId-Type'

responses:

'200':

description: Success case (200 OK). The resources identified in the request for retrieval are returned in the response message body. In case the fields query parameter is used, the selected resources are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/connectionInfo-Type'

'202':

description: Partial success case (202 Partially retrieved). Subset of the resources identified in the request for retrieval are returned in the response message body.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/connectionInfo-Type'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/errorResponse-Type'

'/connections/{connectionId}':

get:

summary: Obtain information about a connection.

description: Enables the streaming data reporting service producer to obtain information about one streaming connection.

parameters:

- name: connectionId

in: path

description: Indicate the ID (URI) of the connection for which the information is being retrieved

required: true

schema:

$ref: '#/components/schemas/connectionId-Type'

- name: Connection

in: header

schema:

$ref: '#/components/schemas/websocketHeaderConnection-Type'

- name: Sec-WebSocket-Extensions

in: header

schema:

$ref: '#/components/schemas/websocketHeader-Sec-WebSocket-Extensions-Type'

- name: Sec-WebSocket-Key

in: header

schema:

$ref: '#/components/schemas/websocketHeader-Sec-WebSocket-Key-Type'

- name: Sec-WebSocket-Protocol

in: header

schema:

$ref: '#/components/schemas/websocketHeader-Sec-WebSocket-Protocol-Type'

- name: Sec-WebSocket-Version

in: header

schema:

$ref: '#/components/schemas/websocketHeader-Sec-WebSocket-Version-Type'

responses:

'101':

description: Success case (101 Switching Protocols). The connection has been successfully switched to WebSocket. The response message body is absent.

headers:

Upgrade:

schema:

$ref: '#/components/schemas/websocketHeaderUpgrade-Type'

Connection:

schema:

$ref: '#/components/schemas/websocketHeaderConnection-Type'

Sec-WebSocket-Accept:

schema:

$ref: '#/components/schemas/websocketHeader-Sec-WebSocket-Accept-Type'

'200':

description: Success case (200 OK). The resource identified in the request for retrieval returned in the response message body.

content:

application/json:

schema:

$ref: '#/components/schemas/connectionInfo-Type'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/errorResponse-Type'

'/connections/{connectionId}/streams':

post:

summary: Inform consumer about new reporting streams on an existing connection.

description: Allows the producer to add one or more reporting streams to an already established streaming connection.

parameters:

- name: connectionId

in: path

description: Indicate the ID (URI) of the connection for which the reporting stream information is being added.

required: true

schema:

$ref: '#/components/schemas/connectionId-Type'

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/streamInfo-Type'

responses:

'201':

description: Success case (201 Posted).

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/streamInfo-Type'

'202':

description: Partial success case (202 Posted).

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/streamInfo-Type'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/errorResponse-Type'

delete:

summary: Remove reporting streams from an existing connection

description: Allows the producer to remove one or more reporting streams from an already established streaming connection.

parameters:

- name: connectionId

in: path

description: Indicate the ID (URI) of the connection for which the reporting stream information is being removed.

required: true

schema:

$ref: '#/components/schemas/connectionId-Type'

- name: streamIds

in: query

description: The list of streamId for the stream(s) to be deleted.

required: true

schema:

type: array

items:

$ref: '#/components/schemas/streamId-Type'

responses:

'204':

description: Success case (204 No Content). The stream information resource has been deleted. The response message body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/errorResponse-Type'

get:

summary: Obtain information about streams.

description: Enables the streaming data reporting service producer to obtain information about one or more reporting streams.

parameters:

- name: connectionId

in: path

description: Indicate the ID (URI) of the connection for which the information is being retrieved

required: true

schema:

$ref: '#/components/schemas/connectionId-Type'

- name: streamIds

in: query

description: The list of streamId for which the stream information is to be retrieved.

required: true

schema:

type: array

items:

$ref: '#/components/schemas/streamId-Type'

responses:

'200':

description: Success case (200 OK).

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/streamInfoWithReporters-Type'

'202':

description: Partial success case (202 Partially retrieved).

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/streamInfoWithReporters-Type'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/errorResponse-Type'

'/connections/{connectionId}/streams/{streamId}':

get:

summary: Obtain information about stream

description: Enables the streaming data reporting service producer to obtain information about a reporting stream.

parameters:

- name: connectionId

in: path

description: Indicate the ID (URI) of the connection for which the information is being retrieved

required: true

schema:

$ref: '#/components/schemas/connectionId-Type'

- name: streamId

in: path

description: Indicate the ID of the reporting stream for which the information is being retrieved

required: true

schema:

$ref: '#/components/schemas/streamId-Type'

responses:

'200':

description: Success case (200 OK).

content:

application/json:

schema:

$ref: '#/components/schemas/streamInfoWithReporters-Type'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/errorResponse-Type'

components:

schemas:

analyticsInfo-Type:

description: Information specific to analytics reporting.

type: object

properties:

activityDetails:

type: string

connectionId-Type:

$ref: '#/components/schemas/uri-Type'

connectionInfo-Type:

type: object

properties:

connection:

$ref: '#/components/schemas/connectionId-Type'

producer:

$ref: '#/components/schemas/producerId-Type'

streams:

type: array

items:

$ref: '#/components/schemas/streamId-Type'

connectionRequest-Type:

type: object

properties:

producer:

$ref: '#/components/schemas/producerId-Type'

streams:

type: array

items:

$ref: '#/components/schemas/streamInfo-Type'

errorResponse-Type:

type: object

properties:

error:

type: object

properties:

errorInfo:

type: string

failedConnectionResponse-Type:

type: object

properties:

error:

type: array

items:

type: object

properties:

streamId:

$ref: '#/components/schemas/streamId-Type'

errorReason:

type: string

measObjDn-Type:

description: DN of the measured object instance (see 3GPP TS 28.550)

allOf:

- $ref: '#/components/schemas/systemDN-Type'

performanceMetrics-Type:

description: an ordered list of performance metric names (see clause 4.4.1 of 3GPP TS 28.622[11]) whose values are to be reported by the Performance Data Stream Units (see Annex C of TS 28.550 [42]) via this stream. Performance metrics include measurement and KPI

type: array

items:

type: string

performanceInfo-Type:

description: Information specific to performance data reporting

type: object

properties:

measObjDn:

$ref: '#/components/schemas/measObjDn-Type'

performanceMetrics:

$ref: '#/components/schemas/performanceMetrics-Type'

jobId:

type: string

required:

- measObjDn

- performanceMetrics

producerId-Type:

description: DN of the streaming data reporting MnS producer.

allOf:

- $ref: '#/components/schemas/systemDN-Type'

serializationFormat-Type:

type: string

enum:

- GPB

- ASN1

streamId-Type:

description: globally unique stream identifier

type: string

example: '26F452550021'

streamInfo-Type:

description: Reporting stream meta-data.

type: object

properties:

streamType:

$ref: '#/components/schemas/streamType-Type'

serializationFormat:

$ref: '#/components/schemas/serializationFormat-Type'

streamId:

oneOf:

- $ref: '#/components/schemas/streamId-Type'

- $ref: '#/components/schemas/traceReference-Type'

additionalInfo:

oneOf:

- $ref: '#/components/schemas/traceInfo-Type'

- $ref: '#/components/schemas/performanceInfo-Type'

- $ref: '#/components/schemas/analyticsInfo-Type'

- $ref: '#/components/schemas/vsDataContainer-Type'

required:

- streamType

- serializationFormat

- streamId

streamInfoWithReporters-Type:

description: Reporting stream meta-data with added information about reporters.

type: object

properties:

streamInfo:

$ref: '#/components/schemas/streamInfo-Type'

reporters:

type: array

items:

$ref: '#/components/schemas/producerId-Type'

systemDN-Type:

description: See 3GPP TS 32.300 for details

type: string

example: 'SubNetwork=ABCNetwork,SubNetwork=MUC01,GNBDUFunction=XYZ0100'

streamType-Type:

type: string

enum:

- TRACE

- PERFORMANCE

- ANALYTICS

- PROPRIETARY

traceInfo-Type:

description: Information specific to trace data reporting

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/TraceJob-Attr'

traceReference-Type:

description: Trace Reference (see clause 5.6 of 3GPP TS 32.422) as stream identifier for streaming trace data reporting

type: string

example: '4358070034D7'

uri-Type:

description: Resource URI

type: string

vsDataContainer-Type:

description: container for vendor specific data (see 3GPP TS 28.622)

type: object

properties:

vsDataType:

type: string

vsData:

type: string

vsDataFormatVersion:

type: string

websocketHeaderConnection-Type:

description: Header value for the upgrade request and response.

type: string

enum:

- Upgrade

websocketHeaderUpgrade-Type:

description: Header value for the upgrade to WebSocket request and response.

type: string

enum:

- websocket

websocketHeader-Sec-WebSocket-Accept-Type:

description: Header value for secure WebSocket response. Carries hash.

type: string

websocketHeader-Sec-WebSocket-Extensions-Type:

description: Header value for secure WebSocket request. Carries protocol extensions.

type: string

websocketHeader-Sec-WebSocket-Key-Type:

description: Header value for secure WebSocket request. Provides information to the server which is needed in order to confirm that the client is entitled to request an upgrade to WebSocket.

type: string

websocketHeader-Sec-WebSocket-Protocol-Type:

description: Header value for secure WebSocket request. Carries a comma-separated list of subprotocol names, in the order of preference.

type: string

websocketHeader-Sec-WebSocket-Version-Type:

description: Header value for secure WebSocket request and response. Carries the WebSocket protocol version to be used.

type: string

# A.7 File data reporting management service

## A.7.1 Introduction

Clause A.7.2 contains the OpenAPI specification of the File data reporting MnS.

Clause A.7.3 provides indications regarding the content of the File data reporting MnS notifications when the consumer of these notifications supports the ONAP VES API. This content is sent as payload of VES events (see Annex B).

## A.7.2 OpenAPI document "FileDataReportingMnS.yaml"

openapi: 3.0.1

info:

title: TS 28.532 File data reporting Service

version: 16.6.0

description: >-

OAS 3.0.1 specification of the File data reporting Management Service © 2020,

3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC). All

rights reserved.

externalDocs:

description: 3GPP TS 28.532 V16.5.0; Generic management services

url: 'http://www.3gpp.org/ftp/Specs/archive/28\_series/28.532/'

servers:

- url: '{MnSRoot}/FileDataReportingMnS/{MnSversion}'

variables:

MnSRoot:

description: See subclause 4.4 of TS 32.158

default: http://example.com/3GPPManagement

version:

description: Indicates the current version of the specification

default: 16.5.0

paths:

/Files:

get:

summary: Read resources of information of available files

description: With HTTP GET, resources of information of available files are read. The resources to be read are identified with the path component (base resource) and the query component (fileaType, beginTime and endTime) of the URI. The fields query component allows to select the resource properties to be returned.

parameters:

- name: fileType

in: query

description: This parameter identifies the type of management data that the file contains to select the resources from the collection resources identified with the path component of the URI.

required: true

schema:

$ref: '#/components/schemas/fileType-Type'

- name: beginTime

in: query

description: This parameter identifies the time stamp no later than which the file became available to select the resources from the collection resources identified with the path component of the URI.

required: true

schema:

$ref: '#/components/schemas/dateTime-Type'

- name: endTime

in: query

description: This parameter identifies the time stamp no earlier than which the file became available to select the resources from the collection resources identified with the path component of the URI.

required: true

schema:

$ref: '#/components/schemas/dateTime-Type'

responses:

'200':

description: 'Success case ("200 OK"). The resources identified in the request for retrieval are returned in the response message body. In case the fields query parameter is used, the selected resources are returned.'

content:

application/json:

schema:

$ref: '#/components/schemas/fileInfoRetrieval-ResponseType'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/error-ResponseType'

/subscriptions:

post:

summary: Create a subscription

description: To create a subscription the representation of the subscription is POSTed on the /subscriptions collection resource.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/subscription-RequestType'

responses:

'201':

description: Success case ("201 Created"). The representation of the newly created subscription resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/subscription-ResponseType'

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/error-ResponseType'

callbacks:

notifyFileReady:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/notifyFileReady-NotifType'

responses:

'204':

description: Success case ("204 No Content"). The notification is successfully delivered. The response message body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/error-ResponseType'

notifyFilePreparationError:

'{request.body#/consumerReference}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/notifyFilePreparationError-NotifType'

responses:

'204':

description: Success case ("204 No Content"). The notification is successfully delivered. The response message body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/error-ResponseType'

delete:

summary: Delete all subscriptions made with a specific consumerReferenceId

description: The subscriptions are deleted by deleting the corresponding subscription resources. The resources to be deleted are identified with the path component of the URI pointing to the /subscription collection resource and filtering on the consumerReferenceId provided in the query part.

parameters:

- name: consumerReferenceId

in: query

description: Identifies the subscriptions to be deleted.

required: true

schema:

$ref: '#/components/schemas/consumerReferenceId-QueryType'

responses:

'204':

description: Success case ("204 No Content"). The subscription resources have been deleted. The response message body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/error-ResponseType'

'/subscriptions/{subscriptionId}':

delete:

summary: Delete a single subscription

description: The subscription is deleted by deleting the corresponding subscription resource. The resource to be deleted is identified with the path component of the URI.

parameters:

- name: subscriptionId

in: path

description: Identifies the subscription to be deleted.

required: true

schema:

$ref: '#/components/schemas/subscriptionId-PathType'

responses:

'204':

description: Success case ("204 No Content"). The subscription resource has been deleted. The response message body is absent.

default:

description: Error case.

content:

application/json:

schema:

$ref: '#/components/schemas/error-ResponseType'

components:

schemas:

dateTime-Type:

type: string

format: date-Time

uri-Type:

type: string

long-Type:

type: string

format: long

additionalText-Type:

type: string

reason-Type:

type: string

fileInfoRetrieval-ResponseType:

type: object

properties:

data:

type: array

items:

$ref: '#/components/schemas/fileInfo-Type'

fileInfo-Type:

type: object

properties:

fileLocation:

$ref: '#/components/schemas/uri-Type'

fileSize:

$ref: '#/components/schemas/long-Type'

fileReadyTime:

$ref: '#/components/schemas/dateTime-Type'

fileExpirationTime:

$ref: '#/components/schemas/dateTime-Type'

fileCompression:

type: string

fileFormat:

type: string

fileType:

$ref: '#/components/schemas/fileType-Type'

error-ResponseType:

type: object

properties:

error:

type: object

properties:

errorInfo:

type: string

fileType-Type:

type: string

enum:

- PERFORMANCE

- TRACE

- ANALYTICS

- PROPRIETARY

header-Type:

description: Header used in notifications as notification header

type: object

properties:

uri:

$ref: '#/components/schemas/uri-Type'

notificationId:

$ref: '#/components/schemas/notificationId-Type'

notificationType:

$ref: '#/components/schemas/notificationType-Type'

eventTime:

$ref: '#/components/schemas/dateTime-Type'

subscriptionId-PathType:

type: string

filter-Type:

type: string

notificationId-Type:

$ref: '#/components/schemas/long-Type'

notificationType-Type:

type: string

enum:

- notifyFileReady

- notifyFilePreparationError

subscription-ResourceType:

type: object

properties:

consumerReference:

$ref: '#/components/schemas/uri-Type'

timeTick:

$ref: '#/components/schemas/long-Type'

filter:

$ref: '#/components/schemas/filter-Type'

subscription-RequestType:

type: object

properties:

data:

$ref: '#/components/schemas/subscription-ResourceType'

subscription-ResponseType:

type: object

properties:

data:

$ref: '#/components/schemas/subscription-ResourceType'

consumerReferenceId-QueryType:

$ref: '#/components/schemas/uri-Type'

notifyFileReady-NotifType:

type: object

properties:

header:

$ref: '#/components/schemas/header-Type'

body:

type: object

properties:

fileInfoList:

type: array

items:

$ref: '#/components/schemas/fileInfo-Type'

additionalText:

$ref: '#/components/schemas/additionalText-Type'

notifyFilePreparationError-NotifType:

type: object

properties:

header:

$ref: '#/components/schemas/header-Type'

body:

type: object

properties:

fileInfoList:

type: array

items:

$ref: '#/components/schemas/fileInfo-Type'

reason:

$ref: '#/components/schemas/reason-Type'

additionalText:

$ref: '#/components/schemas/additionalText-Type'

## A.7.3 Integration with ONAP VES

Detailed guidelines for integration of file data reporting MnS notifications with ONAP VES are provided in Annex B.

Annex B (Informative):  
Guidelines for the integration of 3GPP MnS notifications with ONAP VES

In case the consumer of the 3GPP MnS notifications specified in the present document is an ONAP VES collector, the following guidelines are for the developer of the corresponding notification producer:

- The produced notification conforms to ONAP-defined VES specification;

- The VES Common Event Header fields are populated by the producer is as follows:

- The domain "stndDefined" is used,

- The "stndDefinedNamespace" field value is the concatenation of "3GPP-" and the name of the 3GPP MnS which the 3GPP IS notification is part of. Based on the MnS names defined in the present version of this document, VES name space values corresponding to 3GPP MnS could be:

- "3GPP-Provisioning",

- "3GPP-FaultSupervision",

- "3GPP-PerformanceAssurance",

- "3GPP-Heartbeat",

- "3GPP-DataStreamingReporting",

- "3GPP-DataFileReporting".

- How the other fields of the Common Event Header are populated is not in the scope of the present document;

- The payload part of the VES event specification conforms to the OpenAPI definitions of clause A.1.1 (for provisioning MnS notifications), A.2.1 (for the fault supervision MnS notifications), A4.2 (for the performance assurance MnS notifications), A.5.1 (for the heartbeat notifications) and A.7.2 (for the file data reporting MnS notifications) of the present document. The OpenAPI definitions of Annex A in the present document may also be found on 3GPP FORGE ([see](C:\\SA#90e\\SA5\\CRs\\specs\\see) [46]).




Figure X-1. 3GPP MnS notifications consumed by ONAP VES Collector(s).

Annex C (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-09 | SA#81 |  |  |  |  | Upgrade to change control version | 15.0.0 |
| 2018-09 | SA#81 |  |  |  |  | EditHelp editorial fix | 15.0.1 |
| 2018-12 | SA#82 | SP-181042 | 0002 | 1 | F | Correction of references | 15.1.0 |
| 2018-12 | SA#82 | SP-181042 | 0003 | 1 | F | Align with 3GPP draft rules of the usage of must | 15.1.0 |
| 2018-12 | SA#82 | SP-181042 | 0004 | 1 | F | Correction of the numbering and title of figures and tables | 15.1.0 |
| 2018-12 | SA#82 | SP-181042 | 0005 | 1 | F | Remove unnecessary Editor’s Note and figure | 15.1.0 |
| 2018-12 | SA#82 | SP-181045 | 0006 | 1 | F | Update Resource URI of alarmCount | 15.1.0 |
| 2018-12 | SA#82 | SP-181045 | 0009 | 1 | F | Change the name of IRPAgent and IRPManager | 15.1.0 |
| 2018-12 | SA#82 | SP-181045 | 0010 | 1 | F | Remove unnecessary import table and state diagram | 15.1.0 |
| 2018-12 | SA#82 | SP-181045 | 0012 | - | F | Correct the subscription resource related errors | 15.1.0 |
| 2018-12 | SA#82 | SP-181043 | 0018 | - | F | Add notifyNewSecurityAlarm to notification type | 15.1.0 |
| 2018-12 | SA#82 | SP-181045 | 0020 | 1 | F | Change alarmIRP to FaultSupervision MnS producer | 15.1.0 |
| 2018-12 | SA#82 | SP-181042 | 0021 | 1 | F | Add stage 2 definition for provisioning management service related notifications | 15.1.0 |
| 2018-12 | SA#82 | SP-181042 | 0022 | 1 | F | Correct stage 3 description of the Provisioning Management Service | 15.1.0 |
| 2018-12 | SA#82 | SP-181045 | 0025 | - | F | Correct erroneous reference to notification header | 15.1.0 |
| 2019-03 | SA#83 | SP-190120 | 0029 | 1 | F | Correction of references | 15.2.0 |
| 2019-06 | SA#84 | SP-190372 | 0031 | 2 | B | Add RESTful HTTP-based solution set of fault supervision for integration with ONAP VES | 16.0.0 |
| 2019-06 | SA#84 | SP-190371 | 0038 | 1 | B | Add performance threshold crossing notification | 16.0.0 |
| 2019-09 | SA#85 | SP-190742 | 0038A |  |  | Global reorganization, correcting operation names, notification parameter and wrong references | 16.1.0 |
| 2019-12 | SA#86 | SP-191178 | 0055 | 1 | B | RESTful CM notifications for integration with ONAP VES | 16.2.0 |
| 2019-12 | SA#86 | SP-191219 | 0059 | 1 | A | Corrections to provisioning MnS notification definitions (Stage 2) | 16.2.0 |
| 2019-12 | SA#86 | SP-191219 | 0061 | 2 | A | Correct fault supervision management service | 16.2.0 |
| 2019-12 | SA#86 | SP-191159 | 0069 | 2 | C | Make scoping and filtering optional in the ProvMnS | 16.2.0 |
| 2019-12 | SA#86 | SP-191159 | 0071 | 2 | F | Correct and update the RESTful HTTP-based solution set of provisioning | 16.2.0 |
| 2019-12 | SA#86 | SP-191178 | 0073 | 2 | B | Introduce Heartbeat | 16.2.0 |
| 2019-12 | SA#86 | SP-191173 | 0075 | 1 | A | Correct event time defn | 16.2.0 |
| 2019-12 | SA#86 | SP-191166 | 0076 | 1 | B | Add notifyEvent | 16.2.0 |
| 2019-12 | SA#86 | SP-191159 | 0081 | 1 | F | Correct schema to reflect location in the specifications | 16.2.0 |
| 2019-12 | SA#86 | SP-191159 | 0082 | - | F | Correct XML Schema for consistency and clarity | 16.2.0 |
| 2020-03 | SA#87E | SP-200174 | 0089 | - | A | Add missing definition for matching-criteria-attributes | 16.3.0 |
| 2020-03 | SA#87E | SP-200166 | 0092 | 1 | F | Clarify capability of ack alarms and filter constraint | 16.3.0 |
| 2020-03 | SA#87E | SP-200176 | 0094 | 1 | F | Correction of MnS Stage 3 solution sets for integration with ONAP VES | 16.3.0 |
| 2020-03 | SA#87E | SP-200166 | 0096 | - | F | Rapporteur clean up | 16.3.0 |
| 2020-03 | SA#87E | SP-200169 | 0098 | 1 | B | YANG\_Netconf Operations | 16.3.0 |
| 2020-03 | SA#87E | SP-200166 | 0101 | 1 | F | Clarify and add numerous issues in the REST SS of the ProvMnS | 16.3.0 |
| 2020-03 | SA#87E | SP-200166 | 0103 | 2 | F | Correct OpenAPI definition of the ProvMnS | 16.3.0 |
| 2020-03 | SA#87E | SP-200174 | 0104 | - | A | Correct ackState attribute name | 16.3.0 |
| 2020-03 | SA#87E | SP-200169 | 0105 | - | F | Correct Heartbeat | 16.3.0 |
| 2020-06 | SA#88-e | SP-200484 | 0100 | 2 | B | Add summary CM notification to the ProvMnS | 16.4.0 |
| 2020-06 | SA#88-e | SP-200484 | 0102 | 1 | F | Remove subscribe and unsubscribe operation from ProvMnS | 16.4.0 |
| 2020-06 | SA#88-e | SP-200484 | 0107 | 1 | F | Void meaningless clauses 12.1.2.2.1.2 and 12.2.2.2.1.2 | 16.4.0 |
| 2020-06 | SA#88-e | SP-200484 | 0111 | - | F | Add missing callbacks for notifications to ProvMnS | 16.4.0 |
| 2020-06 | SA#88-e | SP-200484 | 0113 | - | F | Remove attribute referenceObjectInstance which is not supported by solution set | 16.4.0 |
| 2020-06 | SA#88-e | SP-200485 | 0114 | 2 | F | Update URI for generic fault supervision management service | 16.4.0 |
| 2020-06 | SA#88-e | SP-200485 | 0115 | 2 | F | Update URI for performance data file reporting management service | 16.4.0 |
| 2020-06 | SA#88-e | SP-200484 | 0116 | - | F | Remove data object from response types in the ProvMnS | 16.4.0 |
| 2020-06 | SA#88-e | SP-200483 | 0117 | 3 | B | Add streaming trace data reporting service stage 2 definition | 16.4.0 |
| 2020-06 | SA#88-e | SP-200483 | 0118 | 2 | B | Add streaming data reporting service stage 3 mapping of operations | 16.4.0 |
| 2020-06 | SA#88-e | SP-200483 | 0119 | 2 | B |  | 16.4.0 |
| 2020-06 | SA#88-e | SP-200483 | 0120 | 2 | B |  | 16.4.0 |
| 2020-06 | SA#88-e | SP-200483 | 0121 | 2 | B | Add streaming data reporting service stage 3 OpenAPI definition | 16.4.0 |
| 2020-06 | SA#88-e | SP-200499 | 0123 | - | A | Move XML file format from stage2 to stage3 | 16.4.0 |
| 2020-06 | SA#88-e | SP-200485 | 0126 | 1 | C | Update Fault Supervision MnS (stage 2) | 16.4.0 |
| 2020-06 | SA#88-e | SP-200485 | 0127 | 1 | C | Update Fault Supervision MnS (REST SS) | 16.4.0 |
| 2020-06 | SA#88-e | SP-200485 | 0128 | 1 | C | Update Fault Supervision MnS (OpenAPI definitions) | 16.4.0 |
| 2020-06 | SA#88-e | SP-200500 | 0133 | - | F | Correction of ONAP references | 16.4.0 |
| 2020-06 | SA#88-e | SP-200611 | 0134 | 1 | F | Convert JSON schema to YAML file for performance threshold monitoring service | 16.4.0 |
| 2020-09 | SA#89e | SP-200738 | 0135 | - | F | Change stage2 definition for performance data file report MnS to generic file data report MnS | 16.5.0 |
| 2020-09 | SA#89e | SP-200738 | 0136 | - | F | Change RESTFUL definition for performance data file report MnS to generic file data report MnS | 16.5.0 |
| 2020-09 | SA#89e | SP-200724 | 0137 | - | F | Change openAPI definition for performance data file report MnS to generic file data report MnS | 16.5.0 |
| 2020-09 | SA#89e | SP-200737 | 0138 | 1 | F | Clarification on Annex A.1, A.2 and A.5 | 16.5.0 |
| 2020-09 | SA#89e | SP-200723 | 0139 | - | F | Update URI for streamingDataReportingMnS to aligh with URI structure defined in 32.158 | 16.5.0 |
| 2020-09 | SA#89e | SP-200736 | 0141 | 1 | A | Correct the description for generic provisioning MnS | 16.5.0 |
| 2020-09 | SA#89e | SP-200724 | 0143 | - | F | Correct various smaller errors (e.g. validation errors) in faultMnS.yaml (OpenAPI definitions) | 16.5.0 |
| 2020-09 | SA#89e | SP-200724 | 0144 | - | F | Correct definition of ThresholdLevelInd (REST SS) | 16.5.0 |
| 2020-09 | SA#89e | SP-200737 | 0147 | - | F | Remove unintended normative statement from informative clause | 16.5.0 |
| 2020-09 | SA#89e |  |  |  |  | Correction of clause numbering | 16.5.1 |
| 2020-11 |  |  |  |  |  | Cleanup of custom XML, watermarks, hidden text, etc.. no technical changes | 16.5.2 |
| 2020-12 | SA#90e | SP-201050 | 0148 | 1 | F | Correction on generic file data report MnS | 16.6.0 |
| 2020-12 | SA#90e | SP-201088 | 0149 | 2 | F | Update generic streaming MnS | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0150 | 1 | F | Correct CR implementation errors (Fault MnS) | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0152 | 1 | F | Correct ThresholdLevelInd (REST SS, OpenAPI definition) | 16.6.0 |
| 2020-12 | SA#90e | SP-201054 | 0153 | - | F | Correct notifyThresholdCrossing (stage 2) | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0154 | 1 | F | Correct notifyThresholdCrossing (REST SS, OpenAPI definition) | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0155 | 1 | F | Correct notifyHeartbeat (stage 2, REST SS, OpenAPI definition) | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0156 | - | F | Correct small errors in faultMnS.yaml (OpenAPI definition) | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0157 | 1 | F | Correct notifyChangedAlarmGeneral (stage 2) | 16.6.0 |
| 2020-12 | SA#90e | SP-201050 | 0158 | - | F | Correct notifyChangedAlarmGeneral (REST SS, OpenAPI definitions) | 16.6.0 |
| 2020-12 | SA#90e | SP-201055 | 0160 | 1 | F | Fix inconsistencies in guidelines for integration with ONAP VES | 16.6.0 |
| 2020-12 | SA#90e | SP-201088 | 0161 | - | F | Correct small errors in the Fault MnS (REST SS) | 16.6.0 |
| 2020-12 | SA#90e | SP-201088 | 0162 | - | F | Align ProvMnS data type names to UpperCamel (REST SS, OpenAPI definition) | 16.6.0 |