3GPP TSG SA WG5 Meeting 136-e S5-212212

electronic meeting, online, 1 - 9 March 2021

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.130** | **CR** | **0009** | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Update business requirements to applicable for SBMA |
|  |  |
| ***Source to WG:*** | S5 |
| ***Source to TSG:*** | Huawei, China Telecom, China Unicom |
|  |  |
| ***Work item code:*** | MANS |  | ***Date:*** | 2021-02-03  |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | 1. Current requirements for the OAM&P of shared RAN in clause 5.1.1 is system specific requirement, instead of business level requirements. Also these requirments are not applicable for 5G SBMA.
 |
|  |  |
| ***Summary of change:*** | 1. Update the requirements for the OAM&P of shared RAN in clause 5.1.1
 |
|  |  |
| ***Consequences if not approved:*** |  |
|  |  |
| ***Clauses affected:*** | 5.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

### 5.1.1 Requirements for the OAM&P of shared RAN

**REQ-NS\_GEN-CON-1** The 3GPP management system of the MOP shall support a capability allowing its authorized consumer to manage S-RAN of any of the following radio access technologies:

i/ GERAN;

ii/ UTRAN;

iii/ E-UTRAN.

**REQ-NS\_GEN-CON-2** The 3GPP management system of the MOP shall support a capability allowing its authorized consumer to manage S-RAN according to any of the following scenarios:

i/ Multi-Operator Core Network

ii/ Gateway Core Network.

**REQ-NS\_GEN-CON-3** The 3GPP management system of the MOP shall support a capability allowing its authorized consumer to know which POPs the shared resources belong to.

**REQ-NS\_GEN-CON-4** The 3GPP management system of the MOP shall support a capability allowing its authorized consumer to configure which POPs share each cell.

**REQ-NS\_GEN-CON-5**  Any POP shall be able to activate a signaling-based trace / MDT session on its subscribers, whether they are attached to the POP own RAN or to the S-RAN, provided:

a/ this is compliant with the RAN sharing contract; and

b/ user consent for participation in MDT is respected.

**REQ-NS\_GEN-CON-6** The MOP shall be able, on behalf of any POP, to activate an area-based trace / MDT session, on the portion of the S-RAN that the POP shares and on the POP subscribers only, from the 3GPP management system of MOP, provided

a/ only the POP related subscriber data are collected;

b/ this is compliant with the RAN sharing contract; and

c/ user consent for participation in MDT is respected.

**REQ-NS\_GEN-CON-7**  The MOP shall be able, on behalf of multiple POPs, to activate an area-based trace / MDT session, on the portion of the S-RAN that each POP shares and on each POP subscribers only, from the 3GPP management system of MOP, provided:

a/ each POP has access only to its subscriber data (i.e. not to other POPs' subscriber data);

b/ this is compliant with the RAN sharing contract; and

c/ user consent for participation in MDT is respected.

|  |
| --- |
| **End of Changes** |