**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | AssuranceGoalStatusObserved and AssuranceGoalStatusPredicted are not placed appropriately. The status will be observed and predicted for individual AssuranceTarget not for the goal. For example, the goal will be provided by ServiceProfile-A containing latency and throughput as individual AssuranceTarget. The status will be observed for both of the targets for the specified observationTime  |
|  |  |
| ***Summary of change:*** | Moving AssuranceGoalStatusObserved and AssuranceGoalStatusPredicted from AssuranceGoal to AssuranceTarget <<datatype>>. |
|  |  |
| ***Consequences if not approved:*** | Incorrect specification. |
|  |  |
| ***Clauses affected:*** | 4.1.2.3.2.1, 4.1.2.3.2.2, 4.1.2.3.5.1 and 4.1.2.3.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Forge Link: https://forge.3gpp.org/rep/sa5/MnS/commits/S5-213103\_Rel-17\_CR\_28.536\_Moving\_Assurance\_Observed\_and\_Predicted |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Modified Section** |

##### 4.1.2.3.2 AssuranceGoal

4.1.2.3.2.1 Definition

This class represents the subset of attributes (typically characteristics attributes) from an SLS, i.e. a ServiceProfile or a SliceProfile, that are subject to assurance requirements. A single instance of AssuranceGoal represents a list of assurance targets. The assurance goal includes information about the time a goal should be observed. and the status of the the goal fulfilment. The status of the goal fuilfilment is considered FULFILLED if all the constituent target are FULFILLED.

NOTE: A NetworkSlice or NetworkSliceSubnet can support multiple instances of AssuranceGoal.

4.1.2.3.2.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| assuranceTargetList | M | T | F | F | T |
| sliceProfileId | CM | T | T | F | T |
| serviceProfileId | CM | T | T | F | T |
| observationTime | M | T | T | F | T |
| AssuranceGoalStatusObserved | O | T | F | F | T |
| AssuranceGoalStatusPredicted | O | T | F | F | T |
| **Attributes related to role** |  |  |  |  |  |
| networkSliceRef | CM | T | T | F | T |
| networkSliceSubnetRef | CM | T | T | F | T |

.

4.1.2.3.2.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| sliceProfileId | Condition: the AssuranceGoal applies to a NetworkSliceSubNet |
| serviceProfileId | Condition: the AssuranceGoal applies to a NetworkSlice |
| networkSliceSubnet | Condition: the AssuranceGoal applies to a NetworkSliceSubNet |
| networkSlice | Condition: the AssuranceGoal applies to a NetworkSlice |

4.1.2.3.2.4 Notifications

The common notifications defined in subclause 4.1.2.5 are valid for this IOC, without exceptions or additions.

##### 4.1.2.3.3 Void

##### 4.1.2.3.4 Void

##### 4.1.2.3.5 AssuranceTarget <<dataType>>

4.1.2.3.5.1 Definition

This data type represents a single attribute name-value-pair of which one or more are included in an AssuranceGoal. The AssuranceTarget include the status of the goal fulfilment.

4.1.2.3.5.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| assuranceTargetname-value-pair | M | T | F | F | T |
| AssuranceTargetStatusObserved | O | T | F | F | T |
| AssuranceTargetStatusPredicted | O | T | F | F | T |

4.1.2.3.5.3 Attribute constraints

No constraints have been defined for this document.

4.1.2.3.5.4 Notifications

The common notifications defined in clause 4.1.2.5 are valid for the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **End of 1st Modified Section** |

|  |
| --- |
| **2nd Modified Section** |

#### 4.1.2.4 Attribute definitions

##### 4.1.2.4.1 Attribute properties

The following table defines the properties of attributes that are specified in the present document.

Table 4.1.2.4.1.1

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| controlLoopLifeCyclePhase | It indicates the lifecycle phase of the AssuranceClosedControlLoop instance. AllowedValues: Preparation, Commissioning, Operation and Decommissioning.  | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NULL isNullable: False |
| assuranceTargetName | The name of the attribute which is part of AssuranceTarget.The assuranceTargetName shall be equal to the name of an attribute in the relevant ServiceProfile or SliceProfile. The relevant ServiceProfile or SliceProfile is identified by the attribute serviceProfileId or sliceProfileId in the AssuranceGoal. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceTargetValue | The value of the attribute which is part of AssuranceTarget | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| assuranceTargetList | This is an attribute containing a list of AssuranceTarget(s) that are part of an AssuranceGoal | type: AssuranceTargetmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| observationTime | It indicates the time duration over which an AssuranceGoal is observed. The observation time is expressed in seconds. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceGoalStatusObserved | It holds the status of the observed goal fulfilment to the assuranceGoal. The value is FULFILLED only if all the constituent assuranceTargetStatusObserved are FULFILLED. allowedValues: "FULFILLED", “NOT\_FULFILLED  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceGoalStatusPredicted | It holds the status of the predicted future goal fulfilment to the assuranceGoal. The value is FULFILLED only if all the constituent assuranceTargetStatusPredicted are FULFILLED. allowedValues: "FULFILLED", “NOT\_FULFILLED" | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceTargetStatusObserved | It holds the status of the observed target fulfilment to the assuranceGoal. allowedValues: "FULFILLED", “NOT\_FULFILLED  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| assuranceTargetStatusPredicted | It holds the status of the predicted future target fulfilment to the assuranceGoal allowedValues: "FULFILLED", “NOT\_FULFILLED" | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| networkSliceRef | It holds the reference to the NetworkSlice instance subject to assurance requirements | type: Dnmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| networkSliceSubnetRef | It holds the reference to the NetworkSliceSubnet instance subject to assurance requirements | type: Dnmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| operationalState | It indicates the operational state of the AssuranceClosedControlLoop instance. It describes whether the resource is installed and partially or fully operable (Enabled) or the resource is not installed or not operable (Disabled).Allowed values; Enabled/DisabledallowedValues: "ENABLED", "DISABLED".The meaning of these values is as defined in 3GPP TS 28.625 [14] and ITU-T X.731 [15]. | type: ENUM multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: DisabledallowedValues: Enabled, DisabledisNullable: False |
| administrativeState | It indicates the administrative state of the AssuranceClosedControlLoop instance. It describes the permission to use or the prohibition against using the AssuranceClosedControlLoop instance. The administrative state is set by the MnS consumer. Allowed values; Locked/UnlockedallowedValues: "LOCKED", "UNLOCKED".The meaning of these values is as defined in 3GPP TS 28.625 [14] and ITU-T X.731 [15]. | type: ENUM multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: LockedallowedValues: Locked, UnlockedisNullable: False |
| NOTE 1: VoidNOTE 2: Void |

##### 4.1.2.4.2 Constraints

No constraints have been identified for this document.

##### 4.1.2.4.3 Notifications

This subclause presents a list of notifications, defined in [7], that provisioning management service consumer can receive. The notification parameter objectClass/objectInstance, defined in [10], would capture the DN of an instance of an IOC defined in the present document.

#### 4.1.2.5 Common notifications

##### 4.1.2.5.1 Alarm notifications

This clause presents a list of notifications, defined in TS 28.532 [7], that an MnS consumer may receive. The notification header attribute objectClass/objectInstance, defined in TS 32.302 [8], shall capture the DN of an instance of a class defined in the present document.

| Name | Qualifier | Notes |
| --- | --- | --- |
| notifyNewAlarm | M | -- |
| notifyClearedAlarm | M | -- |
| notifyAckStateChanged | M | -- |
| notifyAlarmListRebuilt | M | -- |
| notifyChangedAlarm | O | -- |
| notifyCorrelatedNotificationChanged | O | -- |
| notifyChangedAlarmGeneral | O | -- |
| notifyComments | O | -- |
| notifyPotentialFaultyAlarmList | O | -- |

##### 4.1.2.5.2 Configuration notifications

This clause presents a list of notifications, defined in TS 28.532 [7], that an MnS consumer may receive. The notification header attribute objectClass/objectInstance, defined in TS 32.302 [8], shall capture the DN of an instance of a class defined in the present document.

| Name | Qualifier | Notes |
| --- | --- | --- |
| notifyMOICreation | O | -- |
| notifyMOIDeletion | O | -- |
| notifyMOIAttributeValueChanges | O | -- |
| notifyEvent | O | -- |

|  |
| --- |
| **End of 2nd Modified Section** |

|  |
| --- |
| **2nd Modified Section** |

# B.2 Solution Set (SS) definitions

## B.2.1 OpenAPI document "coslaNrm.yml"

openapi: 3.0.2

info:

 title: coslaNrm

 version: 16.4.0

 description:

 OAS 3.0.1 specification of the Cosla NRM

 © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.536 V16.4.0; Cosla NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.536/

paths: {}

components:

 schemas:

#------------ Type definitions ---------------------------------------------------

 ControlLoopLifeCyclePhase:

 type: string

 enum:

 - PREPARATION

 - COMMISSIONING

 - OPERATION

 - DECOMMISSIONING

 ObservationTime:

 type: integer

 AssuranceGoalStatusObserved:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceGoalStatusPredicted:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceTargetStatusObserved:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceTargetStatusPredicted:

 type: string

 enum:

 - FULFILLED

 - NOT\_FULFILLED

 AssuranceTarget:

 type: object

 properties:

 assuranceTargetName:

 type: string

 assuranceTargetValue:

 type: string

 assuranceTargetStatusObserved:

 $ref: '#/components/schemas/AssuranceGoalStatusObserved'

 assuranceTargetStatusPredicted:

 $ref: '#/components/schemas/AssuranceGoalStatusPredicted'

 AssuranceTargetList:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceTarget'

#-------- Definition of concrete IOCs --------------------------------------------

 SubNetwork-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

 - $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

 - type: object

 properties:

 AssuranceClosedControlLoop:

 $ref: '#/components/schemas/AssuranceClosedControlLoop-Multiple'

 ManagedElement-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-Attr'

 - $ref: 'genericNrm.yaml#/components/schemas/ManagedElement-ncO'

 - type: object

 properties:

 AssuranceClosedControlLoop:

 $ref: '#/components/schemas/AssuranceClosedControlLoop-Multiple'

 AssuranceClosedControlLoop-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 operationalState:

 $ref: 'comDefs.yaml#/components/schemas/OperationalState'

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 controlLoopLifeCyclePhase:

 $ref: '#/components/schemas/ControlLoopLifeCyclePhase'

 AssuranceGoal:

 $ref: '#/components/schemas/AssuranceGoal-Multiple'

 AssuranceGoal-Single:

 allOf:

 - $ref: 'genericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 observationTime:

 $ref: '#/components/schemas/ObservationTime'

 assuranceTargetList:

 $ref: '#/components/schemas/AssuranceTargetList'

 assuranceGoalStatusObserved:

 $ref: '#/components/schemas/AssuranceGoalStatusObserved'

 assuranceGoalStatusPredicted:

 $ref: '#/components/schemas/AssuranceGoalStatusPredicted'

 serviceProfileId:

 type: string

 sliceProfileId:

 type: string

 networkSliceRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 networkSliceSubnetRef:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

 AssuranceClosedControlLoop-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceClosedControlLoop-Single'

 AssuranceGoal-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AssuranceGoal-Single'

#------------ Definitions in TS 28.536 for TS 28.623 -----------------------------

 resources-coslaNrm:

 oneOf:

 - $ref: '#/components/schemas/AssuranceClosedControlLoop-Single'

 - $ref: '#/components/schemas/AssuranceGoal-Single'

 - $ref: '#/components/schemas/SubNetwork-Single'

 - $ref: '#/components/schemas/ManagedElement-Single'

|  |
| --- |
| **End of 2nd Modified Section** |