**3GPP TSG Meeting #137-e *TDoc S5-213199***

electronic meeting, online, May 10th – 19th 2021

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | 28.622 | **CR** | Draft CR | **rev** | - | **Current version:** | 16.7.1 |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-17 Input to DraftCR 28.622 Add data collection job to allow consumers without detailed knowledge of the network to request for data  |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | MADCOL |  | ***Date:*** | 2021-04-30 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)* *Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Job to request for data without detailed knowledge of the network is missing |
|  |  |
| ***Summary of change:*** | Job to request for data without detailed knowledge of the network is added |
|  |  |
| ***Consequences if not approved:*** | Job to request for data without detailed knowledge of the network is missing |
|  |  |
| ***Clauses affected:*** | 4.3, 4.4.1  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | **Input to DraftCR to 28.622 related to the WI MADCOL** |
|  |  |
| ***This CR's revision history:*** |  |

***First change***

4.3.A DataCollectionJob

4.3.A.1 Definition

This IOC represents a data collection request job. The requested data could be of kind Trace, MDT (Minimization of Drive Test), RLF (Radio Link Failure) report, RCEF (RRC Connection Establishment Failure) report, PM (performance metrics) or a combination of these. The DataRequestJob can be name-contained by SubNetwork, ManagedElement, or ManagedFunction.

To activate the production of the requested data, a MnS consumer has to create a DataCollectionJob object instance on the MnS producer. The MnS producer itself has to set up one or several specific data collection jobs (TraceJob, PerfMetricJob) corresponding to the attribute managementDataType. This intermediate step is necessary, as the MnS consumer setting up this DataCollectionJob might not be aware of the necessary detailed knowledge about the network.

*Editor’s Note: The mapping to specific data collection job covers TraceJob and PerfMetricJob. It is FFS if it should be enhanced to other jobs.*

*Editor’s Note: If the mapping from* managementDataType *to the set of data collection jobs is implementation specific or should be explicitely specified with lists is FFS*.

The attribute managementDataType defines the set of data which should be reported. The following sets are available: Coverage, Capacity and Service Experience.

*Editor’s Note: The final sets are FFS. The description of each set is to be edited. If further sets are needed is FFS.*

*Editor’s Note: The attribute name managementDataType is FFS. Further possible names are jobType, manDataType, manDataGroup, manDataSet.*

The attribute areaOfInterest specifies the geograhpic area where data shall be collected. The area is defined by the corners of a polygon specified by latitude and longitude.

The attribute reportingCtrl specifies the method and associated control parameters for reporting the produced measurements to MnS consumers. Three methods are available: file-based reporting with selection of the file location by the MnS producer, file-based reporting with selection of the file location by the MnS consumer and stream-based reporting.

*Editor’s Note: The necessity of the attributes positioningMethod and sensorInformation (to define what positioning method shall be used and which sensor information shall be included in the report) is FFS.*

The optional attribute anonymizationOfData defines the level of anonymization for management based MDT. For details see clause 4.7 in TS 32.422 [30].

The attribute operationalState defines if the object instance is operable or inoperable. This state is set by the object instance or the MnS producer.

*Editor’s Note: An additional attribute dataGranularity to specify data needs (e.g. per S-NSSAI, per 5QI) is FFS.*

4.3.A.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| managementDataType | M | T | T | T | N/A |
| areaOfInterest | M | T | T | T | N/A |
| reportingCtrl | M | T | T | T | N/A |
| anonymizationOfData | O | T | T | T | N/A |
| operationalState | M | T | F | F | T |

4.3.A.3 Attribute constraints

None.

4.3.A.4 Notifications

The common notifications defined in clause 4.5 are valid for this IOC. In addition, the following set of notifications is also valid.

| **Name** | **S** | **Notes** |
| --- | --- | --- |
| notifyFileReady | M | -- |
| notifyFilePreparationError | M | -- |

4.3.B GeoLocation <<dataType>>

4.3.B.1 Definition

This data type defines a geographical location on earth.

4.3.B.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| latitude | M | T | T | T | N/A |
| longitude | M | T | T | T | N/A |

4.3.B.3 Attribute constraints

None.

4.3.B.4 Notifications

The subclause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

***Next change***

4.4.1 Attribute properties

The following table defines the properties of attributes specified in the present document.

| **Attribute Name** | **Documentation and Allowed Values** | **Properties** |
| --- | --- | --- |
| heartbeatNtfPeriod | Periodicity of the heartbeat notification emission. The value of zero has the special meaning of stopping the heartbeat notification emission.Unit is in seconds.AllowedValues: non-negative integers | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0isNullable: False |
| triggerHeartbeatNtf | Setting this attribute to TRUE triggers an immediate additional heartbeat notification emission. Setting the value to FALSE has no observable result.The periodicity of notifyHeartbeat emission is not changed.AllowedValues: TRUE, FALSE | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FALSE isNullable: False |
| notificationRecipientAddress | Address of the notification recipient.allowedValues: N/A | type: String multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| notificationTypes | Notification types of notifications that are candidates for being forwarding to the notification recipient. If this attribute is absent, notifications of all types are candidates for being forwarding to the notification recipient.If the notificationFilter attribute is absent, all candidate notifications are forwarded to the notification recipient, otherwise the candidate notifications are discriminated by the filter specified by the notificationFilter attribute.AllowedValues: - notifyMOICreation- notifyMOIDeletion- notifyMOIAttributeValueChanges- notifyMOIChanges- notifyEvent- notifyNewAlarm- notifyChangedAlarm- notifyAckStateChanged- notifyComments- notifyCorrelatedNotificationChanged- notifyChangedAlarmGeneral- notifyAlarmListRebuilt- notifyPotentialFaultyAlarmList- notifyFileReady- notifyFilePreparationError- notifyThresholdCrossing | type: ENUMmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| notificationFilter | Filter to be applied to candidate notifications identified by the notificationTypes attribute. Only notifications that pass the filter criteria are forwarded to the notification recipient. All other notifications are discarded.The filter can be applied to any field of a notification.allowedValues: N/A | type: String multiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| scope | Scopes the managed object instances included in the notification subscription. If this attribute is absent, all objects below and including the base object are scoped.allowedValues: N/A | type: Scopemultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| scopeType | If the optional scopeLevel attribute is not supported or absent, allowed values of scopeType are BASE\_ONLY and BASE\_ALL.The value BASE\_ONLY indicates only the base object is selected.The value BASE\_ALL indicates the base object and all of its subordinate objects (incl. the leaf objects) are selected.If the scopeLevel attribute is supported and present, allowed values of scopeType are BASE\_NTH\_LEVEL and BASE\_SUBTREE.The value BASE\_NTH\_LEVEL indicates all objects on the level, which is specified by the scopeLevel attribute, below the base object are selected. The base object is at scopeLevel zero.The value BASE\_SUBTREE indicates the base object and all subordinate objects down to and including the objects on the level, which is specified by the scopeLevel attribute, are selected. The base object is at scopeLevel zero.allowedValues: N/A | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| scopeLevel | See definition of scopeType attribute.allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| farEndEntity | The value of this attribute shall be the Distinguished Name of the far end network entity to which the reference point is related.As an example, with EP\_Iucs, if the instance of EP\_Iucs is contained by one RncFunction instance, the farEndEntity is the Distinguished Name of the MscServerFunction instance to which this Iucs reference point is related. allowedValues: N/A | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| linkType | This attribute defines the type of the link. allowedValues: Signalling, Bearer, OAM&P, Other or multiple combinations of this type. | type: Stringmultiplicity: 0..\*isOrdered: FalseisUnique: TruedefaultValue: No isNullable: False |
| locationName | The physical location of this entity (e.g. an address). allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| monitorGranularityPeriod | Granularity period used to monitor measurements for threshold crossings. The period is defined in seconds.See Note 5allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: 1isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| monitorGranularityPeriods | Granularity periods supported for the monitoring of associated measurement types for thresholds. The period is defined in seconds.allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| thresholdInfoList | List of threshold infos. | type: ThresholdInfomultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| thresholdValue | Value against which the monitored performance metric is compared at a threshold level in case the hysteresis is zero.allowedValues: float or integer | type: Unionmultiplicity: 1isOrdered: NAisUnique: NAdefaultValue: NoneisNullable: False |
| hysteresis | Hysteresis of a threshold. If this attribute is present the monitored performance metric is not compared against the threshold value as specified by the thresholdValue attribute but against a high and low threshold value given byhighThresholdValue- = thresholdValue + hysteresislowThresholdValue = thresholdValue - hysteresisWhen going up, the threshold is triggered when the performance metric reaches or crosses the high threshold value. When going down, the threshold is triggered when the performance metric reaches or crosses the low threshold value.A hysteresis may be present only when the monitored performance metric is not of type counter that can go up only. If present for a performance metric of type counter, it shall be ignored.allowedValues: non-negative float or integer | type: Unionmultiplicity: 0..1isOrdered: NAisUnique: NAdefaultValue: NoneisNullable: False |
| thresholdDirection | Direction of a threshold indicating the direction for which a threshold crossing triggers a threshold.When the threshold direction is configured to "UP", the associated treshold is triggered only when the performance metric value is going up upon reaching or crossing the threshold value. The treshold is not triggered, when the performance metric is going down upon reaching or crossing the threshold value.Vice versa, when the threshold direction is configured to "DOWN", the associated treshold is triggered only when the performance metric is going down upon reaching or crossing the threshold value. The treshold is not triggered, when the performance metric is going up upon reaching or crossing the threshold value.When the threshold direction is set to "UP\_AND\_DOWN" the treshold is active in both direcions.In case a threshold with hysteresis is configured, the threshold direction attribute shall be set to "UP\_AND\_DOWN".allowedValues:- UP- DOWN- UP\_AND\_DOWN | type: ENUMmultiplicity: 1isOrdered: NAisUnique: NAdefaultValue: NoneisNullable: False |
| objectClass | Class of a managed object instance.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| objectInstance | Managed object instance identified by its DN.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| objectInstances | List of managed object instances. Each object instance is identified by its DN.allowedValues: N/A | type: Dnmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| peeParametersList | This attribute contains the parameter list for the control and monitoring of power, energy and environmental parameters of ManagedFunction instance(s). This list contains the following parameters:- siteIdentification- siteLatitude (optional)- siteLongitude (optional)- siteDescription - equipmentType- environmentType- powerInterface siteIdentification: The identification of the site where the ManagedFunction resides.allowedValues: N/AsiteLatitude: The latitude of the site where the ManagedFunction instance resides, based on World Geodetic System (1984 version) global reference frame (WGS 84). Positive values correspond to the northern hemisphere. This attribute is optional in case of BTSFunction and RNCFunction instance(s).allowedValues: -90.0000 to +90.0000siteLongitude: The longitude of the site where the ManagedFunction instance resides, based on World Geodetic System (1984 version) global reference frame (WGS 84). Positive values correspond to degrees east of 0 degrees longitude. This attribute is optional in case of BTSFunction and RNCFunction instance(s).allowedValues: -180.0000 to +180.0000siteDescription: An operator defined description of the site where the ManagedFunction instance resides.allowedValues: N/A equipmentType: The type of equipment where the managedFunction instance resides. allowedValues: see clause 4.4.1 of ETSI ES 202 336-12 [18].environmentType: The type of environment where the managedFunction instance resides. allowedValues: see clause 4.4.1 of ETSI ES 202 336-12 [18].powerInterface: The type of power.allowedValues: see clause 4.4.1 of ETSI ES 202 336-12 [18]. | type: Stringmultiplicity: 0..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: True |
| priorityLabel | This is a label that consumer would assign a value on a concrete instance of the managed object. The management system takes the value of this attribute into account. The effect of this attribute value to the subject managed entity is not standardized | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| protocolVersion | Versions(s) and additional descriptive information for the protocol(s) used for the associated communication link. Syntax and semantic is not specified.allowedValues: N/A | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| setOfMcc | Set of Mobile Country Code (MCC). The MCC uniquely identifies the country of domicile of the mobile subscriber. MCC is part of the IMSI (TS 23.003 [5])This list contains all the MCC values in subordinate object instances to this SubNetwork instance.allowedValues: See clause 2.3 of TS 23.003 [5] for MCC allocation principles. | type: Integermultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: No default valueisNullable: False |
| swVersion | The software version of the ManagementNode or ManagedElement (this is used for determining which version of the vendor specific information is valid for the ManagementNode or ManagedElement).allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| systemDN | The Distinguished Name (DN) of IRPAgent (or consumer). Defined in 3GPP TS 32.300.allowedValues: N/A | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| userDefinedState | An operator defined state for operator specific usage.allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| userLabel | A user-friendly (and user assignable) name of this object.allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| vendorName | The name of the vendor.allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| vnfParametersList | This attribute contains the parameter set of the VNF instance(s) corresponding to an NE. Each entry in the list contains:- vnfInstanceId- vnfdId (optional)- flavourId (optional) - autoScalable vnfInstanceId: VNF instance identifier (vnfInstanceId, see section 9.4.2 of [16] and section B2.4.2.1.2.3 of [17]).See Note 1.vnfdId: Identifier of the VNFD on which the VNF instance is based, see section 9.4.2 of [16]. This attribute is optional.Note: the value of this attribute is identical to that of the same attribute in clause 9.4.2 of ETSI GS NFV-IFA 008 [16].flavourId: Identifier of the VNF Deployment Flavour applied to this VNF instance, see section 9.4.3 of [16]. This attribute is optional.Note: the value of this attribute is identical to that of the same attribute in clause 9.4.3 of ETSI GS NFV-IFA 008 [16].autoScalable: Indicator of whether the auto-scaling of this VNF instance is enabled or disabled. The type is Boolean.See Note2.The presence of this attribute indicates that the ManagedFunction represented by the MOI is a virtualized function. See Note 3.allowedValues: N/AA string length of zero for vnfInstanceId means the VNF instance(s) corresponding to the MOI does not exist (e.g. has not been instantiated yet, has already been terminated). | type: Stringmultiplicity: \*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: True |
| vsData | Vendor specific attributes of the type vsDataType. The attribute definitions including constraints (value ranges, data types, etc.) are specified in a vendor specific data format file. allowedValues: -- | type: --multiplicity: --isOrdered: --isUnique: --defaultValue: --isNullable: False |
| vsDataFormatVersion | Name of the data format file, including version.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| vsDataType | Type of vendor specific data contained by this instance, e.g. relation specific algorithm parameters, cell specific parameters for power control or re-selection or a timer. The type itself is also vendor specific.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| supportedPerfMetricGroups | A set of performance metric groups. When this attribute is contained in a managed object it may define performance metrics for this object and all descendant objects.allowedValues: N/A | type: SupportedPerfMetricGroupmultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneallowedValues: N/AisNullable: False |
| performanceMetrics | List of performance metrics.Performance metrics include measurements defined in TS 28.552 [20] and KPIs defined in TS 28.554 [28]. Performance metrics can also be those specified by other SDOs or vendor specific metrics. Performance metrics are identified with their names. A name can als identify a vendor specific group of performance metrics.For measurements defined in TS 28.552 [20] the name is constructed as follows:- "family.measurementName.subcounter" for measurement types with subcounters- "family.measurementName" for measurement types without subcounters- "family" for measurement familiesFor KPIs defined in TS 28.554 [28] the name is defined in the KPI definitions template as the component designated with e).allowedValues: N/A | type: Stringmultiplicity: \*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| rootObjectInstances | List of object instances. Each object instance is identified by its DN and designates the root of a subtree that contains the root object and all descendant objects. | Type: Dnmultiplicity: \*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| reportingMethods | List of reporting methods for performance metricsallowedValues:  - "FILE\_BASED\_LOC\_SET\_BY\_PRODUCER", - "FILE\_BASED\_LOC\_SET\_BY\_CONSUMER", - "STREAM\_BASED" | Type: ENUMmultiplicity: \*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| nFServiceType | The parameter defines the type of the managed NF service instanceallowedValues: See clause 7.2 of TS 23.501[22] | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| operations | This parameter defines set of operations supported by the managed NF service instance.allowedValues: See TS 23.502[23] for supporting operations | type: Operationmultiplicity: 1..\*isOrdered: FalseisUnique: FalsedefaultValue: No default valueisNullable: False |
| Operation.name | This parameter defines the name of the operation of the managed NF service instance.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FalseisUnique: FalsedefaultValue: NoneisNullable: True |
| allowedNFTypes | This parameter identifies the type of network functions allowed to access the operation of the managed NF service instance.allowedValues: See TS 23.501[22] for NF types | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| operationSemantics | This paramerter identifies the semantics type of the operation. See TS 23.502[23]allowedValues: “Request/Response”, “Subscribe/Notify”.  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| sAP | This parameter specifies the service access point of the managed NF service instance.allowedValues: N/A | type: SAPmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| host | This parameter specifies the host address of the managed NF service instance. It can be FQDN (See TS 23.003 [5]) or an IPv4 address (See RFC 791 [24]) or an IPv6 address (See RFC 2373 [25]).allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: FalseisUnique: N/AdefaultValue: NoneisNullable: False |
| port | This parameter specifies the transport port of the managed NF service instance.allowedValues: 1 - 65535 | type: Integermultiplicity: 1isOrdered: FalseisUnique: FalsedefaultValue: NoneisNullable: False |
| usageStae | Usage state of a managed object instance. It describes whether the resource is actively in use at a specific instant, and if so, whether or not it has spare capacity for additional users at that instant. allowedValues: "IDLE", "ACTIVE", "BUSY".The meaning of these values is as defined in 3GPP TS 28.625 [21] and ITU-T X.731 [19]. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| registrationState | This parameter defines the registration status of the managed NF service instance.allowedValues: "Registered", "Deregistered". | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: DeregisteredisNullable: False |
| jobId | Id for a PerfMetricJob job. | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| granularityPeriod | Granularity period used to produce measurements. The period is defined in seconds.See Note 4.allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| granularityPeriods | Granularity periods supported for the production of associated measurement types. The period is defined in seconds.allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: \*isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| reportingCtrl | Selecting the reporting method and defining associated control parameters. | type: ReportingCtrlmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileReportingPeriod | For the file-based reporting method this is the time window during which collected measurements are stored into the same file before the file is closed and a new file is opened. The period is defined in minutes.allowedValues: Multiples of granularityPeriod | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileLocation | File location allowedValues: Not applicable. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| streamTarget | The stream target for the stream-based reporting method.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| administrativeState | Administrative state of a managed object instance. The administrative state describes the permission to use or prohibition against using the object instance. The adminstrative state is set by the MnS consumer.allowedValues: LOCKED, UNLOCKED.  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: LOCKEDisNullable: False |
| operationalState | Operational state of manged object instance. The operational state describes if an object instance is operable ("ENABLED") or inoperable ("DISABLED"). This state is set by the object instance or the MnS producer and is hence READ-ONLY.allowedValues: ENABLED, DISABLED. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: DISABLEDisNullable: False |
| alarmRecords | List of alarm recordsallowedValues: N/A | type: AlarmRecordmultiplicity: \*isOrdered: N/AisUnique: Truedefault value: NoneisNullable: True |
| numOfAlarmRecords | Number of alarm records in the AlarmList.allowedValues: 0 to x where x is vendor specific. | type: integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| lastModification | Time an alarm record was modified the last timeallowedValues: N/A | type: DateTimemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tjJobType | It specifies the MDT mode and it specifies also whether the TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined Trace and MDT job. The attribute is applicable for Trace, MDT, RCEF and RLF reporting.See the clause 5.9a of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: TRACE\_ONLYisNullable: False |
| tjListOfInterfaces | It specifies the interfaces that need to be traced in the given ManagedEntityFunction.The attribute is applicable only for Trace. In case this attribute is not used, it carries a null semantic.See the clause 5.5 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoisNullable: True |
| tjListOfNeTypes | It specifies in which type of ManagedFunction the trace should be activated. The attribute is applicable only for Trace with Signalling Based Trace activation. In case this attribute is not used, it carries a null semantic.See the clause 5.4 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoisNullable: True |
| tjPLMNTarget | It specifies which PLMN that the subscriber of the session to be recorded uses as selected PLMN. PLMN Target might differ from the PLMN specified in the Trace Reference.See the clause 5.9b of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: No isNullable: True |
| tjStreamingTraceConsumerURI | It specifies the URI of the Streaming Trace data reporting MnS consumer (a.k.a. streaming target).See the clause 5.9 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjTraceCollectionEntityAddress | It specifies the address of the Trace Collection Entity when the attribute tjTraceReportingFormat is configured for the file-based reporting. The attribute is applicable for both Trace and MDT.See the clause 5.9 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjTraceDepth | It specifies the trace depth. The attribute is applicable only for Trace. In case this attribute is not used, it carries a null semantic.See the clause 5.3 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: MAXIMUM isNullable: True |
| tjTraceReference | A globally unique identifier, which uniquely identifies the Trace Session that is created by the TraceJob. In case of shared network, it is the MCC and MNC of the Participating Operator that request the trace session that shall be provided.The attribute is applicable for both Trace and MDT.See the clause 5.6 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: None isNullable: False |
| tjTraceReportingFormat | It specifies the trace reporting format - streaming trace reporting or file-based trace reporting.See the clause 5.11 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FILE isNullable: False |
| tjTraceTarget | It specifies the target object of the Trace and MDT. The attribute is applicable for both Trace and MDT. This attribute includes the ID type of the target as an enumeration and the ID value.See the 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjTriggeringEvent | It specifies the triggering event parameter of the trace session. The attribute is applicable only for Trace. In case this attribute is not used, it carries a null semantic.See the clause 5.1 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTAnonymizationOfData | It specifies the level of anonymization for management based MDT.See the clause 5.10.12 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NO\_IDENTITY isNullable: True |
| tjMDTAreaConfigurationForNeighCell | It specifies the area for which UE is requested to perform measurement logging for neighbour cells which have list of frequencies. If it is not configured, the UE shall perform measurement logging for all the neighbour cells.Applicable only to NR Logged MDT.See the clause 5.10.26 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTAreaScope | It specifies MDT area scope when activates an MDT job. For RLF and RCEF reporting it specifies the eNB or list of eNBs where the RLF or RCEF reports should be collected.List of cells/TA/LA/RA for signaling based MDT or management based Logged MDT.List of cells for management based Immediate MDT.Cell, TA, LA, RA are mutually exclusive.One or list of eNBs for RLF and RCEFreportingSee the clause 5.10.2 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTCollectionPeriodRrmLte | It specifies the collection period for collecting RRM configured measurement samples for M2, M3 in LTE. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.20 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTCollectionPeriodRrmUmts | It specifies the collection period for collecting RRM configured measurement samples for M3, M4, M5 in UMTS. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.21 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTEventListForTriggeredMeasurement | It specifies event types for event triggered measurement in the case of logged NR MDT. Each trace session may configure at most one event. The UE shall perform logging of measurements only upon certain condition being fulfilled:- Out of coverage.- A2 event.See the clause 5.10.28 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTEventThreshold | It specifies the threshold which should trigger the reporting in case A2 event reporting in LTE or 1F/1l event in UMTS. The attribute is applicable only for Immediate MDT and when reportingTrigger is configured for A2 event in LTE or 1F event or 1l event in UMTS. In case this attribute is not used, it carries a null semantic.See the clauses 5.10.7 and 5.10.7a of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTListOfMeasurements | It specifies the UE measurements that shall be collected in an Immediate MDT job. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.3 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTLoggingDuration | It specifies how long the MDT configuration is valid at the UE in case of Logged MDT. The attribute is applicable only for Logged MDT and Logged MBSFN MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.9 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTLoggingInterval | It specifies the periodicty for Logged MDT. The attribute is applicable only for Logged MDT and Logged MBSFN MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.8 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTMBSFNAreaList | The MBSFN Area consists of a MBSFN Area ID and Carrier Frequency (EARFCN). The target MBSFN area List can have up to 8 entries. This parameter is applicable only if the job type is Logged MBSFN MDT.See the clause 5.10.25 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1..8isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTMeasurementPeriodLTE | It specifies the measurement period for the Data Volume and Scheduled IP throughput measurements for MDT taken by the eNB. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.23 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTMeasurementPeriodUMTS | It specifies the measurement period for the Data Volume and Throughput measurements for MDT taken by RNC. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.22 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTCollectionPeriodRrmNR | It specifies the collection period for collecting RRM configured measurement samples for M4, M5 in NR. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.30 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTMeasurementQuantity | It specifies the measurements that are collected in an MDT job for a UMTS MDT configured for event triggered reporting.See the clause 5.10.15 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTPLMList | It indicates the PLMNs where measurement collection, status indication and log reporting is allowed.See the clause 5.10.24 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: PLMNmultiplicity: 1..16isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTPositioningMethod | It specifies what positioning method should be used in the MDT job.See the clause 5.10.19 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTReportAmount | It specifies the number of measurement reports that shall be taken for periodic reporting while the UE is in connected. The attribute is applicable only for Immediate MDT and when tjMDTReportingTrigger is configured for periodical measurements. In case this attribute is not used, it carries a null semantic.See the clause 5.10.6 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTReportingTrigger | It specifies whether periodic or event based measurements should be collected. The attribute is applicable only for Immediate MDT and when the tjMDTListOfMeasurements is configured for M1 (for both UMTS and LTE) or M2 (only for UMTS). In case this attribute is not used, it carries a null semantic.See the clause 5.10.4 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTReportInterval | It specifies the interval between the periodical measurements that shall be taken when the UE is in connected mode. The attribute is applicable only for Immediate MDT and when tjMDTReportingTrigger is configured for periodical measurements. In case this attribute is not used, it carries a null semantic.See the clause 5.10.5 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTReportType | It specifies report type for logged NR MDT as:- periodical.- event triggered.See the clause 5.10.27 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTSensorInformation | It specifies which sensor information shall be included in logged NR MDT and immediate NR MDT measurement if they are available. The following sensor measurement can be included or excluded for the UE: - Barometric pressure.- UE speed.- UE orientation.See the clause 5.10.29 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjMDTTraceCollectionEntityID | It specifies the TCE Id which is sent to the UE in Logged MDT.See the clause 5.10.11 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| jobType | It specifies the set of data which shall be reported.allowedValues: COVERAGE, UP\_CONGESTION, RESOURCE\_UTILIZATION, SLICE\_LOAD, LATENCY, SERVICE\_EXPERIENCE, FAULT\_MANAGEMENT, MOBILITY, ENERGY\_EFFICIENCY  | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoisNullable: True |
| areaOfInterest | It specifies the area where data is collected. | type: GeoLocationmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| longitude | It specifies the longitude of a geographical location. The unit is degree. Precede West longitudes with a minus sign.Allowed values: -180, …,180 | type: floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| latitude | It specifies the latitude of a geographical location. The unit is degree. Precede South latitudes with a minus sign.Allowed values: -90, …,90 | type: floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| positioningMethod | It specifies what positioning method should be used in the MDT job.allowedValues: GNSS, E-CID | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoisNullable: True |
| sensorInformation | It specifies which sensor information shall be included in the measurement reports if they are available. AllowedValues: BAROMETRIC\_PRESSURE, UE\_SPEED, UE\_ORIENTATION | type: ENUMmultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| anonymizationOfData | It specifies the level of anonymization for management based MDT. For details see clause 4.7 of TS 32.422 [30].AllowedValues: NO\_IDENTITY, TAC\_OF\_IMEI | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NO\_IDENTITY isNullable: True |
| NOTE 1: The value of this attribute is identical to that of the same attribute in clause 9.4.2 of ETSI GS NFV-IFA 008 [16].NOTE 2: The value of this attribute is identical to that of the same attribute included in vnfConfigurableProperty in clause 9.4.2 of ETSI GS NFV-IFA 008 [16].NOTE 3: The presence of the attribute vnfParametersList, whose vnfInstanceId with a string length of zero, in createMO operation can trigger the instantiation of the related VNF/VNFC instances.NOTE 4: The GP defines the measurement data production rate. The supported rates are dependent on the capacity of the producer involved (e.g. the processing power of the producer, the complexity of the measurement type involved etc) and therefore, it cannot be standardized for all producers involved. The supported GPs reflects the agreement between producer and the consumer involved.NOTE 5: The monitoring granularity period defines the measurements monitoring period. The supported monitoring periods are dependent on the capacity of the producer involved (e.g. the processing power of the producer, the complexity of the measurement type involved etc) and therefore, it cannot be standardized for all producers involved. The supported monitoring GPs reflect the agreement between producer and the consumer involved.NOTE 6: The supported threshold levels are dependent on the capacity of the producer involved (e.g. the processing power of the producer, number of measurements being measured by the producer at the time, the complexity of the measurement type involved etc) and therefore, it cannot be standardized for all producers involved. The supported levels can only reflect the negotiated agreement between producer and the consumer involved. |

4.4.2 Constraints

None

***End of changes***