**3GPP TSG-SA5 Meeting #138-e *S5-214187***

**e-meeting, 23 - 31 August 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **32.130** | **CR** | **0014** | **rev** | 1 | **Current version:** | **17.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Add NG-RAN sharing individual management use case and requirements | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE Corporation | | | | | | | | | |
| ***Source to TSG:*** | SA5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | MANS | | | | |  | ***Date:*** | | | 2021-08-09 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In NG-RAN sharing scenarios, the shared NG-RAN is usually managed by MOP, but the POPs still have the requirements that the shared NG-RAN can be individually managed based on their own policies, e.g. in autonomous network scenario, the POPs may want to have their own autonomous functions. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add the NG-RAN sharing individual management use case and requirements. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.4.x (new), 5.1.y (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Revision of S5-213402 | | | | | | | | |

|  |
| --- |
| **1st of Changes** |

### 5.4.x Individual management of shared NG-RAN

In this use case, Operator A and Operator B are sharing one NG-RAN network. Operator A owns and manages this shared NG-RAN network as the MOP and POP. Operator B as the POP hopes that the shared resources in NG-RAN sharing scenarios can also be individually managed based on their own policies, so that they can use their own autonomous network management functions.

|  |
| --- |
| **Next Change** |

### 5.1.y Requirements for the OAM&P of shared NG-RAN

**REQ-NS\_NG-CON-x** The 3GPP management system of the MOP shall support a capability allowing the shared resources (i.e. gNBs, Cells) associated with the POPs to be managed individually based on the POPs’ requirements.

|  |
| --- |
| **End of Change** |