**3GPP TSG-SA5 Meeting #138-e *S5-214340***

**e-meeting, 23 - 31 August 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **32.291** | **CR** | **0337** | **rev** | **-** | **Current version:** | **16.8.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarify the User Location information | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI16 | | | | |  | ***Date:*** | | | 2021-08-06 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| Reason for change: | | As per the TS 32.291, the data type "Userlocation" as re-used data types specified in TS 29.571 is used for userLocationinfo and  mAPDUNon3GPPUserLocationInfo in PDUSessionChargingInformation, userLocationInformation in PDUContainerInformation and QFIContainerInformation, userLocationInfo in SMSChargingInformation, RegistrationChargingInformation, N2ConnectionChargingInformation and LocationReportingChargingInformation. The data type "Userlocation" includes all of the user location information for diversertiy scenarios. The trigger "USER\_LOCATION\_CHANGE" will cause the usage reporting to CHF, only the corresponding updated user location information will be reported. The clarification for user location information reporting is required. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add the description to clarify the "Userlocation". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Unclear data type "Userlocation" for 5G Charging. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.1.6.3.6,6.2.5.3.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First change** |

##### 6.1.6.3.6 Enumeration: TriggerType

Table 6.1.6.3.6-1: Enumeration TriggerType

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| QUOTA\_THRESHOLD | the quota threshold has been reached |  |
| QHT | the quota holding time specified in a previous response has been hit (i.e. the quota has been unused for that period of time) |  |
| FINAL | a service normal termination has occurred. |  |
| QUOTA\_EXHAUSTED | the quota has been exhausted |  |
| VALIDITY\_TIME | the credit authorization lifetime provided from CHF has expired |  |
| OTHER\_QUOTA\_TYPE | usage reporting of the particular quota type indicated in the used unit container where it appears is that, for a multi-dimensional quota, one reached a trigger condition and the other quota is being reported. |  |
| FORCED\_REAUTHORISATION | a Server initiated re-authorization procedure, i.e. receipt of notify service operation |  |
| UNIT\_COUNT\_INACTIVITY\_TIMER | the unit count inactivity timer has expired |  |
| ABNORMAL\_RELEASE | a service abnormal termination has occurred. |  |
| QOS\_CHANGE | In request message, this value is used to indicate that QoS change has happened. Any of elements of QoSData may result in QoS change.  In response message, this value is used to indicate that a change of authorized QoS shall cause the service consumer to ask for a re-authorization of the associated quota. |  |
| VOLUME\_LIMIT | Volume limit has been reached. |  |
| TIME\_LIMIT | Time limit has been reached |  |
| EVENT\_LIMIT | Event limit has been reached |  |
| PLMN\_CHANGE | PLMN has been changed. |  |
| USER\_LOCATION\_CHANGE | In request message, this value is used to indicate that User location has been changed. Only the change in location information that triggered reporting must be included.  In response message, this value is used to indicate that a change in the end user location shall cause the service consumer to ask for a re-authorization of the associated quota |  |
| RAT\_CHANGE | In request message, this value is used to indicate that RAT type has been changed.  In response message, this value is used to indicate that a change in the radio access technology shall cause the service consumer to ask for a re-authorization of the associated quota |  |
| SESSION\_AMBR\_CHANGE | In request message, this value is used to indicate that Session AMBR has been changed.  In response message, this value is used to indicate that a change in the session AMBR shall cause the service consumer to ask for a re-authorization of the associated quota. |  |
| GFBR\_GUARANTEED\_STATUS\_CHANGE | In request message,thisvalue is used to indicate that GFBR targets for the indicated SDFs are changed ("NOT\_GUARANTEED" or "GUARANTEED" again).  In response message, this value is used to indicate that a NF Consumer (CTF) needs to ensure requesting the notification from the access network and that a change in the GFBR targets shall cause the service consumer to ask for a re-authorization of the associated quota. |  |
| UE\_TIMEZONE\_CHANGE | In request message, this value is used to indicate that UE timezone has been changed.  In response message, this value is used to indicate that a change in the time zone where the end user is located shall cause the service consumer to ask for a re-authorization of the associated quota. |  |
| TARIFF\_TIME\_CHANGE | Tariff time change has happened. |  |
| MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS | Max number of change has been reached |  |
| MANAGEMENT\_INTERVENTION | Management intervention |  |
| CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA | In request message, this value is used to indicate that Change of UE presence in PRA has happened.  In response message, this value is used to indicate a request of reporting the event that the user enters/leaves the area(s) as indicated in the presenceReportingArea Attribute |  |
| CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS | In request message, this value is used to indicate that Change of 3GPP PS Data off status has happened.  In response message, this value is used to indicate that a change in the 3GPP PS Data off status shall cause the service consumer to ask for a re-authorization of the associated quota |  |
| SERVING\_NODE\_CHANGE | A serving node (e.g., AMF) change in the NF Consumer |  |
| REMOVAL\_OF\_UPF | A used UPF is removed |  |
| ADDITION\_OF\_UPF | A new UPF is added. |  |
| INSERTION\_OF\_ISMF | A new I-SMF is inserted |  |
| REMOVAL\_OF\_ISMF | A used I-SMF is removed |  |
| CHANGE\_OF\_ISMF | A used I-SMF is removed, and a new I-SMF is inserted |  |
| START\_OF\_SERVICE\_DATA\_FLOW | A Service Data Flow has started |  |
| HANDOVER\_CANCEL | The handover is canceled. |  |
| HANDOVER\_START | The handover is start. |  |
| HANDOVER\_COMPLETE | The handover is completed. |  |
| ECGI\_CHANGE | In request message, this value is used to indicate that ECGI has been changed.  In response message, this value is used to indicate that a change in the end user location shall cause the service consumer to ask for a re-authorization of the associated quota | 5GIEPC\_CH |
| TAI\_CHANGE | In request message, this value is used to indicate that TAI has been changed.  In response message, this value is used to indicate that a change in the end user location shall cause the service consumer to ask for a re-authorization of the associated quota | 5GIEPC\_CH |
| ADDITION\_OF\_ACCESS | Addition of access to the MA PDU session | ATSSS |
| REMOVAL\_OF\_ACCESS | Removal of access to the MA PDU session | ATSSS |
| START\_OF\_SDF\_ADDITIONAL\_ACCESS | Start of service data flow on additional access in a MA PDU session | ATSSS |

|  |
| --- |
| **Next change** |

##### 6.2.5.3.5 Enumeration: TriggerType

Table 6.2.5.3.5-1: Enumeration TriggerType

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| FINAL | a service termination has happened |  |
| ABNORMAL\_RELEASE | PDU session has abnormal released. |  |
| QOS\_CHANGE | In request message, this value is used to indicate that QoS change has happened. Any of elements of QoSData may result in QoS change. |  |
| VOLUME\_LIMIT | Volume limit has been reached. |  |
| TIME\_LIMIT | Time limit has been reached |  |
| EVENT\_LIMIT | Event limit has been reached |  |
| PLMN\_CHANGE | PLMN has been changed. |  |
| USER\_LOCATION\_CHANGE | In request message, this value is used to indicate that User location has been changed. Only the change in location information that triggered reporting must be included. |  |
| RAT\_CHANGE | In request message, this value is used to indicate that RAT type has been changed. |  |
| SESSION\_AMBR\_CHANGE | In request message, this value is used to indicate that Session AMBR has been changed. |  |
| UE\_TIMEZONE\_CHANGE | In request message, this value is used to indicate that UE timezone has been changed. |  |
| TARIFF\_TIME\_CHANGE | Tariff time change has happened. |  |
| MAX\_NUMBER\_OF\_CHANGES\_IN CHARGING\_CONDITIONS | Max number of change has been reached |  |
| MANAGEMENT\_INTERVENTION | Management intervention |  |
| CHANGE\_OF\_UE\_PRESENCE\_IN PRESENCE\_REPORTING\_AREA | In request message, this value is used to indicate that Change of UE presence in PRA has happened.  In response message, this value is used to indicate a request of reporting the event that the user enters/leaves the area(s) as indicated in the presenceReportingArea Attribute |  |
| CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS | In request message, this value is used to indicate that Change of 3GPP PS Data off status has happened. |  |
| SERVING\_NODE\_CHANGE | A serving node (e.g., AMF) change in the NF Consumer |  |
| REMOVAL\_OF\_UPF | A used UPF is removed |  |
| ADDITION\_OF\_UPF | A new UPF is added. |  |
| INSERTION\_OF\_ISMF | A new I-SMF is inserted |  |
| REMOVAL\_OF\_ISMF | A used I-SMF is removed |  |
| CHANGE\_OF\_ISMF | A used I-SMF is removed, and a new I-SMF is inserted |  |
| HANDOVER\_CANCEL | The handover is cancelled. |  |
| HANDOVER\_START | The handover is started. |  |
| HANDOVER\_COMPLETE | The handover is complete. |  |
| ADDITION\_OF\_ACCESS | Addition of access to the MA PDU session | ATSSS |
| REMOVAL\_OF\_ACCESS | Removal of access to the MA PDU session | ATSSS |
| START\_OF\_SDF\_ADDITIONAL\_ACCESS | Start of service data flow on additional access in a MA PDU session | ATSSS |

|  |
| --- |
| **End of change** |