**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The NRM fragment for edge need to be defined as depicted in 28.814. |
|  |  |
| ***Summary of change:*** | The introduction of edge NRM fragment |
|  |  |
| ***Consequences if not approved:*** | Impossible edge management solution |
|  |  |
| ***Clauses affected:*** | Y (new clause) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First modification** |

Y. Edge NRM

Y.1 Information Model definitions for Edge NRM

## Y.1 Imported information entities and local labels

|  |  |
| --- | --- |
| Label reference | Local label |
| TS 28.622 [30], IOC, Top | Top |
| TS 28.622 [30], IOC, SubNetwork | SubNetwork |
| TS 28.622 [30], IOC, ManagedFunction | ManagedFunction |

## Y.2 Class diagram

### Y.2.1 Relationships



### Y.2.2 Inheritance

 

## Y.3 Class definition

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

Y.3.1 EASFunction

Y.3.1.1 Definition

This IOC represent the properties of a EAS in a 3GPP network. For more information about EAS, see 3GPP TS 23.558.

Y.3.1.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| eASRequirements | M | T | T | F | T |
|  |  |  |  |  |  |
| eASProfile | M | T | T | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### Y.3.1.3 Attribute constraints

#### Y.3.1.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

Y.3.2 EASRequirements <<datatype>>

Y.3.2.1 Definition

This datatype represent the deployment requirements of an EAS which need to be considered during EASFunction instantiation.

Y.3.2.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| requiredEASservingLocation | M | T | F | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### Y.3.2.3 Attribute constraints

#### Y.3.2.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

Y.3.3 ServingLocation <<datatype>>

Y.3.3.1 Definition

This datatype represent the location which is to be served by the node.

Y.3.3.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| geographicalLocation | CM | T | F | F | T |
| topologicalLocation | CM | T | F | F | T |
|  |  |  |  |  |  |

#### Y.3.3.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| geographicalLocation Support Qualifier | Condition: either geographicalLocation or topologicalLocation shall be present. |
| topologicalLocation Support Qualifier | Condition: either geographicalLocation or topologicalLocation shall be present. |

#### Y.3.3.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

Y.3.4 EASProfile <<datatype>>

Y.3.1.1 Definition

This IOC represent the EAS profile, see 3GPP TS 23.558.

Y.3.1.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| eASservingLocation | M | T | T | F | T |
| eASProvider | O | T | T | F | T |
| eASType | O | T | T | F | T |
| eASDescription | O | T | T | F | T |
|  |  |  |  |  |  |

#### Y.3.1.3 Attribute constraints

#### Y.3.1.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

Y.3.5 GeoLoc <<datatype>>

Y.3.5.1 Definition

This datatype represent the geographical location.

Y.3.5.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| geoPoint | CM | T | T | F | T |
| civicAddress | CM | T | T | F | T |

#### Y.3.5.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| geoPoint Support Qualifier | Condition: either geoPoint or civicAddress shall be present. |
| civicAddress Support Qualifier | Condition: either geoPoint or civicAddress shall be present. |

#### Y.3.5.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

Y.3.6 GeoP <<datatype>>

Y.3.6.1 Definition

This datatype represent the geographical location.

Y.3.6.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| lat | M | T | T | F | T |
| long | M | T | T | F | T |

#### Y.3.6.3 Attribute constraints

#### Y.3.6.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

Y.3.7 TopoLoc <<datatype>>

Y.3.7.1 Definition

This datatype represent the topological location.

Y.3.7.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| cellID | O | T | T | F | T |
| tAI | O | T | T | F | T |
| pLMNID | O | T | T | F | T |

#### Y.3.7.3 Attribute constraints

#### Y.3.7.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

## Y.2 Attribute definition

Y.2.1 Attribute Properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
|  |  |  |
| eASREquirements | It defines the deployment requirement of an EAS. | type: EASRequirementsmultiplicity: isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| eASservingLocation | It defines the serving location for an EAS. | type: ServingLocationmultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| eASProvider | It defines the EAS Provider Identifier, see 3GPP TS 23.558. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| eASType | It defines the EAS Type, see 3GPP TS 23.558. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| eASDescription | It defines the EAS description, see 3GPP TS 23.558. | type: Stingmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| requiredEASservingLocation | It defines the location where the EAS service should be available. | type: ServingLocationmultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| requiredVR | It defines the virtual resources requirements of the EAS. | type: FFSmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
|  |  |  |
| topologicalLocation | This refers to the Topological Service Area, see 3GPP TS 23.558. | type: TopoLocmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| geographicalLocation | This refers to the Geographical Service Area, see 3GPP TS 23.558. | type: GeoLocmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| eASProfile | This refers to the EAS profile, see 3GPP TS 23.558 | type: EASProfilemultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| geoPoint | This defines the location in terms of latitude and longitude. | type: geoPmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| lat | This defines the single latitude coordinate. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| long | This defines the single longtitude coordinate. | type: Floatmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| civicAddress | This defines the location in terms of a civic address | type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| cellID | The list of cell IDs defining the topological service area | type: Stringmultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| tAI | The list of Tracking Area IDs defining the topological service area | type: Stringmultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| pLMNID | The list of PLMN IDs defining the topological service area | type: Stringmultiplicity: 1..\*isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |

|  |
| --- |
| **End of first modification** |