**3GPP TSG-SA5 Meeting #140e *S5-216043***

**e-meeting** **15th - 24th November 2021**

**Source: Nokia, Nokia Shanghai Bell****, Huawei**

**Title: Extend Attributes of the Intent IOC**

**Document for: Approval**

**Agenda Item: 6.4.10**

# 1 Decision/action requested

***The group is asked to discuss and approval.***

# 2 References

[1] 3GPP draft TS 28.312: “Management and orchestration; Intent driven management services for mobile networks v0.5.0”.

# 3 Rationale

This contribution proposes to Extend attributes of the Intent IOC for an Intent-driven Management Service

.

# 4 Detailed proposal

It proposes to make the following changes to TS 28.312[1].


|  |
| --- |
| **1st Change** |

## 6.2 Information model definition for Intent (MnS component typeB)

### 6.2.1 Information model definition for Intent

#### 6.2.1.1 Class diagram

##### 6.2.1.1.1 Relationship



@startuml TS 28.541 figure 6.2.1-2 (as of MArch 2021)

' UML diagram for 3GPP TS 28.541 clause 6

skinparam ClassStereotypeFontStyle normal

skinparam ClassBackgroundColor White

skinparam shadowing false

skinparam monochrome true

hide members

hide circle

'skinparam maxMessageSize 250

class ManagedEntity <<ProxyClass>>

class Intent <<InformationObjectClass>>

class intentExpectation <<dataType>>

class intentTarget <<dataType>>

class context<<dataType>>

class IntentReport <<DataType>>

ManagedEntity "1" \*-- "\*" Intent: <<names>>

Intent "1" \*-r- "\*" intentExpectation

Intent "1" \*-d- "\*" context

intentExpectation "1" \*-r- "\*" intentTarget

intentExpectation "1" \*-d- "\*" context

'ManagedEntity -d- IntentReport: <<FFS>>

Intent \*-l- IntentReport: <<FFS>>

intentTarget "1" \*-d- "\*" context

note top of ManagedEntity

Represents the following IOCs:

Subnetwork or

Other ICs are FFS

end note

note "{xor}" as N1

(Intent, context) .. N1

N1 .. (intentTarget, context)

N1 .. (intentExpectation, context)

@enduml





Figure 6.2.1.1.1-1 Relationship UML diagram for intent

Editor’s Note: Whether the intentExpectation is a <<dataType>> or a <<IOC>> is FFS.

##### 6.2.1.1.2 Inheritance



@startuml TS 28.541 figure 6.2.1-2 (as of MArch 2021)

' UML diagram for 3GPP TS 28.541 clause 6

skinparam ClassStereotypeFontStyle normal

skinparam ClassBackgroundColor White

skinparam shadowing false

skinparam monochrome true

hide members

hide circle

class Top <<InformationObjectClass>>

class Intent <<InformationObjectClass>>

'class intentExpectation <<dataType>>

'class Context <<dataType>>

'class IntentTarget <<dataType>>

Top <|-- Intent

'Top <|-- intentExpectation

@enduml

Figure 6.2.1.1.2-1 Inheritance UML diagram for generic intent

#### 6.2.1.2 Class definition

##### 6.2.1.2.1 Intent <<IOC>>

###### 6.2.1.2.1.1 Definition

This IOC represents the properties of an Intent. The Intent IOC contains one or multiple intentExpectation(s) which includes MnS consumer’s requirements, goals and constraints given to a 3GPP system*.*

The Intent IOC includes the attribute objectClass and objectInstance from the TOP IOC. The value of attribute objectClass is “Intent” and the value of attribute objectInstance is the DN of the instance of Intent IOC.

###### 6.2.1.2.1.2 Attributes

The Intent includes attributes inherited fromTOP IOC (defined in TS 28.622) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute Name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| intentExpectations | M | T | T | F | T |
| userLabel | M | T | T | F | T |
| IntentContexts | O | T | T | F | T |
| intentFulfilStatus | M | T | F | F | T |

Editor’s Note: whether other the attributes are needed for the Intent IOC needs further discussion.

###### 6.2.1.2.1.3 Attribute constraints

None

##### 6.2.1.2.2 IntentExpectation

IntentExpectation class represent MnS consumer’s requirements, goals and constraints given to a 3GPP system*.*

Editor’s Note: more description for IntentExpectation will be added later based on the further discussion.

###### 6.2.1.2.2.1 Definition

IntentExpectation class represent MnS consumer’s requirements, goals and constraints given to a 3GPP system.

###### 6.2.1.2.2.2 Attributes

The IntentExpectation includes the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute Name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| ExpectationId | M | T | T | T | T |
| ObjectType | M | T | T | F | T |
| ObjectContexts | CM | T | T | F | T |
| ExpetationTargets | CM | T | T | F | T |
| ExpetationContexts | O | T | T | F | T |

Editor’s Note: whether other the attributes are needed for the IntentExpectation IOC needs further discussion.

Editor’s Note: whether both objectContexts and ExpetationTargets are mandatory is FFS.

###### 6.2.1.2.2.3 Attribute constraints

None

##### 6.2.1.2.3 IntentReport

###### 6.2.1.2.3.1 Definition

IntentReport class represent intent fulfilment feedback information that MnS consumer can obtained from a 3gpp system.

Editor’s Note: more description for IntentReport will be added later based on the further discussion.

###### 6.2.1.2.3.2 Attributes

TBD

###### 6.2.1.2.3.3 Attribute constraints

TBD

#### 6.2.1.3 DataType definition

##### 6.2.1.3.1 expectationTarget <<dataType>>

###### 6.2.1.3.1.1 Definition

This <<dataType>> represents the Targets of the IntentExpectation that are required to be achieved .

###### 6.2.1.3.1.2 Attributes

The expectationTarget includes the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute Name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| targetName | M | T | T | T | T |
| targetCondition | M | T | T | F | T |
| targetValueRange | M | T | T | F | T |
| targetContexts | O | T | T | F | T |

###### 6.2.1.3.1.3 Attribute constraints

None

##### 6.2.1.3.2 context << dataType >>

###### 6.2.1.3.2.1 Definition

This IOC represents the properties of a context. A context describes the list of constraints and conditions that should evaluate to True when the targets are fulfilled but are themselves not to be enforced. The context may apply to the intent, the intent expectation, the intent targets or to the managed object as filter information used to identify the manged objects to which the targets are intended.

###### 6.2.1.3.2.2 Attributes

The context includes the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute Name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
|  |  |  |  |  |  |
| contextAttribute | M | T | F | T | T |
| contextCondition | M | T | T | F | T |
| contextValueRange | M | T | T | F | T |

###### 6.2.1.3.2.3 Attribute constraints

None

#### 6.2.1.4 Attribute definition

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| userLabel | A user-friendly (and user assignable) name of the intent.  allowedValues: Not Applicable | type: String  multiplicity: 1  isOrdered: F  isUnique: F  defaultValue: None  isNullable: False |
| intentExpectation | It indicates the expectations including requirements, goals and constraints given to a 3GPP system. It states the list of specific outcomes desired to be realized for a specific type of managed object | type: FFS  multiplicity: \*  isOrdered: F  isUnique: F  defaultValue: None  isNullable: False |
| intentFulfilStatus | It describes the status of the intent fulfilment result, which is configured by MnS producer and can be read by MnS consumer.  allowedValues: "FULFILLED", “NOT\_FULFILLED  Editor’s Note: whether other allowed values should be supported is FFS, and the name for the attribute intentFulfilStatus is FFS. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| intentContext | It describes the list of constraints and conditions that should apply for the entire intent even if there may be specific constraints and conditions defined for specific parts of the intent.  allowedValues: triple of (attribute, condition, value range) | type: Context  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| intentExpectationIdentifier | A user-friendly (and user assignable) name of the intentExpectation.  allowedValues: Not Applicable | type: String  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| objectType | It describes the type of object to which the given intentExpectation should apply. It is used together with the ObjectContext to identify the specific entity to which the intentExpectation should apply. E.g. the intentExpectation may be stated for a slice (type of Object) with identitier IIOT\_Atomotive\_2021 (identifier as context). Alternatively, the intentExpectation may be stated for a slice (type of Object) serving IIoT users (context 1) with slice profile supporting automotive connectivity (context 2).  allowedValues: NA | type: string  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| objectContext | It describes the list of constraints and conditions to be used as filter information to identify the specific intentObject to which a given intentExpectation should apply. Note there may be other constraints and conditions defined either for the entire intent , for the specific intentExpectation or for the expectationTarget of the considered intentExpectation.  E.g. the intentExpectation may be stated for a slice (type of Object) with identitier IIOT\_Atomotive\_2021 (identifier as context). Alternatively, the intentExpectation may be stated for a slice (type of Object) serving IIoT users (context 1) with slice profile supporting automotive connectivity (context 2).  ObjectContext may also be used to select a specific instance of Object, i.e., given the type of object in "ObjectType", the object instance is identified using the identifier of the object instance under Object context e.g. to refer to cell instance number 234, we state the Object context as {cell\_id, "=", 234}. The object identifier is in that case the context  allowedValues: depends on Object in the IntentExpectation | type: Context  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| expectionTargets | It describes the list of specific outcomes on metrics and observables related to the stated Object (e.g. the metrics that characterize the performance of the object(s) or some abstract index that expresses the behavior of the object(s)) that are desired to be realized for a given intentExpectation.  allowedValues: depends on Object in the IntentExpectation | type: expectationTarget  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| expectationContext | It describes the list of constraints and conditions that should apply for a specific intentExpectation. Note there may be other constraints and conditions defined for the entire intent or for specific parts of the intentExpectation.  allowedValues: depends on Object in the IntentExpectation | type: Context  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
| targetName | It describes a specific name of metric or observable related to the stated Object (e.g. the metrics that characterize the performance of the object(s) or some abstract index that expresses the behavior of the object(s))attribute of an object on which an outcomes may be stated  allowedValues: depends on Object in the IntentExpectation | type: string  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: Null  isNullable: True |
| targetCondition | It expresses the limits within which the targetName is allowed/supposed to be  allowedValues: is equal to; is less than; is greater than;  Note: Others conditions like "is within the range" or "is outside the range" can be expressed in terms of these basic conditions | type: enum  multiplicity: upto 2  isOrdered: False  isUnique: False  defaultValue: "is equal to"  isNullable: False |
| targetValueRange | It describes the range of values that applicable to the targetName and the TargetCondition. | type: FFS  multiplicity: upto 2  isOrdered: False  isUnique: False  defaultValue: Null  isNullable: True |
| targetContext | It describes the list of constraints and conditions that should apply for a specific expectationTarget. Note there may be other constraints and conditions defined for the entire intent or the intentExpectation.  allowedValues: triple of (attribute, condition, value range) | type: Context  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: None  isNullable: False |
|  |  |  |
| contextAttribute | It describes a specific attribute of or related to an object or to characteristics thereof (e.g. its control parameter, gauge, counter, KPI, weighted metric,, etc) or an attribute related to the operating conditions of the object (such as weather conditions, load conditions, etc). | type: String  multiplicity: 1  isOrdered: False  isUnique: False  defaultValue: Null  isNullable: True |
| contextCondition | It expresses the limits within which the ContextAttribute is allowed/supposed to be  allowedValues: is equal to; is less than; is greater than;  Note: Others conditions like "is within the range" or "is outside the range" can be expressed in terms of these basic conditions | type: enum  multiplicity: upto 2  isOrdered: False  isUnique: False  defaultValue: "is equal to"  isNullable: False |
| contextValueRange | It describes the range of values that explicatable to the ContextAttribute and the ContextCondition. | type: FFS  multiplicity: upto 2  isOrdered: False  isUnique: False  defaultValue: Null  isNullable: True |

|  |
| --- |
| **2nd Change** |

Annex <A> (informative):

Mapping the 3GPP and the TM Forum intentExpectation Models

The TM forum defines the structure of an intent as a list of expectations with each expectation containing the requirements goals and constraints to be achieved. The expectation is defined to contain 2 attributes - the imm:target and the imm:params. On the hand, the intentExpectation defined in 3GPP (see clause 6.2.1.2.2) contain more attributes some of which (the objectType, objectContexts, expectationTargets and expectationContexts)have the relation with TM Forum model.

Following the table to illustrate the attributes relation between 3GPP Intent Expectation and TM Forum IntentExpectation

|  |  |
| --- | --- |
| **3GPP Intent Expectation** | **TM Forum Intent Expectation** |
| **Class Property** | **Attribute** |
| objectType | imm:target |
| objectContexts | imm:params |
| expectationTargets |
| expectationContexts |



|  |
| --- |
| **End of changes** |