**3GPP TSG-SA5 Meeting #145-e *225082***

**, , – 24th Aug 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **0408** | **rev** | - | **Current version:** | 17.3.0 |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Rel-17 CR 32.291 Adding missing NodeFunctionality value for IMS | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Amdocs | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GIMSCH | | | | |  | ***Date:*** | | | 2022-07-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | NodeFunctionality is missing a value to describe IMS Node as CHF Consumer | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | NodeFunctioanlity is missing a value to describe “IMS Node” as CHF Consumer | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | There could be a confusion on the implementation of Node Functionality value between CHF and the consumer for IMS | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.6.3.4, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First change** |

##### 6.1.6.3.4 Enumeration: NodeFunctionality

Table 6.1.6.3.4-1: Enumeration NodeFunctionality

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| SMF | This field identifies that NF is a SMF. |  |
| AMF | This field identifies that NF is a AMF. |  |
| SMSF | This field identifies that NF service consumer is a SMSF. |  |
| PGW\_C\_SMF | This field identifies that NF is a SMF+PGW-C. |  |
| NEF | This field identifies that NF is a NEF. |  |
| SGW | This field identifies that node is an SGW, only applicable for interworking with EPC. |  |
| I\_SMF | This field identifies that node is an I-SMF, only applicable for PDU session served by SMF + I-SMF. | ETSUN |
| ePDG | This field identifies that node is an ePDG, only applicable for interworking with EPC/ePDG. | 5GIEPC\_CH |
| CEF | This field identifies that NF is a CEF. |  |
| MnS\_Producer | This field identifies that NF is a MnS Producer |  |
| SGSN | This field identifies that node is an SGSN, only applicable when SMF+PGW-C serves GERAN/UTRAN access. | TEI17\_NIESGU |
| V\_SMF | This field identifies that node is a V-SMF, may be used instead of SMF in roaming scenarios. |  |
| 5G DDNMF | This field identifies that NF is a 5G DDNMF | 5G ProSe |
| IMS\_Node | This field identifies that NF is an IMS Node. A further breakdown of IMS Node type may be available in IMS Charging Information | IMS |

|  |
| --- |
| **Second change** |

A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

title: Nchf\_ConvergedCharging

version: 3.1.0

description: |

ConvergedCharging Service © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 32.291 V17.3.0: Telecommunication management; Charging management;

5G system, charging service; Stage 3.

url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

- url: '{apiRoot}/nchf-convergedcharging/v3'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

- {}

- oAuth2ClientCredentials:

- nchf-convergedcharging

paths:

/chargingdata:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

responses:

'201':

description: Created

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataResponse'

'400':

description: Bad request

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'404':

description: Not Found

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'405':

$ref: 'TS29571\_CommonData.yaml#/components/responses/405'

'408':

$ref: 'TS29571\_CommonData.yaml#/components/responses/408'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

chargingNotification:

'{$request.body#/notifyUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingNotifyRequest'

responses:

'200':

description: OK.

content:

application/ json:

schema:

$ref: '#/components/schemas/ChargingNotifyResponse'

'204':

description: 'No Content, Notification was succesfull'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

description: Bad request

content:

application/problem+json:

schema:

oneOf:

- $ref: TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

- $ref: '#/components/schemas/ChargingNotifyResponse'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

'/chargingdata/{ChargingDataRef}/update':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

parameters:

- name: ChargingDataRef

in: path

description: a unique identifier for a charging data resource in a PLMN

required: true

schema:

type: string

responses:

'200':

description: OK. Updated Charging Data resource is returned

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataResponse'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

description: Bad request

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'404':

description: Not Found

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'405':

$ref: 'TS29571\_CommonData.yaml#/components/responses/405'

'408':

$ref: 'TS29571\_CommonData.yaml#/components/responses/408'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

'/chargingdata/{ChargingDataRef}/release':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

parameters:

- name: ChargingDataRef

in: path

description: a unique identifier for a charging data resource in a PLMN

required: true

schema:

type: string

responses:

'204':

description: No Content.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'404':

description: Not Found

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nchf-convergedcharging: Access to the Nchf\_ConvergedCharging API

schemas:

ChargingDataRequest:

type: object

properties:

subscriberIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

tenantIdentifier:

type: string

chargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

mnSConsumerIdentifier:

type: string

nfConsumerIdentification:

$ref: '#/components/schemas/NFIdentification'

invocationTimeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

invocationSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

retransmissionIndicator:

type: boolean

oneTimeEvent:

type: boolean

oneTimeEventType:

$ref: '#/components/schemas/oneTimeEventType'

notifyUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

serviceSpecificationInfo:

type: string

multipleUnitUsage:

type: array

items:

$ref: '#/components/schemas/MultipleUnitUsage'

minItems: 0

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

pDUSessionChargingInformation:

$ref: '#/components/schemas/PDUSessionChargingInformation'

roamingQBCInformation:

$ref: '#/components/schemas/RoamingQBCInformation'

sMSChargingInformation:

$ref: '#/components/schemas/SMSChargingInformation'

nEFChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

registrationChargingInformation:

$ref: '#/components/schemas/RegistrationChargingInformation'

n2ConnectionChargingInformation:

$ref: '#/components/schemas/N2ConnectionChargingInformation'

locationReportingChargingInformation:

$ref: '#/components/schemas/LocationReportingChargingInformation'

nSPAChargingInformation:

$ref: '#/components/schemas/NSPAChargingInformation'

nSMChargingInformation:

$ref: '#/components/schemas/NSMChargingInformation'

mMTelChargingInformation:

$ref: '#/components/schemas/MMTelChargingInformation'

iMSChargingInformation:

$ref: '#/components/schemas/IMSChargingInformation'

edgeInfrastructureUsageChargingInformation':

$ref: '#/components/schemas/EdgeInfrastructureUsageChargingInformation'

eASDeploymentChargingInformation:

$ref: '#/components/schemas/EASDeploymentChargingInformation'

directEdgeEnablingServiceChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

exposedEdgeEnablingServiceChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

proSeChargingInformation:

$ref: '#/components/schemas/ProseChargingInformation'

required:

- nfConsumerIdentification

- invocationTimeStamp

- invocationSequenceNumber

ChargingDataResponse:

type: object

properties:

invocationTimeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

invocationSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

invocationResult:

$ref: '#/components/schemas/InvocationResult'

sessionFailover:

$ref: '#/components/schemas/SessionFailover'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

multipleUnitInformation:

type: array

items:

$ref: '#/components/schemas/MultipleUnitInformation'

minItems: 0

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

pDUSessionChargingInformation:

$ref: '#/components/schemas/PDUSessionChargingInformation'

roamingQBCInformation:

$ref: '#/components/schemas/RoamingQBCInformation'

locationReportingChargingInformation:

$ref: '#/components/schemas/LocationReportingChargingInformation'

required:

- invocationTimeStamp

- invocationSequenceNumber

ChargingNotifyRequest:

type: object

properties:

notificationType:

$ref: '#/components/schemas/NotificationType'

reauthorizationDetails:

type: array

items:

$ref: '#/components/schemas/ReauthorizationDetails'

minItems: 0

required:

- notificationType

ChargingNotifyResponse:

type: object

properties:

invocationResult:

$ref: '#/components/schemas/InvocationResult'

NFIdentification:

type: object

properties:

nFName:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

nFIPv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

nFIPv6Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

nFPLMNID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

nodeFunctionality:

$ref: '#/components/schemas/NodeFunctionality'

nFFqdn:

type: string

required:

- nodeFunctionality

MultipleUnitUsage:

type: object

properties:

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

requestedUnit:

$ref: '#/components/schemas/RequestedUnit'

usedUnitContainer:

type: array

items:

$ref: '#/components/schemas/UsedUnitContainer'

minItems: 0

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

multihomedPDUAddress:

$ref: '#/components/schemas/PDUAddress'

required:

- ratingGroup

InvocationResult:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

failureHandling:

$ref: '#/components/schemas/FailureHandling'

Trigger:

type: object

properties:

triggerType:

$ref: '#/components/schemas/TriggerType'

triggerCategory:

$ref: '#/components/schemas/TriggerCategory'

timeLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

volumeLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

volumeLimit64:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

eventLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

maxNumberOfccc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

tariffTimeChange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

required:

- triggerType

- triggerCategory

MultipleUnitInformation:

type: object

properties:

resultCode:

$ref: '#/components/schemas/ResultCode'

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

grantedUnit:

$ref: '#/components/schemas/GrantedUnit'

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

validityTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

quotaHoldingTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

finalUnitIndication:

$ref: '#/components/schemas/FinalUnitIndication'

timeQuotaThreshold:

type: integer

volumeQuotaThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

unitQuotaThreshold:

type: integer

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

announcementInformation:

$ref: '#/components/schemas/AnnouncementInformation'

required:

- ratingGroup

RequestedUnit:

type: object

properties:

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

UsedUnitContainer:

type: object

properties:

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

quotaManagementIndicator:

$ref: '#/components/schemas/QuotaManagementIndicator'

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

triggerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

eventTimeStamps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

minItems: 0

localSequenceNumber:

type: integer

pDUContainerInformation:

$ref: '#/components/schemas/PDUContainerInformation'

nSPAContainerInformation:

$ref: '#/components/schemas/NSPAContainerInformation'

pC5ContainerInformation:

$ref: '#/components/schemas/PC5ContainerInformation'

required:

- localSequenceNumber

GrantedUnit:

type: object

properties:

tariffTimeChange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

FinalUnitIndication:

type: object

properties:

finalUnitAction:

$ref: '#/components/schemas/FinalUnitAction'

restrictionFilterRule:

$ref: '#/components/schemas/IPFilterRule'

restrictionFilterRuleList:

type: array

items:

$ref: '#/components/schemas/IPFilterRule'

minItems: 1

filterId:

type: string

filterIdList:

type: array

items:

type: string

minItems: 1

redirectServer:

$ref: '#/components/schemas/RedirectServer'

required:

- finalUnitAction

RedirectServer:

type: object

properties:

redirectAddressType:

$ref: '#/components/schemas/RedirectAddressType'

redirectServerAddress:

type: string

required:

- redirectAddressType

- redirectServerAddress

ReauthorizationDetails:

type: object

properties:

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

quotaManagementIndicator:

$ref: '#/components/schemas/QuotaManagementIndicator'

PDUSessionChargingInformation:

type: object

properties:

chargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

homeProvidedChargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

mAPDUNon3GPPUserLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

non3GPPUserLocationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

mAPDUNon3GPPUserLocationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

pduSessionInformation:

$ref: '#/components/schemas/PDUSessionInformation'

unitCountInactivityTimer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'  
 rANSecondaryRATUsageReport:

$ref: '#/components/schemas/RANSecondaryRATUsageReport'

UserInformation:

type: object

properties:

servedGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

servedPEI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

unauthenticatedFlag:

type: boolean

roamerInOut:

$ref: '#/components/schemas/RoamerInOut'

PDUSessionInformation:

type: object

properties:

networkSlicingInfo:

$ref: '#/components/schemas/NetworkSlicingInfo'

pduSessionID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

pduType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

sscMode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

hPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

servingNetworkFunctionID:

$ref: '#/components/schemas/ServingNetworkFunctionID'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

mAPDUNon3GPPRATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

dnnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

dnnSelectionMode:

$ref: '#/components/schemas/dnnSelectionMode'

chargingCharacteristics:

type: string

pattern: '^[0-9a-fA-F]{1,4}$'

chargingCharacteristicsSelectionMode:

$ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

stopTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

sessionStopIndicator:

type: boolean

pduAddress:

$ref: '#/components/schemas/PDUAddress'

diagnostics:

$ref: '#/components/schemas/Diagnostics'

authorizedQoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

subscribedQoSInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

authorizedSessionAMBR:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

subscribedSessionAMBR:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

servingCNPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

mAPDUSessionInformation:

$ref: '#/components/schemas/MAPDUSessionInformation'

enhancedDiagnostics:

$ref: '#/components/schemas/EnhancedDiagnostics5G'

redundantTransmissionType:

$ref: '#/components/schemas/RedundantTransmissionType'

pDUSessionPairID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

5GLANTypeService:

$ref: '#/components/schemas/5GLANTypeService'

required:

- pduSessionID

- dnnId

PDUContainerInformation:

type: object

properties:

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

afChargingIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

afChargingIdString:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNodeID:

type: array

items:

$ref: '#/components/schemas/ServingNetworkFunctionID'

minItems: 0

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

sponsorIdentity:

type: string

applicationserviceProviderIdentity:

type: string

chargingRuleBaseName:

type: string

mAPDUSteeringFunctionality:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

mAPDUSteeringMode:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringMode'

trafficForwardingWay:

$ref: '#/components/schemas/TrafficForwardingWay'

qosMonitoringReport:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 0

NSPAContainerInformation:

type: object

properties:

latency:

type: integer

throughput:

$ref: '#/components/schemas/Throughput'

maximumPacketLossRate:

type: string

serviceExperienceStatisticsData:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

theNumberOfPDUSessions:

type: integer

theNumberOfRegisteredSubscribers:

type: integer

loadLevel:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

NSPAChargingInformation:

type: object

properties:

singleNSSAI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- singleNSSAI

NetworkSlicingInfo:

type: object

properties:

sNSSAI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- sNSSAI

PDUAddress:

type: object

properties:

pduIPv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

pduIPv6AddresswithPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

pduAddressprefixlength:

type: integer

iPv4dynamicAddressFlag:

type: boolean

iPv6dynamicPrefixFlag:

type: boolean

addIpv6AddrPrefixes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

ServingNetworkFunctionID:

type: object

properties:

servingNetworkFunctionInformation:

$ref: '#/components/schemas/NFIdentification'

aMFId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

required:

- servingNetworkFunctionInformation

RoamingQBCInformation:

type: object

properties:

multipleQFIcontainer:

type: array

items:

$ref: '#/components/schemas/MultipleQFIcontainer'

minItems: 0

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

roamingChargingProfile:

$ref: '#/components/schemas/RoamingChargingProfile'

MultipleQFIcontainer:

type: object

properties:

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

triggerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

localSequenceNumber:

type: integer

qFIContainerInformation:

$ref: '#/components/schemas/QFIContainerInformation'

required:

- localSequenceNumber

QFIContainerInformation:

type: object

properties:

qFI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

reportTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNetworkFunctionID:

type: array

items:

$ref: '#/components/schemas/ServingNetworkFunctionID'

minItems: 0

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

3gppChargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

diagnostics:

$ref: '#/components/schemas/Diagnostics'

enhancedDiagnostics:

type: array

items:

type: string

required:

- reportTime

RoamingChargingProfile:

type: object

properties:

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

partialRecordMethod:

$ref: '#/components/schemas/PartialRecordMethod'

SMSChargingInformation:

type: object

properties:

originatorInfo:

$ref: '#/components/schemas/OriginatorInfo'

recipientInfo:

type: array

items:

$ref: '#/components/schemas/RecipientInfo'

minItems: 0

userEquipmentInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

roamerInOut:

$ref: '#/components/schemas/RoamerInOut'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

sMSCAddress:

type: string

sMDataCodingScheme:

type: integer

sMMessageType:

$ref: '#/components/schemas/SMMessageType'

sMReplyPathRequested:

$ref: '#/components/schemas/ReplyPathRequested'

sMUserDataHeader:

type: string

sMStatus:

type: string

pattern: '^[0-7]?[0-9a-fA-F]$'

sMDischargeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

numberofMessagesSent:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sMServiceType:

$ref: '#/components/schemas/SMServiceType'

sMSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sMSresult:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

submissionTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

sMPriority:

$ref: '#/components/schemas/SMPriority'

messageReference:

type: string

messageSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

messageClass:

$ref: '#/components/schemas/MessageClass'

deliveryReportRequested:

$ref: '#/components/schemas/DeliveryReportRequested'

OriginatorInfo:

type: object

properties:

originatorSUPI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

originatorGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

originatorOtherAddress:

$ref: '#/components/schemas/SMAddressInfo'

originatorReceivedAddress:

$ref: '#/components/schemas/SMAddressInfo'

originatorSCCPAddress:

type: string

sMOriginatorInterface:

$ref: '#/components/schemas/SMInterface'

sMOriginatorProtocolId:

type: string

RecipientInfo:

type: object

properties:

recipientSUPI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

recipientGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

recipientOtherAddress:

$ref: '#/components/schemas/SMAddressInfo'

recipientReceivedAddress:

$ref: '#/components/schemas/SMAddressInfo'

recipientSCCPAddress:

type: string

sMDestinationInterface:

$ref: '#/components/schemas/SMInterface'

sMrecipientProtocolId:

type: string

SMAddressInfo:

type: object

properties:

sMaddressType:

$ref: '#/components/schemas/SMAddressType'

sMaddressData:

type: string

sMaddressDomain:

$ref: '#/components/schemas/SMAddressDomain'

RecipientAddress:

type: object

properties:

recipientAddressInfo:

$ref: '#/components/schemas/SMAddressInfo'

sMaddresseeType:

$ref: '#/components/schemas/SMAddresseeType'

MessageClass:

type: object

properties:

classIdentifier:

$ref: '#/components/schemas/ClassIdentifier'

tokenText:

type: string

SMAddressDomain:

type: object

properties:

domainName:

type: string

3GPPIMSIMCCMNC:

type: string

SMInterface:

type: object

properties:

interfaceId:

type: string

interfaceText:

type: string

interfacePort:

type: string

interfaceType:

$ref: '#/components/schemas/InterfaceType'

RANSecondaryRATUsageReport:

type: object

properties:

rANSecondaryRATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

qosFlowsUsageReports:

type: array

items:

$ref: '#/components/schemas/QosFlowsUsageReport'

Diagnostics:

type: integer

IPFilterRule:

type: string

QosFlowsUsageReport:

type: object

properties:

qFI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

startTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

5GLANTypeService:

type: object

properties:

internalGroupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

NEFChargingInformation:

type: object

properties:

externalIndividualIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

externalGroupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

groupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

aPIDirection:

$ref: '#/components/schemas/APIDirection'

aPITargetNetworkFunction:

$ref: '#/components/schemas/NFIdentification'

aPIResultCode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

aPIName:

type: string

aPIReference:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

aPIContent:

type: string

required:

- aPIName

RegistrationChargingInformation:

type: object

properties:

registrationMessagetype:

$ref: '#/components/schemas/RegistrationMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pSCellInformation:

$ref: '#/components/schemas/PSCellInformation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

5GMMCapability:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

mICOModeIndication:

$ref: '#/components/schemas/MICOModeIndication'

smsIndication:

$ref: '#/components/schemas/SmsIndication'

taiList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 0

serviceAreaRestriction:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

minItems: 0

requestedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

allowedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

rejectedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

nSSAIMapList:

type: array

items:

$ref: '#/components/schemas/NSSAIMap'

minItems: 0

amfUeNgapId:

type: integer

ranUeNgapId:

type: integer

ranNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

required:

- registrationMessagetype

PSCellInformation:

type: object

properties:

nrcgi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

ecgi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

NSSAIMap:

type: object

properties:

servingSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

homeSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- servingSnssai

- homeSnssai

N2ConnectionChargingInformation:

type: object

properties:

n2ConnectionMessageType:

$ref: '#/components/schemas/N2ConnectionMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pSCellInformation:

$ref: '#/components/schemas/PSCellInformation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

amfUeNgapId:

type: integer

ranUeNgapId:

type: integer

ranNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

restrictedRatList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

minItems: 0

forbiddenAreaList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

minItems: 0

serviceAreaRestriction:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

minItems: 0

restrictedCnList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

minItems: 0

allowedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

rrcEstCause:

type: string

pattern: '^[0-9a-fA-F]+$'

required:

- n2ConnectionMessageType

LocationReportingChargingInformation:

type: object

properties:

locationReportingMessageType:

$ref: '#/components/schemas/LocationReportingMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pSCellInformation:

$ref: '#/components/schemas/PSCellInformation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

required:

- locationReportingMessageType

N2ConnectionMessageType:

type: integer

LocationReportingMessageType:

type: integer

NSMChargingInformation:

type: object

properties:

managementOperation:

$ref: '#/components/schemas/ManagementOperation'

idNetworkSliceInstance:

type: string

listOfserviceProfileChargingInformation:

type: array

items:

$ref: '#/components/schemas/ServiceProfileChargingInformation'

minItems: 0

managementOperationStatus:

$ref: '#/components/schemas/ManagementOperationStatus'

# To be introduced once the reference to 'generic.yaml is resolved

# managementOperationalState:

# $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

# managementAdministrativeState:

# $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

required:

- managementOperation

ServiceProfileChargingInformation:

type: object

properties:

serviceProfileIdentifier:

type: string

sNSSAIList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

# To be introduced once the reference to 'nrNrm.yaml is resolved

# sST:

# $ref: 'nrNrm.yaml#/components/schemas/Sst'

latency:

type: integer

availability:

type: number

# To be introduced once the reference to sliceNrm.yaml is resolved

# resourceSharingLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/SharingLevel'

jitter:

type: integer

reliability:

type: string

maxNumberofUEs:

type: integer

coverageArea:

type: string

# To be introduced once the reference to sliceNrm.yaml is resolved

# uEMobilityLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/MobilityLevel'

# delayToleranceIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

dLThptPerSlice:

$ref: '#/components/schemas/Throughput'

dLThptPerUE:

$ref: '#/components/schemas/Throughput'

uLThptPerSlice:

$ref: '#/components/schemas/Throughput'

uLThptPerUE:

$ref: '#/components/schemas/Throughput'

maxNumberofPDUsessions:

type: integer

kPIMonitoringList:

type: string

supportedAccessTechnology:

type: integer

# To be introduced once the reference to sliceNrm.yaml is resolved

# v2XCommunicationModeIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

addServiceProfileInfo:

type: string

Throughput:

type: object

properties:

guaranteedThpt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

maximumThpt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

MAPDUSessionInformation:

type: object

properties:

mAPDUSessionIndicator:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MaPduIndication'

aTSSSCapability:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AtsssCapability'

EnhancedDiagnostics5G:

$ref: '#/components/schemas/RanNasCauseList'

RanNasCauseList:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

QosMonitoringReport:

description: Contains reporting information on QoS monitoring.

type: object

properties:

ulDelays:

type: array

items:

type: integer

minItems: 0

dlDelays:

type: array

items:

type: integer

minItems: 0

rtDelays:

type: array

items:

type: integer

minItems: 0

AnnouncementInformation:

type: object

properties:

announcementIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

announcementReference:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

variableParts:

type: array

items:

$ref: '#/components/schemas/VariablePart'

minItems: 0

timeToPlay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

quotaConsumptionIndicator:

$ref: '#/components/schemas/QuotaConsumptionIndicator'

announcementPriority:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

playToParty:

$ref: '#/components/schemas/PlayToParty'

announcementPrivacyIndicator:

$ref: '#/components/schemas/AnnouncementPrivacyIndicator'

Language:

$ref: '#/components/schemas/Language'

VariablePart:

type: object

properties:

variablePartType:

$ref: '#/components/schemas/VariablePartType'

variablePartValue:

type: array

items:

type: string

minItems: 1

variablePartOrder:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

required:

- variablePartType

- variablePartValue

Language:

type: string

MMTelChargingInformation:

type: object

properties:

supplementaryServices:

type: array

items:

$ref: '#/components/schemas/SupplementaryService'

minItems: 1

SupplementaryService:

type: object

properties:

supplementaryServiceType:

$ref: '#/components/schemas/SupplementaryServiceType'

supplementaryServiceMode:

$ref: '#/components/schemas/SupplementaryServiceMode'

numberOfDiversions:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

associatedPartyAddress:

type: string

conferenceId:

type: string

participantActionType:

$ref: '#/components/schemas/ParticipantActionType'

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

numberOfParticipants:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

cUGInformation:

$ref: '#/components/schemas/OctetString'

IMSChargingInformation:

type: object

properties:

eventType:

$ref: '#/components/schemas/SIPEventType'

iMSNodeFunctionality:

$ref: '#/components/schemas/IMSNodeFunctionality'

roleOfNode:

$ref: '#/components/schemas/RoleOfIMSNode'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

isupCause:

$ref: '#/components/schemas/ISUPCause'

controlPlaneAddress:

$ref: '#/components/schemas/IMSAddress'

vlrNumber:

$ref: '#/components/schemas/E164'

mscAddress:

$ref: '#/components/schemas/E164'

userSessionID:

type: string

outgoingSessionID:

type: string

sessionPriority:

$ref: '#/components/schemas/IMSSessionPriority'

callingPartyAddresses:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

minItems: 1

calledPartyAddress:

type: string

numberPortabilityRoutinginformation:

type: string

carrierSelectRoutingInformation:

type: string

alternateChargedPartyAddress:

type: string

requestedPartyAddress:

type: array

items:

type: string

minItems: 1

calledAssertedIdentities:

type: array

items:

type: string

minItems: 1

calledIdentityChanges:

type: array

items:

$ref: '#/components/schemas/CalledIdentityChange'

minItems: 1

associatedURI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

minItems: 1

timeStamps:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

applicationServerInformation:

type: array

items:

type: string

minItems: 1

interOperatorIdentifier:

type: array

items:

$ref: '#/components/schemas/InterOperatorIdentifier'

minItems: 1

imsChargingIdentifier:

type: string

relatedICID:

type: string

relatedICIDGenerationNode:

type: string

transitIOIList:

type: array

items:

type: string

minItems: 1

earlyMediaDescription:

type: array

items:

$ref: '#/components/schemas/EarlyMediaDescription'

minItems: 1

sdpSessionDescription:

type: array

items:

type: string

minItems: 1

sdpMediaComponent:

type: array

items:

$ref: '#/components/schemas/SDPMediaComponent'

minItems: 1

servedPartyIPAddress:

$ref: '#/components/schemas/IMSAddress'

serverCapabilities:

$ref: '#/components/schemas/ServerCapabilities'

trunkGroupID:

$ref: '#/components/schemas/TrunkGroupID'

bearerService:

type: string

imsServiceId:

type: string

messageBodies:

type: array

items:

$ref: '#/components/schemas/MessageBody'

minItems: 1

accessNetworkInformation:

type: array

items:

type: string

minItems: 1

additionalAccessNetworkInformation:

type: string

cellularNetworkInformation:

type: string

accessTransferInformation:

type: array

items:

$ref: '#/components/schemas/AccessTransferInformation'

minItems: 1

accessNetworkInfoChange:

type: array

items:

$ref: '#/components/schemas/AccessNetworkInfoChange'

minItems: 1

imsCommunicationServiceID:

type: string

imsApplicationReferenceID:

type: string

causeCode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

reasonHeader:

type: array

items:

type: string

minItems: 1

initialIMSChargingIdentifier:

type: string

nniInformation:

type: array

items:

$ref: '#/components/schemas/NNIInformation'

minItems: 1

fromAddress:

type: string

imsEmergencyIndication:

type: boolean

imsVisitedNetworkIdentifier:

type: string

sipRouteHeaderReceived:

type: string

sipRouteHeaderTransmitted:

type: string

tadIdentifier:

$ref: '#/components/schemas/TADIdentifier'

feIdentifierList:

type: string

EdgeInfrastructureUsageChargingInformation:

type: object

properties:

meanVirtualCPUUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

meanVirtualMemoryUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

meanVirtualDiskUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

durationStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

durationEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

EASDeploymentChargingInformation:

type: object

properties:

# To be introduced once the reference to EdgeNrm.yaml is resolved

# eEASDeploymentRequirements:

# $ref: 'EdgeNrm.yaml#/components/schemas/EASRequirements'

lCMStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

lCMEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

PC5ContainerInformation:

type: object

properties:

coverageInfoList:

type: array

items:

$ref: '#/components/schemas/CoverageInfo'

radioParameterSetInfoList:

type: array

items:

$ref: '#/components/schemas/RadioParameterSetInfo'

transmitterInfoList:

type: array

items:

$ref: '#/components/schemas/TransmitterInfo'

minItems: 0

timeOfFirst Transmission:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeOfFirst Reception:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

CoverageInfo:

type: object

properties:

coverageStatus:

type: boolean

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

locationInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

minItems: 0

RadioParameterSetInfo:

type: object

properties:

radioParameterSetValues:

type: array

items:

$ref: '#/components/schemas/OctetString'

minItems: 0

changeTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

TransmitterInfo:

type: object

properties:

proseSourceIPAddress:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

proseSourceL2Id:

type: string

ProseChargingInformation:

type: object

properties:

announcingPlmnID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

announcingUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

announcingUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

monitoringUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

monitoringUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovererUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovererUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovereeUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovereeUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

monitoredPlmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

proseApplicationID:

type: string

ApplicationId:

type: string

applicationSpecificDataList:

type: array

items:

type: string

minItems: 0

proseFunctionality:

$ref: '#/components/schemas/ProseFunctionality'

proseEventType:

$ref: '#/components/schemas/ProseEventType'

directDiscoveryModel:

$ref: '#/components/schemas/DirectDiscoveryModel'

validityPeriod:

type: integer

roleOfUE:

$ref: '#/components/schemas/RoleOfUE'

proseRequestTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

pC3ProtocolCause:

type: integer

monitoringUEIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

requestedPLMNIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

timeWindow:

type: integer

rangeClass:

$ref: '#/components/schemas/RangeClass'

proximityAlertIndication:

type: boolean

proximityAlertTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

proximityCancellationTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

relayIPAddress:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

proseUEToNetworkRelayUEID :

type: string

proseDestinationLayer2ID:

type: string

pFIContainerInformation:

type: array

items:

$ref: '#/components/schemas/PFIContainerInformation'

minItems: 0

transmissionDataContainer:

type: array

items:

$ref: '#/components/schemas/PC5DataContainer'

minItems: 0

receptionDataContainer:

type: array

items:

$ref: '#/components/schemas/PC5DataContainer'

minItems: 0

required:

- aPIName

PFIContainerInformation:

type: object

properties:

pFI:

type: string

reportTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

PC5DataContainer:

type: object

properties:

localSequenceNumber:

type: string

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

coverageStatus:

type: boolean

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

dataVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

changeCondition:

type: string

radioResourcesId:

$ref: '#/components/schemas/RadioResourcesId'

radioFrequency:

type: string

pC5RadioTechnology:

type: string

OctetString:

type: string

pattern: '^[0-9a-fA-F]+$'

E164:

type: string

pattern: '^[0-9a-fA-F]+$'

IMSAddress:

type: object

properties:

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

e164:

$ref: '#/components/schemas/E164'

anyOf:

- required: [ ipv4Addr ]

- required: [ ipv6Addr ]

- required: [ e164 ]

ServingNodeAddress:

type: object

properties:

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

anyOf:

- required: [ ipv4Addr ]

- required: [ ipv6Addr ]

SIPEventType:

type: object

properties:

sIPMethod:

type: string

eventHeader:

type: string

expiresHeader:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

ISUPCause:

type: object

properties:

iSUPCauseLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

iSUPCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

iSUPCauseDiagnostics:

$ref: '#/components/schemas/OctetString'

CalledIdentityChange:

type: object

properties:

calledIdentity:

type: string

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

InterOperatorIdentifier:

type: object

properties:

originatingIOI:

type: string

terminatingIOI:

type: string

EarlyMediaDescription:

type: object

properties:

sDPTimeStamps:

$ref: '#/components/schemas/SDPTimeStamps'

sDPMediaComponent:

type: array

items:

$ref: '#/components/schemas/SDPMediaComponent'

minItems: 0

sDPSessionDescription:

type: array

items:

type: string

minItems: 0

SDPTimeStamps:

type: object

properties:

sDPOfferTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

sDPAnswerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

SDPMediaComponent:

type: object

properties:

sDPMediaName:

type: string

SDPMediaDescription:

type: array

items:

type: string

minItems: 0

localGWInsertedIndication:

type: boolean

ipRealmDefaultIndication:

type: boolean

transcoderInsertedIndication:

type: boolean

mediaInitiatorFlag:

$ref: '#/components/schemas/MediaInitiatorFlag'

mediaInitiatorParty:

type: string

threeGPPChargingId:

$ref: '#/components/schemas/OctetString'

accessNetworkChargingIdentifierValue:

$ref: '#/components/schemas/OctetString'

sDPType:

$ref: '#/components/schemas/SDPType'

ServerCapabilities:

type: object

properties:

mandatoryCapability:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

minItems: 0

optionalCapability :

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

minItems: 0

serverName:

type: array

items:

type: string

minItems: 0

TrunkGroupID:

type: object

properties:

incomingTrunkGroupID:

type: string

outgoingTrunkGroupID:

type: string

MessageBody:

type: object

properties:

contentType:

type: string

contentLength:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

contentDisposition:

type: string

originator:

$ref: '#/components/schemas/OriginatorPartyType'

required:

- contentType

- contentLength

AccessTransferInformation:

type: object

properties:

accessTransferType:

$ref: '#/components/schemas/AccessTransferType'

accessNetworkInformation:

type: array

items:

$ref: '#/components/schemas/OctetString'

minItems: 0

cellularNetworkInformation:

$ref: '#/components/schemas/OctetString'

interUETransfer:

$ref: '#/components/schemas/UETransferType'

userEquipmentInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

instanceId:

type: string

relatedIMSChargingIdentifier:

type: string

relatedIMSChargingIdentifierNode:

$ref: '#/components/schemas/IMSAddress'

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

AccessNetworkInfoChange:

type: object

properties:

accessNetworkInformation:

type: array

items:

$ref: '#/components/schemas/OctetString'

minItems: 0

cellularNetworkInformation:

$ref: '#/components/schemas/OctetString'

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

NNIInformation:

type: object

properties:

sessionDirection:

$ref: '#/components/schemas/NNISessionDirection'

nNIType:

$ref: '#/components/schemas/NNIType'

relationshipMode:

$ref: '#/components/schemas/NNIRelationshipMode'

neighbourNodeAddress:

$ref: '#/components/schemas/IMSAddress'

NotificationType:

anyOf:

- type: string

enum:

- REAUTHORIZATION

- ABORT\_CHARGING

- type: string

NodeFunctionality:

anyOf:

- type: string

enum:

- AMF

- SMF

- SMS

- PGW\_C\_SMF

- NEFF # Included for backwards compatibility, shall not be used

- SGW

- I\_SMF

- ePDG

- CEF

- NEF

- MnS\_Producer

- SGSN

- IMS\_Node - type: string

ChargingCharacteristicsSelectionMode:

anyOf:

- type: string

enum:

- HOME\_DEFAULT

- ROAMING\_DEFAULT

- VISITING\_DEFAULT

- type: string

TriggerType:

anyOf:

- type: string

enum:

- QUOTA\_THRESHOLD

- QHT

- FINAL

- QUOTA\_EXHAUSTED

- VALIDITY\_TIME

- OTHER\_QUOTA\_TYPE

- FORCED\_REAUTHORISATION

- UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

- UNIT\_COUNT\_INACTIVITY\_TIMER

- ABNORMAL\_RELEASE

- QOS\_CHANGE

- VOLUME\_LIMIT

- TIME\_LIMIT

- EVENT\_LIMIT

- PLMN\_CHANGE

- USER\_LOCATION\_CHANGE

- RAT\_CHANGE

- SESSION\_AMBR\_CHANGE

- UE\_TIMEZONE\_CHANGE

- TARIFF\_TIME\_CHANGE

- MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

- MANAGEMENT\_INTERVENTION

- CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

- CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

- SERVING\_NODE\_CHANGE

- REMOVAL\_OF\_UPF

- ADDITION\_OF\_UPF

- INSERTION\_OF\_ISMF

- REMOVAL\_OF\_ISMF

- CHANGE\_OF\_ISMF

- START\_OF\_SERVICE\_DATA\_FLOW

- ECGI\_CHANGE

- TAI\_CHANGE

- HANDOVER\_CANCEL

- HANDOVER\_START

- HANDOVER\_COMPLETE

- GFBR\_GUARANTEED\_STATUS\_CHANGE

- ADDITION\_OF\_ACCESS

- REMOVAL\_OF\_ACCESS

- START\_OF\_SDF\_ADDITIONAL\_ACCESS

- REDUNDANT\_TRANSMISSION\_CHANGE

- CGI\_SAI\_CHANGE

- RAI\_CHANGE

- type: string

FinalUnitAction:

anyOf:

- type: string

enum:

- TERMINATE

- REDIRECT

- RESTRICT\_ACCESS

- type: string

RedirectAddressType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- URL

- URI

- type: string

TriggerCategory:

anyOf:

- type: string

enum:

- IMMEDIATE\_REPORT

- DEFERRED\_REPORT

- type: string

QuotaManagementIndicator:

anyOf:

- type: string

enum:

- ONLINE\_CHARGING

- OFFLINE\_CHARGING

- QUOTA\_MANAGEMENT\_SUSPENDED

- type: string

FailureHandling:

anyOf:

- type: string

enum:

- TERMINATE

- CONTINUE

- RETRY\_AND\_TERMINATE

- type: string

SessionFailover:

anyOf:

- type: string

enum:

- FAILOVER\_NOT\_SUPPORTED

- FAILOVER\_SUPPORTED

- type: string

3GPPPSDataOffStatus:

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

ResultCode:

anyOf:

- type: string

enum:

- SUCCESS

- END\_USER\_SERVICE\_DENIED

- QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

- QUOTA\_LIMIT\_REACHED

- END\_USER\_SERVICE\_REJECTED

- USER\_UNKNOWN

- RATING\_FAILED

- QUOTA\_MANAGEMENT

- type: string

PartialRecordMethod:

anyOf:

- type: string

enum:

- DEFAULT

- INDIVIDUAL

- type: string

RoamerInOut:

anyOf:

- type: string

enum:

- IN\_BOUND

- OUT\_BOUND

- type: string

SMMessageType:

anyOf:

- type: string

enum:

- SUBMISSION

- DELIVERY\_REPORT

- SM\_SERVICE\_REQUEST

- DELIVERY

- type: string

SMPriority:

anyOf:

- type: string

enum:

- LOW

- NORMAL

- HIGH

- type: string

DeliveryReportRequested:

anyOf:

- type: string

enum:

- YES

- NO

- type: string

InterfaceType:

anyOf:

- type: string

enum:

- UNKNOWN

- MOBILE\_ORIGINATING

- MOBILE\_TERMINATING

- APPLICATION\_ORIGINATING

- APPLICATION\_TERMINATING

- type: string

ClassIdentifier:

anyOf:

- type: string

enum:

- PERSONAL

- ADVERTISEMENT

- INFORMATIONAL

- AUTO

- type: string

SMAddressType:

anyOf:

- type: string

enum:

- EMAIL\_ADDRESS

- MSISDN

- IPV4\_ADDRESS

- IPV6\_ADDRESS

- NUMERIC\_SHORTCODE

- ALPHANUMERIC\_SHORTCODE

- OTHER

- IMSI

- type: string

SMAddresseeType:

anyOf:

- type: string

enum:

- TO

- CC

- BCC

- type: string

SMServiceType:

anyOf:

- type: string

enum:

- VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

- VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

- VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

- VAS4SMS\_SHORT\_MESSAGE\_FILTERING

- VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

- VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

- VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

- VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

- VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

- VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

- VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

- type: string

ReplyPathRequested:

anyOf:

- type: string

enum:

- NO\_REPLY\_PATH\_SET

- REPLY\_PATH\_SET

- type: string

oneTimeEventType:

anyOf:

- type: string

enum:

- IEC

- PEC

- type: string

dnnSelectionMode:

anyOf:

- type: string

enum:

- VERIFIED

- UE\_DNN\_NOT\_VERIFIED

- NW\_DNN\_NOT\_VERIFIED

- type: string

APIDirection:

anyOf:

- type: string

enum:

- INVOCATION

- NOTIFICATION

- type: string

RegistrationMessageType:

anyOf:

- type: string

enum:

- INITIAL

- MOBILITY

- PERIODIC

- EMERGENCY

- DEREGISTRATION

- type: string

MICOModeIndication:

anyOf:

- type: string

enum:

- MICO\_MODE

- NO\_MICO\_MODE

- type: string

SmsIndication:

anyOf:

- type: string

enum:

- SMS\_SUPPORTED

- SMS\_NOT\_SUPPORTED

- type: string

ManagementOperation:

anyOf:

- type: string

enum:

- CreateMOI

- ModifyMOIAttributes

- DeleteMOI

- type: string

ManagementOperationStatus:

anyOf:

- type: string

enum:

- OPERATION\_SUCCEEDED

- OPERATION\_FAILED

- type: string

RedundantTransmissionType:

anyOf:

- type: string

enum:

- NON\_TRANSMISSION

- END\_TO\_END\_USER\_PLANE\_PATHS

- N3/N9

- TRANSPORT\_LAYER

- type: string

VariablePartType:

anyOf:

- type: string

enum:

- INTEGER

- NUMBER

- TIME

- DATE

- CURRENCY

- type: string

QuotaConsumptionIndicator:

anyOf:

- type: string

enum:

- QUOTA\_NOT\_USED

- QUOTA\_IS\_USED

- type: string

PlayToParty:

anyOf:

- type: string

enum:

- SERVED

- REMOTE

- type: string

AnnouncementPrivacyIndicator:

anyOf:

- type: string

enum:

- NOT\_PRIVATE

- PRIVATE

- type: string

SupplementaryServiceType:

anyOf:

- type: string

enum:

- OIP

- OIR

- TIP

- TIR

- HOLD

- CB

- CDIV

- CW

- MWI

- CONF

- FA

- CCBS

- CCNR

- MCID

- CAT

- CUG

- PNM

- CRS

- ECT

- type: string

SupplementaryServiceMode:

anyOf:

- type: string

enum:

- CFU

- CFB

- CFNR

- CFNL

- CD

- CFNRC

- ICB

- OCB

- ACR

- BLIND\_TRANFER

- CONSULTATIVE\_TRANFER

- type: string

ParticipantActionType:

anyOf:

- type: string

enum:

- CREATE

- JOIN

- INVITE\_INTO

- QUIT

- type: string

TrafficForwardingWay:

anyOf:

- type: string

enum:

- N6

- N19

- LOCAL\_SWITCH

- type: string

IMSNodeFunctionality:

anyOf:

- type: string

enum:

- S\_CSCF

- P\_CSCF

- I\_CSCF

- MRFC

- MGCF

- BGCF

- AS

- IBCF

- S-GW

- P-GW

- HSGW

- E-CSCF

- MME

- TRF

- TF

- ATCF

- PROXY

- EPDG

- TDF

- TWAG

- SCEF

- IWK\_SCEF

- type: string

RoleOfIMSNode:

anyOf:

- type: string

enum:

- ORIGINATING

- TERMINATING

- FORWARDING

- type: string

IMSSessionPriority:

anyOf:

- type: string

enum:

- PRIORITY\_0

- PRIORITY\_1

- PRIORITY\_2

- PRIORITY\_3

- PRIORITY\_4

- type: string

MediaInitiatorFlag:

anyOf:

- type: string

enum:

- CALLED\_PARTY

- CALLING\_PARTY

- UNKNOWN

- type: string

SDPType:

anyOf:

- type: string

enum:

- OFFER

- ANSWER

- type: string

OriginatorPartyType:

anyOf:

- type: string

enum:

- CALLING

- CALLED

- type: string

AccessTransferType:

anyOf:

- type: string

enum:

- PS\_TO\_CS

- CS\_TO\_PS

- PS\_TO\_PS

- CS\_TO\_CS

- type: string

UETransferType:

anyOf:

- type: string

enum:

- INTRA\_UE

- INTER\_UE

- type: string

NNISessionDirection:

anyOf:

- type: string

enum:

- INBOUND

- OUTBOUND

- type: string

NNIType:

anyOf:

- type: string

enum:

- NON\_ROAMING

- ROAMING\_NO\_LOOPBACK

- ROAMING\_LOOPBACK

- type: string

NNIRelationshipMode:

anyOf:

- type: string

enum:

- TRUSTED

- NON\_TRUSTED

- type: string

TADIdentifier:

anyOf:

- type: string

enum:

- CS

- PS

- type: string

ProseFunctionality:

anyOf:

- type: string

enum:

- DIRECT\_DISCOVERY

- DIRECT\_COMMUNICATION

- type: string

ProseEventType:

anyOf:

- type: string

enum:

- ANNOUNCING

- MONITORING

- MATCH\_REPORT

- type: string

DirectDiscoveryModel:

anyOf:

- type: string

enum:

- MODEL\_A

- MODEL\_B

- type: string

RoleOfUE:

anyOf:

- type: string

enum:

- ANNOUNCING\_UE

- MONITORING\_UE

- REQUESTOR\_UE

- REQUESTED\_UE

- type: string

RangeClass:

anyOf:

- type: string

enum:

- RESERVED

- 50\_METER

- 100\_METER

- 200\_METER

- 500\_METER

- 1000\_METER

- UNUSED

- type: string

RadioResourcesId:

anyOf:

- type: string

enum:

- OPERATOR\_PROVIDED

- CONFIGURED

- type: string

|  |
| --- |
| **End of changes** |