**3GPP TSG-SA5 Meeting #145-e *S5-225348***

**e-meeting, 15 Aug – 24 Aug 2022**

**Source: Amdocs**

**Title: Adding potential solution for locating a cancel failed event**

**Document for: Approval**

**Agenda Item: 7.5.2**

# 1 Decision/action requested

**Include the proposed changes in TR 28.826.**

# 2 References

[1] 3GPP TR 28.826: " Study on Nchf charging services phase 2 improvements and optimizations"

# 3 Rationale

Adding a potential solution for key issue #4a, addressing how to locate the event that should be cancelled.

# 4 Detailed proposal

|  |
| --- |
| **First change** |

#### 5.4.5.x Solutions #4.x: Cancelling using a reference identifier for Charging Event

A possible solution for key issues 4a, covering requirements **REQ-3GPPCH-ESC-01**, cancelling of event would be to add a reference identifier (e.g. refundInformation) in Charging Data Response -> multipleUnitInformation for IEC, that can later be sent back in Charging Data Request -> multipleUnitUsage, to identify the event to be cancelled or refunded



|  |
| --- |
| **End of changes** |