**3GPP TSG-SA5 Meeting #148e *S5-233257***

**Online, ,17 April 2023 – 25 April 2023**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.291** | **CR** |  **0468** | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-17 CR 32.291 Update EAS Infrastructure Usage Charging Information |
|  |  |
| ***Source to WG:*** | Amdocs |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | EDGE\_CH |  | ***Date:*** | 2023-04-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The data type for mean CPU, disk and memory usage does not the match the corresponding definitions in TS 28.552. Also, the edge infrastructure usage charging information is missing data volumes specified in TS 32.257  |
|  |  |
| ***Summary of change:*** | Use Integer data type for mean CPU, disk and memory usage. Also, add incoming and outgoing data volumes in the edge infrastructure usage charging information |
|  |  |
| ***Consequences if not approved:*** | There can be confusion on the implementation of EAS Infrastructure Usage Charging events between CHF and consumers. |
|  |  |
| ***Clauses affected:*** | 6.1.6.2.12.3, 7.10, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** | **X** |  |  O&M Specifications | TS 32.257 CR 0007 TS 32.298 CR 0931 |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

###### 6.1.6.2.12.3 Type EdgeInfrastructureUsageChargingInformation

Table  6.1.6.2.12.3-2: Definition of type EdgeInfrastructureUsageChargingInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| meanVirtualCPUUsage | Integer |  OM | 0..1 | This field holds the information of mean virtual CPU usage for the EAS, see VR.VCpuUsageMean in clause 5.7.1.1.1 of T TS 28.552 [263]. |  |
| meanVirtualMemoryUsage | Integer |  OM | 0..1 | This field holds the information of mean virtual memory usage for the EAS, see VR.VMemoryUsageMean in clause 5.7.1.2.1 of TS 28.552 [263]. |  |
| meanVirtualDiskUsage | Integer |  OM | 0..1 | This field holds the information of mean virtual disk usage for the EAS, see VR.VDiskUsageMean in clause 5.7.1.2.1 of TS 28.552 [263]. |  |
| incomingDataVolume | Integer | OM | 0..1 | This field holds the information of number of incoming bytes received by the EAS, See DataVolum.InBytesEAS in clause 5.7.2.1 of 3GPP TS 28.552 [263] |  |
| outgoingDataVolume | Integer | OM | 0..1 | This field holds the information of number of outgoing bytes transmitted from the EAS, see DataVolum.OutBytesEAS in clause 5.7.2.2 of 3GPP TS 28.552 [263] |  |
| durationStartTime | DateTime | OC | 0..1 | This field holds the start time of the collection period, see TS 28.550 [262]. |  |
| durationEndTime | DateTime | OC | 0..1 | This field holds the end time of the collection period, see TS 28.550 [262]. |  |

|  |
| --- |
| **Second change** |

## 7.10 Bindings for Edge Computing domain charging

Table 7.10-1: Bindings of Edge Computing domain charging CDR field, Information Element and Resource Attribute

| Information Element | CDR Field | Resource Attribute |
| --- | --- | --- |
|  |  | **ChargingDataRequest** |
| EAS ID | EAS ID | /eASID |
| EDN ID | EDN ID | /eDNID |
| EAS Provider Identifier | EAS Provider Identifier | /eASProviderIdentifier |
| Edge Enabling Infrastructure Resource Usage Charging Information | Edge Enabling Infrastructure Resource Usage Charging Information | /edgeInfrastructureUsageChargingInformation |
| Mean Virtual CPU Usage | Mean Virtual CPU Usage | /edgeInfrastructureUsageChargingInformation/meanVirtualCPUUsage |
| Mean Virtual Memory Usage | Mean Virtual Memory Usage | /edgeInfrastructureUsageChargingInformation/meanVirtualMemoryUsage |
| Mean Virtual Disk Usage | Mean Virtual Disk Usage | /edgeInfrastructureUsageChargingInformation/meanVirtualDiskUsage |
| Incoming Data Volume | Incoming Data Volume | /edgeInfrastructureUsageChargingInformation/incomingDataVolume |
| Outgoing Data Volume | Outgoing Data Volume | /edgeInfrastructureUsageChargingInformation/outgoingDataVolume |
| Duration Start Time | Duration Start Time | /edgeInfrastructureUsageChargingInformation/durationStartTime |
| Duration End Time | Duration End Time | /edgeInfrastructureUsageChargingInformation/durationEndTime |
| EAS Deployment Charging Information | EAS Deployment Charging Information | /eASDeploymentChargingInformation |
| EAS Deployment Requirements | EAS Deployment Requirements | /eASDeploymentChargingInformation/eASDeploymentRequirements |
| LCM Start Time | LCM Start Time | /eASDeploymentChargingInformation/lCMStartTime |
| LCM End Time | LCM End Time | /eASDeploymentChargingInformation/lCMEndTime |
| Direct Edge Enabling Service Charging Information | Exposure Function API Information | /nEFChargingInformation |
| Exposed Edge Enabling Service Charging Information | Exposure Function API Information  | /nEFChargingInformation |
|  |  | **ChargingDataResponse** |

|  |
| --- |
| **Third change** |

## A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

 title: Nchf\_ConvergedCharging

 version: 3.1.3

 description: |

 ConvergedCharging Service © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 32.291 V17.6.0: Telecommunication management; Charging management;

 5G system, charging service; Stage 3.

 url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

 - url: '{apiRoot}/nchf-convergedcharging/v3'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

 - {}

 - oAuth2ClientCredentials:

 - nchf-convergedcharging

paths:

 /chargingdata:

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '405':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/405'

 '408':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/408'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 chargingNotification:

 '{$request.body#/notifyUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingNotifyRequest'

 responses:

 '200':

 description: OK.

 content:

 application/ json:

 schema:

 $ref: '#/components/schemas/ChargingNotifyResponse'

 '204':

 description: 'No Content, Notification was succesfull'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

 - $ref: '#/components/schemas/ChargingNotifyResponse'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated Charging Data resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '405':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/405'

 '408':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/408'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/release':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nchf-convergedcharging: Access to the Nchf\_ConvergedCharging API

 schemas:

 ChargingDataRequest:

 type: object

 properties:

 subscriberIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 tenantIdentifier:

 type: string

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 mnSConsumerIdentifier:

 type: string

 nfConsumerIdentification:

 $ref: '#/components/schemas/NFIdentification'

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 retransmissionIndicator:

 type: boolean

 oneTimeEvent:

 type: boolean

 oneTimeEventType:

 $ref: '#/components/schemas/oneTimeEventType'

 notifyUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 serviceSpecificationInfo:

 type: string

 multipleUnitUsage:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitUsage'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 easid:

 type: string

 ednid:

 type: string

 eASProviderIdentifier:

 type: string

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 sMSChargingInformation:

 $ref: '#/components/schemas/SMSChargingInformation'

 nEFChargingInformation:

 $ref: '#/components/schemas/NEFChargingInformation'

 registrationChargingInformation:

 $ref: '#/components/schemas/RegistrationChargingInformation'

 n2ConnectionChargingInformation:

 $ref: '#/components/schemas/N2ConnectionChargingInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 nSPAChargingInformation:

 $ref: '#/components/schemas/NSPAChargingInformation'

 nSMChargingInformation:

 $ref: '#/components/schemas/NSMChargingInformation'

 mMTelChargingInformation:

 $ref: '#/components/schemas/MMTelChargingInformation'

 iMSChargingInformation:

 $ref: '#/components/schemas/IMSChargingInformation'

 edgeInfrastructureUsageChargingInformation':

 $ref: '#/components/schemas/EdgeInfrastructureUsageChargingInformation'

 eASDeploymentChargingInformation:

 $ref: '#/components/schemas/EASDeploymentChargingInformation'

 directEdgeEnablingServiceChargingInformation:

 $ref: '#/components/schemas/NEFChargingInformation'

 exposedEdgeEnablingServiceChargingInformation:

 $ref: '#/components/schemas/NEFChargingInformation'

 proSeChargingInformation:

 $ref: '#/components/schemas/ProseChargingInformation'

 required:

 - nfConsumerIdentification

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingDataResponse:

 type: object

 properties:

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 sessionFailover:

 $ref: '#/components/schemas/SessionFailover'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 multipleUnitInformation:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitInformation'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 required:

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingNotifyRequest:

 type: object

 properties:

 notificationType:

 $ref: '#/components/schemas/NotificationType'

 reauthorizationDetails:

 type: array

 items:

 $ref: '#/components/schemas/ReauthorizationDetails'

 minItems: 0

 required:

 - notificationType

 ChargingNotifyResponse:

 type: object

 properties:

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 NFIdentification:

 type: object

 properties:

 nFName:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nFIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 nFIPv6Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 nFPLMNID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 nodeFunctionality:

 $ref: '#/components/schemas/NodeFunctionality'

 nFFqdn:

 type: string

 required:

 - nodeFunctionality

 MultipleUnitUsage:

 type: object

 properties:

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 requestedUnit:

 $ref: '#/components/schemas/RequestedUnit'

 usedUnitContainer:

 type: array

 items:

 $ref: '#/components/schemas/UsedUnitContainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 multihomedPDUAddress:

 $ref: '#/components/schemas/PDUAddress'

 required:

 - ratingGroup

 InvocationResult:

 type: object

 properties:

 error:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 failureHandling:

 $ref: '#/components/schemas/FailureHandling'

 Trigger:

 type: object

 properties:

 triggerType:

 $ref: '#/components/schemas/TriggerType'

 triggerCategory:

 $ref: '#/components/schemas/TriggerCategory'

 timeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 volumeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 volumeLimit64:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 maxNumberOfccc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 required:

 - triggerType

 - triggerCategory

 MultipleUnitInformation:

 type: object

 properties:

 resultCode:

 $ref: '#/components/schemas/ResultCode'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 grantedUnit:

 $ref: '#/components/schemas/GrantedUnit'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 validityTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 quotaHoldingTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 finalUnitIndication:

 $ref: '#/components/schemas/FinalUnitIndication'

 timeQuotaThreshold:

 type: integer

 volumeQuotaThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 unitQuotaThreshold:

 type: integer

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 announcementInformation:

 $ref: '#/components/schemas/AnnouncementInformation'

 required:

 - ratingGroup

 RequestedUnit:

 type: object

 properties:

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 UsedUnitContainer:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventTimeStamps:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 0

 localSequenceNumber:

 type: integer

 pDUContainerInformation:

 $ref: '#/components/schemas/PDUContainerInformation'

 nSPAContainerInformation:

 $ref: '#/components/schemas/NSPAContainerInformation'

 pC5ContainerInformation:

 $ref: '#/components/schemas/PC5ContainerInformation'

 required:

 - localSequenceNumber

 GrantedUnit:

 type: object

 properties:

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 FinalUnitIndication:

 type: object

 properties:

 finalUnitAction:

 $ref: '#/components/schemas/FinalUnitAction'

 restrictionFilterRule:

 $ref: '#/components/schemas/IPFilterRule'

 restrictionFilterRuleList:

 type: array

 items:

 $ref: '#/components/schemas/IPFilterRule'

 minItems: 1

 filterId:

 type: string

 filterIdList:

 type: array

 items:

 type: string

 minItems: 1

 redirectServer:

 $ref: '#/components/schemas/RedirectServer'

 required:

 - finalUnitAction

 RedirectServer:

 type: object

 properties:

 redirectAddressType:

 $ref: '#/components/schemas/RedirectAddressType'

 redirectServerAddress:

 type: string

 required:

 - redirectAddressType

 - redirectServerAddress

 ReauthorizationDetails:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 PDUSessionChargingInformation:

 type: object

 properties:

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 sMFchargingId:

 type: string

 homeProvidedChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 sMFHomeProvidedChargingId:

 type: string

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 mAPDUNon3GPPUserLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 non3GPPUserLocationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 mAPDUNon3GPPUserLocationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 pduSessionInformation:

 $ref: '#/components/schemas/PDUSessionInformation'

 unitCountInactivityTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'
 rANSecondaryRATUsageReport:

 $ref: '#/components/schemas/RANSecondaryRATUsageReport'

 UserInformation:

 type: object

 properties:

 servedGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 servedPEI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 unauthenticatedFlag:

 type: boolean

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 PDUSessionInformation:

 type: object

 properties:

 networkSlicingInfo:

 $ref: '#/components/schemas/NetworkSlicingInfo'

 pduSessionID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 pduType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 sscMode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

 hPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 servingNetworkFunctionID:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 mAPDUNon3GPPRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 dnnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 dnnSelectionMode:

 $ref: '#/components/schemas/dnnSelectionMode'

 chargingCharacteristics:

 type: string

 pattern: '^[0-9a-fA-F]{1,4}$'

 chargingCharacteristicsSelectionMode:

 $ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 stopTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sessionStopIndicator:

 type: boolean

 pduAddress:

 $ref: '#/components/schemas/PDUAddress'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 authorizedQoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

 subscribedQoSInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

 authorizedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 subscribedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 servingCNPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 mAPDUSessionInformation:

 $ref: '#/components/schemas/MAPDUSessionInformation'

 enhancedDiagnostics:

 $ref: '#/components/schemas/EnhancedDiagnostics5G'

 redundantTransmissionType:

 $ref: '#/components/schemas/RedundantTransmissionType'

 pDUSessionPairID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 cpCIoTOptimisationIndicator:

 type: boolean

 5GSControlPlaneOnlyIndicator:

 type: boolean

 smallDataRateControlIndicator:

 type: boolean

 5GLANTypeService:

 $ref: '#/components/schemas/5GLANTypeService'

 required:

 - pduSessionID

 - dnnId

 PDUContainerInformation:

 type: object

 properties:

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 afChargingIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 afChargingIdString:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNodeID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sponsorIdentity:

 type: string

 applicationserviceProviderIdentity:

 type: string

 chargingRuleBaseName:

 type: string

 mAPDUSteeringFunctionality:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

 mAPDUSteeringMode:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringMode'

 trafficForwardingWay:

 $ref: '#/components/schemas/TrafficForwardingWay'

 qosMonitoringReport:

 type: array

 items:

 $ref: '#/components/schemas/QosMonitoringReport'

 minItems: 0

 NSPAContainerInformation:

 type: object

 properties:

 latency:

 type: integer

 throughput:

 $ref: '#/components/schemas/Throughput'

 maximumPacketLossRate:

 type: string

 serviceExperienceStatisticsData:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

 theNumberOfPDUSessions:

 type: integer

 theNumberOfRegisteredSubscribers:

 type: integer

 loadLevel:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

 NSPAChargingInformation:

 type: object

 properties:

 singleNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - singleNSSAI

 NetworkSlicingInfo:

 type: object

 properties:

 sNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - sNSSAI

 PDUAddress:

 type: object

 properties:

 pduIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 pduIPv6AddresswithPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 pduAddressprefixlength:

 type: integer

 iPv4dynamicAddressFlag:

 type: boolean

 iPv6dynamicPrefixFlag:

 type: boolean

 addIpv6AddrPrefixes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 addIpv6AddrPrefixList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 ServingNetworkFunctionID:

 type: object

 properties:

 servingNetworkFunctionInformation:

 $ref: '#/components/schemas/NFIdentification'

 aMFId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

 required:

 - servingNetworkFunctionInformation

 RoamingQBCInformation:

 type: object

 properties:

 multipleQFIcontainer:

 type: array

 items:

 $ref: '#/components/schemas/MultipleQFIcontainer'

 minItems: 0

 uPFID:

# Included for backwards compatibility and

 # can be included based on operators requirement

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 roamingChargingProfile:

 $ref: '#/components/schemas/RoamingChargingProfile'

 MultipleQFIcontainer:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 localSequenceNumber:

 type: integer

 qFIContainerInformation:

 $ref: '#/components/schemas/QFIContainerInformation'

 required:

 - localSequenceNumber

 QFIContainerInformation:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 reportTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNetworkFunctionID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 3gppChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 enhancedDiagnostics:

 type: array

 items:

 type: string

 required:

 - reportTime

 RoamingChargingProfile:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 partialRecordMethod:

 $ref: '#/components/schemas/PartialRecordMethod'

 SMSChargingInformation:

 type: object

 properties:

 originatorInfo:

 $ref: '#/components/schemas/OriginatorInfo'

 recipientInfo:

 type: array

 items:

 $ref: '#/components/schemas/RecipientInfo'

 minItems: 0

 userEquipmentInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 sMSCAddress:

 type: string

 sMDataCodingScheme:

 type: integer

 sMMessageType:

 $ref: '#/components/schemas/SMMessageType'

 sMReplyPathRequested:

 $ref: '#/components/schemas/ReplyPathRequested'

 sMUserDataHeader:

 type: string

 sMStatus:

 type: string

 pattern: '^[0-7]?[0-9a-fA-F]$'

 sMDischargeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 numberofMessagesSent:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMServiceType:

 $ref: '#/components/schemas/SMServiceType'

 sMSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMSresult:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 submissionTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sMPriority:

 $ref: '#/components/schemas/SMPriority'

 messageReference:

 type: string

 messageSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 messageClass:

 $ref: '#/components/schemas/MessageClass'

 deliveryReportRequested:

 $ref: '#/components/schemas/DeliveryReportRequested'

 OriginatorInfo:

 type: object

 properties:

 originatorSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 originatorGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 originatorOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorSCCPAddress:

 type: string

 sMOriginatorInterface:

 $ref: '#/components/schemas/SMInterface'

 sMOriginatorProtocolId:

 type: string

 RecipientInfo:

 type: object

 properties:

 recipientSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 recipientGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 recipientOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientSCCPAddress:

 type: string

 sMDestinationInterface:

 $ref: '#/components/schemas/SMInterface'

 sMrecipientProtocolId:

 type: string

 SMAddressInfo:

 type: object

 properties:

 sMaddressType:

 $ref: '#/components/schemas/SMAddressType'

 sMaddressData:

 type: string

 sMaddressDomain:

 $ref: '#/components/schemas/SMAddressDomain'

 RecipientAddress:

 type: object

 properties:

 recipientAddressInfo:

 $ref: '#/components/schemas/SMAddressInfo'

 sMaddresseeType:

 $ref: '#/components/schemas/SMAddresseeType'

 MessageClass:

 type: object

 properties:

 classIdentifier:

 $ref: '#/components/schemas/ClassIdentifier'

 tokenText:

 type: string

 SMAddressDomain:

 type: object

 properties:

 domainName:

 type: string

 3GPPIMSIMCCMNC:

 type: string

 SMInterface:

 type: object

 properties:

 interfaceId:

 type: string

 interfaceText:

 type: string

 interfacePort:

 type: string

 interfaceType:

 $ref: '#/components/schemas/InterfaceType'

 RANSecondaryRATUsageReport:

 type: object

 properties:

 rANSecondaryRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 qosFlowsUsageReports:

 type: array

 items:

 $ref: '#/components/schemas/QosFlowsUsageReport'

 Diagnostics:

 type: integer

 IPFilterRule:

 type: string

 QosFlowsUsageReport:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 startTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 5GLANTypeService:

 type: object

 properties:

 internalGroupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 NEFChargingInformation:

 type: object

 properties:

 externalIndividualIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 externalGroupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

 groupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 aPIDirection:

 $ref: '#/components/schemas/APIDirection'

 aPITargetNetworkFunction:

 $ref: '#/components/schemas/NFIdentification'

 aPIResultCode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 aPIName:

 type: string

 aPIReference:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 aPIContent:

 type: string

 required:

 - aPIName

 RegistrationChargingInformation:

 type: object

 properties:

 registrationMessagetype:

 $ref: '#/components/schemas/RegistrationMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 5GMMCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 mICOModeIndication:

 $ref: '#/components/schemas/MICOModeIndication'

 smsIndication:

 $ref: '#/components/schemas/SmsIndication'

 taiList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 requestedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rejectedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 nSSAIMapList:

 type: array

 items:

 $ref: '#/components/schemas/NSSAIMap'

 minItems: 0

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 required:

 - registrationMessagetype

 PSCellInformation:

 type: object

 properties:

 nrcgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

 ecgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

 NSSAIMap:

 type: object

 properties:

 servingSnssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 homeSnssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - servingSnssai

 - homeSnssai

 N2ConnectionChargingInformation:

 type: object

 properties:

 n2ConnectionMessageType:

 $ref: '#/components/schemas/N2ConnectionMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 restrictedRatList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 minItems: 0

 forbiddenAreaList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 restrictedCnList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rrcEstCause:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 required:

 - n2ConnectionMessageType

 LocationReportingChargingInformation:

 type: object

 properties:

 locationReportingMessageType:

 $ref: '#/components/schemas/LocationReportingMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 required:

 - locationReportingMessageType

 N2ConnectionMessageType:

 type: integer

 LocationReportingMessageType:

 type: integer

 NSMChargingInformation:

 type: object

 properties:

 managementOperation:

 $ref: '#/components/schemas/ManagementOperation'

 idNetworkSliceInstance:

 type: string

 listOfserviceProfileChargingInformation:

 type: array

 items:

 $ref: '#/components/schemas/ServiceProfileChargingInformation'

 minItems: 0

 managementOperationStatus:

 $ref: '#/components/schemas/ManagementOperationStatus'

# To be introduced once the reference to 'generic.yaml is resolved

# managementOperationalState:

# $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

# managementAdministrativeState:

# $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 required:

 - managementOperation

 ServiceProfileChargingInformation:

 type: object

 properties:

 serviceProfileIdentifier:

 type: string

 sNSSAIList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

# To be introduced once the reference to 'nrNrm.yaml is resolved

# sST:

# $ref: 'nrNrm.yaml#/components/schemas/Sst'

 latency:

 type: integer

 availability:

 type: number

# To be introduced once the reference to sliceNrm.yaml is resolved

# resourceSharingLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/SharingLevel'

 jitter:

 type: integer

 reliability:

 type: string

 maxNumberofUEs:

 type: integer

 coverageArea:

 type: string

# To be introduced once the reference to sliceNrm.yaml is resolved

# uEMobilityLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/MobilityLevel'

# delayToleranceIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

 dLThptPerSlice:

 $ref: '#/components/schemas/Throughput'

 dLThptPerUE:

 $ref: '#/components/schemas/Throughput'

 uLThptPerSlice:

 $ref: '#/components/schemas/Throughput'

 uLThptPerUE:

 $ref: '#/components/schemas/Throughput'

 maxNumberofPDUsessions:

 type: integer

 kPIMonitoringList:

 type: string

 supportedAccessTechnology:

 type: integer

# To be introduced once the reference to sliceNrm.yaml is resolved

# v2XCommunicationModeIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

 addServiceProfileInfo:

 type: string

 Throughput:

 type: object

 properties:

 guaranteedThpt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 maximumThpt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 MAPDUSessionInformation:

 type: object

 properties:

 mAPDUSessionIndicator:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MaPduIndication'

 aTSSSCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AtsssCapability'

 EnhancedDiagnostics5G:

 $ref: '#/components/schemas/RanNasCauseList'

 RanNasCauseList:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

 QosMonitoringReport:

 description: Contains reporting information on QoS monitoring.

 type: object

 properties:

 ulDelays:

 type: array

 items:

 type: integer

 minItems: 0

 dlDelays:

 type: array

 items:

 type: integer

 minItems: 0

 rtDelays:

 type: array

 items:

 type: integer

 minItems: 0

 AnnouncementInformation:

 type: object

 properties:

 announcementIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 announcementReference:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 variableParts:

 type: array

 items:

 $ref: '#/components/schemas/VariablePart'

 minItems: 0

 timeToPlay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 quotaConsumptionIndicator:

 $ref: '#/components/schemas/QuotaConsumptionIndicator'

 announcementPriority:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 playToParty:

 $ref: '#/components/schemas/PlayToParty'

 announcementPrivacyIndicator:

 $ref: '#/components/schemas/AnnouncementPrivacyIndicator'

 Language:

 $ref: '#/components/schemas/Language'

 VariablePart:

 type: object

 properties:

 variablePartType:

 $ref: '#/components/schemas/VariablePartType'

 variablePartValue:

 type: array

 items:

 type: string

 minItems: 1

 variablePartOrder:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 required:

 - variablePartType

 - variablePartValue

 Language:

 type: string

 MMTelChargingInformation:

 type: object

 properties:

 supplementaryServices:

 type: array

 items:

 $ref: '#/components/schemas/SupplementaryService'

 minItems: 1

 SupplementaryService:

 type: object

 properties:

 supplementaryServiceType:

 $ref: '#/components/schemas/SupplementaryServiceType'

 supplementaryServiceMode:

 $ref: '#/components/schemas/SupplementaryServiceMode'

 numberOfDiversions:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 associatedPartyAddress:

 type: string

 conferenceId:

 type: string

 participantActionType:

 $ref: '#/components/schemas/ParticipantActionType'

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 numberOfParticipants:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 cUGInformation:

 $ref: '#/components/schemas/OctetString'

 IMSChargingInformation:

 type: object

 properties:

 eventType:

 $ref: '#/components/schemas/SIPEventType'

 iMSNodeFunctionality:

 $ref: '#/components/schemas/IMSNodeFunctionality'

 roleOfNode:

 $ref: '#/components/schemas/RoleOfIMSNode'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 isupCause:

 $ref: '#/components/schemas/ISUPCause'

 controlPlaneAddress:

 $ref: '#/components/schemas/IMSAddress'

 vlrNumber:

 $ref: '#/components/schemas/E164'

 mscAddress:

 $ref: '#/components/schemas/E164'

 userSessionID:

 type: string

 outgoingSessionID:

 type: string

 sessionPriority:

 $ref: '#/components/schemas/IMSSessionPriority'

 callingPartyAddresses:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 minItems: 1

 calledPartyAddress:

 type: string

 numberPortabilityRoutinginformation:

 type: string

 carrierSelectRoutingInformation:

 type: string

 alternateChargedPartyAddress:

 type: string

 requestedPartyAddress:

 type: array

 items:

 type: string

 minItems: 1

 calledAssertedIdentities:

 type: array

 items:

 type: string

 minItems: 1

 calledIdentityChanges:

 type: array

 items:

 $ref: '#/components/schemas/CalledIdentityChange'

 minItems: 1

 associatedURI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 minItems: 1

 timeStamps:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 applicationServerInformation:

 type: array

 items:

 type: string

 minItems: 1

 interOperatorIdentifier:

 type: array

 items:

 $ref: '#/components/schemas/InterOperatorIdentifier'

 minItems: 1

 imsChargingIdentifier:

 type: string

 relatedICID:

 type: string

 relatedICIDGenerationNode:

 type: string

 transitIOIList:

 type: array

 items:

 type: string

 minItems: 1

 earlyMediaDescription:

 type: array

 items:

 $ref: '#/components/schemas/EarlyMediaDescription'

 minItems: 1

 sdpSessionDescription:

 type: array

 items:

 type: string

 minItems: 1

 sdpMediaComponent:

 type: array

 items:

 $ref: '#/components/schemas/SDPMediaComponent'

 minItems: 1

 servedPartyIPAddress:

 $ref: '#/components/schemas/IMSAddress'

 serverCapabilities:

 $ref: '#/components/schemas/ServerCapabilities'

 trunkGroupID:

 $ref: '#/components/schemas/TrunkGroupID'

 bearerService:

 type: string

 imsServiceId:

 type: string

 messageBodies:

 type: array

 items:

 $ref: '#/components/schemas/MessageBody'

 minItems: 1

 accessNetworkInformation:

 type: array

 items:

 type: string

 minItems: 1

 additionalAccessNetworkInformation:

 type: string

 cellularNetworkInformation:

 type: string

 accessTransferInformation:

 type: array

 items:

 $ref: '#/components/schemas/AccessTransferInformation'

 minItems: 1

 accessNetworkInfoChange:

 type: array

 items:

 $ref: '#/components/schemas/AccessNetworkInfoChange'

 minItems: 1

 imsCommunicationServiceID:

 type: string

 imsApplicationReferenceID:

 type: string

 causeCode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 reasonHeader:

 type: array

 items:

 type: string

 minItems: 1

 initialIMSChargingIdentifier:

 type: string

 nniInformation:

 type: array

 items:

 $ref: '#/components/schemas/NNIInformation'

 minItems: 1

 fromAddress:

 type: string

 imsEmergencyIndication:

 type: boolean

 imsVisitedNetworkIdentifier:

 type: string

 sipRouteHeaderReceived:

 type: string

 sipRouteHeaderTransmitted:

 type: string

 tadIdentifier:

 $ref: '#/components/schemas/TADIdentifier'

 feIdentifierList:

 type: string

 EdgeInfrastructureUsageChargingInformation:

 type: object

 properties:

 meanVirtualCPUUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 meanVirtualMemoryUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 meanVirtualDiskUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 incomingDataVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 outgoingDataVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 durationStartTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 durationEndTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 EASDeploymentChargingInformation:

 type: object

 properties:

 eEASDeploymentRequirements:

 $ref: '#/components/schemas/EASRequirements'

 lCMStartTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 lCMEndTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 PC5ContainerInformation:

 type: object

 properties:

 coverageInfoList:

 type: array

 items:

 $ref: '#/components/schemas/CoverageInfo'

 radioParameterSetInfoList:

 type: array

 items:

 $ref: '#/components/schemas/RadioParameterSetInfo'

 transmitterInfoList:

 type: array

 items:

 $ref: '#/components/schemas/TransmitterInfo'

 minItems: 0

 timeOfFirst Transmission:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeOfFirst Reception:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 CoverageInfo:

 type: object

 properties:

 coverageStatus:

 type: boolean

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 locationInfo:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 minItems: 0

 RadioParameterSetInfo:

 type: object

 properties:

 radioParameterSetValues:

 type: array

 items:

 $ref: '#/components/schemas/OctetString'

 minItems: 0

 changeTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 TransmitterInfo:

 type: object

 properties:

 proseSourceIPAddress:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 proseSourceL2Id:

 type: string

 ProseChargingInformation:

 type: object

 properties:

 announcingPlmnID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 announcingUeHplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 announcingUeVplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 monitoringUeHplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 monitoringUeVplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 discovererUeHplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 discovererUeVplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 discovereeUeHplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 discovereeUeVplmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 monitoredPlmnIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 proseApplicationID:

 type: string

 ApplicationId:

 type: string

 applicationSpecificDataList:

 type: array

 items:

 type: string

 minItems: 0

 proseFunctionality:

 $ref: '#/components/schemas/ProseFunctionality'

 proseEventType:

 $ref: '#/components/schemas/ProseEventType'

 directDiscoveryModel:

 $ref: '#/components/schemas/DirectDiscoveryModel'

 validityPeriod:

 type: integer

 roleOfUE:

 $ref: '#/components/schemas/RoleOfUE'

 proseRequestTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 pC3ProtocolCause:

 type: integer

 monitoringUEIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 requestedPLMNIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 timeWindow:

 type: integer

 rangeClass:

 $ref: '#/components/schemas/RangeClass'

 proximityAlertIndication:

 type: boolean

 proximityAlertTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 proximityCancellationTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 relayIPAddress:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 proseUEToNetworkRelayUEID :

 type: string

 proseDestinationLayer2ID:

 type: string

 pFIContainerInformation:

 type: array

 items:

 $ref: '#/components/schemas/PFIContainerInformation'

 minItems: 0

 transmissionDataContainer:

 type: array

 items:

 $ref: '#/components/schemas/PC5DataContainer'

 minItems: 0

 receptionDataContainer:

 type: array

 items:

 $ref: '#/components/schemas/PC5DataContainer'

 minItems: 0

 required:

 - aPIName

 PFIContainerInformation:

 type: object

 properties:

 pFI:

 type: string

 reportTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 PC5DataContainer:

 type: object

 properties:

 localSequenceNumber:

 type: string

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 coverageStatus:

 type: boolean

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 dataVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 changeCondition:

 type: string

 radioResourcesId:

 $ref: '#/components/schemas/RadioResourcesId'

 radioFrequency:

 type: string

 pC5RadioTechnology:

 type: string

 OctetString:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 E164:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 IMSAddress:

 type: object

 properties:

 ipv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 e164:

 $ref: '#/components/schemas/E164'

 anyOf:

 - required: [ ipv4Addr ]

 - required: [ ipv6Addr ]

 - required: [ e164 ]

 ServingNodeAddress:

 type: object

 properties:

 ipv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 anyOf:

 - required: [ ipv4Addr ]

 - required: [ ipv6Addr ]

 SIPEventType:

 type: object

 properties:

 sIPMethod:

 type: string

 eventHeader:

 type: string

 expiresHeader:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 ISUPCause:

 type: object

 properties:

 iSUPCauseLocation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 iSUPCauseValue:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 iSUPCauseDiagnostics:

 $ref: '#/components/schemas/OctetString'

 CalledIdentityChange:

 type: object

 properties:

 calledIdentity:

 type: string

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 InterOperatorIdentifier:

 type: object

 properties:

 originatingIOI:

 type: string

 terminatingIOI:

 type: string

 EarlyMediaDescription:

 type: object

 properties:

 sDPTimeStamps:

 $ref: '#/components/schemas/SDPTimeStamps'

 sDPMediaComponent:

 type: array

 items:

 $ref: '#/components/schemas/SDPMediaComponent'

 minItems: 0

 sDPSessionDescription:

 type: array

 items:

 type: string

 minItems: 0

 SDPTimeStamps:

 type: object

 properties:

 sDPOfferTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sDPAnswerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 SDPMediaComponent:

 type: object

 properties:

 sDPMediaName:

 type: string

 SDPMediaDescription:

 type: array

 items:

 type: string

 minItems: 0

 localGWInsertedIndication:

 type: boolean

 ipRealmDefaultIndication:

 type: boolean

 transcoderInsertedIndication:

 type: boolean

 mediaInitiatorFlag:

 $ref: '#/components/schemas/MediaInitiatorFlag'

 mediaInitiatorParty:

 type: string

 threeGPPChargingId:

 $ref: '#/components/schemas/OctetString'

 accessNetworkChargingIdentifierValue:

 $ref: '#/components/schemas/OctetString'

 sDPType:

 $ref: '#/components/schemas/SDPType'

 ServerCapabilities:

 type: object

 properties:

 mandatoryCapability:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 minItems: 0

 optionalCapability :

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 minItems: 0

 serverName:

 type: array

 items:

 type: string

 minItems: 0

 TrunkGroupID:

 type: object

 properties:

 incomingTrunkGroupID:

 type: string

 outgoingTrunkGroupID:

 type: string

 MessageBody:

 type: object

 properties:

 contentType:

 type: string

 contentLength:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 contentDisposition:

 type: string

 originator:

 $ref: '#/components/schemas/OriginatorPartyType'

 required:

 - contentType

 - contentLength

 AccessTransferInformation:

 type: object

 properties:

 accessTransferType:

 $ref: '#/components/schemas/AccessTransferType'

 accessNetworkInformation:

 type: array

 items:

 $ref: '#/components/schemas/OctetString'

 minItems: 0

 cellularNetworkInformation:

 $ref: '#/components/schemas/OctetString'

 interUETransfer:

 $ref: '#/components/schemas/UETransferType'

 userEquipmentInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 instanceId:

 type: string

 relatedIMSChargingIdentifier:

 type: string

 relatedIMSChargingIdentifierNode:

 $ref: '#/components/schemas/IMSAddress'

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 AccessNetworkInfoChange:

 type: object

 properties:

 accessNetworkInformation:

 type: array

 items:

 $ref: '#/components/schemas/OctetString'

 minItems: 0

 cellularNetworkInformation:

 $ref: '#/components/schemas/OctetString'

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 NNIInformation:

 type: object

 properties:

 sessionDirection:

 $ref: '#/components/schemas/NNISessionDirection'

 nNIType:

 $ref: '#/components/schemas/NNIType'

 relationshipMode:

 $ref: '#/components/schemas/NNIRelationshipMode'

 neighbourNodeAddress:

 $ref: '#/components/schemas/IMSAddress'

 EASRequirements:

 type: object

 properties:

 requiredEASservingLocation:

 $ref: 'TS28538\_EdgeNrm.yaml#/components/schemas/ServingLocation'

 softwareImageInfo:

 $ref: 'TS28538\_EdgeNrm.yaml#/components/schemas/SoftwareImageInfo'

 affinityAntiAffinity:

 $ref: 'TS28538\_EdgeNrm.yaml#/components/schemas/AffinityAntiAffinity'

 serviceContinuity:

 type: boolean

 virtualResource:

 $ref: 'TS28538\_EdgeNrm.yaml#/components/schemas/VirtualResource'

 NotificationType:

 anyOf:

 - type: string

 enum:

 - REAUTHORIZATION

 - ABORT\_CHARGING

 - type: string

 NodeFunctionality:

 anyOf:

 - type: string

 enum:

 - AMF

 - SMF

 - SMS # Included for backwards compatibility, shall not be used

 - SMSF

 - PGW\_C\_SMF

 - NEFF # Included for backwards compatibility, shall not be used

 - SGW

 - I\_SMF

 - ePDG

 - CEF

 - NEF

 - MnS\_Producer

 - SGSN

 - V\_SMF

 - 5G\_DDNMF

 - IMS\_Node

 - EES

 - type: string

 ChargingCharacteristicsSelectionMode:

 anyOf:

 - type: string

 enum:

 - HOME\_DEFAULT

 - ROAMING\_DEFAULT

 - VISITING\_DEFAULT

 - type: string

 TriggerType:

 anyOf:

 - type: string

 enum:

 - QUOTA\_THRESHOLD

 - QHT

 - FINAL

 - QUOTA\_EXHAUSTED

 - VALIDITY\_TIME

 - OTHER\_QUOTA\_TYPE

 - FORCED\_REAUTHORISATION

 - UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

 - UNIT\_COUNT\_INACTIVITY\_TIMER

 - ABNORMAL\_RELEASE

 - QOS\_CHANGE

 - VOLUME\_LIMIT

 - TIME\_LIMIT

 - EVENT\_LIMIT

 - PLMN\_CHANGE

 - USER\_LOCATION\_CHANGE

 - RAT\_CHANGE

 - SESSION\_AMBR\_CHANGE

 - UE\_TIMEZONE\_CHANGE

 - TARIFF\_TIME\_CHANGE

 - MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

 - MANAGEMENT\_INTERVENTION

 - CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

 - CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

 - SERVING\_NODE\_CHANGE

 - REMOVAL\_OF\_UPF

 - ADDITION\_OF\_UPF

 - INSERTION\_OF\_ISMF

 - REMOVAL\_OF\_ISMF

 - CHANGE\_OF\_ISMF

 - START\_OF\_SERVICE\_DATA\_FLOW

 - ECGI\_CHANGE

 - TAI\_CHANGE

 - HANDOVER\_CANCEL

 - HANDOVER\_START

 - HANDOVER\_COMPLETE

 - GFBR\_GUARANTEED\_STATUS\_CHANGE

 - ADDITION\_OF\_ACCESS

 - REMOVAL\_OF\_ACCESS

 - START\_OF\_SDF\_ADDITIONAL\_ACCESS

 - REDUNDANT\_TRANSMISSION\_CHANGE

 - CGI\_SAI\_CHANGE

 - RAI\_CHANGE

 - type: string

 FinalUnitAction:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - REDIRECT

 - RESTRICT\_ACCESS

 - type: string

 RedirectAddressType:

 anyOf:

 - type: string

 enum:

 - IPV4

 - IPV6

 - URL

 - URI

 - type: string

 TriggerCategory:

 anyOf:

 - type: string

 enum:

 - IMMEDIATE\_REPORT

 - DEFERRED\_REPORT

 - type: string

 QuotaManagementIndicator:

 anyOf:

 - type: string

 enum:

 - ONLINE\_CHARGING

 - OFFLINE\_CHARGING

 - QUOTA\_MANAGEMENT\_SUSPENDED

 - type: string

 FailureHandling:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - CONTINUE

 - RETRY\_AND\_TERMINATE

 - type: string

 SessionFailover:

 anyOf:

 - type: string

 enum:

 - FAILOVER\_NOT\_SUPPORTED

 - FAILOVER\_SUPPORTED

 - type: string

 3GPPPSDataOffStatus:

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

 ResultCode:

 anyOf:

 - type: string

 enum:

 - SUCCESS

 - END\_USER\_SERVICE\_DENIED

 - QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

 - QUOTA\_LIMIT\_REACHED

 - END\_USER\_SERVICE\_REJECTED

 - USER\_UNKNOWN #Included for backwards compatibility, shall not be used

 - RATING\_FAILED

 - QUOTA\_MANAGEMENT

 - type: string

 PartialRecordMethod:

 anyOf:

 - type: string

 enum:

 - DEFAULT

 - INDIVIDUAL

 - type: string

 RoamerInOut:

 anyOf:

 - type: string

 enum:

 - IN\_BOUND

 - OUT\_BOUND

 - type: string

 SMMessageType:

 anyOf:

 - type: string

 enum:

 - SUBMISSION

 - DELIVERY\_REPORT

 - SM\_SERVICE\_REQUEST

 - DELIVERY

 - type: string

 SMPriority:

 anyOf:

 - type: string

 enum:

 - LOW

 - NORMAL

 - HIGH

 - type: string

 DeliveryReportRequested:

 anyOf:

 - type: string

 enum:

 - YES

 - NO

 - type: string

 InterfaceType:

 anyOf:

 - type: string

 enum:

 - UNKNOWN

 - MOBILE\_ORIGINATING

 - MOBILE\_TERMINATING

 - APPLICATION\_ORIGINATING

 - APPLICATION\_TERMINATING

 - type: string

 ClassIdentifier:

 anyOf:

 - type: string

 enum:

 - PERSONAL

 - ADVERTISEMENT

 - INFORMATIONAL

 - AUTO

 - type: string

 SMAddressType:

 anyOf:

 - type: string

 enum:

 - EMAIL\_ADDRESS

 - MSISDN

 - IPV4\_ADDRESS

 - IPV6\_ADDRESS

 - NUMERIC\_SHORTCODE

 - ALPHANUMERIC\_SHORTCODE

 - OTHER

 - IMSI

 - type: string

 SMAddresseeType:

 anyOf:

 - type: string

 enum:

 - TO

 - CC

 - BCC

 - type: string

 SMServiceType:

 anyOf:

 - type: string

 enum:

 - VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

 - VAS4SMS\_SHORT\_MESSAGE\_FILTERING

 - VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

 - VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

 - VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

 - VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

 - VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

 - VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

 - VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

 - type: string

 ReplyPathRequested:

 anyOf:

 - type: string

 enum:

 - NO\_REPLY\_PATH\_SET

 - REPLY\_PATH\_SET

 - type: string

 oneTimeEventType:

 anyOf:

 - type: string

 enum:

 - IEC

 - PEC

 - type: string

 dnnSelectionMode:

 anyOf:

 - type: string

 enum:

 - VERIFIED

 - UE\_DNN\_NOT\_VERIFIED

 - NW\_DNN\_NOT\_VERIFIED

 - type: string

 APIDirection:

 anyOf:

 - type: string

 enum:

 - INVOCATION

 - NOTIFICATION

 - type: string

 RegistrationMessageType:

 anyOf:

 - type: string

 enum:

 - INITIAL

 - MOBILITY

 - PERIODIC

 - EMERGENCY

 - DEREGISTRATION

 - type: string

 MICOModeIndication:

 anyOf:

 - type: string

 enum:

 - MICO\_MODE

 - NO\_MICO\_MODE

 - type: string

 SmsIndication:

 anyOf:

 - type: string

 enum:

 - SMS\_SUPPORTED

 - SMS\_NOT\_SUPPORTED

 - type: string

 ManagementOperation:

 anyOf:

 - type: string

 enum:

 - CreateMOI #Included for backwards compatibility, shall not be used

 - ModifyMOIAttributes #Included for backwards compatibility, shall not be used

 - DeleteMOI #Included for backwards compatibility, shall not be used

 - CREATE\_MOI

 - MODIFY\_MOI\_ATTR

 - DELETE\_MOI

 - type: string

 ManagementOperationStatus:

 anyOf:

 - type: string

 enum:

 - OPERATION\_SUCCEEDED

 - OPERATION\_FAILED

 - type: string

 RedundantTransmissionType:

 anyOf:

 - type: string

 enum:

 - NON\_TRANSMISSION

 - END\_TO\_END\_USER\_PLANE\_PATHS

 - N3/N9

 - TRANSPORT\_LAYER

 - type: string

 VariablePartType:

 anyOf:

 - type: string

 enum:

 - INTEGER

 - NUMBER

 - TIME

 - DATE

 - CURRENCY

 - type: string

 QuotaConsumptionIndicator:

 anyOf:

 - type: string

 enum:

 - QUOTA\_NOT\_USED

 - QUOTA\_IS\_USED

 - type: string

 PlayToParty:

 anyOf:

 - type: string

 enum:

 - SERVED

 - REMOTE

 - type: string

 AnnouncementPrivacyIndicator:

 anyOf:

 - type: string

 enum:

 - NOT\_PRIVATE

 - PRIVATE

 - type: string

 SupplementaryServiceType:

 anyOf:

 - type: string

 enum:

 - OIP

 - OIR

 - TIP

 - TIR

 - HOLD

 - CB

 - CDIV

 - CW

 - MWI

 - CONF

 - FA

 - CCBS

 - CCNR

 - MCID

 - CAT

 - CUG

 - PNM

 - CRS

 - ECT

 - type: string

 SupplementaryServiceMode:

 anyOf:

 - type: string

 enum:

 - CFU

 - CFB

 - CFNR

 - CFNL

 - CD

 - CFNRC

 - ICB

 - OCB

 - ACR

 - BLIND\_TRANFER

 - CONSULTATIVE\_TRANFER

 - type: string

 ParticipantActionType:

 anyOf:

 - type: string

 enum:

 - CREATE

 - JOIN

 - INVITE\_INTO

 - QUIT

 - type: string

 TrafficForwardingWay:

 anyOf:

 - type: string

 enum:

 - N6

 - N19

 - LOCAL\_SWITCH

 - type: string

 IMSNodeFunctionality:

 anyOf:

 - type: string

 enum:

# The applicable IMS Nodes are MRFC, IMS-GWF (connected to S-CSCF using ISC) and SIP AS.

 - S\_CSCF

 - P\_CSCF

 - I\_CSCF

 - MRFC

 - MGCF

 - BGCF

 - AS

 - IBCF

 - S-GW

 - P-GW

 - HSGW

 - E-CSCF

 - MME

 - TRF

 - TF

 - ATCF

 - PROXY

 - EPDG

 - TDF

 - TWAG

 - SCEF

 - IWK\_SCEF

 - IMS\_GWF

 - type: string

 RoleOfIMSNode:

 anyOf:

 - type: string

 enum:

 - ORIGINATING

 - TERMINATING

 - FORWARDING

 - type: string

 IMSSessionPriority:

 anyOf:

 - type: string

 enum:

 - PRIORITY\_0

 - PRIORITY\_1

 - PRIORITY\_2

 - PRIORITY\_3

 - PRIORITY\_4

 - type: string

 MediaInitiatorFlag:

 anyOf:

 - type: string

 enum:

 - CALLED\_PARTY

 - CALLING\_PARTY

 - UNKNOWN

 - type: string

 SDPType:

 anyOf:

 - type: string

 enum:

 - OFFER

 - ANSWER

 - type: string

 OriginatorPartyType:

 anyOf:

 - type: string

 enum:

 - CALLING

 - CALLED

 - type: string

 AccessTransferType:

 anyOf:

 - type: string

 enum:

 - PS\_TO\_CS

 - CS\_TO\_PS

 - PS\_TO\_PS

 - CS\_TO\_CS

 - type: string

 UETransferType:

 anyOf:

 - type: string

 enum:

 - INTRA\_UE

 - INTER\_UE

 - type: string

 NNISessionDirection:

 anyOf:

 - type: string

 enum:

 - INBOUND

 - OUTBOUND

 - type: string

 NNIType:

 anyOf:

 - type: string

 enum:

 - NON\_ROAMING

 - ROAMING\_NO\_LOOPBACK

 - ROAMING\_LOOPBACK

 - type: string

 NNIRelationshipMode:

 anyOf:

 - type: string

 enum:

 - TRUSTED

 - NON\_TRUSTED

 - type: string

 TADIdentifier:

 anyOf:

 - type: string

 enum:

 - CS

 - PS

 - type: string

 ProseFunctionality:

 anyOf:

 - type: string

 enum:

 - DIRECT\_DISCOVERY

 - DIRECT\_COMMUNICATION

 - type: string

 ProseEventType:

 anyOf:

 - type: string

 enum:

 - ANNOUNCING

 - MONITORING

 - MATCH\_REPORT

 - type: string

 DirectDiscoveryModel:

 anyOf:

 - type: string

 enum:

 - MODEL\_A

 - MODEL\_B

 - type: string

 RoleOfUE:

 anyOf:

 - type: string

 enum:

 - ANNOUNCING\_UE

 - MONITORING\_UE

 - REQUESTOR\_UE

 - REQUESTED\_UE

 - type: string

 RangeClass:

 anyOf:

 - type: string

 enum:

 - RESERVED

 - 50\_METER

 - 100\_METER

 - 200\_METER

 - 500\_METER

 - 1000\_METER

 - UNUSED

 - type: string

 RadioResourcesId:

 anyOf:

 - type: string

 enum:

 - OPERATOR\_PROVIDED

 - CONFIGURED

 - type: string

|  |
| --- |
| **End of changes** |