**3GPP TSG-SA WG6 Meeting #37-e S6-200803**

**e-meeting, 14th – 26th May 2020 (revision of S6-xxxxxx)**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **23.434** | **CR** | **0022** | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification and correction on media direction mode |
|  |  |
| ***Source to WG:*** | Huawei, Hisilicon |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | SEAL |  | ***Date:*** | 2020-04-30 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The user plane delivery mode is used by the NRM server to instruct the VAL server to switch from MBMS bearer to Unicast bearer or from Unicast Bearer to MBMS bearer. However, the description about the MBMS media stream and unicast stream in table 14.3.2.12.1-1 is not clear to indicate the switching. |
|  |  |
| ***Summary of change:*** | Update the user plane delivery mode desciption in table 14.3.2.12-1. |
|  |  |
| ***Consequences if not approved:*** | Confussion and misunderstanding may be caused to downstream working group. |
|  |  |
| ***Clauses affected:*** | 14.3.2.12 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* 1st change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

#### 14.3.2.12 User plane delivery mode

Table 14.3.2.12-1 describes the information flow for the user plane delivery mode from NRM server to VAL server.

Table 14.3.2.12-1: User plane delivery mode

|  |  |  |
| --- | --- | --- |
| Information element | Status | Description |
| Delivery mode | M | Indicates whether to deliver the user data to the UE(s) via unicast mode or multicast mode |
| MBMS media stream identifier (NOTE) | M  | Indicates the MBMS media stream to be used to deliver the media previously over unicast |
| Unicast media stream identifier(s) (NOTE) | M | Indicates the unicast media stream to be used to deliver the media previously over multicast, or the unicast to be stopped and switched to multicast. |
| NOTE: During the switchover from unicast mode to multicast mode, the Unicast media stream identifiers(s) can also be used to deliver the media which is being delivered using MBMS media stream identifier. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*