**3GPP TSG-SA3 Meeting #104-e- Ad-hoc *S3-213402***

**e-meeting, 27 – 30 September 2021** Revision of S3-20xxxx

**Source: Huawei, HiSilicon**

**Title: User Consent Related Requirements**

**Document for: Approval**

**Agenda Item: 4.9**

# 1 Decision/action requested

***SA3 is kindly requested to approve the proposed changes in clause 5.8.X.***

# 2 References

[1] 3GPP TR 33.867 “Study on User Consent for 3GPP services”

[2] S2-2105408 “KI#15 – User consent”

# 3 Rationale

It is agreed in clause 8.5.1 and 8.5.3 in TR 33.867 [1], UDM services for user consent check and revocation are concluded.

It is also agreed in clause 8.4 in TR 33.867 [1], relationship between the subscriber and the end-users is concluded.

In agreed S2-2105408 [2], Nudm\_SDM\_Get and Nudm\_SDM\_Subscribe service is for user consent check and revocation usage.

Thus, the contribution proposes to add the agreed UDM parts in the main text.

# 4 Detailed proposal

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of 1st Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

5.8.X User consent related requirements

The UDM shall provide the following services for the checking and revocation of the user consent.

- Service used to retrieve user consent parameters for NF to check of user consent.

- Service used to notify about user consent change for NF to revoke user consent

The user consent parameters shall be stored in the UDM as subscription data.

The user consent parameters shall be effective only after the point in time that user consent was given, and they shall be effective until they are revoked.

NOTE: The user consent related requirements in the present document are applicable only when it is required by regional regulations or operator’s local policy.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of 1st Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*