**3GPP SA3LI#86e-a *S3i220329***

**eMeeting, 13-15 July 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **33.128** | **CR** | **0366** | **rev** |  | **Current version:** | **16.11.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Alignment of the requestType Paramter usage within SMF events |
|  |  |
| ***Source to WG:*** | SA3 LI (ZITiS) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** | LI16 |  | ***Date:*** | 2022-07-10 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The evaluation of 5G SA IRI tickets revealed a mismatch of the textual description of the requestType parameter within SMF event messages and the corresponding ASN.1 specification.  |
|  |  |
| ***Summary of change:*** | This CR proposes to adapt the textual description of the requestType parameter to be in line with the ASN.1 specification and considering 3GPP TS 24.501 and 3GPP TS 29.502. |
|  |  |
| ***Consequences if not approved:*** | Misalignment between texual specification and corresponding ASN.1 representation. |
|  |  |
| ***Clauses affected:*** | 6.2.3.2.2, 6.2.3.2.3, 6.2.3.2.5, 6.2.3.2.6, 6.2.3.2.7.2, 6.2.3.2.7.3, 6.2.3.2.7.5, 6.2.3.2.7.6, 6.2.3.2.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### \*\*\* FIRST CHANGE \*\*\*

##### 6.2.3.2.2 PDU session establishment

The IRI-POI in the SMF shall generate an xIRI containing an SMFPDUSessionEstablishment record when the IRI-POI present in the SMF detects that a PDU session has been established for the target UE. The IRI-POI present in the SMF shall generate the xIRI for the following events:

- For a non-roaming scenario, the SMF (or for a roaming scenario, V-SMF in the VPLMN), sends the N1 NAS message (via AMF) PDU SESSION ESTABLISHMENT ACCEPT to the UE and the 5G Session Management (5GSM) state within the SMF is changed to PDU SESSION ACTIVE (see TS 24.501 [13]).

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) sends the N16: Nsmf\_PDU\_Session\_Create response message with n1SmInfoToUe IE containing the PDU SESSION ESTABLISHMENT ACCEPT (see TS 29.502 [16]).

Table 6.2.3-1: Payload for SMFPDUSessionEstablishment record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions (see NOTE). | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI has not been authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available (see NOTE). | C |
| gPSI | GPSI associated with the PDU session if available (see NOTE). | C |
| pDUSessionID | PDU Session ID See TS 24.501 [13] clause 9.4. | M |
| gTPTunnelID | Contains the F-TEID identifying the GTP tunnel used to encapsulate the traffic, as defined in TS 29.244 [15] clause 8.2.3. Non-GTP encapsulation is for further study. | M |
| pDUSessionType | Identifies selected PDU session type, see TS 24.501 [13] clause 9.11.4.11. | M |
| sNSSAI | Slice identifiers associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| uEEndpoint | UE endpoint address(es) if available. | C |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| dNN | Data Network Name associated with the target traffic, as defined in TS 23.003[19] clause 9A and described in TS 23.501 [2] clause 4.3.2.2. Shall be given in dotted-label presentation format as described in TS 23.003 [19] clause 9.1. | M |
| aMFID | Identifier of the AMF associated with the target UE, as defined in TS 23.003 [19] clause 2.10.1 when available. | C |
| hSMFURI | URI of the Nsmf\_PDUSession service of the selected H-SMF, if available. See TS 29.502 [16] clause 6.1.6.2.2. | C |
| requestType | Type of request as described in TS 24.501 [13] clause 9.11.3.47 provided within the Nsmf\_PDU\_Session\_CreateSMContext Request (TS 29.502 [16]) message shall be reported.. In the case where the network does not support Multi Access (MA) PDU sessions, but receives a MA PDU session request, a request type of “Initial request” shall be reported.In the case where the network does not provide a request type value for a non-MA PDU session, a request type of “initial request”, according to TS 24.501 [13] clause 6.4.1.2 shall be reported. | M |
| accessType | Access type associated with the session (i.e. 3GPP or non-3GPP access) if provided by the AMF (see TS 24.501 [13] clause 9.11.2.1A). | C |
| rATType | RAT Type associated with the access if provided by the AMF as part of session establishment (see TS 23.502 [4] clause 4.3.2). Values given as per TS 29.571 [17] clause 5.4.3.2. | C |
| sMPDUDNRequest | Contents of the SM PDU DN Request container, if available, as described in TS 24.501 [13] clause 9.11.4.15. | C |
| uEEPSPDNConnection | This IE shall be present, if available, during an EPS to 5GS Idle mode mobility or handover using the N26 interface. When present, it shall contain the EPS bearer context(s) information present in the uEEPSPDNConnection parameter of the intercepted SmContextCreateData message. (see TS 29.502 [16] clause 6.1.6.2.2). | C |
| NOTE: At least one of the SUPI, PEI or GPSI fields shall be present. |

#### \*\*\* END OF FIRST CHANGE \*\*\*

#### \*\*\* SECOND CHANGE \*\*\*

##### 6.2.3.2.3 PDU session modification

The IRI-POI in the SMF shall generate an xIRI containing an SMFPDUSessionModification record when the IRI-POI present in the SMF detects that a PDU session has been modified for the target UE. The IRI-POI present in the SMF shall generate the xIRI for the following events:

- For a non-roaming scenario, the SMF (or for a roaming scenario, V-SMF in the VPLMN), receives the N1 NAS message (via AMF) PDU SESSION MODIFICATION COMMAND COMPLETE from the UE and the 5GSM state within the SMF is returned to PDU SESSION ACTIVE (see TS 24.501 [13]). This applies to the following two cases:

- UE initiated PDU session modification.

- Network (VPLMN) initiated PDU session modification.

- For a non-roaming scenario, the SMF (or for a roaming scenario, V-SMF in the VPLMN), sends the N1 NAS message (via AMF) PDU SESSION ESTABLISHMENT ACCEPT to the UE and the 5GSM state within the SMF remains in the PDU SESSION ACTIVE (see TS 24.501 [13]). This applies to the following case:

- Handover from one access type to another access type happens (e.g. 3GPP to non-3GPP).

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) receives the N16: Nsmf\_PDU\_Session\_Update response message with n1SmInfoFromUe IE containing the PDU SESSION MODIFICATION COMMAND COMPLETE (see TS 29.502 [16]). This applies to the following three cases:

- UE initiated PDU session modification.

- Network (VPLMN) initiated PDU session modification.

- Network (HPLMN) initiated PDU session modification.

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) sends the N16: Nsmf\_PDU\_Session\_Create response message with n1SmInfoToUe IE containing the PDU SESSION ESTABLISHMENT ACCEPT (see TS 29.502 [16]) while it had received a N16 Nsmf\_PDU\_Session\_Create request message with an existing PDU Session Id with access type being changed. This applies to the following case:

- Handover from one access type to another access type happens (e.g. 3GPP to non-3GPP).

Table 6.2.3-2: Payload for SMFPDUSessionModification record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions. | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI was not authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available. | C |
| gPSI | GPSI associated with the PDU session if available. | C |
| sNSSAI | Slice identifier associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| requestType | For both a UE- as well as a network-requested PDU session the POI (SMF) shall set the requestType parameter to "modification request". | M |
| accessType | Access type associated with the session (i.e. 3GPP or non-3GPP access) if provided by the AMF (see TS 24.501 [13] clause 9.11.2.1A). | C |
| rATType | RAT type associated with the access, if available. Values given as per TS 29.571 [17] clause 5.4.3.2. | C |
| pDUSessionID | PDU Session ID See TS 24.501 [13] clause 9.4. This parameter is conditional only for backwards compatibility. | C |

#### \*\*\* END OF SECOND CHANGE \*\*\*

#### \*\*\* THIRD CHANGE \*\*\*

##### 6.2.3.2.5 Start of interception with an established PDU session

The IRI-POI in the SMF shall generate an xIRI containing an SMFStartOfInterceptionWithEstablishedPDUSession record when the IRI-POI present in the SMF detects that a PDU session has already been established for the target UE when interception starts.

In a non-roaming scenario, the IRI-POI in the SMF (or in a roaming scenario, the IRI-POI in the V-SMF in the VPLMN) shall generate the xIRI containing the SMFStartOfInterceptionWithEstablishedPDUSession record when it detects that a new interception for a UE is activated (i.e. provisioned by the LIPF) for the following case:

- The 5GSM state within the SMF for that UE is 5GSM: PDU SESSION ACTIVE or PDU SESSION MODIFICATION PENDING.

NOTE: The above trigger happens when the SMF (V-SMF in VPLMN) had not sent an N1 NAS message PDU SESSION RELEASE COMMAND to the UE for a PDU session and the SMF (V-SMF in the VPLMN) had previously sent an N1 NAS message PDU SESSION ESTABLISHMENT ACCEPT to that UE for the same PDU session.

In a home-routed roaming scenario, the IRI-POI in the H-SMF shall generate the xIRI containing the SMFStartOfInterceptionWithEstablishedPDUSession record when it detects that a new interception for a UE is activated (i.e. provisioned by the LIPF) for the following case:

- The H-SMF had not sent a Nsmf\_PDU\_Session\_Update Request (n1SmInfoToUe: PDU SESSION RELEASE COMMAND) to the V-SMF for a PDU session and H-SMF had previously sent a Nsmf\_PDU\_Session\_Create response (n1SmInfoToUE: PDU SESSION ESTABLISHMENT ACCEPT) to the V-SMF for that PDU session.

The IRI-POI in the SMF shall generate the xIRI containing the SMFStartOfInterceptionWithEstablishedPDUSession record for each of the PDU sessions (that meets the above criteria) associated with the newly identified target UEs.

Table 6.2.3-4: Payload for SMFStartOfInterceptionWithEstablishedPDUSession record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions. | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI has not been authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available. | C |
| gPSI | GPSI associated with the PDU session if available. | C |
| pDUSessionID | PDU Session ID as assigned by the AMF, as defined in TS 24.007 [14] clause 11.2.3.1b. | M |
| gTPTunnelID | Contains the F-TEID identifying the tunnel used to encapsulate the traffic, as defined in TS 29.244 [15] clause 8.2.3. Non-GTP encapsulation is for further study. | M |
| pDUSessionType | Identifies selected PDU session type, see TS 24.501 [13] clause 9.11.4.11. | M |
| sNSSAI | Slice identifier associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| uEEndpoint | UE endpoint address(es) if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). MAC addresses are given as 6 octets with the most significant octet first. | C |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| location | Location information provided by the AMF at session establishment, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| dNN | Data Network Name associated with the target traffic, as defined in TS 23.003 [19] clause 9A and described in TS 23.501 [2] clause 4.3.2.2. Shall be given in dotted-label presentation format as described in TS 23.003 [19] clause 9.1. | M |
| aMFID | Identifier of the AMF associated with the target UE, as defined in TS 23.003 [19] clause 2.10.1, if available. | C |
| hSMFURI | URI of the Nsmf\_PDUSession service of the selected H-SMF, if available. See TS 29.502 [16] clause 6.1.6.2.2. | C |
| requestType | Type of request as initially set within the PDU SESSION ESTABLISHMENT as described in TS 24.501 [13] clause 9.11.3.47.If the initial value is no longer available the request type shall be set to “existing PDU session”. | M |
| accessType | Access type associated with the session (i.e. 3GPP or non-3GPP access) if provided by the AMF (see TS 24.501 [13] clause 9.11.2.1A). | C |
| rATType | RAT type associated with the access if provided by the AMF as part of session establishment (see TS 23.502 [4] clause 4.3.2). Values given as per TS 29.571 [17] clause 5.4.3.2. | C |
| sMPDUDNRequest | Contents of the SM PDU DN request container, if available, as described in TS 24.501 [13] clause 9.11.4.15. | C |
| timeOfSessionEstablishment | Time at which the session establishment occurred, if available. Shall be given qualified with time zone information (i.e. as UTC or offset from UTC, not as local time). | C |

The IRI-POI present in the SMF generating an xIRI containing a SMFStartOfInterceptionWithEstablishedPDUSession record shall set the Payload Direction field in the PDU header to *not applicable* (see ETSI TS 103 221-2 [8] clause 5.2.6).

#### \*\*\* END OF THIRD CHANGE \*\*\*

#### \*\*\* FORTH CHANGE \*\*\*

##### 6.2.3.2.6 SMF unsuccessful procedure

The IRI-POI in the SMF shall generate an xIRI containing an SMFUnsuccessfulProcedure record when the IRI-POI present in the SMF detects an unsuccessful procedure or error condition for a UE matching one of the target identifiers provided via LI\_X1.

Accordingly, the IRI-POI in the SMF generates the xIRI when one of the following events are detected:

- SMF sends a PDU SESSION ESTABLISHMENT REJECT message to the target UE.

- SMF sends a PDU SESSION MODIFICATION REJECT message to the target UE.

- SMF sends a PDU SESSION RELEASE REJECT message to the target UE.

- SMF receives a PDU SESSION MODIFICATION COMMAND REJECT message from the target UE.

- An ongoing SM procedure is aborted at the SMF, due to e.g. a 5GSM STATUS message sent from or received by the SMF.

Table 6.2.3-5: Payload for SMFUnsuccessfulProcedure record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| failedProcedureType | Specifies the procedure which failed or is aborted at the SMF. | M |
| failureCause | Provides the value of the 5GSM cause, see TS 24.501 [13], clause 9.11.4.2. In case the procedure is aborted due to a 5GSM STATUS message, the 5GSM cause is the one included in the 5GSM status message. | M |
| requestedSlice | Slice requested for the procedure, if available, given as a NSSAI (a list of S-NSSAI values as described in TS 24.501 [13] clause 9.11.3.37). | C |
| initiator | Specifies whether the network (SMF) or the UE is initiating the rejection or indicating the failure. | M |
| sUPI | SUPI associated with the procedure, if available (see NOTE). | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI has not been authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI used in the procedure, if available (see NOTE). | C |
| gPSI | GPSI used in the procedure, if available (see NOTE). | C |
| pDUSessionID | PDU Session ID See clause 9.4 of TS 24.501 [13], if available. | C |
| uEEndpoint | UE endpoint address(es) if available. | C |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| dNN | Data Network Name associated with the target traffic, as defined in TS 23.003 [19] clause 9A and described in TS 23.501 [2] clause 4.3.2.2, if available. Shall be given in dotted-label presentation format as described in TS 23.003 [19] clause 9.1. | C |
| aMFID | Identifier of the AMF associated with the target UE, as defined in TS 23.003 [19] clause 2.10.1 when available. | C |
| hSMFURI | URI of the Nsmf\_PDUSession service of the selected H-SMF, if available. See TS 29.502 [16] clause 6.1.6.2.2. | C |
| requestType | Type of request as described in TS 24.501 [13] clause 9.11.3.47, if available.Otherwise depending on the REJECT event the following request type shall be reported: PDU SESSION ESTABLISHMENT REJECT: The request type shall be set to the one reported within the PDU SESSION ESTABLISHMENT or if there hasn't been one reported or is no longer available it should be set to "initial request".PDU SESSION MODIFICATION REJECT: "modification request”PDU SESSION RELEASE REJECT: -PDU SESSION MODIFICATION COMMAND REJECT: "modification request” | C |
| accessType | Access type associated with the session (i.e. 3GPP or non-3GPP access) if provided by the AMF (see TS 24.501 [13] clause 9.11.2.1A). | C |
| rATType | RAT Type associated with the access if provided by the AMF as part of session establishment (see TS 23.502 [4] clause 4.3.2). Values given as per TS 29.571 [17] clause 5.4.3.2. | C |
| sMPDUDNRequest | Contents of the SM PDU DN Request container, if available, as described in TS 24.501 [13] clause 9.11.4.15. | C |
| NOTE: At least one identity shall be provided, the others shall be provided if available. |

#### \*\*\* END OF FORTH CHANGE \*\*\*

#### \*\*\* FIFTH CHANGE \*\*\*

6.2.3.2.7.2 MA PDU session establishment

The IRI-POI in the SMF shall generate an xIRI containing an SMFMAPDUSessionEstablishment record when the IRI-POI present in the SMF detects that a PDU session has been established for the target UE that is an MA PDU session (Request Type set to MA PDU session or upgraded at establishment), or where the upgrade allowed parameter is set to upgrade allowed and session is established as an ordinary PDU session (not upgraded at establishment, but may occur later on). The IRI-POI present in the SMF shall generate the xIRI for the following events:

- For a non-roaming scenario , the SMF sends the N1 NAS message (via AMF) PDU Session Establishment Accept to the UE for a new PDU session and the 5G Session Management (5GSM) state within the SMF is changed to PDU SESSION ACTIVE (see TS 24.501 [13]) in response to a PDU Session Establishment request received along with:

- PDU Session ID which does not identify an existing PDU session, and

- Request Type = MA PDU request, or

- Request Type = initial request and MA PDU session information set to "MA PDU session network upgrade is allowed", with either upgrade occuring at establishment or upgrade does not occur at establishment but may occur later.

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) sends the N16: Nsmf\_PDU\_Session\_Create response message with n1SmInfoToUe IE containing the PDU SESSION ESTABLISHMENT ACCEPT (see TS 29.502 [16]) for a new PDU session in response to a PDU Session Establishment request received along with:

- PDU Session ID which does not identify an existing PDU session, and

- Request Type = MA PDU request, or

- Request Type = initial request and MA PDU session information set to "MA PDU session network upgrade is allowed", with either upgrade occuring at establishment or upgrade does not occur at establishment but may occur later.

Table 6.2.3-5A: Payload for SMFMAPDUSessionEstablishment record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions (see NOTE). | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI has not been authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available (see NOTE). | C |
| gPSI | GPSI associated with the PDU session if available (see NOTE). | C |
| pDUSessionID | PDU Session ID See clause 9.4 of TS 24.501 [13]. Identifies a new PDU session. | M |
| pDUSessionType | Identifies selected PDU session type, see TS 24.501 [13] clause 9.11.4.11. | M |
| accessInfo | Identifies the access(es) associated with the PDU session including the information for each specific access (see Table 6.2.3-5B) | M |
| sNSSAI | Slice identifiers associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| uEEndpoint | UE endpoint address(es) if available. | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| dNN | Data Network Name associated with the target traffic, as defined in TS 23.003[19] clause 9A and described in TS 23.501 [2] clause 4.3.2.2. Shall be given in dotted-label presentation format as described in TS 23.003 [19] clause 9.1. | M |
| aMFID | Identifier of the AMF associated with the target UE, as defined in TS 23.003 [19] clause 2.10.1 when available. | C |
| hSMFURI | URI of the Nsmf\_PDUSession service of the selected H-SMF, if available. See TS 29.502 [16] clause 6.1.6.2.2. | C |
| requestType | Type of request as described in TS 24.501 [13] clause 9.11.3.47 provided within the Nsmf\_PDU\_Session\_CreateSMContext Request (TS 29.502 [16]) message shall be reported.In the case where the network does not provide a request type value for a MA PDU session and the network does support MA PDU sessions, the request type shall be set to “MA PDU request” according to TS 24.501 [13] clause 6.4.1.2. | C |
| sMPDUDNRequest | Contents of the SM PDU DN Request container, if available, as described in TS 24.501 [13] clause 9.11.4.15. | C |
| servingNetwork | PLMN ID of the serving core network operator, and, for a Non-Public Network (NPN), the NID that together with the PLMN ID identifies the NPN. | M |
| oldPDUSessionID | The old PDU Session ID received from the UE. See clauses 4.3.2.2.1 and 4.3.5.2 of TS 23.502 [4] and clause 6.4.1.2 of TS 24.501 [13]. Include if known.  | C |
| mAUpgradeIndication | Indicates whether the PDU session is allowed to be upgraded to MA-Confirmed MA PDU session (see clause 4.22.3 of TS 23.502 [4]). Include if known. | C |
| ePSPDNCnxInfo | Indicates if the PDU session may be moved to EPS during its lifetime (see TS 29.502 [16] clause 6.1.6.2.31). Include if known.  | C |
| mAAcceptedIndication | Indicates that a request to establish an MA PDU session was accepted or if a single access PDU session request was upgraded into a MA PDU session (see clauses 4.22.2 and 4.22.3 of TS 23.502 [4]).It shall be set as follows:- true: MA-Confirmed MA PDU session was established- false: single access MA-Upgrade-Allowed MA PDU session was established that may be upgraded to an MA-Confirmed MA PDU session. | M |
| aTSSSContainer | Identifies the steering, switching, and splitting features for the MA-Confirmed MA PDU session. Also indicates whether MPTCP or ATSSS-LL is to be used for ATSSS. See 9.11.4.22 of 24.501[13]. | C |
| NOTE: At least one of the SUPI, PEI or GPSI fields shall be present. |

Table 6.2.3-5B: Contents of Access Info parameter

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| accessType | Access type associated with the session (i.e. 3GPP or non-3GPP access) as provided by the AMF (see TS 24.501 [13] clause 9.11.2.1A). | M |
| rATType | RAT Type associated with the access as provided by the AMF as part of session establishment (see TS 23.502 [4] clause 4.3.2). Values given as per TS 29.571 [17] clause 5.4.3.2. | C |
| gTPTunnelID | Contains the F-TEID identifying the GTP tunnel used to encapsulate the traffic, as defined in TS 29.244 [15] clause 8.2.3. Non-GTP encapsulation is for further study. | M |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| establishmentStatus | Indicates whether the access type is established or released. | M |
| aNTypeToReactivate | Indicates the Access Network Type for which the UP connection is requested to be re-activated, for an MA PDU session. Applicable to session modification reporting. | C |

#### \*\*\* END OF FIFTH CHANGE \*\*\*

#### \*\*\* SIXTH CHANGE \*\*\*

6.2.3.2.7.3 MA PDU session modification

The IRI-POI in the SMF shall generate an xIRI containing an SMFMAPDUSessionModification record when the IRI-POI present in the SMF detects that an MA PDU session has been modified for the target UE. The IRI-POI present in the SMF shall generate the xIRI for the following events:

- For a non-roaming scenario, the SMF (or for a roaming scenario, V-SMF in the VPLMN), receives the N1 NAS message (via AMF) PDU SESSION MODIFICATION COMMAND COMPLETE from the UE and the 5GSM state within the SMF is returned to PDU SESSION ACTIVE (see TS 24.501 [13]). This applies to the following cases for an MA-Upgrade-Allowed PDU session:

- UE initiated PDU session modification.

- Network (VPLMN) initiated PDU session modification.

- Upgrade to an MA PDU session.

- For a non-roaming scenario, the SMF (or for a roaming scenario, V-SMF in the VPLMN), receives the N1 NAS message (via AMF) PDU SESSION RELEASE COMPLETE from the UE in response to a PDU SESSION RELEASE COMMAND message containing an Access type IE identifying a single access to be released of an MA PDU session which was established over both accesses and the 5GSM state within the SMF remains in the PDU SESSION ACTIVE (see TS 24.501 [13]). This applies to the following case:

- A single access type is released from an MA PDU session, but the MA PDU session continues.

- For a non-roaming scenario, the SMF (or for a roaming scenario, V-SMF in the VPLMN), sends the N1 NAS message (via AMF) PDU SESSION ESTABLISHMENT ACCEPT to the UE and the 5GSM state within the SMF remains in the PDU SESSION ACTIVE (see TS 24.501 [13]). This applies to the following cases:

- Handover from one access type to another access type happens (e.g. 3GPP to non-3GPP) for an MA-Upgrade-Allowed MA PDU session.

- MA PDU Session establishment over second access type.

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) receives the N16: Nsmf\_PDU\_Session\_Update response message with n1SmInfoFromUe IE containing the PDU SESSION MODIFICATION COMMAND COMPLETE (see TS 29.502 [16]). This applies to the following cases for an MA-Upgrade-Allowed PDU session:

- UE initiated PDU session modification.

- Network (VPLMN) initiated PDU session modification.

- Network (HPLMN) initiated PDU session modification.

- Upgrade to an MA PDU session.

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) receives the N16: Nsmf\_PDU\_Session\_Update response message with n1SmInfoFromUe IE containing the PDU SESSION RELEASE COMPLETE message, a response to a PDU SESSION RELEASE COMMAND message containing an Access type IE identifying a single access to be released of an MA PDU session which was established over both accesses and the 5GSM state within the SMF remains in the PDU SESSION ACTIVE (see TS 29.502 [16]). This applies to the following cases:

- A single access type is released from an MA PDU session, but the MA PDU session continues.

- For a home-routed roaming scenario, the SMF in the HPLMN (i.e. H-SMF) sends the N16: Nsmf\_PDU\_Session\_Create response message with n1SmInfoToUe IE containing the PDU SESSION ESTABLISHMENT ACCEPT (see TS 29.502 [16]) while it had received an N16 Nsmf\_PDU\_Session\_Create request message with an existing PDU Session Id with access type being changed. This applies to the following cases:

- Handover from one access type to another access type happens (e.g. 3GPP to non-3GPP) for an MA-Upgrade-Allowed PDU session.

- MA PDU Session establishment over second access type.

Table 6.2.3-5C: Payload for SMFMAPDUSessionModification record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions. | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message, and set to “true” if the SUPI was not authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available. | C |
| gPSI | GPSI associated with the PDU session if available. | C |
| pDUSessionID | PDU Session ID See clause 9.4 of TS 24.501 [13]. | M |
| accessInfo | Identifies the access(es) associated with the PDU session including the information for each specific access (see Table 6.2.3-5B) being modified.  | C |
| sNSSAI | Slice identifier associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| requestType | For both a UE- as well as a network-requested PDU session, the POI (SMF) shall set the requestType parameter to "modification request". | C |
| servingNetwork | PLMN ID of the serving core network operator, and, for a Non-Public Network (NPN), the NID that together with the PLMN ID identifies the NPN. | M |
| oldPDUSessionID | The old PDU Session ID received from the UE. See clauses 4.3.2.2.1 and 4.3.5.2 of TS 23.502 [4] and clause 6.4.1.2 of TS 24.501 [13]. Include if known.  | C |
| mAUpgradeIndication | Indicates whether the PDU session is allowed to be upgraded to MA PDU session (see clause 4.22.3 of 3GPP TS 23.502 [4]). Include if known. | C |
| ePSPDNCnxInfo | Indicates if the PDU session may be moved to EPS during its lifetime (see TS 29.502 [16] clause 6.1.6.2.31). Include if known.  | C |
| mAAcceptedIndication | Indicates that a request to establish an MA PDU session was accepted or if a single access PDU session request was upgraded into a MA PDU session (see clauses 4.22.2 and 4.22.3 of TS 23.502 [4]).It shall be set as follows:- true: MA-Confirmed MA PDU session was established- false: single access MA-Upgrade-Allowed MA PDU session was established that may be upgraded to an MA-Confirmed MA PDU session. | M |
| aTSSSContainer | Identifies the steering, switching, and splitting features for the MA-Confirmed MA PDU session. Also indicates whether MPTCP or ATSSS-LL is to be used for ATSSS. See clause 9.11.4.22 of TS 24.501 [13]. | C |

#### \*\*\* END OF SIXTH CHANGE \*\*\*

#### \*\*\* SEVENTH CHANGE \*\*\*

6.2.3.2.7.5 Start of interception with an established MA PDU session

The IRI-POI in the SMF shall generate an xIRI containing an SMFStartOfInterceptionWithEstablishedMAPDUSession record when the IRI-POI present in the SMF detects that a MA PDU session has already been established for the target UE when interception starts.

In a non-roaming scenario, the IRI-POI in the SMF (or in a roaming scenario, the IRI-POI in the V-SMF in the VPLMN) shall generate the xIRI containing the SMFStartOfInterceptionWithEstablishedMAPDUSession record when it detects that a new interception for a UE is activated (i.e. provisioned by the LIPF) for the following case for an MA PDU session that is either MA-Confirmed or MA-Upgrade-Allowed:

- The 5GSM state within the SMF for that UE is 5GSM: PDU SESSION ACTIVE or PDU SESSION MODIFICATION PENDING.

NOTE: The above trigger happens when the SMF (V-SMF in VPLMN) had not sent an N1 NAS message PDU SESSION RELEASE COMMAND to the UE to release the entire MA PDU session and the SMF (V-SMF in the VPLMN) had previously sent an N1 NAS message PDU SESSION ESTABLISHMENT ACCEPT to that UE for the same MA PDU session.

In a home-routed roaming scenario, the IRI-POI in the H-SMF shall generate the xIRI containing the SMFStartOfInterceptionWithEstablishedMAPDUSession record when it detects that a new interception for a UE is activated (i.e. provisioned by the LIPF) for the following case for an MA PDU session that is either MA-Confirmed or MA-Upgrade-Allowed:

- The H-SMF had not sent an Nsmf\_PDU\_Session\_Update Request (n1SmInfoToUe: PDU SESSION RELEASE COMMAND to release the entire MA PDU session) to the V-SMF for a PDU session and H-SMF had previously sent an Nsmf\_PDU\_Session\_Create response (n1SmInfoToUE: PDU SESSION ESTABLISHMENT ACCEPT) to the V-SMF for that PDU session.

The IRI-POI in the SMF shall generate the xIRI containing the SMFStartOfInterceptionWithEstablishedMAPDUSession record for each of the MA PDU sessions (that meets the above criteria) associated with the newly identified target UEs.

Table 6.2.3-5E: Payload for SMFStartOfInterceptionWithEstablishedMAPDUSession record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions. | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI has not been authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available. | C |
| gPSI | GPSI associated with the PDU session if available. | C |
| pDUSessionID | PDU Session ID as assigned by the AMF, as defined in TS 24.007 [14] clause 11.2.3.1b. | M |
| pDUSessionType | Identifies selected PDU session type, see TS 24.501 [13] clause 9.11.4.11. | M |
| accessInfo | Identifies the access(es) associated with the PDU session including the information for each specific access (see Table 6.2.3-5B). | M |
| sNSSAI | Slice identifier associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| uEEndpoint | UE endpoint address(es) if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). MAC addresses are given as 6 octets with the most significant octet first. | C |
| location | Location information provided by the AMF at session establishment, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| dNN | Data Network Name associated with the target traffic, as defined in TS 23.003 [19] clause 9A and described in TS 23.501 [2] clause 4.3.2.2. Shall be given in dotted-label presentation format as described in TS 23.003 [19] clause 9.1. | M |
| aMFID | Identifier of the AMF associated with the target UE, as defined in TS 23.003 [19] clause 2.10.1, if available. | C |
| hSMFURI | URI of the Nsmf\_PDUSession service of the selected H-SMF, if available. See TS 29.502 [16] clause 6.1.6.2.2. | C |
| requestType | Type of request as initially set within PDU SESSION ESTABLISHMENT as described in TS 24.501 [13] clause 9.11.3.47.If the initial value is no longer available the request type shall be set to “existing PDU session”. | C |
| sMPDUDNRequest | Contents of the SM PDU DN request container, if available, as described in TS 24.501 [13] clause 9.11.4.15. | C |
| servingNetwork | PLMN ID of the serving core network operator, and, for a Non-Public Network (NPN), the NID that together with the PLMN ID identifies the NPN. | M |
| oldPDUSessionID | The old PDU Session ID received from the UE. See clauses 4.3.2.2.1 and 4.3.5.2 of TS 23.502 [4] and clause 6.4.1.2 of TS 24.501 [13]. Include if known. | C |
| mAUpgradeIndication | Indicates whether the PDU session is allowed to be upgraded to MA PDU session (see clause 4.22.3 of TS 23.502 [4]). Include if known. | C |
| ePSPDNCnxInfo | Indicates if the PDU session may be moved to EPS during its lifetime (see TS 29.502 [16] clause 6.1.6.2.31). Include if known. | C |
| mAAcceptedIndication | Indicates that a request to establish an MA PDU session was accepted or if a single access PDU session request was upgraded into an MA PDU session (see clauses 4.22.2 and 4.22.3 of TS 23.502 [4]).It shall be set as follows:- true: MA-Confirmed MA PDU session was established.- false: single access MA-Upgrade-Allowed MA PDU session was established that may be upgraded to an MA-Confirmed MA PDU session. | M |
| aTSSSContainer | Identifies the steering, switching, and splitting features for the MA-Confirmed MA PDU session. Also indicates whether MPTCP or ATSSS-LL is to be used for ATSSS. See clause 9.11.4.22 of TS 24.501 [13].  | C |

The IRI-POI present in the SMF generating an xIRI containing a SMFStartOfInterceptionWithEstablishedMAPDUSession record shall set the Payload Direction field in the PDU header to not applicable (see ETSI TS 103 221-2 [8] clause 5.2.6).

#### \*\*\* END OF SEVENTH CHANGE \*\*\*

#### \*\*\* EIGHTH CHANGE \*\*\*

6.2.3.2.7.6 SMF MA unsuccessful procedure

The IRI-POI in the SMF shall generate an xIRI containing an SMFMAUnsuccessfulProcedure record when the IRI-POI present in the SMF detects an unsuccessful procedure or error condition for a UE matching one of the target identifiers provided via LI\_X1.

Accordingly, the IRI-POI in the SMF generates the xIRI when one of the following events are detected:

- SMF sends a PDU SESSION ESTABLISHMENT REJECT message to the target UE for MA-Confirmed and MA-Upgrade-Allowed MA PDU sessions.

- SMF sends a PDU SESSION MODIFICATION REJECT message to the target UE for MA-Confirmed and MA-Upgrade-Allowed MA PDU sessions.

- SMF sends a PDU SESSION RELEASE REJECT message to the target UE for MA-Confirmed and MA-Upgrade-Allowed MA PDU sessions.

- SMF receives a PDU SESSION MODIFICATION COMMAND REJECT message from the target UE for MA-Confirmed and MA-Upgrade-Allowed MA PDU sessions.

- An ongoing SM procedure is aborted at the SMF, due to e.g. a 5GSM STATUS message sent from or received by the SMF for MA-Confirmed and MA-Upgrade-Allowed MA PDU sessions.

Table 6.2.3-5F: Payload for SMFMAUnsuccessfulProcedure record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| failedProcedureType | Specifies the procedure which failed or is aborted at the SMF. | M |
| failureCause | Provides the value of the 5GSM cause, see TS 24.501 [13], clause 9.11.4.2. In case the procedure is aborted due to a 5GSM STATUS message, the 5GSM cause is the one included in the 5GSM status message. | M |
| requestedSlice | Slice requested for the procedure, if available, given as a NSSAI (a list of S-NSSAI values as described in TS 24.501 [13] clause 9.11.3.37). | C |
| initiator | Specifies whether the network (SMF) or the UE is initiating the rejection or indicating the failure. | M |
| sUPI | SUPI associated with the procedure, if available (see NOTE). | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message and set to “true” if the SUPI has not been authenticated, or “false” if it has been authenticated. | C |
| pEI | PEI used in the procedure, if available (see NOTE). | C |
| gPSI | GPSI used in the procedure, if available (see NOTE). | C |
| pDUSessionID | PDU Session ID See clause 9.4 of TS 24.501 [13], if available. | C |
| accessInfo | Identifies the access(es) associated with the PDU session including the information for each specific access (see Table 6.2.3-5B). | M |
| uEEndpoint | UE endpoint address(es) if available. | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| dNN | Data Network Name associated with the target traffic, as defined in TS 23.003 [19] clause 9A and described in TS 23.501 [2] clause 4.3.2.2, if available. Shall be given in dotted-label presentation format as described in TS 23.003 [19] clause 9.1. | C |
| aMFID | Identifier of the AMF associated with the target UE, as defined in TS 23.003 [19] clause 2.10.1 when available. | C |
| hSMFURI | URI of the Nsmf\_PDUSession service of the selected H-SMF, if available. See TS 29.502 [16] clause 6.1.6.2.2. | C |
| requestType | Type of request as described in TS 24.501 [13] clause 9.11.3.47, if available.Otherwise depending on the REJECT event the following request type shall be reported: PDU SESSION ESTABLISHMENT REJECT: The request type shall be set to the one reported within the PDU SESSION ESTABLISHMENT or if there hasn't been one reported it should be set to "MA PDU request".PDU SESSION MODIFICATION REJECT: "modification request”PDU SESSION RELEASE REJECT: -PDU SESSION MODIFICATION COMMAND REJECT: "modification request” | C |
| sMPDUDNRequest | Contents of the SM PDU DN Request container, if available, as described in TS 24.501 [13] clause 9.11.4.15. | C |
| NOTE: At least one identity shall be provided, the others shall be provided if available. |

#### \*\*\* END OF EIGHTH CHANGE \*\*\*

#### \*\*\* NINTH CHANGE \*\*\*

##### 6.2.3.2.8 PDU to MA PDU session modification

The IRI-POI in the SMF shall generate an xIRI containing an SMFPDUtoMAPDUSessionModification record when the IRI-POI present in the SMF detects that an existing PDU session for the target UE has been successfully modified to an MA PDU session using the PDU session modification procedures as described in TS 24.501 [13]. A PDU session is considered to be successfully modified to a MA PDU session, when all of the following are true:

1. The UE is registered to both 3GPP access and non-3GPP access:

- In the same PLMN (non-roaming UE).

- In the different PLMNs (roaming UE).

2. SMF receives the PDU SESSION MODIFICATION REQUEST from the UE (clause 8.2.10 in TS 24.501 [13]) that includes one of the following:

- *modification request* and includes MA PDU session information IE set to *MA PDU session network upgrade allowed*.

- *MA PDU request*.

3. SMF sends a PDU SESSION MODIFICATION COMMAND to the UE that includes the ATSSS IE (clause 6.4.2.3 in TS 24.501 [13]).

4. SMF receives the PDU SESSION MODIFICATION COMPLETE from the UE (clause 8.3.10.1 in TS 24.501 [13]).

5. The 5GSM state within the SMF is PDU Session Active.

Once the SMFPDUtoMAPDUSessionModification record has been generated by the IRI-POI in the SMF, the IRI-POI shall follow clause 6.2.3.2.7 of the present document for further reporting for this MA PDU session.

Table 6.2.3-5G: Payload for SMFPDUtoMAPDUSessionModification record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI associated with the PDU session (e.g. as provided by the AMF in the associated Nsmf\_PDU\_Session\_CreateSMContext service operation). Shall be present except for PEI-only unauthenticated emergency sessions. | C |
| sUPIUnauthenticated | Shall be present if a SUPI is present in the message, and set to *true* if the SUPI was not authenticated, or *false* if it has been authenticated. | C |
| pEI | PEI associated with the PDU session if available. | C |
| gPSI | GPSI associated with the PDU session if available. | C |
| sNSSAI | Slice identifier associated with the PDU session, if available. See TS 23.003 [19] clause 28.4.2 and TS 23.501 [2] clause 5.12.2.2. | C |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| location | Location information provided by the AMF, if available.Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*), see Annex A. | C |
| requestType | In accordance with the request type as described in TS 24.501 [13] clause 6.4.2.2 and clause 9.11.3.47 a request type of “modification request” shall be reported. | M |
| accessType | Access type associated with the session (i.e. 3GPP or non-3GPP access) if provided by the AMF (see TS 24.501 [13] clause 9.11.2.1A). | C |
| rATType | RAT type associated with the access, if available. Values given as per TS 29.571 [17] clause 5.4.3.2. | C |
| pDUSessionID | PDU Session ID See TS 24.501 [13] clause 9.4. | M |
| requestIndication | Indicates the request type for PDU session modification as indicated by the requestIndication sent in the PDU SESSION MODIFICATION REQUEST (see TS 29.502 [16] clause 6.1.6.3.6). | M |
| aTSSSContainer | Identifies the steering, switching, and splitting features for the MA-Confirmed MA PDU session. Also indicates whether MPTCP or ATSSS-LL is to be used for ATSSS. See TS 24.501 [13] clause 9.11.4.22. | M |

#### \*\*\* END OF NINTH CHANGE \*\*\*

#### \*\*\* END OF ALL CHANGES \*\*\*