**3GPP TSG-SA3 Meeting #87-LI-e-a *s3i220524r2***

**Online, , 5th Oct 2022 - 7th Oct 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **33.128** | **CR** | **0424** | **rev** | **1** | **Current version:** | **18.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction of AMFLocationUpdate Record |
|  |  |
| ***Source to WG:*** | SA3-LI (Rogers Communications Canada) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** | LI17 |  | ***Date:*** | 2022-10-07 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | AMFLocationUpdate IRI was extended by mistake in CR 0166 with some irrelevant parameters. |
|  |  |
| ***Summary of change:*** | The respective changes to AMFLocationUpdate inttroduced in CR 0166 are reverted. |
|  |  |
| ***Consequences if not approved:*** | Confusing specification, potential inconsistent implmentation and redundant reporting. |
|  |  |
| ***Clauses affected:*** | 6.2.2.2.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Mirror of CR 0423 |
|  |  |
| ***This CR's revision history:*** |  |

START OF CHANGE

6.2.2.2.4 Location update

The IRI-POI in the AMF shall generate an xIRI containing an AMFLocationUpdate record each time the IRI-POI present in an AMF detects that the target’s UE location is updated due to target UE mobility or as a part of an AMF service procedure and the reporting of location information is not restricted by service scoping. The generation of such separate xIRI is not required if the updated UE location information is obtained as a part of a procedure producing some other xIRIs (e.g. mobility registration). In that case the location information is included into the respective xIRI. For the responses to location acquisition requests initiated by LARF, as described in TS 33.127 [5] the location update xIRIs shall not be generated.

The UE mobility events resulting in generation of an AMFLocationUpdate xIRI include the *N2 Path Switch Request* (*Xn based inter NG-RAN handover* procedure described in TS 23.502 [4] clause 4.9.1.2) and the *N2 Handover Notify* (*Inter NG-RAN node N2 based handover* procedure described in TS 23.502 [4] clause 4.9.1.3).

The AMFLocationUpdate xIRI is also generated when the AMF receives an NG-RAN NGAP *PDU Session Resource Modify Indication* message as a result of Dual Connectivity activation/release for the target UE, as described in TS 37.340 [37] clause 10.

Optionally, based on operator policy, other NG-RAN NGAP messages that do not generate separate xIRI but carry location information (e.g. RRC INACTIVE TRANSITION REPORT) may trigger the generation of an xIRI AMFLocationUpdate record.

Additionally, based on regulatory requirements and operator policy, the location information obtained by AMF from NG-RAN or LMF in the course of some service operation (e.g. emergency services, LCS) may generate xIRI AMFLocationUpdate record. The AMF services providing the location information in these cases include the AMF Location Service (ProvideLocInfo, ProvidePosInfo, NotifiedPosInfo and EventNotify service operations) and the AMF Exposure Service (AmfEventReport with LOCATION\_REPORT) (see TS 29.518 [22]). Additionally, the AMF Communication Service (Namf\_Communication\_N1MessageNotify service operation) may be monitored to capture the location information in the scenarios described in TS 23.273 [42] clause 6.3.1. Also, in the case of Mobile Originated LCS service invoked by the target, the location information may be derived from a Nlmf\_Location\_DetermineLocation Response to AMF (see TS 23.273 [42] clause 6.2).

**Table 6.2.2-3: Payload for AMFLocationUpdate record**

|  |  |  |
| --- | --- | --- |
| **Field name** | **Description** | **M/C/O** |
| sUPI | SUPI associated with the location update (see clause 6.2.2.4). | M |
| sUCI | SUCI associated with the location update, if available, see TS 24.501 [13]. | C |
| pEI | PEI associated with the location update, if available. | C |
| gPSI | GPSI associated with the location update, if available as part of the subscription profile. | C |
| gUTI | 5G-GUTI associated with the location update, if available, see TS 24.501 [13]. | C |
| location | Updated location information determined by the network.Depending on the service or message type from which the location information is extracted, it may be encoded in several forms (Annex A):1) as a *userLocation* parameter (*location>locationInfo>userLocation*) in the case the information is obtained from an NGAP message, except the LOCATION REPORT message (see TS 38.413 [23]);2) as a *locationInfo* parameter (*location>locationInfo*) in the case the information is obtained from a **ProvideLocInfo** (TS 29.518 [22] clause 6.4.6.2.6);3) as a *locationPresenceReport* parameter (*location>locationPresenceReport*) in the case the information is obtained from an **AmfEventReport** (TS 29.518 [22] clause 6.2.6.2.5) with event type **Location-Report** or **Presence-In-AOI-Report;**4) as a *positionInfo* parameter (*location>positioningInfo>positionInfo*) in the case the information is obtained from a **ProvidePosInfo** (TS 29.518 [22] clause 6.4.6.2.3) or a **NotifiedPosInfo** (TS 29.518 [22] clause 6.4.6.2.4). | M |
| sMSoverNASIndicator | No longer used in present version of this specification. | O |
| oldGUTI | GUTI or 5G-GUTI, if provided (e.g. in REGISTRATION REQUEST message, when performing S1 to N1 inter-system change), see TS 24.501 [13] clause 8.2.6.12. | C |

END OF CHANGE