**3GPP TSG- Meeting # *87***

**, , -**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Alignment of Cell Site Information reporting Stage 2 |
|  |  |
| ***Source to WG:*** | SA3- LI () |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 26 Jan 2023 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | There is currently a mismatch between the naming conventions of cell supplemental information in 33.127 vs the cell site report in 33.128. This CR aligns the terminology while adding new capability to report cell radio related information as part of cell database reporting. |
|  |  |
| ***Summary of change:*** | Add abbreviations for CSR and CRRR, Modification of text in clause 7.3.1, Modification of text in clause 7.3.4, Correction to diagram in Figure 7.3.4-1 |
|  |  |
| ***Consequences if not approved:*** | There will be a mismatch of text in 33.127 and 33.128. Information available and reportable to LEAs will be missing. |
|  |  |
| ***Clauses affected:*** | 3.3, 7.3.1, 7.3.4, Figure 7.3.4-1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Was s3i230040 |

START OF FIRST CHANGE

END OF FIRST CHANGE

3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core Network

5GMS 5G Media Streaming

5GS 5G System

AAnF AKMA Anchor Function

AC Application Client

ACR Application Context Relocation

ADMF LI Administration Function

AF Application Function

AF\_ID Application Function Identity

AKA Authentication and Key Agreement

A-KID AKMA Key IDentifier

AKMA Authentication and Key Management for Applications

AMF Access and Mobility Management Function

AS Application Server

AUSF Authentication Server Function

BBIFF Bearer Binding Intercept and Forward Function

BSS Business Support System

CAG Closed Access Group

CC Content of Communication

CP Control Plane

CPIM Common Presence and Instant Messaging

CPS Call Placement Service

CRRR Cell Radio Related Report

CSI Cell Supplemental Information

CSP Communication Service Provider

CSR Cell Site Report

CUPS Control and User Plane Separation

DN Data Network

DNAI Data Network Access Identifier

DoNAS Data over NAS

EAP Extensible Authentication Protocol

EAS Edge Application Server

eCNAM Enhanced Calling Name

ECSP Edge Computing Service Provider

E-CSCF Emergency – Call Session Control Function

EDN Edge Data Network

EEC Edge Enabler Client

EECID Edge Enabler Client IDentifier

EES Edge Enabler Server

GPSI Generic Public Subscription Identifier

HMEE Hardware Mediated Execution Enclave

HR Home Routed

IBCF Interconnection Border Control Functions

ICF Identity Caching Function

IEF Identity Event Function

IMS-AGW IMS Access Gateway

IM-MGW IM Media Gateway

IP Interception Product

IQF Identity Query Function

IRI Intercept Related Information

KAF AKMA Application Key

KAKMA AKMA Anchor Key

KID Key IDentifier

KLI Decryption key(s) for services encrypted by CSP-provided keys

KSF Key Server Function

LAF Location Acquisition Function

LALS Lawful Access Location Services

LARF Location Acquisition Requesting Function

LBO Local Break Out

LEA Law Enforcement Agency

LEMF Law Enforcement Monitoring Facility

LI Lawful Interception

LI CA Lawful Interception Certificate Authority

LICF Lawful Interception Control Function

LI\_HI1 Lawful Interception Handover Interface 1

LI\_HI2 Lawful Interception Handover Interface 2

LI\_HI3 Lawful Interception Handover Interface 3

LI\_HI4 Lawful Interception Handover Interface 4

LI\_HILA Lawful Interception Handover Interface Location Acquisition

LI\_HIQR Lawful Interception Handover Interface Query Response

LIID Lawful Interception Identifier

LIPF Lawful Interception Provisioning Function

LIR Location Immediate Request

LI\_SI Lawful Interception System Information Interface

LISSF Lawful Interception State Storage Function

LI\_ST Lawful Interception State Transfer Interface

LI\_T1 Lawful Interception Internal Triggering Interface 1

LI\_T2 Lawful Interception Internal Triggering Interface 2

LI\_T3 Lawful Interception Internal Triggering Interface 3

LI\_X0 Lawful Interception Internal Interface 0

LI\_X1 Lawful Interception Internal Interface 1

LI\_X2 Lawful Interception Internal Interface 2

LI\_X2\_LA Lawful Interception Internal Interface 2 Location Acquisition

LI\_X3 Lawful Interception Internal Interface 3

LI\_X3A Lawful Interception Internal Interface 3 Aggregator

LI\_XEM1 Lawful Interception Internal Interface Event Management Interface 1

LI\_XER Lawful Interception Internal Interface Event Record

LI\_XLA Lawful Interception Internal Interface Location Acquisition

LI\_XQR Lawful Interception Internal Interface Query Response

LMF Location Management Function

LMISF LI Mirror IMS State Function

LMISF-CC LMISF for the handling of CC

LMISF-IRI LMISF for the handling of IRI

LTF Location Triggering Function

MA Multi-Access

MANO Management and Orchestration

MDF Mediation and Delivery Function

MDF2 Mediation and Delivery Function 2

MDF3 Mediation and Delivery Function 3

MRFP Multimedia Resource Function Processor

MSRP Message Session Relay Protocol

N3A Non-3GPP Access

N3IWF Non 3GPP Inter Working Function

N9HR N9 Home Routed

NAS Non-Access Stratum

NCGI NR Cell Global Identity

NEF Network Exposure Function

NFV Network Function Virtualisation

NFVI Network Function Virtualisation Infrastructure

NFVO Network Function Virtualisation Orchestrator

NIDD Non-IP Data Delivery

NPLI Network Provided Location Information

NR New Radio

NRF Network Repository Function

NSSF Network Slice Selection Function

OSS Operations Support System

PAG POI Aggregator

PCF Policy Control Function

P-CSCF Proxy - Call Session Control Function

PEI Permanent Equipment Identifier

PGW PDN Gateway

PGW-C PDN Gateway Control Plane

PGW-U PDN Gateway User Plane

POI Point Of Interception

PLMN Public Land Mobile Network

PTC Push to Talk over Cellular

RCD Rich Call Data

RCS Rich Communication Suite

S8HR S8 Home Routed

SCEF Service Capability Exposure Function

SCS Service Capability Server

SGW Serving Gateway

SGW-C Serving Gateway Control Plane

SGW-U Serving Gateway User Plane

SHAKEN Signature-based Handling of Asserted information using toKENs

SIRF System Information Retrieval Function

S-CSCF Serving - Call Session Control Function

SIP Session Initiation Protocol

SMF Session Management Function

SMSF SMS-Function

STF Security Terminating Function

STIR Secure Telephony Identity Revisited

SUCI Subscriber Concealed Identifier

SUPI Subscriber Permanent Identifier

TAI Tracking Area Identity

TF Triggering Function

TLS Transport Layer Security

TNGF Trusted Non-3GPP Gateway Function

TrGW Transit Gateway

TWIF Trusted WLAN Interworking Function

UDM Unified Data Management

UDR Unified Data Repository

UDSF Unstructured Data Storage Function

UPF User Plane Function

VNF Virtual Network Function

VNFC Virtual Network Function Component

W-AFG Wireline Access Gateway Function

xCC LI\_X3 Content of Communication

xIRI LI\_X2 Intercept Related Information

END OF FIRST CHANGE

START OF SECOND CHANGE

7.3 Location

7.3.1 General

This clause provides location reporting functionality for both UE location obtained as part of normal network access or user service usage and location actively triggered through location based services or other LALS reporting.

In addition, clause 7.3.4 describes Cell Supplemental Information (CSI) (e.g., civic address, geographical coordinates, azimuth, or operator specific information) derived from CSP databases.

For all UE locations obtained, generated or reported to the MDF2, the POI shall report the time at which the location was established by the location source (e.g. AMF, MME or HSS/UDM) and provide this to the MDF along with the location information.

For all UE locations obtained, generated or reported to the ICF, the IEF shall report the time at which the location was established by the location source (e.g. AMF) and provide this to the ICF along with the location information.

END OF SECOND CHANGE

START OF THIRD CHANGE

7.3.4 Cell database information reporting

When a cell identity is provided for the target's location in an IRI message, the CSP may also provide CSI for the reported cell identity. The CSI can be delivered in two types of information reports, Cell Site Reports (CSR) and Cell Radio Related Reports (CRRR). The MDF2 may retrieve CSI by access to a CSP maintained database (referred to as CSP Cell Database) as shown in figure 7.3.4-1. The CSP delivers the CSI either via the IRI message generated from the corresponding xIRI, or asynchronously in a stand-alone Cell Site Report (CSR) IRI message.

The following information shall be delivered when CSI is provided in IRI message or a MDF2 generated CSR:

- LIID.

- Cell identity.

- Date/time(s) established by MDF2.

- Cell site information.

CSR shall include the physical location (e.g. geographical coordinates) information and coverage area for the reported cell. If the reported cell is not fixed to a permanent location, the report should indicate the cell mobility type (e.g. nomadic cell, vehicle-mounted cell) as well as the time period of the location validity.

If CSI for a cell identity has been previously reported to the LEMF for the current interception, CSI may be omitted, if allowed by the warrant unless the CSI is for a cell that is not fixed to a permanent location.

CRRR includes specific information related to the reported cell. This information may be reported from the NG Interface or F1 interface and may include globalRANNode ID, radio band, PLMNs supported, and other operator specific information that may be reported independently from CSR.

If the CSP does not support CSR or CSI, the database can be provided by non-real-time means.

**Figure 7.3.4-1: CSP Cell Database**

END OF THIRD CHANGE

END OF ALL CHANGES