**3GPP TSG CT WG3 Meeting #138 *C3-246242***

**Orlando, US, 18 - 22 November, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **29.549** | **CR** | **0347** | **rev** | **-** | **Current version:** | **19.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Introduction of ADAE service in SEAL |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | NBI19 |  | ***Date:*** | 2024-10-28 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | ADAE service is specified in SA6 as a part of SEAL. Thus, it shall be consistenly intoroduced in 29.549 with the reference to stage 2 spec in overview clause to keep consistency. |
|  |  |
| ***Summary of change:*** | This CR introduces ADAE service in SEAL. |
|  |  |
| ***Consequences if not approved:*** | Inconsistent definition of ADAE service in clause 4 in 29.549. |
|  |  |
| ***Clauses affected:*** | 4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | * This CR does not impact any OpenAPI file.
 |
| ***()*** |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\* \* \* First Change \* \* \* \*

# 4 Overview

3GPP has considered in 3GPP TS 23.434 [2], 3GPP TS 23.433 [34] (for SEALDD), 3GPP TS 23.435 [41] (for NSCE) and 3GPP TS 23.436 [38] (for ADAE) the development of Service enabler architecture layer for verticals (SEAL) over 3GPP networks to support vertical applications (e.g. V2X applications). It specifies the functional architecture for SEAL and the procedures, information flows and APIs for each service within SEAL in order to support vertical applications over the 3GPP systems. To ensure efficient use and deployment of vertical applications over 3GPP systems, SEAL services includes, group management, configuration management, location management, identity management, key management, network resource management, network slice capability enablement (NSCE), application data analytics enablement (ADAE) and data delivery management (SEALDD).

Clause 6 of 3GPP TS 23.434 [2] specifies the functional entities and domains of the functional model, reference points descriptions and SEAL APIs for SEAL services.

The present document specifies the APIs needed to support SEAL. 3GPP TS 29.548 [35] specifies the APIs needed for SEALDD. 3GPP TS 29.435 [42] specifies the APIs needed for NSCE.

\* \* \* End of changes \* \* \* \*