3GPP TSG CT WG3 Meeting #138 C3-246487

Orlando, US, 18 - 22 November, 2024

**Title: LS on handling of Nsmf events targeting anyUe for I-SMF**

**Release: Release 18**

**Work Item: UPEAS**

**Source: CT3**

**To: SA2**

**Cc:**

**Contact person: Apostolos Papageorgiou**

 **apostolos.papageorgiou@nokia.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** **None**

# 1 Overall description

The agreed SA2 23.502 CR#5108 specified (in 23.502 clause 4.15.4.5.3) that:

*"*

*An SMF receiving Nsmf\_EventExposure Subscription request to subscribe to UPF data for "Any UE", does not consider PDU sessions for which it is acting as I-SMF when it selects the PDU session(s) and the UPFs it has to send the request to*

*"*

CT3 understands that this avoids a duplication of subscriptions and wants to ask the following question:

**Question1:** Is this issue specific to UPF events or can it apply to any event type that is supported by the I-SMF?

# 2 Actions

**To SA2**

**ACTION:** CT3 kindly asks SA2 to answer the above question and update the SA2 specifications respectively, if necessary.

# 3 Dates of next TSG CT WG 3 meetings

CT3#139 17th Feb – 21st Feb 2024 Athens, GR

CT3#140 07th Apr – 11st Apr 2024 TBD, China