**3GPP TSG CT WG3 Meeting #138 *C3-246371***

**Orlando, US, 18th – 22nd November, 2024 was C3-246076**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **0338** | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| ***Title:*** | Define the OpenAPI description of the SS\_ConfirmLocation API | | | | | | | | |
|  |  | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | |
|  |  | | | | | | | | |
| ***Work item code:*** | eLSAPP | | | | |  | ***Date:*** | | 2024-11-18 |
|  |  | | | |  | |  | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | |
| ***Reason for change:*** | | | The "Location history querying" functionality was defined in Rel-19 in clause 9.3.21 of TS 23.434 and led to the introduction of a new LM Server exposed API, i.e., the SS\_ConfirmLocation API. | | | | | | |
|  | | |  | | | | | | |
| ***Summary of change:*** | | | This CR proposes to:   * Define the OpenAPI description of the new SS\_ConfirmLocation API. | | | | | | |
|  | | |  | | | | | | |
| ***Consequences if not approved:*** | | | * The above-detailed Rel-19 updates are not specified in stage 3. | | | | | | |
|  | |  | | | | | | | |
| ***Clauses affected:*** | | A.24 (new Annex) | | | | | | | |
|  | |  | | | | | | | |
|  | | **Y** | | **N** |  | | |  | |
| ***Other specs*** | | **X** | |  | Other core specifications | | | TS 23.434 CR#0342 | |
| ***affected:*** | |  | | **X** | Test specifications | | | TS/TR ... CR ... | |
| ***(show related CRs)*** | |  | | **X** | O&M Specifications | | | TS/TR ... CR ... | |
|  | |  | | | | | | | |
| ***Other comments:*** | | This CR introduces a new OpenAPI description for the new SS\_ConfirmLocation the API introduced in this specification. | | | | | | | |
|  | |  | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | |

\* \* \* \* Start of changes \* \* \* \*

# A.24 SS\_ConfirmLocation API

openapi: 3.0.0

info:

title: LM Server Location Confirmation Service Management Service

version: 1.0.0-alpha.1

description: |

LM Server Location Confirmation Service Management Service.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.549 V19.1.0 Service Enabler Architecture Layer for Verticals (SEAL);

Application Programming Interface (API) specification; Stage 3.

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

servers:

- url: '{apiRoot}/ss-cl/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549.

security:

- {}

- oAuth2ClientCredentials: []

paths:

/subscriptions:

post:

summary: Request the creation of a Location Confirmation Service Subscription.

operationId: CreateLocConfirmSubsc

tags:

- Location Confirmation Service Subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmSubsc'

responses:

'201':

description: >

Created. The Location Confirmation Service Subscription is successfully created and a

representation of the created Individual Location Confirmation Service Subscription

resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmSubsc'

headers:

Location:

description: >

Contains the URI of the created Individual Location Confirmation Service

Subscription resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

LocConfirmUsageNotif:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmUsageNotif'

responses:

'204':

description: >

No Content. The Location Confirmation Service Usage Notification is successfully

received and acknowledged.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/subscription/{subscId}:

parameters:

- name: subscId

in: path

description: >

Represents the identifier of the Individual Location Confirmation Service Subscription

resource.

required: true

schema:

type: string

get:

summary: Retrieve an existing Individual Location Confirmation Service Subscription resource.

operationId: GetIndLocConfirmSubsc

tags:

- Individual Location Confirmation Service Subscription (Document)

responses:

'200':

description: >

OK. The requested Individual Location Confirmation Service Subscription resource shall

be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmSubsc'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Request the update of an existing Individual Location Confirmation Service Subscription resource.

operationId: UpdateIndLocConfirmSubsc

tags:

- Individual Location Confirmation Service Subscription (Document)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmSubsc'

responses:

'200':

description: >

OK. The Individual Location Confirmation Service Subscription resource is successfully

updated and a representation of the updated resource shall be returned in the response

body.

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmSubsc'

'204':

description: >

No Content. The Individual Location Confirmation Service Subscription resource is

successfully updated and no content is returned in the response body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Request the modification of an existing Individual Location Confirmation Service Subscription resource.

operationId: ModifyIndLocConfirmSubsc

tags:

- Individual Location Confirmation Service Subscription (Document)

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/LocConfirmSubscPatch'

responses:

'200':

description: >

OK. The Individual Location Confirmation Service Subscription resource is successfully

modified and a representation of the updated resource shall be returned in the response

body.

content:

application/json:

schema:

$ref: '#/components/schemas/LocConfirmSubsc'

'204':

description: >

No Content. The Individual Location Confirmation Service Subscription resource is

successfully modified and no content is returned in the response body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Request the deletion of an existing Individual Location Confirmation Service Subscription resource.

operationId: DeleteIndLocConfirmSubsc

tags:

- Individual Location Confirmation Service Subscription (Document)

responses:

'204':

description: >

No Content. The Individual Location Confirmation Service Subscription resource is

successfully deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

#

# STRUCTURED DATA TYPES

#

LocConfirmSubsc:

description: >

Represents a Location Confirmation Service Subscription.

type: object

properties:

appId:

type: array

items:

type: string

minItems: 1

valServiceId:

type: array

items:

type: string

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

oneOf:

- required: [appId]

- required: [valServiceId]

LocConfirmSubscPatch:

description: >

Represents the parameters to request the modification of a Location Confirmation Service

Subscription.

type: object

properties:

appId:

type: array

items:

type: string

minItems: 1

valServiceId:

type: array

items:

type: string

minItems: 1

LocConfirmUsageNotif:

description: >

Represents a Location Confirmation Service Usage Notification.

type: object

properties:

reports:

type: array

items:

$ref: '#/components/schemas/LocConfirmUsageReport'

minItems: 0

timestamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- reports

LocConfirmUsageReport:

description: >

Represents a Location Confirmation Service Usage Notification.

type: object

properties:

valUeId:

type: string

timestamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- valUeId

# SIMPLE DATA TYPES

#

#

# ENUMERATIONS

#

# Data types describing alternative data types or combinations of data types

#

\* \* \* \* End of changes \* \* \* \*