**3GPP TSG-SA5 Meeting #158 *S5-247111***

Orlando, USA, 18 - 22 November 2024

**Source:**  **Rakuten Mobile**

**Title: pCR TR 28.869 Add new solution for modification of NF instance**

**Document for: Approval**

**Agenda Item: 6.19.6**

# 1 Decision/action requested

***For approval***

# 2 References

1. 3GPP TR 28.869 v1.1.0 Study on cloud aspects of management and orchestration.

# 3 Rationale

The contribution proposes to add a new solution for modification of NF instance

# 4 Detailed proposal

It is proposed to make the following changes to TR 28.869 [1].

|  |
| --- |
| **1st Change** |

##### 5.2.4.3.X Use of deployment management reference point based on declarative descriptor

In this case, as illustrated in figure 5.2.4.3.X-1, the modified requirements of the deployment of a NF deployment instance are conveyed from the 3GPP management system to the orchestration and management system via a modified version of the declarative descriptor that was used for creation of the NF deployment instance.



Figure 5.2.4.3.X-1. interaction between 3GPP management system and orchestration and management system using deployment management reference point based on declarative descriptor

|  |
| --- |
| **End of Changes** |