**3GPP TSG-SA5 Meeting #158 *S5-247265***

Orlando, Florida, USA, 18 - 22 November 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel19 CR 28.105 Enhance the OpenAPI related to multiplicity |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | SA5 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2024-11-07 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | According to agreed Rel19 TS32.160 CR0071 (S5-245469 TS32.160 clarify the Attribute property "multiplicity" for OpenAPI) ”Attributes of structured type with multiplicity greater than "1" are mapped to a name/value pair whose value is a JSON array, and the items are JSON objects, whose properties are described by the structured data type. The length of the array can be specified using the "minItems" and "maxItems" keywords, each of which must be a non-negative integer. If the low bound is 0, the keyword "minItems" can be omitted. If there is no upper (e.g, specified as \*), the keyword "maxItems" shall not be used.”The OpenAPI stage 3 needs enhancement if the attributes of structured type with multiplicity greater than "1" and mapped to a name/value pair whose value is a JSON array.Additionally, attribute name MLUpdateReport.mLModelModelRef in 7.5.1 is not correct, and the multiplicity is not aligned with the class diagram.Similar issues for MLTrainingReport.mLModelCoordinationGroupGeneratedRefMLTestingRequest.mLModelCoordinationGroupRef, supportedPerformanceIndicators. |
|  |  |
| ***Summary of change:*** | Updating the Stage 3 according to clause 6.1.11.2 in TS32.160Correct the attribute name and multiplicity. |
|  |  |
| ***Consequences if not approved:*** | Multiplicity constraint not supported |
|  |  |
| ***Clauses affected:*** | 7.5.1 , (Normative Stage3 is in forge) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Forge MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1475> at commit 54d3940d4e3288479f676c28eadfd0e5aa35892a |
|  |  |
| ***This CR's revision history:*** | Revision of S5-246454 |

***Start of change***

### 7.5.1 Attribute properties

Table 7.5.1-1

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| mLModelId | It identifies the ML model.It is unique in each MnS producer.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| candidateTrainingDataSource | It provides the address(es) of the candidate training data source provided by MnS consumer. The detailed training data format is vendor specific.allowedValues: N/A. | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| aIMLInferenceName | It indicates the type of inference that the ML model supports. allowedValues: the values of the MDA type (see 3GPP TS 28.104 [2]), Analytics ID(s) of NWDAF (see 3GPP TS 23.288 [3]), types of inference for NG-RAN (see TS 38.300 [16] and TS 38.401 [17]), and vendor's specific extensions. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| areConsumerTrainingDataUsed | It indicates whether the consumer provided training data have been used for the ML model training.allowedValues: ALL, PARTIALLY, NONE. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| usedConsumerTrainingData | It provides the address(es) where lists of the consumer-provided training data are located, which have been used for the ML model training.allowedValues: N/A. | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| trainingRequestRef | It is the DN(s) of the related MLTrainingRequest MOI(s).allowedValues: DN. | type: DN multiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| trainingProcessRef | It is the DN(s) of the related MLTrainingProcess MOI(s) that produced the MLTrainingReport.allowedValues: DN. | type: DN multiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| trainingReportRef | It is the DN of the MLTrainingReport MOI that represents the reports of the ML model training.allowedValues: DN. | type: DN multiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| lastTrainingRef | It is the DN of the MLTrainingReport MOI that represents the reports for the last training of the ML model.allowedValues: DN. | type: DN multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| modelConfidenceIndication | It indicates the average confidence value (in unit of percentage) that the ML model would perform for inference on the data with the same distribution as training data.Essentially, this is a measure of degree of the convergence of the trained ML model.allowedValues: { 0..100 }. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| trainingRequestSource | It describes the model that requested to instantiate the MLTrainingRequest MOI.This attribute can be of type String or DN. | type: <<CHOICE>>multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLTrainingRequest.requestStatus | It describes the status of a particular ML model training request.allowedValues: NOT\_STARTED, IN\_PROGRESS, CANCELLING, SUSPENDED, FINISHED, and CANCELLED. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| mLTrainingProcessId | It identifies the training process.It is unique in each instantiated process in the MnS producer.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| priority | It indicates the priority of the training process.The priority may be used by the ML model training to schedule the training processes. Lower value indicates a higher priority.allowedValues: { 0..65535 }. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0 isNullable: False |
| terminationConditions | It indicates the conditions to be considered by the ML training MnS producer to terminate a specific training process.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| progressStatus | It indicates the status of the process.allowedValues: N/A. | type: ProcessMonitor multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLUpdateProcess.cancelProcess | It allows the ML update MnS consumer to cancel the ML update process.Setting this attribute to "TRUE" cancels the ML update process. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLUpdateProcess.suspendProcess | It allows the ML update MnS consumer to suspend the ML update process.Setting this attribute to "TRUE" suspends the ML update process. The process can be resumed by setting this attribute to “FALSE” when it is suspended. Setting the attribute to "FALSE" has no observable result.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| mLModelVersion | It indicates the version number of the ML model.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| performanceRequirements | It indicates the expected performance for a trained ML model when performing on the training data.allowedValues: N/A. | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| modelPerformanceTraining | It indicates the performance score of the ML model when performing on the training data.allowedValues: N/A. | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| MLTrainingProcess.progressStatus.progressStateInfo | It provides the following specialization for the “progressStateInfo“ attribute of the “ProcessMonitor“ data type for the “MLTrainingProcess.progressStatus“.When the ML model training is in progress, and the " mLTrainingProcess.progressStatus.status " is equal to "RUNNING", it provides the more detailed progress information.allowedValues for " mLTrainingProcess.progressStatus.status " = "RUNNING":- “COLLECTING\_DATA”- “PREPARING\_TRAINING\_DATA”- “TRAINING” + DN of the MLModel being trainedThe allowed values for " mLTrainingProcess.progressStatus.status " = "CANCELLING" are vendor specific.The allowed values for " mLTrainingProcess.progressStatus.status " = "NOT\_STARTED" are vendor specific. | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| inferenceOutputName | It indicates the name of an inference output of an ML model.allowedValues: the name of the MDA output IEs (see 3GPP TS 28.104 [2]), name of analytics output IEs of NWDAF (see TS 23.288 [3]), RAN inference output IE name(s), and vendor's specific extensions. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| performanceMetric | It indicates the performance metric used to evaluate the performance of an ML model, e.g. "accuracy", "precision", "F1 score", etc.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| performanceScore | It indicates the performance score (in unit of percentage) of an ML model when performing inference on a specific data set (Note).The performance metrics may be different for different kinds of ML models depending on the nature of the model. For instance, for numeric prediction, the metric may be accuracy; for classification, the metric may be a combination of precision and recall, like the "F1 score".allowedValues: { 0..100 }. | type: Realmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| MLTrainingRequest.cancelRequest | It allows the ML training MnS consumer to cancel the ML model training request.Setting this attribute to "TRUE" cancels the ML model training request. The request can be resumed by setting this attribute to "FALSE" when it is suspended. Cancellation is possible when the requestStatus is the "NOT\_STARTED", " IN\_PROGRESS", and "SUSPENDED" state. Setting the attribute to "FALSE" has no observable result.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLTrainingRequest.suspendRequest | It allows the ML training MnS consumer to suspend the ML model training request.Setting this attribute to "TRUE" suspends the ML model training process. Suspension is possible when the requestStatus is not the "FINISHED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLTrainingProcess.cancelProcess | It allows the ML training MnS consumer to cancel the ML model training process.Setting this attribute to “TRUE“ cancels the ML model training process. Cancellation is possible when the “mLTrainingProcess.progressStatus.status“ is not the “FINISHED“ state. Setting the attribute to “FALSE“ has no observable result.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLTrainingProcess.suspendProcess | It allows the ML training MnS consumer to suspend the ML model training process.Setting this attribute to "TRUE" suspends the ML model training process. The process can be resumed by setting this attribute to “FALSE” when it is suspended. Suspension is possible when the " mLTrainingProcess.progressStatus.status" is not the "FINISHED", "CANCELLING" or "CANCELLED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| inferenceModelRef | It describes the target entities that will use the ML model for inference. | type: DN multiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| dataProviderRef | It describes the entities that have provided or should provide data needed by the ML model e.g. for training or inference | type: DN multiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| areNewTrainingDataUsed | It indicates whether the other new training data have been used for the ML model training.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| trainingDataQualityScore | It indicates numerical value that represents the dependability/quality of a given observation and measurement type. The lowest value indicates the lowest level of dependability of the data, i.e. that the data is not usable at all. allowedValues: { 0..100 }. | type: Realmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| decisionConfidenceScore | It is the numerical value that represents the dependability/quality of a given decision generated by the AI/ML inference function. The lowest value indicates the lowest level of dependability of the decisions, i.e. that the data is not usable at all.allowedValues: { 0..100 }. | type: Realmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| expectedRuntimeContext | This describes the context where an MLModel is expected to be applied.allowedValues: N/A | type: MLContextmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| trainingContext | This specifies the context under which the MLModel has been trained.allowedValues: N/A | type: MLContextmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| runTimeContext | This specifies the context where the MLmodel or model is being applied.allowedValues: N/A | type: MLContextmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| MLTrainingRequest.mLModelRef | It identifies the DN of the MLModel requested to be trained.allowedValues: DN | type: DNmultiplicity: 0..1isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| MLTrainingReport.mLModelGeneratedRef | It identifies the DN of the MLModel generated by the ML training.allowedValues: DN | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| mLModelRepositoryRef | It identifies the DN of the MLModelRepository. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| mLRepositoryId | It indicates the unique ID of the ML repository. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| modelPerformanceValidation | It indicates the performance score of the ML model when performing on the validation data.allowedValues: N/A | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| dataRatioTrainingAndValidation | It indicates the ratio (in terms of quantity of data samples) of the training data and validation data used during the training and validation process. It is represented by the percentage of the validation data samples in the total training data set (including both training data samples and validation data samples). The value is an integer reflecting the rounded number of percent \* 100. allowedValues: { 0 .. 100 }. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLTestingRequest.requestStatus | It describes the status of a particular ML testing request.allowedValues: NOT\_STARTED, IN\_PROGRESS, CANCELLING, SUSPENDED, FINISHED, and CANCELLED. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLTestingRequest.cancelRequest | It allows the ML testing MnS consumer to cancel the ML testing request.Setting this attribute to "TRUE" cancels the ML testing request. Cancellation is possible when the requestStatus is the "NOT\_STARTED", " IN\_PROGRESS", and "SUSPENDED" state. Setting the attribute to "FALSE" has no observable result.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLTestingRequest.suspendRequest | It allows the ML testing MnS consumer to suspend the ML testing request.Setting this attribute to "TRUE" suspends the ML testing request. The request can be resumed by setting this attribute to “FALSE” when it is suspended. Suspension is possible when the requestStatus is not the "FINISHED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLTestingRequest.mLModelRef | It identifies the DN of the MLModel requested to be tested.AllowedValues: DN | type: DNMultiplicity: 0..1isOrdered: FalsoisUnique: TruedefaultValue: NoneisNullable: True |
| modelPerformanceTesting | It indicates the performance score of the ML model when performing on the testing data.allowedValues: N/A. | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| mLTestingResult | It provides the address where the testing result (including the inference result for each testing data example) is provided.The detailed testing result format is vendor specific.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| testingRequestRef | It identifies the DN of the MLTestingRequest MOI. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| supportedPerformanceIndicators | This parameter lists specific PerformanceIndicator(s) of an ML model.allowedValues: N/A. | type: SupportedPerfIndicator multiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| performanceIndicatorName | It indicates the identifier of the specific performance indicator.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| isSupportedForTraining | It indicates whether the specific performance indicator is supported a performance metric of ML model training for the ML model. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| isSupportedForTesting | It indicates whether the specific performance indicator is supported a performance metric of ML model testing for the ML model. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| mLUpdateProcessRef | It is the DN of the mLUpdateProcess MOI that represents the process of updating an ML model.allowedValues: DN. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| mLUpdateRequestRefList | It is the list of DN of the MLUpdateRequest MOI that represents an ML update request.allowedValues: DN. | type: DNmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| mLUpdateReportRef | It is the DN of the MLUpdateReport MOI that represents an ML update report.allowedValues: DN. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| mLUpdateReportingPeriod | It specifies the time duration upon which the MnS consumer expects the ML update is reported. | type: TimeWindowmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| availMLCapabilityReport | It represents the available ML capabilities.allowedValues: N/A. | type: AvailMLCapabilityReport multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| updatedMLCapability | It represents the updated ML capabilities.allowedValues: N/A. | type: AvailMLCapabilityReport multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| availMLCapabilityReportID | It identifies the available ML capability report.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| newCapabilityVersionId | It indicates the specific version of AI/ML capabilities to be applied for the update. It is typically the one indicated by the MLCapabilityVersionID in a newCapabilityVersion | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| mlCapabilityVersionId | It indicates the version of ML capabilities that is available for the update.  | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| performanceGainThreshold | It defines the minimum performance gain as a percentage that shall be achieved with the capability update, i.e., the difference in the performances between the existing capabilities and the new capabilities should be at least performanceGainThreshold otherwise the new capabilities should not be applied.Allowed value: float between 0.0 and 100.0 | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| expectedPerformanceGains | It indicates the expected performance gain if/when the AI/ML capabilities of the respective network function are updated with/to the specific set of newly available AI/ML capabilities. | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| updateTimeDeadline | It indicates the maximum as stated in the MLUpdate request that should be taken to complete the update | type: TimeWindowmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| MLUpdateReport.mLModelRefList | It indicates the DN of MLModel instances that can be updated. | type: DNmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| MLUpdateRequest.requestStatus | It describes the status of a particular ML update request.allowedValues: NOT\_STARTED, IN\_PROGRESS, CANCELLING, SUSPENDED, FINISHED, and CANCELLED. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLUpdateRequest.cancelRequest | It allows the MnS consumer to cancel the ML update request.Setting this attribute to "TRUE" cancels the ML update request. Cancellation is possible when the requestStatus is the "NOT\_STARTED", " IN\_PROGRESS", and "SUSPENDED" state. Setting the attribute to "FALSE" has no observable result.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLUpdateRequest.suspendRequest | It allows the MnS consumer to suspend the ML update request.Setting this attribute to "TRUE" suspends the ML update request. The request can be resumed by setting this attribute to “FALSE” when it is suspended. Suspension is possible when the requestStatus is not the "FINISHED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| memberMLModelRefList | It identifies the list of member ML models within a level of an ML model coordination group.allowedValues: DN list | type: DNmultiplicity: 2..\*isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| MLTrainingRequest.mLModelCoordinationGroupRef | It identifies the DN of the MLModelCoordinationGroup requested to be trained.allowedValues: DN | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLTrainingReport.mLModelCoordinationGroupGeneratedRef | It identifies the DN of the MLModelCoordinationGroup generated by ML training.AllowedValues: DN | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLTestingRequest.mLModelCoordinationGroupRef | It identifies the DN of the MLEntityCoordinationGroup requested to be tested.AllowedValues: DN | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| retrainingEventsMonitorRef | It indicates the DN of the ThresholdMonitor MOI that indicates the performance measurements and its corresponding thresholds to be used by MnS producer to initiate the re-training of the MLModel. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| sourceTrainedMLModelRef | It identifies the DN of the source trained MLModel whose copy has been loaded from the ML model repository to the inference function. allowedValues: DN | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| MLModelLoadingRequest.requestStatus | It describes the status of a particular ML model loading request.allowedValues: NOT\_STARTED, IN\_PROGRESS, CANCELLING, SUSPENDED, FINISHED, and CANCELLED. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| MLModelLoadingRequest.cancelRequest | It allows the MnS consumer to cancel the ML model loading request.Setting this attribute to "TRUE" cancels the ML model loading. Cancellation is possible when the requestStatus is the "NOT\_STARTED", " IN\_PROGRESS", and "SUSPENDED" state. Setting the attribute to "FALSE" has no observable result.allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLModelLoadingRequest.suspendRequest | It allows the MnS consumer to suspend the ML model loading request.Setting this attribute to "TRUE" suspends the ML model loading request. The request can be resumed by setting this attribute to “FALSE” when it is suspended. Suspension is possible when the requestStatus is not the "FINISHED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| mLModelToLoadRef | It identifies the DN of a trained MLModel requested to be loaded to the target inference function(s). | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| policyForLoading | It provides the policy for controlling ML model loading triggered by the MnS producer.This policy contains two thresholds in the thresholdList attribute. The first threshold is related to the ML model to be loaded, and the second threshold is related to the existing ML model being used for inference. | type: AIMLManagementPolicymultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| thresholdList | It provides the list of threshold.  | type: ThresholdInfomultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| MLModelLoadingProcess.progressStatus.progressStateInfo | It provides the following specialization for the "progressStateInfo" attribute of the "ProcessMonitor" data type for the "MLModelLoadingProcess.progressStatus".When the ML model loading is in progress, and the " MLModelLoadingProcess.progressStatus.status " is equal to "RUNNING", it provides the more detailed progress information.allowedValues for " MLModelLoadingProcess.progressStatus.status " = "RUNNING":The allowed values for " MLModelLoadingProcess.progressStatus.status " = "CANCELLING" are vendor specific.The allowed values for " MLModelLoadingProcess.progressStatus.status " = "NOT\_STARTED" are vendor specific. | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| MLModelLoadingProcess.cancelProcess | It allows the MnS consumer to cancel the ML model loading process.Setting this attribute to "TRUE" cancels the process. Cancellation is possible when the "MLModelLoadingProcess.progressStatus.status" is not the "FINISHED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| MLModelLoadingProcess.suspendProcess | It allows the MnS consumer to suspend the ML model loading process.Setting this attribute to "TRUE" suspends the process. The process can be resumed by setting this attribute to "FALSE" when it is suspended. Suspension is possible when the "MLModelLoadingProcess.progressStatus.status" is not the "FINISHED", "CANCELLING" or "CANCELLED" state. Setting the attribute to "FALSE" has no observable result. allowedValues: TRUE, FALSE. | type: Booleanmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| mLModelLoadingRequestRef | It identifies the DN of the associated MLModelLoadingRequest.allowedValues: DN. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| mLModelLoadingPolicyRef | It identifies the DN of the associated MLModelLoadingPolicyRef.allowedValues: DN. | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| loadedMLModelRef | It identifies the DN of the MLModel that has been loaded to the inference function. allowedValues: DN | type: DNmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| activationStatus | It describes the activation status.allowedValues: ACTIVATED, DEACTIVATED. | type: Enummultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| AIMLManagementPolicy.managedActivationScope | It provides a list of sub scopes for which ML inference is activated as triggered by a policy on the MnS producer. For example, the sub scopes may be a list of cells or of geographical areas. The list is an ordered list indicating the inference is activated for the first sub scope and gradually extended to the next sub scope if the policy evaluates to true.allowedValues: N/A | type: ManagedActivationScopemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| AIMLInferenceFunction.managedActivationScope | It provides a list of sub scopes for which ML inference is activated as triggered by a policy on the MnS producer. For example, the sub scopes may be a list of cells or of geographical areas. The list is an ordered list indicating the inference is activated for the first sub scope and gradually extended to the next sub scope if the policy evaluates to true.allowedValues: N/A | type: AIMLManagementPolicymultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| ManagedActivationScope.dNList | It indicates the list of DN, the list is an ordered list indicating the inference is activated for the first sub scope and gradually extended to the next sub scope.allowedValues: N/A | type: DNmultiplicity: \*isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| ManagedActivationScope.timeWindow | It indicates the list of time window; the list is an ordered list indicating the inference is activated for the first sub scope and gradually extended to the next sub scope.allowedValues: N/A | type: TimeWindowmultiplicity: \*isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| ManagedActivationScope.geoPolygon | It indicates the list of GeoArea, the list is an ordered list indicating the inference is activated for the first sub scope and gradually extended to the next sub scope.allowedValues: N/A | type: GeoAreamultiplicity: \*isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| usedByFunctionRefList | It provides the DNs of the functions supported by the AIMLInferenceFunction.allowedValues: N/A | type: DNmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| inferenceOutputId  | It identifies an inference output within an AIMLinferenceReport. | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| inferenceOutputs | It indicates the Outputs that have been derived by the AIMLInferenceFunction instance from a specific ML model.Each ML model, inferenceOutputs may be a set of values.allowedValues: N/A. | type: InferenceOutputmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| inferencePerformance | It indicates the performance score of the ML model during Inference.allowedValues: N/A. | type: ModelPerformancemultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| inferenceOutputTime | It indicates the time at which the inference output is generated.allowedValues: N/A | type: DateTimemultiplicity: \*isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| outputResult | It indicates the result of an inference. | type: AttributeValuePairmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NullisNullable: False |
| mLCapabilitiesInfoList | It indicates information about what an ML model can generate inference for. allowedValues: N/A. | type: MLCapabilityInfomultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| capabilityName | It indicates the name of a capability for which an ML model can generate inference. The capability is defined by Mns producer which can be traffic analysis capability, coverage analysis capability, mobility analysis capability or vendor specific extensions.allowedValues: N/A. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| mLCapabilityParameters | It indicates a set of optional parameters that apply for an aIMLInferenceName and capabilityName. allowedValues: N/A | type: AttributeValuePair multiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| aIMLInferenceReportRefList | It indicates a list of DN of the MLInferenceReport MOI that represents an ML inference report.allowedValues: DN. | type: DNmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| mLModelRefList | It identifies the list of MLModel DN.allowedValues: DN list | type: DNmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| NOTE: When the performanceScore is to indicate the performance score for ML model training, the data set is the training data set. When the performanceScore is to indicate the performance score for ML validation, the data set is the validation data set. When the performanceScore is to indicate the performance score for ML model testing, the data set is the testing data set. |

***Next change***

Forge MR link: <https://forge.3gpp.org/rep/sa5/MnS/-/merge_requests/1475> at commit 54d3940d4e3288479f676c28eadfd0e5aa35892a

\*\*\* START OF CHANGE 1 \*\*\*

\*\*\* OpenAPI/TS28105\_AiMlNrm.yaml \*\*\*

<CODE BEGINS>

openapi: 3.0.1

info:

 title: AI/ML NRM

 version: 18.5.0

 description: >-

 OAS 3.0.1 specification of the AI/ML NRM

 © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.105; AI/ML Management

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.105/

paths: {}

components:

 schemas:

#-------- Definition of types-----------------------------------------------------

 MLContext:

 type: object

 properties:

 inferenceModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 dataProviderRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 RequestStatus:

 type: string

 readOnly: true

 enum:

 - NOT\_STARTED

 - IN\_PROGRESS

 - SUSPENDED

 - FINISHED

 - CANCELLED

 - CANCELLING

 ModelPerformance:

 type: object

 properties:

 inferenceOutputName:

 type: string

 performanceMetric:

 type: string

 performanceScore:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Float'

 decisionConfidenceScore:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Float'

 ProcessMonitor:

 description: >-

 This data type is the "ProcessMonitor" data type defined in “genericNrm.yaml”

 with specialisations for usage in TS 28.105.

 type: object

 properties:

 status:

 type: string

 progressPercentage:

 type: integer

 minimum: 0

 maximum: 100

 progressStateInfo:

 type: string

 resultStateInfo:

 type: string

 AIMLManagementPolicy:

 description: >-

 This data type represents the properties of a policy for AI/ML management.

 type: object

 properties:

 thresholdList:

 type: array

 uniqueItems: true

 items:

 $ref: 'TS28623\_ThresholdMonitorNrm.yaml#/components/schemas/ThresholdInfo'

 managedActivationScope:

 $ref: '#/components/schemas/ManagedActivationScope'

 SupportedPerfIndicator:

 type: object

 properties:

 performanceIndicatorName:

 type: string

 readOnly: true

 isSupportedForTraining:

 type: boolean

 readOnly: true

 isSupportedForTesting:

 type: boolean

 readOnly: true

 ManagedActivationScope:

 oneOf:

 - type: object

 properties:

 dNList:

 type: array

 uniqueItems: true

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 - type: object

 properties:

 timeWindow:

 type: array

 uniqueItems: true

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/TimeWindow'

 - type: object

 properties:

 geoPolygon:

 type: array

 uniqueItems: true

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/GeoArea'

 MLCapabilityInfo:

 type: object

 properties:

 aIMLInferenceName:

 type: string

 readOnly: true

 capabilityName:

 type: string

 readOnly: true

 mLCapabilityParameters:

 description: A map (list of key-value pairs) for an aIMLInferenceName and capabilityName

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/AttributeNameValuePairSet'

 AvailMLCapabilityReport:

 type: object

 properties:

 availMLCapabilityReportID:

 type: string

 readOnly: true

 mLCapabilityVersionId:

 type: array

 uniqueItems: true

 items:

 type: string

 readOnly: true

 expectedPerformanceGains:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/ModelPerformance'

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 InferenceOutput:

 type: object

 properties:

 inferenceOutputId:

 type: array

 uniqueItems: true

 items:

 type: string

 readOnly: true

 aIMLInferenceName:

 type: string

 readOnly: true

 inferenceOutputTime:

 type: array

 uniqueItems: true

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTimeRo'

 # FIXME, isOrder/isUnique both as True

 inferencePerformance:

 $ref: '#/components/schemas/ModelPerformance'

 outputResult:

 description: A map (list of key-value pairs) for Inference result name and it's value

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/AttributeNameValuePairSet'

#-------- Definition of types for name-containments ------

 SubNetwork-ncO-AiMlNrm:

 type: object

 properties:

 MLTrainingFunction:

 $ref: '#/components/schemas/MLTrainingFunction-Multiple'

 MLTestingFunction:

 $ref: '#/components/schemas/MLTestingFunction-Multiple'

 MLModelRepository:

 $ref: '#/components/schemas/MLModelRepository-Multiple'

 MLUpdateFunction:

 $ref: '#/components/schemas/MLUpdateFunction-Multiple'

 AIMLInferenceFunction:

 $ref: '#/components/schemas/AIMLInferenceFunction-Multiple'

 AIMLInferenceEmulationFunction:

 $ref: '#/components/schemas/AIMLInferenceEmulationFunction-Multiple'

 ManagedElement-ncO-AiMlNrm:

 type: object

 properties:

 MLTrainingFunction:

 $ref: '#/components/schemas/MLTrainingFunction-Multiple'

 MLTestingFunction:

 $ref: '#/components/schemas/MLTestingFunction-Multiple'

 MLModelRepository:

 $ref: '#/components/schemas/MLModelRepository-Multiple'

 MLUpdateFunction:

 $ref: '#/components/schemas/MLUpdateFunction-Multiple'

 AIMLInferenceFunction:

 $ref: '#/components/schemas/AIMLInferenceFunction-Multiple'

 AIMLInferenceEmulationFunction:

 $ref: '#/components/schemas/AIMLInferenceEmulationFunction-Multiple'

#-------- Definition of concrete IOCs --------------------------------------------

 MLTrainingFunction-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 mLModelRepositoryRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 MLTrainingRequest:

 $ref: '#/components/schemas/MLTrainingRequest-Multiple'

 MLTrainingProcess:

 $ref: '#/components/schemas/MLTrainingProcess-Multiple'

 MLTrainingReport:

 $ref: '#/components/schemas/MLTrainingReport-Multiple'

 ThresholdMonitors:

 $ref: 'TS28623\_ThresholdMonitorNrm.yaml#/components/schemas/ThresholdMonitor-Multiple'

 MLTestingRequest:

 $ref: '#/components/schemas/MLTestingRequest-Multiple'

 MLTestingReport:

 $ref: '#/components/schemas/MLTestingReport-Multiple'

 MLTrainingRequest-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 aIMLInferenceName:

 type: string

 readOnly: true

 candidateTrainingDataSource:

 type: array

 uniqueItems: true

 items:

 type: string

 trainingDataQualityScore:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Float'

 trainingRequestSource:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 requestStatus:

 $ref: '#/components/schemas/RequestStatus'

 expectedRuntimeContext:

 $ref: '#/components/schemas/MLContext'

 performanceRequirements:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/ModelPerformance'

 cancelRequest:

 type: boolean

 suspendRequest:

 type: boolean

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelCoordinationGroupRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLTrainingProcess-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 priority:

 type: integer

 terminationConditions:

 type: string

 progressStatus:

 $ref: '#/components/schemas/ProcessMonitor'

 cancelProcess:

 type: boolean

 suspendProcess:

 type: boolean

 trainingRequestRef: ## Figure 7.3a.1.1.1-1 has no such pointer

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 trainingReportRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelGeneratedRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelRef: ## Figure 7.3a.1.1.1-1 is 1-0..1 mapping, hence should be single

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLTrainingReport-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 usedConsumerTrainingData:

 type: array

 uniqueItems: true

 items:

 type: string

 readOnly: true

 modelConfidenceIndication:

 type: integer

 readOnly: true

 modelPerformanceTraining:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/ModelPerformance'

 modelPerformanceValidation:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/ModelPerformance'

 dataRatioTrainingAndValidation:

 type: integer

 areNewTrainingDataUsed:

 type: boolean

 readOnly: true

 trainingRequestRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 trainingProcessRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 lastTrainingRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelGeneratedRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelCoordinationGroupGeneratedRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 MLTestingFunction-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties: ##FIXME pointer to MLModelCoordinationGroup missing

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 MLTestingRequest:

 $ref: '#/components/schemas/MLTestingRequest-Multiple'

 MLTestingReport:

 $ref: '#/components/schemas/MLTestingReport-Multiple'

 MLTestingRequest-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 requestStatus:

 $ref: '#/components/schemas/RequestStatus'

 cancelRequest:

 type: boolean

 suspendRequest:

 type: boolean

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelCoordinationGroupRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLTestingReport-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 modelPerformanceTesting:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/ModelPerformance'

 mLTestingResult:

 type: string

 readOnly: true

 testingRequestRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLModelLoadingRequest-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 requestStatus:

 $ref: '#/components/schemas/RequestStatus'

 cancelRequest:

 type: boolean

 suspendRequest:

 type: boolean

 mLModelToLoadRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLModelLoadingPolicy-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 aIMLInferenceName:

 type: string

 policyForLoading:

 $ref: '#/components/schemas/AIMLManagementPolicy'

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 MLModelLoadingProcess-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 progressStatus:

 $ref: '#/components/schemas/ProcessMonitor'

 cancelProcess:

 type: boolean

 suspendProcess:

 type: boolean

 mLModelLoadingRequestRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelLoadingPolicyRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 loadedMLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLModel-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 mLModelId:

 type: string

 readOnly: true

 aIMLInferenceName:

 type: string

 readOnly: true

 mLModelVersion:

 type: string

 readOnly: true

 expectedRunTimeContext:

 $ref: '#/components/schemas/MLContext'

 trainingContext:

 $ref: '#/components/schemas/MLContext'

 runTimeContext:

 $ref: '#/components/schemas/MLContext'

 supportedPerformanceIndicators:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/SupportedPerfIndicator'

 minItems: 1

 mLCapabilitiesInfoList:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/MLCapabilityInfo'

 minItems: 1

 retrainingEventsMonitorRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 sourceTrainedMLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 aIMLInferenceReportRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 usedByFunctionRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 MLModelRepository-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 MLModel:

 $ref: '#/components/schemas/MLModel-Multiple'

 MLModelCoordinationGroup:

 $ref: '#/components/schemas/MLModelCoordinationGroup-Multiple'

 MLModelCoordinationGroup-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 memberMLModelRefList:

 type: array

 uniqueItems: true

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 minItems: 2

 ## 7.3a.4.1 IOC

 MLUpdateFunction-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 availMLCapabilityReport:

 $ref: '#/components/schemas/AvailMLCapabilityReport'

 mLModelRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 MLUpdateRequest:

 $ref: '#/components/schemas/MLUpdateRequest-Multiple'

 MLUpdateProcess:

 $ref: '#/components/schemas/MLUpdateProcess-Multiple'

 MLUpdateReport:

 $ref: '#/components/schemas/MLUpdateReport-Multiple'

 MLUpdateRequest-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 performanceGainThreshold:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/ModelPerformance'

 newCapabilityVersionId:

 type: array

 uniqueItems: true

 items:

 type: string

 updateTimeDeadline:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/TimeWindow'

 requestStatus:

 $ref: '#/components/schemas/RequestStatus'

 mLUpdateReportingPeriod:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/TimeWindow'

 cancelRequest:

 type: boolean

 suspendRequest:

 type: boolean

 mLUpdateProcessRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 mLModelRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 MLUpdateProcess-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 progressStatus:

 $ref: '#/components/schemas/ProcessMonitor'

 cancelProcess:

 type: boolean

 suspendProcess:

 type: boolean

 mLModelRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 mLUpdateRequestRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 mLUpdateReportRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 MLUpdateReport-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 updatedMLCapability:

 $ref: '#/components/schemas/AvailMLCapabilityReport'

 mLModelRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 mLUpdateProcessRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnRo'

 AIMLInferenceFunction-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 activationStatus:

 type: string

 enum:

 - ACTIVATED

 - DEACTIVATED

 managedActivationScope:

 $ref: '#/components/schemas/AIMLManagementPolicy'

 usedByFunctionRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 mLModelRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

 - type: object

 properties:

 AIMLInferenceReport:

 $ref: '#/components/schemas/AIMLInferenceReport-Multiple'

 MLModelLoadingRequest:

 $ref: '#/components/schemas/MLModelLoadingRequest-Multiple'

 MLModelLoadingProcess:

 $ref: '#/components/schemas/MLModelLoadingProcess-Multiple'

 MLModelLoadingPolicy:

 $ref: '#/components/schemas/MLModelLoadingPolicy-Multiple'

 MLModel:

 $ref: '#/components/schemas/MLModel-Multiple'

 AIMLInferenceReport-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - type: object

 properties:

 inferenceOutputs:

 type: array

 uniqueItems: true

 items:

 $ref: '#/components/schemas/InferenceOutput'

 minItems: 1

 mLModelRefList:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnListRo'

 AIMLInferenceEmulationFunction-Single:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 allOf:

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-Attr'

 - type: object

 properties:

 AIMLInferenceReport:

 $ref: '#/components/schemas/AIMLInferenceReport-Multiple'

 - $ref: 'TS28623\_GenericNrm.yaml#/components/schemas/ManagedFunction-ncO'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

 MLTrainingFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTrainingFunction-Single'

 MLTrainingRequest-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTrainingRequest-Single'

 MLTrainingProcess-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTrainingProcess-Single'

 MLTrainingReport-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTrainingReport-Single'

 MLModel-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLModel-Single'

 MLModelRepository-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLModelRepository-Single'

 MLModelCoordinationGroup-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLModelCoordinationGroup-Single'

 MLTestingFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTestingFunction-Single'

 MLTestingRequest-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTestingRequest-Single'

 MLTestingReport-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLTestingRequest-Single'

 MLModelLoadingRequest-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLModelLoadingRequest-Single'

 MLModelLoadingProcess-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLModelLoadingProcess-Single'

 MLModelLoadingPolicy-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLModelLoadingPolicy-Single'

 MLUpdateFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLUpdateFunction-Single'

 MLUpdateRequest-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLUpdateRequest-Single'

 MLUpdateProcess-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLUpdateProcess-Single'

 MLUpdateReport-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MLUpdateReport-Single'

 AIMLInferenceFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AIMLInferenceFunction-Single'

 AIMLInferenceReport-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AIMLInferenceReport-Single'

 AIMLInferenceEmulationFunction-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/AIMLInferenceEmulationFunction-Single'

#-------- Definitions in TS 28.104 for TS 28.532 ---------------------------------

 resources-AiMlNrm:

 oneOf:

 - $ref: '#/components/schemas/MLTrainingFunction-Single'

 - $ref: '#/components/schemas/MLTrainingRequest-Single'

 - $ref: '#/components/schemas/MLTrainingProcess-Single'

 - $ref: '#/components/schemas/MLTrainingReport-Single'

 - $ref: '#/components/schemas/MLModel-Single'

 - $ref: '#/components/schemas/MLModelRepository-Single'

 - $ref: '#/components/schemas/MLModelCoordinationGroup-Single'

 - $ref: '#/components/schemas/MLTestingFunction-Single'

 - $ref: '#/components/schemas/MLTestingRequest-Single'

 - $ref: '#/components/schemas/MLTestingReport-Single'

 - $ref: '#/components/schemas/MLModelLoadingRequest-Single'

 - $ref: '#/components/schemas/MLModelLoadingProcess-Single'

 - $ref: '#/components/schemas/MLModelLoadingPolicy-Single'

 - $ref: '#/components/schemas/MLUpdateFunction-Single'

 - $ref: '#/components/schemas/MLUpdateRequest-Single'

 - $ref: '#/components/schemas/MLUpdateProcess-Single'

 - $ref: '#/components/schemas/MLUpdateReport-Single'

 - $ref: '#/components/schemas/AIMLInferenceFunction-Single'

 - $ref: '#/components/schemas/AIMLInferenceReport-Single'

 - $ref: '#/components/schemas/AIMLInferenceEmulationFunction-Single'

<CODE ENDS>

\*\*\* END OF CHANGE 1 \*\*\*

***End of change***