**3GPP TSG-CT WG3 Meeting #120e *C3-221721***

**E-Meeting, 17th – 25st February 2022**

**Source: TSG CT WG3**

**Title: Presentation sheet to TSG for Approval: TS 29.575 Version 0.5.0**

**Document for: Approval**

**Agenda Item: 17.23**

**Work Item: eNA\_Ph2**

**Abstract of document:**

3GPP TS 29.575 specifies the stage 3 protocol and data model for the ADRF Service Based Interface of the 5G System. It provides stage 3 protocol definitions and message flows, and specifies the Nadrf\_DataManagement Service API offered by the ADRF.

3GPP TS 29.575 specifies the service API as RESTful API, following the technical realization of the service based architecture as specified in 3GPP TS 29.500 and the principles and guidelines for service definition as specified in 3GPP TS 29.501.

3GPP TS 29.575 specification work has completed in the definition of the required service operations, the specification of the related procedures, and the identification of resource(s) structure and data model.

**Changes since last presentation to CT Plenary:**

First presentation to CT Plenary.

**Outstanding Issues:**

None.

**Contentious Issues:**

None.