**3GPP TSG-CT3 Meeting #122e C3-223730**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.575** | **CR** | **0020** | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | China Mobile |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2022-05-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CRs modifying the Nadrf\_DataManagement API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in 3GPP TS 29.501, clause 4.3.1.The following agreed CRs update the OpenAPI file for Nadrf\_DataManagement API for the present release:* CR#0002 impacts the OpenAPI file with a backwards compatible feature.
* CR#0005 impacts the OpenAPI file with a backwards compatible feature.
* CR#0006 impacts the OpenAPI file with a backwards compatible feature.
* CR#0008 impacts the OpenAPI file with a backwards compatible correction.
* CR#0019 impacts the OpenAPI file with a backwards compatible correction.
* CR#0354 of 3GPP TS 29.571 impacts the OpenAPI file with a backwards compatible correction.

As some backward compatible corrections and features (but no backward incompatible changes or backward compatible new features) are added of the present release, and the release will be frozen, the draft version number is removed. |
|  |  |
| ***Summary of change:*** | The Nadrf\_DataManagement API version incremented from value "1.0.0-alpha.3" to value "1.0.0", and the TS version in the externalDocs field from 17.0.0 to 17.1.0. |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and TS version in externalDocs field. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible corrections to Nadrf\_DataManagement API. |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

## A.2 Nadrf\_DataManagement API

openapi: 3.0.0

info:

 version: 1.0.0

 title: Nadrf\_DataManagement

 description: |

 ADRF Data Management Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.575 V17.1.0; 5G System; Analytics Data Repository Services; Stage 3.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.575/'

#

servers:

 - url: '{apiRoot}/nadrf-datamanagement/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause clause 4.4 of 3GPP TS 29.501.

#

security:

 - oAuth2ClientCredentials:

 - nadrf-datamanagement

 - {}

#

paths:

 /data-store-records:

 post:

 summary: Creates a new Individual Data Store Record resource.

 operationId: CreateADRFDataStoreRecord

 tags:

 - ADRF Data Store Records (Collection)

 requestBody:

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataStoreRecord'

 required: true

 description: ADRF data store record to be stored.

 responses:

 '201':

 description: Successful creation of new Individual ADRF Data Store Record resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nadrf-datamanagement/v1/data-store-records/{storeTransId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataStoreRecord'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 get:

 summary: "Retrieves existing Individual ADRF Data Store Records"

 operationId: GetAdrfDataStoreRecords

 tags:

 - ADRF Data Store Records (Collection)

 parameters:

 - name: store-trans-id

 description: A storage transaction identifier of a data store record in ADRF.

 in: query

 required: false

 schema:

 type: string

 - name: fetch-correlation-ids

 description: Fetch correlation identifiers received as part of fetch instruction.

 in: query

 required: false

 style: form

 explode: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: ana-sub

 description: Represents analytics event subscription.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

 - name: amf-data-sub

 description: Represents AMF event subscription.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/AmfEventSubscription'

 - name: smf-data-sub

 description: Represents SMF event subscription.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NsmfEventExposure'

 - name: nef-data-sub

 description: Represents NEF event subscription.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29591\_Nnef\_EventExposure.yaml#/components/schemas/NefEventExposureSubsc'

 - name: udm-data-sub

 description: Represents UDM event subscription.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29503\_Nudm\_EE.yaml#/components/schemas/EeSubscription'

 - name: af-data-sub

 description: Represents AF event subscription.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AfEventExposureSubsc'

 - name: time-period

 description: Represents a start time and a stop time during which requested data is collected or to be collected.

 in: query

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 responses:

 '200':

 description: Data store records are returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataStoreRecord'

 '204':

 description: No matching ADRF data were found.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /data-store-records/{storeTransId}:

 delete:

 summary: Delete an existing Individual ADRF Data Store Record

 operationId: DeleteADRFDataStoreRecord

 tags:

 - Individual ADRF Data Store Record (Document)

 parameters:

 - name: storeTransId

 in: path

 description: String identifying a Data Store Record in ADRF

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual ADRF Data Store Record resource matching the storeTransId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /data-retrieval-subscriptions:

 post:

 summary: Creates a new Individual ADRF Data Retrieval Subscription resource.

 operationId: CreateADRFDataRetrievalSubscription

 tags:

 - ADRF Data Retrieval Subscriptions (Collection)

 requestBody:

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataRetrievalSubscription'

 required: true

 description: Individual ADRF Data Retrieval Subscription resource to be created.

 responses:

 '201':

 description: Created a new Individual ADRF Data Retrieval Subscription resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nadrf-datamanagement/v1/data-retrieval-subscriptions/{subscriptionId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataRetrievalSubscription'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 adrfDataRetrievalNotification:

 '{$request.body#/notificationURI}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataRetrievalNotification'

 responses:

 '204':

 description: The receipt of the Notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /data-retrieval-subscriptions/{subscriptionId}:

 delete:

 summary: Delete an existing Individual ADRF Data Retrieval Subscription

 operationId: DeleteADRFDataRetrievalSubscription

 tags:

 - Individual ADRF Data Retrieval Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a data retrieval subscription to the Nadrf\_DataManagement Service.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual ADRF Data Retrieval Subscription resource matching the subscriptionId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /request-storage-sub:

 post:

 summary: Triggers the creation of a new ADRF Storage Subscription.

 operationId: CreateADRFStorageSubscription

 tags:

 - ADRF Storage Subscriptions

 requestBody:

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataStoreSubscription'

 required: true

 responses:

 '200':

 description: Successful response with reference used to identify the subscription at the ADRF.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataStoreSubscriptionRef'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /request-storage-sub-removal:

 post:

 summary: triggers the removal of ADRF storage subscription.

 operationId: DeleteADRFStorageSubscription

 tags:

 - ADRF Storage Subscriptions

 requestBody:

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfDataStoreSubscriptionRef'

 required: true

 responses:

 '204':

 description: No Content. The ADRF Storage Subscription matching the provided reference was deleted.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /remove-stored-data-analytics:

 post:

 summary: remove ADRF data based on data or analytics specification.

 operationId: DeleteADRFData

 tags:

 - ADRF Stored Data

 requestBody:

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NadrfStoredDataSpec'

 required: true

 responses:

 '204':

 description: No Content. The ADRF data matching the provided specification is deleted.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nadrf-datamanagement: Access to the nadrf-datamanagement API

#

 schemas:

#

 NadrfDataStoreRecord:

 description: Represents an Individual ADRF Data Store Record.

 type: object

 oneOf:

 - required: [anaNotifications]

 - required: [amfEventNotifs]

 - required: [smfEventNotifs]

 - required: [udmEventNotifs]

 - required: [nefEventNotifs]

 - required: [afEventNotifs]

 properties:

 anaNotifications:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscriptionNotification'

 minItems: 1

 description: List of analytics subscription notifications.

 amfEventNotifs:

 type: array

 items:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/AmfEventNotification'

 minItems: 1

 description: List of notifications of AMF events.

 smfEventNotifs:

 type: array

 items:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NsmfEventExposureNotification'

 minItems: 1

 description: List of notifications of SMF events.

 udmEventNotifs:

 type: array

 items:

 $ref: 'TS29503\_Nudm\_EE.yaml#/components/schemas/MonitoringReport'

 minItems: 1

 description: List of notifications of UDM events.

 nefEventNotifs:

 type: array

 items:

 $ref: 'TS29591\_Nnef\_EventExposure.yaml#/components/schemas/NefEventExposureNotif'

 minItems: 1

 description: List of notifications of NEF events.

 afEventNotifs:

 type: array

 items:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AfEventExposureNotif'

 minItems: 1

 description: List of notifications of AF events.

#

 NadrfDataStoreSubscription:

 description: Contains information to be used by the ADRF to create a Data or Analytics subscription.

 type: object

 allOf:

 - oneOf:

 - required: [anaSub]

 - required: [dataSub]

 - oneOf:

 - required: [targetNfId]

 - required: [targetNfSetId]

 properties:

 anaSub:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

 dataSub:

 $ref: '#/components/schemas/DataSubscription'

 targetNfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 targetNfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 formatInstruct:

 $ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/FormattingInstruction'

 procInstruct:

 $ref: 'TS29574\_Ndccf\_DataManagement.yaml#/components/schemas/ProcessingInstruction'

#

 NadrfDataRetrievalSubscription:

 description: Represents an Individual ADRF Data Retrieval Subscription.

 type: object

 required:

 - notifCorrId

 - notificationURI

 - timePeriod

 oneOf:

 - required: [anaSub]

 - required: [dataSub]

 properties:

 anaSub:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

 dataSub:

 $ref: '#/components/schemas/DataSubscription'

 notificationURI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 timePeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 notifCorrId:

 type: string

 description: Notification correlation identifier.

#

 NadrfDataRetrievalNotification:

 description: Represents a notification that corresponds with an Individual ADRF Data Retrieval Subscription.

 type: object

 required:

 - notifCorrId

 oneOf:

 - required: [anaNotifications]

 - required: [amfEventNotifs]

 - required: [smfEventNotifs]

 - required: [udmEventNotifs]

 - required: [nefEventNotifs]

 - required: [afEventNotifs]

 properties:

 notifCorrId:

 type: string

 description: Notification correlation identifier.

 anaNotifications:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscriptionNotification'

 minItems: 1

 description: List of analytics subscription notifications.

 amfEventNotifs:

 type: array

 items:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/AmfEventNotification'

 minItems: 1

 description: List of notifications of AMF events.

 smfEventNotifs:

 type: array

 items:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NsmfEventExposureNotification'

 minItems: 1

 description: List of notifications of SMF events.

 udmEventNotifs:

 type: array

 items:

 $ref: 'TS29503\_Nudm\_EE.yaml#/components/schemas/MonitoringReport'

 minItems: 1

 description: List of notifications of UDM events.

 nefEventNotifs:

 type: array

 items:

 $ref: 'TS29591\_Nnef\_EventExposure.yaml#/components/schemas/NefEventExposureNotif'

 minItems: 1

 description: List of notifications of NEF events.

 afEventNotifs:

 type: array

 items:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AfEventExposureNotif'

 minItems: 1

 description: List of notifications of AF events.

#

 NadrfDataStoreSubscriptionRef:

 description: Contains a reference to a request for a Data or Analytics subscription.

 type: object

 required:

 - transRefId

 properties:

 transRefId:

 type: string

 description: Transaction reference identifier.

#

 NadrfStoredDataSpec:

 description: Contains information about Data or Analytics specification.

 type: object

 required:

 - timePeriod

 oneOf:

 - required: [dataSpec]

 - required: [anaSpec]

 properties:

 dataSpec:

 $ref: '#/components/schemas/DataSubscription'

 anaSpec:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NnwdafEventsSubscription'

 timePeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

#

 DataSubscription:

 description: Contains a data specification.

 type: object

 oneOf:

 - required: [amfDataSub]

 - required: [smfDataSub]

 - required: [udmDataSub]

 - required: [nefDataSub]

 - required: [afDataSub]

 properties:

 amfDataSub:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/AmfEventSubscription'

 smfDataSub:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NsmfEventExposure'

 udmDataSub:

 $ref: 'TS29503\_Nudm\_EE.yaml#/components/schemas/EeSubscription'

 afDataSub:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AfEventExposureSubsc'

 nefDataSub:

 $ref: 'TS29591\_Nnef\_EventExposure.yaml#/components/schemas/NefEventExposureSubsc'

#

 \*\*\* End of Changes \*\*\*