TSG-RAN WG1 #112b-e R1-23xxxxx

e-meeting, April 17 – 26, 2023

Source: Nokia

Title: Draft CR 38.214 – NR\_DSS\_enh-Core

Agenda Item: 9.18

Document for: Discussion and Decision

# Introduction

This thread will discuss the draft CR to 38.214 for the *NR\_DSS\_enh.*

First checkpoint for this discussion: **April 20, UTC 17.00!**

# Discussion – first round

The comments in this section are based on the draft CR available in [**R1-2304003**](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_112b-e/Inbox/R1-2304003.zip)

.

|  |  |  |
| --- | --- | --- |
| Company | Comments | Editor reply/Notes |
| ZTE | It seems the following correction per the agreed TP in RAN1#110 is missed.  ….  *-* REs indicated by *'RateMatchPatternLTE-CRS'* in *lte-CRS-PatternList1-r16* or *lte-CRS-PatternList3-r18* in *ServingCellConfig* configuring cell-specific RS, in 15 kHz subcarrier spacing applicable only to 15 kHz subcarrier spacing PDSCH, of one LTE carrier in a serving cell are declared as not available for PDSCH.  ….. |  |
| Xiaomi | We share the similar view with ZTE. |  |
|  |  |  |