**3GPP TSG-RAN2#119e Meeting *R2-2208811***

**Electronic, 17th– 29th Aug, 2022**

**Title: LS on SR config for MG (de-)activation request MAC CE**

**Response to:**

**Release:** Rel-17

**Work Items:** NR\_pos\_enh-Core

**Source:** RAN WG2

**To:** RAN WG1

**CC:**

**Contact Person:**

#### Name: Yinghao Guo

E-mail Address: yinghaoguo@huawei.com

**Attachment:**

**1. Overall Description:**

RAN2 has reached the following conclusion during the discussion on SR configuration for positioning Measurement Gap activation/deactivation request MAC CE in RAN2#119e.

Agreement:

Introduce a dedicated SR configuration for the Measurement Gap Activation/Deactivation Request MAC CE.

LS to RAN1 notifying them of the RAN2 decision.

**2. Actions:**

**To RAN1,**

**ACTION:**

* RAN2 respectfully asks RAN1 to take above agreement into account in further discussions.

**3. Date of Next RAN WG2 Meetings:**

RAN2 #119-bis-e 10– 19 October 2022 Electronic Meeting

RAN2 #120 14-18 November 2022 Europe