**3GPP TSG-RAN WG2 Meeting #119e R2-2208849**

**E-Meeting, August 17-29, 2022**

**Title: [Draft]**LS on missing RRC parameter in IUC Scheme 2

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_SL\_enh-Core

**Source:** Apple [To be RAN2]

**To:** RAN1

**Cc:**

**Contact Person:**

#### Name: Zhibin Wu

E-mail Address: <zhibin\_wu@apple.com>

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** none

**1. Overall Description:**

According to TS 38.213, to support one of the options used to determine the conflict resource in IUC Scheme 2, the “delta RSRP threshold” parameter is needed to be (pre-)configured by the RRC layer. However, this parameter was not included in the original RRC parameter list from RAN1 and is thereby missing in the current version of TS 38.331.

RAN2 has agreed to add the “*deltaRSRP-Threshold*” parameter in the RRC specification TS 38.331 to ensure that the IUC Scheme 2 can be correctly implemented in Rel-17.

**2. Actions:**

**To RAN1**: RAN2 respectfully requests RAN1 to take the above RAN2 agreement into account and provide guidance on the implementation of the *deltaRSRP-Threshold* parameter.

**3. Dates of Next TSG-RAN WG2 Meetings:**

TSG RAN WG2 Meeting #119bis October 10 – October 19 2022 E-meeting

TSG RAN WG2 Meeting #120 November 14 – November 18 2022 Europe (TBD)