**SA WG2 Meeting #S2-142E S2-2008802**

**November 16 ~ 20, 2020, Elbonia**

**Source: vivo**

**Title: Reference points**

**Document for: Approval**

**Agenda Item: 8.9**

**Work Item / Release: FS\_5MBS / Rel-17**

*Abstract of the contribution: Reference points.*

# 1 Introduction

This paper proposes Reference points.

# 2 Discussion

According to the architecture, it is proposed to reuse existing reference points as possible as we can with enhancement for 5MBS.

# 3 Proposal

It is proposed to approve following changes:

\* \* \* \* First change \* \* \* \*

5.3.1 Reference point

The 5MBS System Architecture contains the following new reference points:

**Nmb:** Reference point between the MBSF and the NEF if not collocated.

The 5MBS System Architecture reuses the existing reference points of N1, N2, N10, N16, and N29 with enhancement to support 5G MBS, as well as reuses the existing reference points of N7 and N33 with enhancement to support 5G MBS depends on deployment of PCF and MBSF.

\* \* \* \* End of changes \* \* \* \*