**3GPP TSG-SA3 Meeting #107-e *draft\_S3-220887-r1***

**e-meeting, 16 - 20 May 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **TR 33.926** | **CR** | **draftCR** | **rev** | **<Rev#>** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Addition of MnF critical assets | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | S3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SCAS\_5G\_MF | | | | |  | ***Date:*** | | | 2022-05-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding MnF-Specific critical assets. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding MnF-Specific critical assets. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No critical assets for MnF network product class. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | X.2.1(new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**\*\*\*\*\* START OF 1st CHANGES \*\*\*\*\***

## X.2.1 Critical assets

In addition to the critical assets of a GNP described in clause 5.2 of the present document, the critical assets specific to the MnF to be protected are:

* MnF Application
* The interfaces of MnF to be protected and which are within SECAM scope: for example
  + External Client access interface
  + Interface between MnF and NF
  + Interface between RAN/CN MnFs and Cross Domain MnFs
  + Interface between MnF and AAA infrastructure, if any
  + Service based interfaces, if any
* Management data: User account data, Performance data, Fault supervision data, Configuration data, Log data, etc.

NOTE 1: The detailed interfaces of the MnF class are described in clause 4, Network Product Class Description of the present document.

**\*\*\*\*\* END OF CHANGES \*\*\*\*\***