**3GPP TSG-SA3 Meeting #108e  *S3-22xxxx***

**e-meeting, 22 – 26 August 2022**

**Title: [Draft] LS on Match Report for UE-to-Network Relay Discovery**

**Response to:**

**Release: Release 17**

**Work Item: 5G\_ProSe\_Sec**

**Source: Xiaomi [to be SA3]**

**To: SA2**

**Cc:**

**Contact person: Wei Lu**

[**luwei10@xiaomi.com**](mailto:luwei10@xiaomi.com)

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** NONE

# 1 Overall description

In 5G ProSe Restricted Direct Discovery procedure, SA3 has defined the options that the MIC checking of the discovered ProSe Restricted Code can be performed by the UE or by the 5G DDNMF via Match Reporting.

SA3 would like to ask SA2 whether Match Reporting is also defined to be used in 5G ProSe UE-to-Network Relay Discovery procedure. If yes, SA3 would like to know which inputs and outputs are required to be included in the Match Report and Match Report Acknowledgement respectively, as defined in TS 23.304 clause 7.1.2.8.

# 2 Actions

**To SA2**

**ACTION:** SA3 kindly requests SA2 to provide feedback on the questions raised above.

# 3 Dates of next TSG SA WG 3 meetings

SA3#108e-Bis 10 - 14 October 2022 Online

SA3#109e 14 - 18 November 2022 TBD