**3GPP TSG-SA3 Meeting #119AdHoc-e draft\_S3-250164-r5**

**Online, Electronic meeting, 13 -16 January 2025 *merger of S3-250019, S3-250118, S3-250164***

**Source: Nokia, Huawei, HiSilicon, Xiaomi Communications**

**Title: KI1.3 conclusion**

**Document for: Approval**

**Agenda item: 5.19**

**Spec: 3GPP TR 33.700-22**

**Version: 0.3.0**

**Work Item: FS\_CAPIF\_Ph3-sec**

**Comments**

**Proposed Changes**

\* \* \* First Change \* \* \* \*

### 7.1.3 Conclusions for KI#1.3 Finer granular authorization

Normative work is recommended to support service operation level and resource level granularity in RNAA scenarios.

ROF/UE may support finer level (i.e. granular) authorization, e.g. data processing purpose level (e.g., expose the location) and feature level. Details on finer level service API access and information intended to be provided by the API invoker at invocation, whilst accounting for the provided purpose for data processing, are to be determined in normative work.

NOTE: The granularity (called finer level) will be in line with that specified in TS 23.222 [3].

\* \* \* End of Changes \* \* \* \*