**3GPP TSG-SA3 Meeting #119AdHoc-e S3-250168**

**Online, Electronic meeting, 13 -16 January 2025 *merger of S3-250168 and S3-250108***

**Source: Nokia, Ericsson**

**Title: KI5 conclusion**

**Document for: Approval**

**Agenda item: 5.19**

**Spec: 3GPP TR 33.700-22**

**Version: 0.3.0**

**Work Item: FS\_CAPIF\_Ph3-sec**

**Comments**

There is one solution (#28) provided for this key issue; it is proposed to use it for normative work.

**Proposed Changes**

\* \* \* First Change \* \* \* \*

7.5 Conclusion for KI #5: Authenticating multiple API invokers of the same Resource Owner

When the ROF is engaging multiple API invokers at the same UE and the ROF has a valid certificate received from the CCF, it can be used for interaction between API invoker and AEF after API invoker/ROF interaction within the UE to allow multiple API invokers accessing the same resources of ROF to efficiently be handled by AEF. Solution #28 is the baseline for normative work.

There is no agreement for this key issue, therefore no normative work is required.

\* \* \* End of Changes \* \* \* \*