**3GPP SA3#95-LI S3i240709**

**Las Vegas; October 29-November 1, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **33.127** | **CR** | **0249**  | **rev** | **1** | **Current version:** | **17.14.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Corrections on MMS target identities |
|  |  |
| ***Source to WG:*** | SA3-LI (Nokia) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** | LI17 |  | ***Date:*** | 2024-10-29 |
|  |  |  |  |  |
| ***Category:*** | ***F*** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | For MMS LI, not all the target identities listed are available at the MMS Relay/Server to perform the interception. When the LIPF logic diagrams were constructed for TR 33.928, the scope of target identities applicable to MMS was reevaluated and only GPSI and MSISDN and Email Address were considered.  |
|  |  |
| ***Summary of change:*** | Target identity list is updated.  |
|  |  |
| ***Consequences if not approved:*** | Specification has requirements that are not implementable.  |
|  |  |
| ***Clauses affected:*** |  7.5.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  S3i240614 |

### \*\* First Change \*\*

#### 7.5.2.2 Target Identities

The LIPF provisions the intercept related information associated with the following target identities to the IRI-POI/CC-POI present in the MMS Proxy-Relay:

- Email Address.

- GPSI.

- MSISDN.

- E.164 Number.

- IMSI.

- SUPI.

NOTE: SUPI and IMSI may not be available.

The interception performed on the above identities are mutually independent, even though, an xIRI may contain the information about the other identities when available.

The IRI-POI and CC-POI present in the MMS Proxy-Relay shall also support interception of non-local identities.

### \*\* End of all Changes \*\*