**3GPP TSG RAN WG1 #118bis R1-240xxxx**

**Hefei, China, October 14th – 18th, 2024**

**Source: Moderator (CATT)**

**Title:** **Summary of UE capability of partial cancellation** **of configured UL transmissions**

**Agenda Item:** **7**

**Document for:** **Decision**

# Introduction

In RAN1#118bis, the following contribution is submitted to correct the UE capability name of partial cancellation of configured UL transmissions. This contribution collects companies’ views on the Tdoc.

R1-2408007 Correction on UE capability of partial cancellation of configured UL transmissions CATT

# Discussion

CATT identified that the UE capability of partial cancellation of the configured PUCCH, PUSCH or PRACH in TS38.213 is not aligned with higher layer specifications and proposed to change ‘[partialCancellation]’ to ‘*partialCancellationPUCCH-PUSCH-PRACH-TX-r16*’.

## Q1: Do you agree with the draft CR in R1-2408007?

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree or Not Agree** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

It is expected that some companies may suggest adopting the text proposal in an editor CR. However, based on the previous guidance from Mr. Chair, there is no editor CR for Rel-15 and Rel-16 anymore. Moderator would like to collect companies’ views on whether individual CR is acceptable.

## Q2: Do you agree to endorse the text proposal in an individual CR from Rel-16? If not, the change can be only made from Rel-17 in an editor CR.

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree or Not Agree** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |