**3GPP TSG-SA5 Meeting #156 *S5-244659***

Maastricht, , 19 - 23 August 2024

**Title:** Reply LS on MDT configuration control in NR-DC

**Response to:** R3-243937 Reply LS to MDT configuration control in NR-DC

**Release:** REL-18

**Work Item:** NR\_ENDC\_SON\_MDT\_enh2-Core

**Source: SA5**

**To: RAN3, CT4**

**Cc:**

**Contact person: Zu Qiang**

 **zu.qiang@ericsson.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** S5-244907, S5-244908, S5-244909, S5-244910, S5-244911

# 1 Overall description

SA5 thanks RAN3 for its LS on MDT configuration control in NR-DC in document R3-243937.

SA5 has discussed and agreed to specify a mNOnly indicator in mdtConfig data type. This attribute is only applicable to signalling based NR MDT procedure.

According to 3GPP TS21.801, Annex K, ‘master’ is non-inclusive term. The possible alternative term is ‘main’. Therefore, SA5 has specified that “MN-only” as “Main Node Only”. SA5 Kindly ask RAN3 to take this into consideration.

However, this change may have an impact on CT4. SA5 would like to ask CT4 to update corresponding specification accordingly.

# 2 Actions

**To RAN3**

**ACTION:** SA5 kindly asks RAN3 to take the above progress into account and take actions accordingly if necessary.

**To CT4**

**ACTION:** SA5 kindly asks CT4 to take the above progress into account and take actions accordingly if necessary.

# 3 Dates of next TSG SA WG 5 meetings

SA5#157 14 - 18 October 2024 Hyderabad, IN

SA5#158 18 - 22 November 2024 Orlando, US