**3GPP TSG RAN WG1#110 R1-22xxxxx**

**Toulouse, France, August 22nd – 26th, 2022**

**Title:** DRAFT LS to RAN2 on RRC parameter impact for NR up to 71GHz

**Release:** 17

**Work Item:** NR\_ext\_to\_71GHz-Core

**Source:** Moderator (vivo) [RAN1]

**To:** TSG RAN WG2

**Cc:**

**Contact person:** Huaming Wu

huaming.wu@vivo.com

# 1 Overall description

In RAN1 #110, RAN1 reached the following agreements with RRC parameter impact

Agreement

Support the value range of *reportSlotOffsetList-r17*, *reportSlotOffsetListDCI-0-1-r17* and *reportSlotOffsetListDCI-0-2-r17* for 480kHz and 960kHz SCS to INTEGER (0..128).

* Send an LS to RAN2
* Endorse in draft CR in R1-2207965 and prepare the final CR

Agreement

Send an LS to RAN2 to request that 38.331 captures the following: If *duration-r17* is absent, the UE assumes the duration in slots is equal to L (where L is the configured length of the bitmap *monitoringSlotsWithinSlotGroup-r17*).

# 2 Actions

**To TSG RAN2**

**ACTION:** RAN1 respectfully asks RAN2 to consider the above agreement and capture it in RAN2 spec.

# 3 Dates of next TSG RAN WG1 meetings

TSG RAN WG1 Meeting #110-bis-e 10 - 19 October 2022 Online

TSG RAN WG1 Meeting #111 11 - 18 November 2022 Canada