**3GPP RAN WG2 Meeting #109-e R2-200xxxx**

**Feb. 24th – Mar. 6th, 2020**

**Title:** draft LS on CAPC selection for MsgA Payload

**Release:** Rel-16

**Work Item:** NR\_unlic-Core, NR\_2step\_RACH-Core

**Source:** [RAN2]

**To:** RAN1

**Contact Person:**

**Name:**

**E-mail Address:**

**Send any reply LS to:3GPP Liaisons Coordinator,****mailto:3GPPLiaison@etsi.org**

**1. Overall Description:**

Based on RAN1 agreement, separate LBTs can be used for preamble and the PUSCH payload of MsgA in 2-step RA. When separate LBTs are performed, the UE needs to select the CAPC for each transmission. RAN2 has agreed to the following:

CAPC selection for transmission of the PUSCH payload of MsgA follows the same mechanism defined for UL CG transmissions.

**2. Actions:**

**To RAN1 group.**

**ACTION:**RAN2 asks RAN1 to take the above agreement into account

**3. Date of Next TSG WG RAN2 Meetings:**

RAN-WG2 Meeting #109bis Sapporo, Japan 20-24 Apr, 2020

RAN-WG2 Meeting #110 Athens, Greece 25-29 May, 2020

RAN-WG2 Meeting #111 Toulouse, France 24-28 Aug, 2020