3GPP TSG-RAN WG2 Meeting #111-e draftR2-2008309

**17-28 August 2020, online**

**Source: Document Rapporteur (Ericsson)**

**Title: RAN2 agreements for Rel-17 additional enhancements for NB-IoT and LTE-MTC**

**Agenda Item: 9.1**

**Document for: Endorsement**

# 1 Introduction

This document lists RAN2 agreements made for Rel-17 “Additional enhancements for NB-IoT and LTE-M” work item (WI code NB\_IOTenh4\_LTE\_eMTC6; WID in [RP-201306](http://3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_88e/Docs/RP-201306.zip)), until and including the RAN2#111-e, 17-28 August 2020.

NOTE: Email agreements for CRs/specific topics are not listed in this document.

# 2 Additional enhancements for NB-IoT and LTE-MTC

## 2.1 Organizational

|  |
| --- |
| RAN2#111-e agreements:* Will maintain a document similar to the one used in R16 for capturing agreements.
* The endorsed report can be provided in R2-2008309.
* [Post111-e][350][NBIOT/eMTC R17] Capture the agreements (Ericsson)
	+ - Scope: Capture the agreements.
		- Intended outcome: endorsed report in R2-2008309
		- Deadline: Friday, 2020-09-04 13:00 UTC
 |

## 2.2 NB-IoT neighbour cell measurements and corresponding measurement triggering before RLF

|  |
| --- |
| RAN2#111-e agreements:* Study current RLF procedure to understand the time taken to select the cell for access. Start and end points FFS.
* Support neighbour cell measurements in RRC\_CONNECTED, at least for intra-frequency.
	+ - FFS inter-frequency
		- FFS whether measurements are done on the anchor carrier
		- FFS how neighbour cell measurement is triggered
		- FFS how to perform neighbour cell measurements
* Working assumption: Neighbour cell measurement results are not reported to the network in RRC\_CONNECTED.
	+ - FFS whether and when other information can be sent
 |

## 2.3 NB-IoT carrier selection based on the coverage level, and associated carrier specific configuration

|  |
| --- |
| RAN2#111-e agreements:* Paging carrier selection Improvements based on CE level is considered
* Paging carrier selection Improvements based on DRX cycle may be considered
	+ - whether DRX cycle is considered as part of CE level (Rmax) or can be also considered separately
* Enhancements for NPRACH Carrier selection carrier may be considered
* Paging carrier selection Improvements solely based on WUS or GWUS is not considered
* FFS service based
 |

|  |
| --- |
|  |

# 4 References: List of approved outgoing Rel-17 LSs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Tdoc** | **Meeting** | **Title** | **WI** | **To** | **Cc** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

# 5 References: Reports from the breakout session

|  |  |  |  |
| --- | --- | --- | --- |
| **Meeting** | **Date** | **Title** | **Tdoc** |
| RAN2#111-e, Online | 17-28 August 2020 | Report NB-IoT breakout session | R2-2008127 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# 6 Change history

|  |  |  |
| --- | --- | --- |
| **Tdoc** | **Title** | **Comment** |
| R2-2008309 | RAN2 agreements for Rel-17 additional enhancements for NB-IoT & LTE-MTC | Post RAN2#111-e  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |