3GPP TSG RAN WG2 #112e R2-20xxxxx

Electronic meeting, 2 – 13 November, 2020

Agenda Item: 8.14 NR QoE

Source: Ericsson

Title: Handling of RAN3 LS on QoE Measurement Collection

Document for: Discussion and Decision

# Introduction

This to handle offline discussion #038 related to incoming LS R2-2008728 [1].

# Discussion

## LS comments and reply

In the LS R2-2008728 the following is stated:

“RAN3 has discussed the transport of NR QoE reports and agreed that the NR QoE reports are carried over the control plane in the RAN.”

Rapporteur’s comment: It is the rapporteur’s understanding that this means that NR QoE reports are sent over an SRB via RRC signalling. It is also the rapporteur’s understanding that it is RAN2 who decides what is sent in RRC signalling. Therefore, this needs to be discussed in RAN2 also. At least the following options are possible:

1. Send QoE reports via a separate SRB4 as in LTE.
2. Send QoE reports on another SRB.
3. Send QoE reports over user plane (not inline with RAN3 agreement).
4. Cannot be decided now. Needs to be discussed in RAN2 based on contributions.
5. …

Q1: What is your preferred option?

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Summary and proposal

TBD

# References

1. R2-2008728, LS on Transport of NR QoE Reports in the RAN (R3-205785; contact: Ericsson) RAN3 LS in Rel-17 FS\_NR\_QoE To:RAN2