**3GPP TSG-RAN WG2 Meeting #113 Electronic R2-2102009**

**25 January – 05 February 2021**

**Title:** Reply LS on LS on restricting the rate per UE per network slice

**Response to:** -

**Release:** Release 17

**Work Item:** FS\_eNS\_Ph2

**Source:** RAN2

**To:** SA2

**Cc:** RAN3

**Contact Person:**

**Name:** György Wolfner

**E-mail Address:** gyorgy(dot)wolfner(at)nokia(dot)com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** -

**1. Overall Description:**

RAN2 thanks SA2 for the LS on restricting the rate per UE per network slice (S2-2007946/ R2-2010694). RAN2 would like to extend the feedback provided in R2-2011104 on Solution #22.

RAN2's view is that SMBR enforcement can be provided by configuring different resources per slice. A solution for support of the UL SMBR without different resources will require further study in RAN2.

**2. Actions:**

**To SA2 group.**

**ACTION:** RAN2 respectfully asks SA2 to take the above feedback into account.

**3. Date of Next TSG-RAN WG2 Meetings:**

3GPP RAN2#113bis-e from 2021-04-12 to 2021-04-20 Electronic Meeting

3GPP RAN2#114-e from 2021-05-19 to 2021-05-27 Electronic Meeting