**3GPP TSG-RAN WG2 Meeting #114-e draftR2-2106537**

**Electronic meeting, 2021-05-19 – 2021-05-27**

**Title: draft** LS on lower bound for eDRX cycle length

**Response to:** -

**Release:** Release 17

**Work Item:** NR\_redcap-Core

**Source:** Ericsson [to be: RAN2]

**To:** SA2, CT1

**Cc:** RAN3

**Contact Person:**

#### Name: Tuomas Tirronen

E-mail Address: tuomas dot tirronen at ericsson dot com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**1. Overall Description:**

|  |
| --- |
|  |

RAN2 would like to inform SA2 and CT1 that RAN2 has agreed 2.56 seconds as lower bound for eDRX cycle length for RRC\_IDLE and RRC\_INACTIVE for RedCap. RAN2 would like SA2 and CT1 to take the above agreement into consideration in their work and inform RAN2 if there is any concern.

**2. Actions:**

**To SA2 and CT1 groups:**

**ACTION:** RAN2 respectfully requests SA2 and CT1 to take the RAN2 agreement on lower bound for eDRX cycle length into account in their work and inform RAN2 if there is any concern.

**3. Date of Next RAN2 Meetings:**

3GPP RAN2#115-e 16th – 27th August 2021 Electronic Meeting

3GPP RAN2#116-e 1st – 12th November 2021 Electronic Meeting