**3GPP TSG-RAN WG3 Meeting #120 R3-23xxxx**

**Incheon, Korea, May 22 – 26, 2023**

Title: [draft]LS on cell ID configuration for mobile IAB cell

Response to:

Release: Rel-18

Work Item: NR\_mobile\_IAB

Source: ZTE [to be: RAN3]

To: SA5

Cc:

**Contact Person:**

Name: Ying Huang

E-mail Address: huang.ying11@zte.com.cn

**Send any reply LS to:** 3GPP Liaisons Coordinator, **<mailto:3GPPLiaison@etsi.org>**

Attachments: None

1. **Overall Description:**

RAN3 discussed how to configure the cell ID for mobile IAB cells and the following agreements have been achieved:

**The mIAB-DU’s cell ID is configured by OAM, and it may be reconfigured by the donor CU via F1 based on a list of NCGIs that has been configured on this donor CU by OAM or by preconfiguration. This should not affect the existing procedure of configuring NCGI of cells served by a stationary DU via OAM.**

**2. Actions:**

**To SA5 group.**

**ACTION:** RAN3 asks SA5 to take the above RAN3 agreement into account and provide feedback, if any.

**3. Date of Next RAN3 Meetings:**

TSG-RAN3 Meeting #121 – August 21 to 25, 2023 Toulouse, France

TSG-RAN3 Meeting #121bis – Oct 9 to 13, 2023 Xiamen, China