{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PUCCH Format 2 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #111",null,null,null,null,null,null,null,"R4-2407128"]
[null,"Fukuoka, Japan, May, 2024"]
[]
[null,"Source: Nokia"]
[null,"Title: Simulation Summary for Less Than 5 MHz BS Demod"]
[null,"Agenda: 7.16.8.2"]
[null,"Document for: Information"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUCCH Format 2 1T2R","index":2,"n_rows":11,"n_cols":25,"rows_kept":11,"cut":false,"hidden":false,"merged":[[4,21,4,22],[4,23,4,24],[8,0,9,4],[8,5,9,5],[8,6,9,6],[8,7,8,8],[8,9,8,10],[8,11,8,12],[8,13,8,14],[8,15,8,16],[8,17,8,18],[8,19,8,20],[8,21,8,22],[8,23,8,24],[4,11,4,12],[4,13,4,14],[4,15,4,16],[4,17,4,18],[4,19,4,20],[4,0,5,4],[4,5,5,5],[4,6,5,6],[4,7,4,8],[4,9,4,10],[0,23,0,24],[0,0,1,4],[0,5,1,5],[0,6,1,6],[0,7,0,8],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22]]}
["  FR1 PUCCH Format 2 1T2R",null,null,null,null,"38.104 req","38.141 req","Nokia",null,"ZTE",null,"Ericsson",null,"Samsung",null,"Huawei",null,"Company F",null,"Company G",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["15 kHz SCS","9 PRB","2 OFDM Symbols","22 bit UCI","TDLC 300-100",{"$f":"DerivingPerfReq(H3:Y3)","v":1.5},{"$f":"IF(F3>-100,F3+0.6,F3)","v":2.1},-1.22,0.48,-0.4,2.1,0.41,2.5299999999999998,0.23,2.23,-1.1599999999999999,0.34,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,T3,P3,R3)-MIN(H3,J3,L3,N3,T3,P3,R3)","v":1.63},{"$f":"MAX(I3,K3,M3,O3,U3,Q3,S3)-MIN(I3,K3,M3,O3,U3,Q3,S3)","v":2.19},{"$f":"AVERAGE(H3,J3,L3,N3,T3,P3,R3)","v":-0.42800000000000005},{"$f":"AVERAGE(I3,K3,M3,O3,U3,Q3,S3)","v":1.536}]
[]
["  FR1 PUCCH Format 2 1T4R",null,null,null,null,"38.104 req","38.141 req","Nokia",null,"ZTE",null,"Ericsson",null,"Samsung",null,"Huawei",null,"Company F",null,"Company G",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["15 kHz SCS","9 PRB","2 OFDM Symbols","22 bit UCI","TDLC 300-100",{"$f":"DerivingPerfReq(H7:Y7)","v":-3.2},{"$f":"IF(F7>-100,F7+0.6,F7)","v":-2.6},-6.16,-4.46,-5.0999999999999996,-2.6,-4.55,-2.35,-4.38,-2.38,-5.85,-4.3499999999999996,null,null,null,null,{"$f":"MAX(H7,J7,L7,N7,T7,P7,R7)-MIN(H7,J7,L7,N7,T7,P7,R7)","v":1.7800000000000002},{"$f":"MAX(I7,K7,M7,O7,U7,Q7,S7)-MIN(I7,K7,M7,O7,U7,Q7,S7)","v":2.11},{"$f":"AVERAGE(H7,J7,L7,N7,T7,P7,R7)","v":-5.2080000000000002},{"$f":"AVERAGE(I7,K7,M7,O7,U7,Q7,S7)","v":-3.2280000000000002}]
[]
["  FR1 PUCCH Format 2 1T8R",null,null,null,null,"38.104 req","38.141 req","Nokia",null,"ZTE",null,"Ericsson",null,"Samsung",null,"Huawei",null,"Company F",null,"Company G",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["15 kHz SCS","9 PRB","2 OFDM Symbols","22 bit UCI","TDLC 300-100",{"$f":"DerivingPerfReq(H11:Y11)","v":-6.8},{"$f":"IF(F11>-100,F11+0.6,F11)","v":-6.2},-9.81,-8.11,-8.6999999999999993,-6.2,-8.11,-5.81,-7.97,-5.97,-9.5299999999999994,-8.0299999999999994,null,null,null,null,{"$f":"MAX(H11,J11,L11,N11,T11,P11,R11)-MIN(H11,J11,L11,N11,T11,P11,R11)","v":1.8400000000000007},{"$f":"MAX(I11,K11,M11,O11,U11,Q11,S11)-MIN(I11,K11,M11,O11,U11,Q11,S11)","v":2.2999999999999998},{"$f":"AVERAGE(H11,J11,L11,N11,T11,P11,R11)","v":-8.8239999999999998},{"$f":"AVERAGE(I11,K11,M11,O11,U11,Q11,S11)","v":-6.8239999999999998}]