{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Parameters","PRACH FR1 1T2R","PRACH FR2-1 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #111",null,null,null,null,null,null,null,"R4-2407109"]
[null,"Fukuoka City, JP, May 20-24, 2024"]
[]
[null,"Source: China Telecom"]
[null,"Title: Summary of simulation results for Rel-18 NR coverage enhancements BS demodulation requirements"]
[null,"Agenda: 7.17.2"]
[]
[null,"Reference: R4-2406137 WF on NR_cov_enh2_demod, China Telecom"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PRACH FR1 1T2R","index":2,"n_rows":27,"n_cols":25,"rows_kept":27,"cut":false,"hidden":false,"merged":[[0,21,0,22],[0,23,0,24],[0,0,1,1],[0,2,1,2],[0,3,1,3],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,7,0,8],[0,5,1,5],[0,6,1,6],[0,4,1,4],[2,1,6,1],[3,2,6,2],[3,3,6,3],[2,0,10,0],[7,1,10,1],[8,2,10,2],[8,3,10,3],[24,3,26,3],[19,3,22,3],[12,3,14,3],[16,3,17,3],[11,0,17,0],[11,1,14,1],[15,1,17,1],[12,2,14,2],[16,2,17,2],[18,0,26,0],[18,1,22,1],[23,1,26,1],[24,2,26,2],[19,2,22,2]]}
[" PRACH FR1 1T2R",null,"Propagation condition","Frequency offset (Hz)","Repetition Interval","38.104 req","38.141 req","Nokia (R4-2407140)",null,"Ericsson (R4-2408346)",null,"Huawei (R4-2408957)",null,"ZTE (R4-2409082)",null,"Samsung (R4-2409475)",null,"Company 6",null,"Company 7",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","15kHz","AWGN",0,"N/A",{"$f":"DerivingPerfReq(H3:U3)","v":-100},{"$f":"IF(F3>-100,F3+0.3,F3)","v":-100},-18.8,-16.3,null,null,-17.3,null,-18.5,null,-16.850000000000001,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3)-MIN(H3,J3,L3,N3,P3,R3,T3)","v":1.9499999999999993},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3)-MIN(I3,K3,M3,O3,Q3,S3,U3)","v":0},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3)","v":-17.862500000000001},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3)","v":-16.3}]
[null,null,"TDLC300-100 Low",400,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H4:U4)","v":-100},{"$f":"IF(F4>-100,F4+0.6,F4)","v":-100},null,null,null,null,-9.1999999999999993,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H4,J4,L4,N4,P4,R4,T4)-MIN(H4,J4,L4,N4,P4,R4,T4)","v":0},{"$f":"MAX(I4,K4,M4,O4,Q4,S4,U4)-MIN(I4,K4,M4,O4,Q4,S4,U4)","v":0},{"$f":"AVERAGE(H4,J4,L4,N4,P4,R4,T4)","v":-9.1999999999999993},{"$f":"AVERAGE(I4,K4,M4,O4,Q4,S4,U4)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"1 slot",-100,{"$f":"IF(F5>-100,F5+0.6,F5)","v":-100},null,null,-10.69,null,null,null,null,null,null,null,null,null,null,null,0,0,-10.69,{"$error":"#DIV/0!"}]
[null,null,null,null,"5 slots",{"$f":"DerivingPerfReq(H6:U6)","v":-100},{"$f":"IF(F6>-100,F6+0.6,F6)","v":-100},null,null,-12.18,null,-10.6,null,-11.1,null,null,null,null,null,null,null,{"$f":"MAX(H6,J6,L6,N6,P6,R6,T6)-MIN(H6,J6,L6,N6,P6,R6,T6)","v":1.58},{"$f":"MAX(I6,K6,M6,O6,Q6,S6,U6)-MIN(I6,K6,M6,O6,Q6,S6,U6)","v":0},{"$f":"AVERAGE(H6,J6,L6,N6,P6,R6,T6)","v":-11.293333333333335},{"$f":"AVERAGE(I6,K6,M6,O6,Q6,S6,U6)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"10ms",{"$f":"DerivingPerfReq(H7:U7)","v":-100},{"$f":"IF(F7>-100,F7+0.6,F7)","v":-100},null,null,-12.64,null,-11,null,-11.2,null,-10.54,null,null,null,null,null,{"$f":"MAX(H7,J7,L7,N7,P7,R7,T7)-MIN(H7,J7,L7,N7,P7,R7,T7)","v":2.1000000000000014},{"$f":"MAX(I7,K7,M7,O7,Q7,S7,U7)-MIN(I7,K7,M7,O7,Q7,S7,U7)","v":0},{"$f":"AVERAGE(H7,J7,L7,N7,P7,R7,T7)","v":-11.345000000000001},{"$f":"AVERAGE(I7,K7,M7,O7,Q7,S7,U7)","v":{"$error":"#DIV/0!"}}]
[null,"30kHz","AWGN",0,"N/A",-100,{"$f":"IF(F8>-100,F8+0.3,F8)","v":-100},-18.8,-16.3,null,null,-17.7,null,-18.5,null,-16.78,null,null,null,null,null,2.0199999999999996,0,-17.945,-16.3]
[null,null,"TDLC300-100 Low",400,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H9:U9)","v":-100},{"$f":"IF(F9>-100,F9+0.6,F9)","v":-100},null,null,null,null,-9.5,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H9,J9,L9,N9,P9,R9,T9)-MIN(H9,J9,L9,N9,P9,R9,T9)","v":0},{"$f":"MAX(I9,K9,M9,O9,Q9,S9,U9)-MIN(I9,K9,M9,O9,Q9,S9,U9)","v":0},{"$f":"AVERAGE(H9,J9,L9,N9,P9,R9,T9)","v":-9.5},{"$f":"AVERAGE(I9,K9,M9,O9,Q9,S9,U9)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"1 slot",-100,-100,null,null,-11.24,null,null,null,-12.9,null,null,null,null,null,null,null,1.6600000000000001,0,-12.07,{"$error":"#DIV/0!"}]
[null,null,null,null,"10ms",-100,{"$f":"IF(F11>-100,F11+0.6,F11)","v":-100},null,null,-12.83,null,-10.4,null,-11.5,null,-12.11,null,null,null,null,null,2.4299999999999997,0,-11.71,{"$error":"#DIV/0!"}]
["Format B4","15kHz","AWGN",0,"N/A",-100,{"$f":"IF(F12>-100,F12+0.3,F12)","v":-100},-23.5,-21,null,null,-20.2,null,-21.7,null,-21.62,null,null,null,null,null,3.3000000000000007,0,-21.755000000000003,-21]
[null,null,"TDLC300-100 Low",400,"1 slot",{"$f":"DerivingPerfReq(H13:U13)","v":-100},{"$f":"IF(F13>-100,F13+0.6,F13)","v":-100},null,null,-14.95,null,-13.7,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H13,J13,L13,N13,P13,R13,T13)-MIN(H13,J13,L13,N13,P13,R13,T13)","v":1.25},{"$f":"MAX(I13,K13,M13,O13,Q13,S13,U13)-MIN(I13,K13,M13,O13,Q13,S13,U13)","v":0},{"$f":"AVERAGE(H13,J13,L13,N13,P13,R13,T13)","v":-14.324999999999999},{"$f":"AVERAGE(I13,K13,M13,O13,Q13,S13,U13)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"5 slots",-100,-100,null,null,-15.43,null,-13.3,null,-13,null,null,null,null,null,null,null,2.4299999999999997,0,-13.910000000000002,{"$error":"#DIV/0!"}]
[null,null,null,null,"10ms",-100,{"$f":"IF(F15>-100,F15+0.6,F15)","v":-100},null,null,-15.72,null,-13.8,null,-14.7,null,-15.32,null,null,null,null,null,1.92,0,-14.885,{"$error":"#DIV/0!"}]
[null,"30kHz","AWGN",0,"N/A",-100,{"$f":"IF(F16>-100,F16+0.3,F16)","v":-100},-23.5,-21,null,null,-20.399999999999999,null,-21.7,null,-21.43,null,null,null,null,null,3.1000000000000014,0,-21.7575,-21]
[null,null,"TDLC300-100 Low",400,"1 slot",{"$f":"DerivingPerfReq(H17:U17)","v":-100},{"$f":"IF(F17>-100,F17+0.6,F17)","v":-100},null,null,-15.66,null,-11.9,null,-17.100000000000001,null,null,null,null,null,null,null,{"$f":"MAX(H17,J17,L17,N17,P17,R17,T17)-MIN(H17,J17,L17,N17,P17,R17,T17)","v":5.2000000000000011},{"$f":"MAX(I17,K17,M17,O17,Q17,S17,U17)-MIN(I17,K17,M17,O17,Q17,S17,U17)","v":0},{"$f":"AVERAGE(H17,J17,L17,N17,P17,R17,T17)","v":-14.886666666666668},{"$f":"AVERAGE(I17,K17,M17,O17,Q17,S17,U17)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"10ms",-100,{"$f":"IF(F18>-100,F18+0.6,F18)","v":-100},null,null,-17.079999999999998,null,-13.2,null,-16,null,-16.579999999999998,null,null,null,null,null,3.879999999999999,0,-15.715,{"$error":"#DIV/0!"}]
["Format C2","15kHz","AWGN",0,"N/A",-100,{"$f":"IF(F19>-100,F19+0.3,F19)","v":-100},-18.8,-16.3,null,null,-17.3,null,-18.600000000000001,null,-16.8,null,null,null,null,null,2,0,-17.875,-16.3]
[null,null,"TDLC300-100 Low",400,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H20:U20)","v":-100},{"$f":"IF(F20>-100,F20+0.6,F20)","v":-100},null,null,null,null,-9.1,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H20,J20,L20,N20,P20,R20,T20)-MIN(H20,J20,L20,N20,P20,R20,T20)","v":0},{"$f":"MAX(I20,K20,M20,O20,Q20,S20,U20)-MIN(I20,K20,M20,O20,Q20,S20,U20)","v":0},{"$f":"AVERAGE(H20,J20,L20,N20,P20,R20,T20)","v":-9.1},{"$f":"AVERAGE(I20,K20,M20,O20,Q20,S20,U20)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"1 slot",-100,{"$f":"IF(F21>-100,F21+0.6,F21)","v":-100},null,null,-10.63,null,null,null,null,null,null,null,null,null,null,null,0,0,-10.63,{"$error":"#DIV/0!"}]
[null,null,null,null,"5 slots",{"$f":"DerivingPerfReq(H22:U22)","v":-100},{"$f":"IF(F22>-100,F22+0.6,F22)","v":-100},null,null,-11.98,null,-10.6,null,-11.2,null,null,null,null,null,null,null,{"$f":"MAX(H22,J22,L22,N22,P22,R22,T22)-MIN(H22,J22,L22,N22,P22,R22,T22)","v":1.3800000000000008},{"$f":"MAX(I22,K22,M22,O22,Q22,S22,U22)-MIN(I22,K22,M22,O22,Q22,S22,U22)","v":0},{"$f":"AVERAGE(H22,J22,L22,N22,P22,R22,T22)","v":-11.26},{"$f":"AVERAGE(I22,K22,M22,O22,Q22,S22,U22)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"10ms",-100,{"$f":"IF(F23>-100,F23+0.6,F23)","v":-100},null,null,-12.26,null,-11,null,-11.3,null,-10.67,null,null,null,null,null,1.5899999999999999,0,-11.307500000000001,{"$error":"#DIV/0!"}]
[null,"30kHz","AWGN",0,"N/A",-100,{"$f":"IF(F24>-100,F24+0.3,F24)","v":-100},-18.8,-16.3,null,null,-17.7,null,-18.600000000000001,null,-16.690000000000001,null,null,null,null,null,2.1099999999999994,0,-17.947500000000002,-16.3]
[null,null,"TDLC300-100 Low",400,"Repetition within 1 slot",-100,{"$f":"IF(F25>-100,F25+0.6,F25)","v":-100},null,null,null,null,-9.4,null,null,null,null,null,null,null,null,null,0,0,-9.4,{"$error":"#DIV/0!"}]
[null,null,null,null,"1 slot",{"$f":"DerivingPerfReq(H26:U26)","v":-100},{"$f":"IF(F26>-100,F26+0.6,F26)","v":-100},null,null,-10.84,null,null,null,-12.7,null,null,null,null,null,null,null,{"$f":"MAX(H26,J26,L26,N26,P26,R26,T26)-MIN(H26,J26,L26,N26,P26,R26,T26)","v":1.8599999999999994},{"$f":"MAX(I26,K26,M26,O26,Q26,S26,U26)-MIN(I26,K26,M26,O26,Q26,S26,U26)","v":0},{"$f":"AVERAGE(H26,J26,L26,N26,P26,R26,T26)","v":-11.77},{"$f":"AVERAGE(I26,K26,M26,O26,Q26,S26,U26)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"10ms",-100,{"$f":"IF(F27>-100,F27+0.6,F27)","v":-100},null,null,-12.96,null,-10.5,null,-11.5,null,-12.3,null,null,null,null,null,2.4600000000000009,0,-11.815000000000001,{"$error":"#DIV/0!"}]

{"sheet":"PRACH FR2-1 1T2R","index":3,"n_rows":19,"n_cols":25,"rows_kept":19,"cut":false,"hidden":false,"merged":[[2,0,7,0],[8,0,12,0],[13,0,18,0],[2,1,18,1],[0,0,1,1],[0,2,1,2],[0,3,1,3],[0,5,1,5],[0,6,1,6],[0,4,1,4],[0,7,0,8],[0,21,0,22],[0,23,0,24],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[3,2,7,2],[9,2,12,2],[14,2,18,2],[3,3,7,3],[9,3,12,3],[14,3,18,3]]}
[" PRACH FR2-1 1T2R",null,"Propagation condition","Frequency offset (Hz)","Repetition Interval","38.104 req","38.141 req","Nokia (R4-2407140)",null,"Ericsson (R4-2408346)",null,"Huawei (R4-2408957)",null,"ZTE (R4-2409082)",null,"Samsung (R4-2409475)",null,"Company 6",null,"Company 7",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","120kHz","AWGN",0,"N/A",{"$f":"DerivingPerfReq(H3:U3)","v":-100},{"$f":"IF(F3>-100,F3+0.3,F3)","v":-100},-18.8,-16.100000000000001,null,null,-17.3,null,-18.600000000000001,null,-16.7,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3)-MIN(H3,J3,L3,N3,P3,R3,T3)","v":2.1000000000000014},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3)-MIN(I3,K3,M3,O3,Q3,S3,U3)","v":0},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3)","v":-17.850000000000001},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3)","v":-16.100000000000001}]
[null,null,"TDLA30-300 Low",4000,"Repetition within 1 slot",-100,{"$f":"IF(F4>-100,F4+0.6,F4)","v":-100},null,null,null,null,-9.1999999999999993,null,null,null,null,null,null,null,null,null,0,0,-9.1999999999999993,{"$error":"#DIV/0!"}]
[null,null,null,null,"1 slot",-100,-100,null,null,-11.02,null,null,null,null,null,null,null,null,null,null,null,0,0,-11.02,{"$error":"#DIV/0!"}]
[null,null,null,null,"5 slots",{"$f":"DerivingPerfReq(H6:U6)","v":-100},{"$f":"IF(F6>-100,F6+0.6,F6)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H6,J6,L6,N6,P6,R6,T6)-MIN(H6,J6,L6,N6,P6,R6,T6)","v":0},{"$f":"MAX(I6,K6,M6,O6,Q6,S6,U6)-MIN(I6,K6,M6,O6,Q6,S6,U6)","v":0},{"$f":"AVERAGE(H6,J6,L6,N6,P6,R6,T6)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(I6,K6,M6,O6,Q6,S6,U6)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"10 slots",-100,-100,null,null,-11.64,null,null,null,-11.2,null,null,null,null,null,null,null,0.44000000000000128,0,-11.42,{"$error":"#DIV/0!"}]
[null,null,null,null,"10ms",{"$f":"DerivingPerfReq(H8:U8)","v":-100},{"$f":"IF(F8>-100,F8+0.6,F8)","v":-100},null,null,null,null,null,null,-11.7,null,-11.81,null,null,null,null,null,{"$f":"MAX(H8,J8,L8,N8,P8,R8,T8)-MIN(H8,J8,L8,N8,P8,R8,T8)","v":0.11000000000000121},{"$f":"MAX(I8,K8,M8,O8,Q8,S8,U8)-MIN(I8,K8,M8,O8,Q8,S8,U8)","v":0},{"$f":"AVERAGE(H8,J8,L8,N8,P8,R8,T8)","v":-11.754999999999999},{"$f":"AVERAGE(I8,K8,M8,O8,Q8,S8,U8)","v":{"$error":"#DIV/0!"}}]
["Format B4",null,"AWGN",0,"N/A",-100,{"$f":"IF(F9>-100,F9+0.3,F9)","v":-100},-23.5,-20.8,null,null,-19.5,null,-21.7,null,-20.9,null,null,null,null,null,4,0,-21.4,-20.8]
[null,null,"TDLA30-300 Low",4000,"1 slot",-100,{"$f":"IF(F10>-100,F10+0.6,F10)","v":-100},null,null,-13.13,null,null,null,null,null,null,null,null,null,null,null,0,0,-13.13,{"$error":"#DIV/0!"}]
[null,null,null,null,"5 slots",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"10 slots",-100,-100,null,null,-14.97,null,-11.2,null,-14,null,null,null,null,null,null,null,3.7700000000000014,0,-13.39,{"$error":"#DIV/0!"}]
[null,null,null,null,"10ms",-100,-100,null,null,null,null,null,null,-14.3,null,-15.45,null,null,null,null,null,1.1499999999999986,0,-14.875,{"$error":"#DIV/0!"}]
["Format C2",null,"AWGN",0,"N/A",-100,{"$f":"IF(F14>-100,F14+0.3,F14)","v":-100},-18.8,-16.100000000000001,null,null,-17.399999999999999,null,-18.600000000000001,null,-16.61,null,null,null,null,null,2.1900000000000013,0,-17.852499999999999,-16.100000000000001]
[null,null,"TDLA30-300 Low",4000,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H15:U15)","v":-100},{"$f":"IF(F15>-100,F15+0.6,F15)","v":-100},null,null,null,null,-9.1999999999999993,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H15,J15,L15,N15,P15,R15,T15)-MIN(H15,J15,L15,N15,P15,R15,T15)","v":0},{"$f":"MAX(I15,K15,M15,O15,Q15,S15,U15)-MIN(I15,K15,M15,O15,Q15,S15,U15)","v":0},{"$f":"AVERAGE(H15,J15,L15,N15,P15,R15,T15)","v":-9.1999999999999993},{"$f":"AVERAGE(I15,K15,M15,O15,Q15,S15,U15)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,"1 slot",-100,-100,null,null,-10.59,null,null,null,null,null,null,null,null,null,null,null,0,0,-10.59,{"$error":"#DIV/0!"}]
[null,null,null,null,"5 slots",-100,-100,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,"10 slots",-100,-100,null,null,-11.86,null,-8.6,null,-11.2,null,null,null,null,null,null,null,3.26,0,-10.553333333333333,{"$error":"#DIV/0!"}]
[null,null,null,null,"10ms",-100,-100,null,null,null,null,null,null,-11.7,null,-11.69,null,null,null,null,null,9.9999999999997868E-3,0,-11.695,{"$error":"#DIV/0!"}]