**3GPP SA WG2 Meeting #165 S2-2409910**

**Hyderabad, India, 14-18 October 2024**

Title: [Draft] Reply LS on Binding Information

Response to: Reply LS on Binding Information (S4-241671/S2-2409607)

Release: Release 18

Work Item: NG\_RTC

Source: SA2

To: SA4

Cc: -

**Contact Person:**

Name: Kefeng Zhang

Tel. Number:

E-mail Address: kefezhan AT qti DOT qualcomm DOT com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

Attachments: S2-240XXXX

**1. Overall Description:**

SA2 would like to thank SA4 for the Reply LS on Binding information in [S4-241671/S2-2409607].

SA2 would like to ask for further clarification above the following text:

Therefore, while it is not in any way ruled out, letting a local UE choose an application from a remote UE’s list should be avoided, or at least made with great care to limit the risk of choice mismatch or collision. Instead, it should be a preferable principle to let a local UE choose from its local list and the remote UE can be informed about the chosen application together with a choice to accept or reject that. That principle can be mirrored such that both UEs gets to make a choice in a single session, but that would result in both UEs having two simultaneously active applications in the session, one that was chosen by UE#1 and one that was chosen by UE#2.

**Q1:** SA2 assumes that the above preferable principle is applicable to person-to-person DC sessions. However, if the user calls to a DC-enabled business number, it should be possible for the user to use the applications provided by the business, i.e. from the user's remote network. Is this understanding correct?

**Q2:** SA2 assumes that the above preferable principle is applicable to person-to-person DC sessions when any given DCSF connect to both UE using a pair of bootstrap data channel. However, if the given DCSF only connect to one UE instead of two UE through BDC, e.g. one UE support DC and the other does not, it should be possible for the UE which connected to the DCSF to download application, regardless whether it is local or remote UE. Is this understanding correct?

**2. Actions:**

**To SA WG4:**

**ACTION:** SA WG2 respectfully asks SA WG4 to provide feedback on the question above.

**3. Date of Next TSG SA WG2 Meetings:**

TSG-SA2 Meeting #166 18-22 November 2024 Orlando, FL, USA

TSG-SA2 Meeting #AH 24-28 January 2025 Electronic meeting