**3GPP TSG-CT WG1 Meeting #128-eC1-21xxxx**

**Electronic meeting; 25 February – 5 March 2021 Revision of C1-210692**

**Source: China Mobile**

**Title: Update Solution 3 and Abbreviations**

**Spec:** **3GPP TR 23.700-10 v0.3.0**

**Agenda item: 17.3.3**

**Document for: Agreement**

**1. Introduction**

This pCR proposes to update Solution 3 and the abbreviations according to the comments on C1-210401.

**2. Reason for Change**

1.A NOTE needs to be added to subclause 6.3.2 to mention that the impact to PCF is expected but in CT3 responsibility.

2. Some abbreviations need to be added.

**3. Proposal**

It is proposed to agree the following changes to 3GPP TR 23.700-10 v0.3.0.

\* \* \* First Change \* \* \* \*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.502: "Procedures for the 5G System".

[x] 3GPP TR 23.700-11: "Study on enhanced IP Multimedia Subsystem (IMS) to 5GC integration Phase 2; CT WG3 aspects".

\* \* \* Next Change \* \* \* \*

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

DNN Data Network Name

IMPI IM Private Identity

ISIM IM Services Identity Module

MCC Mobile Country Code

MNC Mobile Network Code

NSSAI Network Slice Selection Assistance Information

S-NSSAI Single NSSAI

SUPI Subscription Permanent Identifier

URSP UE Route Selection Policy

USIM Universal Subscriber Identity Module

\* \* \* Next Change \* \* \* \*

### 6.3.2 Impacts on existing nodes and functions

The PCF and the UE need to support the extended URSP in the case#2.

NOTE: For impacts on PCF, see TR 23.700-11[x].