**TSG-CT WG3 Meeting #108-e *C3-201370***

**E-Meeting, 19th – 28th February 2020 (Revision of C3-201292)**

**Source: Huawei**

**Title: Pseudo-CR on OpenAPI file for Nnef\_EventExposure API**

**Spec: 3GPP TS 29.591 0.3.0**

**Agenda item: 16.5, 16.14**

**Document for: Agreement**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

The OpenAPI file for Nnef\_EventExposure API is still missed.

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.591 0.3.0.

\* \* \* First Change \* \* \* \*

## A.2 Nnef\_EventExposure API

openapi: 3.0.0

info:

 title: Nnef\_EventExposure

 version: 1.0.0.alpha-1

 description: |

 NEF Event Exposure Service.

 © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.591 V0.4.0; 5G System; Application Function (AF) event exposure service; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.591/

servers:

 - url: '{apiRoot}/nnef-eventexposure/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - nnef-eventexposure

paths:

 /subscriptions:

 post:

 summary: subscribe to notifications

 operationId: CreateIndividualSubcription

 tags:

 - Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NefEventExposureSubsc'

 responses:

 '201':

 description: Success

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NefEventExposureSubsc'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnef-eventexposure/{apiVersion}/subscriptions/{subscriptionId}'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NefEventExposureNotif'

 responses:

 '204':

 description: No Content, Notification was succesfull

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 get:

 summary: retrieve subscription

 operationId: GetIndividualSubcription

 tags:

 - IndividualSubscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NefEventExposureSubsc'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: update subscription

 operationId: ReplaceIndividualSubcription

 tags:

 - IndividualSubscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NefEventExposureSubsc'

 parameters:

 - name: subscriptionId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource was succesfully modified and representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NefEventExposureSubsc'

 '204':

 description: No Content. Resource was succesfully modified

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: unsubscribe from notifications

 operationId: DeleteIndividualSubcription

 tags:

 - IndividualSubscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was succesfully deleted

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnef-eventexposure: Access to the Nnef\_EventExposure API

 schemas:

 NefEventExposureSubsc:

 type: object

 properties:

 eventsSubs:

 type: array

 items:

 $ref: '#/components/schemas/NefEventSubs'

 minItems: 1

 eventsRepInfo:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AnalyticsReportingRequirement'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 notifId:

 type: string

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 rspNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - notifId

 - notifUri

 - suppFeat

 NefEventExposureNotif:

 type: object

 properties:

 notifId:

 type: string

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/NefEventNotification'

 minItems: 1

 required:

 - notifId

 - eventNotifs

 NefEventNotification:

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NefEvent'

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 svcExprcInfos:

 type: array

 items:

 $ref: '#/components/schemas/ServiceExperienceInfo'

 minItems: 1

 ueMobilityInfos:

 type: array

 items:

 $ref: '#/components/schemas/UeMobilityInfo'

 minItems: 1

 ueCommInfos:

 type: array

 items:

 $ref: '#/components/schemas/UeCommunicationInfo'

 minItems: 1

 excepInfos:

 type: array

 items:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/ExceptionInfo'

 minItems: 1

 required:

 - event

 - timeStamp

 NefEventSubs:

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NefEvent'

 eventFilter:

 $ref: '#/components/schemas/NefEventFilter'

 required:

 - event

 NefEventFilter:

 type: object

 properties:

 tgtUe:

 $ref: '#/components/schemas/TargetUeIdentification'

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 locArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 required:

 - tgtUe

 TargetUeIdentification:

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 interGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 anyUeId:

 type: boolean

 ServiceExperienceInfo:

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 svcExpPerFlows:

 type: array

 items:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/ServiceExperienceInfoPerFlow'

 minItems: 1

 required:

 - svcExpPerFlows

 UeMobilityInfo:

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ueTrajs:

 type: array

 items:

 $ref: '#/components/schemas/UeTrajectoryInfo'

 minItems: 1

 required:

 - supi

 - ueTrajs

 UeCommunicationInfo:

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 comms:

 type: array

 items:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/CommunicationCollection'

 minItems: 1

 required:

 - comms

 UeTrajectoryInfo:

 type: object

 properties:

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 location:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 required:

 - ts

 - location

# Simple data types and Enumerations

 NefEvent:

 anyOf:

 - type: string

 enum:

 - SVC\_EXPERIENCE

 - UE\_MOBILITY

 - UE\_COMM

 - EXCEPTIONS

 - type: string

\* \* \* End of Changes \* \* \* \*