**3GPP TSG-CT3 Meeting #117e C3-214189\_r1**

**E-Meeting, 18th – 27th August 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.513** | **CR** | **0280** | **rev** | **1** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction to abbreviations for TSC | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | IIoT | | | | |  | ***Date:*** | | | 2021-8-10 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature)* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Abbreviation TSN defined in 3.2 is not referred in this specification, instead, TSC and TSCAI are referred but missing in 3.2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | In Clause 3.2,  -remove abbreviation TSN  -add abbreviations for TSC and TSCAI | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Unused abbreviation is defined but used abbreviations are not. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core Network

5QI 5G QoS Identifier

5G VN 5G Virtual Network

AF Application Function

AMBR Aggregate Maximum Bit Rate

AMF Access and Mobility Management Function

ARP Allocation and Retention Priority

AW Average Window

BDT Background Data Transfer

BSF Binding Support Function

CHEM Coverage and Handoff Enhancements using Multimedia error robustness feature

CHF Charging Function

DN-AAA Data Network Authentication, Authorization and Accounting

DTS Data Transport Service

LBO Local Breakout

MBR Maximum Bitrate

MCS Mission Critical Service

MPD Media Presentation Description

MPS Multimedia Priority Service

NEF Network Exposure Function

NPLI Network Provided Location Information

NRF Network Repository Function

NSSAI Network Slice Selection Assistance Information

NWDAF Network Data Analytics Function

PCC Policy and Charging Control

PCF Policy Control Function

PDB Packet Delay Budget

PER Packet Error Rate

PFD Packet Flow Description

PFDF Packet Flow Description Function

PMIC Port Management Information Container

PL Priority Level

PSAP Public Safety Access Point

P-CSCF Proxy Call Session Control Function

QNC QoS Notification Control

QoS Quality of Service

SCP Service Communication Proxy

SDP Session Description Protocol

SEPP Security Edge Protection Proxy

SMF Session Management Function

S-NSSAI Single Network Slice Selection Assistance Information

TSC Time Sensitive Communication

TSCAI Time Sensitive Communication Assistance Information

TSN Time Sensitive Networking

UDR Unified Data Repository

UMIC User plane node Management Information Container

UPF User Plane Function

UPSI UE policy section identifier

URSP UE Route Selection Policy

\*\*\* End of Changes \*\*\*